{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["数据"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"数据","index":0,"n_rows":1100,"n_cols":24,"rows_kept":1100,"flags":["formulas_cached_only"]}
["机具大类","机具小类","机具品目","分档名称","生产企业","产品名称","机具型号","产品投档技术参数","产品配置参数","中央补贴额","证书编号","有效期截止日期\r\n","销售价格（元）","功率（kW）","机具类型","企业所属省份","产品状态","评阅结果","评阅意见","备注","翻倾防护装置强度检验报告编号","翻倾防护装置强度检验报告检测机构","可靠性试验报告编号","可靠性试验报告检测机构"]
["耕整地机械","耕地机械","铧式犁","单体幅宽35cm以下,1-2铧翻转犁","河南鸿发机械制造有限公司","液压翻转犁","1LFY-227","单体幅宽:27cm;铧体个数:2铧;","外形尺寸：（1670X1180X1320）mm；机器质量：280kg；配套拖拉机标定功率：（29.4-44.1）kw；悬挂类型：三点悬挂；翻转机构形式：液压翻转；犁体数量：2X2个；犁体工作幅宽:270mm;","590","T201941410022","2024-11-13","5500.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","铧式犁","单体幅宽35cm以下,3-4铧翻转犁","河南鸿发机械制造有限公司","液压翻转犁","1LFY-327","单体幅宽:27cm;铧体个数:3铧;","外形尺寸：（2400X1330X1320）mm；机器质量：380kg；配套拖拉机标定功率：（44.1-58.8）kw；悬挂类型：三点悬挂；翻转机构形式：液压翻转；犁体数量：3X2个；犁体工作幅宽:270mm;","990","T202041410037","2025-03-30","6500.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","铧式犁","单体幅宽35cm以下,3-4铧翻转犁","河南鸿发机械制造有限公司","液压翻转犁","1LFY-330","单体幅宽:30cm;铧体个数:3铧;","外形尺寸：（2460X1425X1350）mm；机器质量：480kg；配套拖拉机标定功率：（51.5-66.2）kw；悬挂类型：三点悬挂；翻转机构形式：液压翻转；犁体数量：3X2个；犁体工作幅宽:300mm;","990","T202041410036","2025-03-30","8500.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","铧式犁","单体幅宽35cm以下,3-4铧翻转犁","山东弘泰农业装备有限公司","液压翻转犁","1LF-430","单体幅宽:30cm;铧体个数:3+3铧;","配套动力范围（kW）：69.8-80.8；外形尺寸（工作状态，长×宽×高)mm：2590*1490*1450；结构质量（kg）： 575；犁体数量（个）：4＋4；翻转机构型式：液压翻转","990","鲁T2017067","2021-12-31","6000.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","铧式犁","单体幅宽35cm以下,3-4铧翻转犁","河北冀农农机具有限公司","液压翻转犁","1LF-325","单体幅宽:25cm;铧体个数:3铧;","单体幅宽：250mm，犁体数量：左右各3","990","T201913130045","2024-08-29","5000.00","","非通用类","河北省","评阅不通过","初评员：不通过","专家：不通过，铭牌工作幅宽与鉴定证书不符","","","","",""]
["耕整地机械","耕地机械","铧式犁","单体幅宽35cm以下,3-4铧翻转犁","河北冀农农机具有限公司","液压翻转犁","1LF-327","单体幅宽:27cm;铧体个数:3铧;","单体幅宽：270mm，犁体数量：左右各3","990","T201913130048","2024-12-08","6000.00","","非通用类","河北省","评阅不通过","初评员：不通过","专家：不通过，铭牌工作幅宽与鉴定证书不符","","","","",""]
["耕整地机械","耕地机械","铧式犁","单体幅宽35cm以下,3-4铧翻转犁","河北冀农农机具有限公司","液压翻转犁","1LF-427","单体幅宽:27cm;铧体个数:4铧;","单体幅宽：270mm，犁体数量：左右各4个","990","T201913130049","2024-12-08","7000.00","","非通用类","河北省","评阅不通过","初评员：不通过","专家：不通过，铭牌工作幅宽与鉴定证书不符","","","","",""]
["耕整地机械","耕地机械","铧式犁","单体幅宽35cm以下,3-4铧翻转犁","济南义丰农业装备有限公司","翻转铧式犁","1LF-427","单体幅宽:27cm;铧体个数:4+4铧;","型号规格\t/\t1LF-427\n结构型式\t/\t悬挂式液压翻转犁\n工作状态a外形尺寸（长×宽×高）\t㎜\t2430×1600×1300\n工作幅宽\t㎜\t1080\n与拖拉机连接方式\t/\t悬挂式\n翻转机构型式\t/\t液压\n翻转机构油缸型号\t/\t50/30-140\n翻转机构油缸数量\t/\t1\n犁体数量\t/\t4+4\n犁体类型\t/\t铧式犁\n犁体工作幅宽\t㎜\t270\n犁体调幅犁调整幅宽范围\t㎜\t不适用\n犁轮（限深轮/运输轮/尾轮）类型\t/\t限深轮\n犁轮（限深轮/运输轮/尾轮）数量\t/\t1+1\n犁轮（限深轮/运输轮/尾轮）限深轮调节范围\t㎜\t0~250","990","鲁T2018073","2022-12-31","5000.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，铭牌与样机不符","","","","",""]
["耕整地机械","耕地机械","铧式犁","单体幅宽35cm以下,3-4铧翻转犁","郑州瑞丰王农业机械有限公司","液压翻转犁","1LFY-325","单体幅宽:25cm;铧体个数:3×2铧;","配套动力范围（kW）：36.7-44.1；外形尺寸（工作状态，长×宽×高)mm：2090×1260×1300；结构质量（kg）:370；犁体数量（个）：6；翻转机构型式：液压式、全翻转式","990","T202041410081","2025-06-29","5600.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","铧式犁","单体幅宽35cm以下,5铧及以上翻转犁","江苏神农农业装备有限公司","液压翻转犁","1LF-525","单体幅宽:25cm;铧体个数:5铧;","耕幅：125CM","2100","苏农机（2019）第（0356）号","2023-12-31","10000.00","","非通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","铧式犁","单体幅宽35cm以下,5铧及以上翻转犁","山东弘泰农业装备有限公司","液压翻转犁","1LF-530","单体幅宽:30cm;铧体个数:5+5铧;","配套动力范围（kW）：73.5-95.6；外形尺寸（工作状态，长×宽×高)mm：3300*1880*1470；结构质量（kg）： 723；犁体数量（个）：5＋5；翻转机构型式：液压翻转","2100","鲁T2017069","2021-12-31","7500.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","铧式犁","单体幅宽35cm及以上,3-4铧翻转犁","河南鸿发机械制造有限公司","液压翻转犁","1LFY-435","单体幅宽:35cm;铧体个数:4铧;","外形尺寸：（3100X2000X1550）mm；机器质量：850kg；配套拖拉机标定功率：（103-117.6）kw；悬挂类型：三点悬挂；翻转机构形式：液压翻转；犁体数量：4X2个；犁体工作幅宽:350mm;","2300","T202041410035","2025-03-30","14500.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","铧式犁","单体幅宽35cm及以上,3-4铧翻转犁","河南鸿发机械制造有限公司","液压翻转犁","1LF-440","单体幅宽:40cm;铧体个数:4铧;","外形尺寸：（4080X2000X1760）mm；机器质量：1200kg；配套拖拉机标定功率：（117.6-132.3）kw；悬挂类型：三点悬挂；翻转机构形式：液压翻转；犁体数量：4X2个；犁体工作幅宽:400mm;","2300","T202041410034","2025-03-30","19800.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：不通过承诺书过期","","","","",""]
["耕整地机械","耕地机械","铧式犁","单体幅宽35cm及以上,3-4铧翻转犁","河南鸿发机械制造有限公司","液压翻转犁","1LF-335","单体幅宽:35cm;铧体个数:3铧;","外形尺寸：（2500X1590X1420）mm；机器质量：600kg；配套拖拉机标定功率：（66.2-88.2）kw；悬挂类型：三点悬挂；翻转机构形式：液压翻转；犁体数量：3X2个；犁体工作幅宽:350mm;","2300","T201941410021","2024-11-13","8500.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","铧式犁","单体幅宽35cm及以上,3-4铧翻转犁","山东弘泰农业装备有限公司","液压翻转犁","1LT-440","单体幅宽:40cm;铧体个数:4+4铧;","配套动力范围（kW）：110-150；外形尺寸（工作状态，长×宽×高)mm：4500*2200*1770；犁体数量（个）：4+4；翻转机构型式：液压翻转","2300","T201937370078","2024-10-24","18000.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","铧式犁","单体幅宽35cm及以上,3-4铧翻转犁","山东弘泰农业装备有限公司","液压翻转犁","1LT-450","单体幅宽:50cm;铧体个数:5+5铧;","配套动力范围（kW）：132.3-176.5；外形尺寸（工作状态，长×宽×高)mm：4600*2650*1770；犁体数量（个）：4+4；翻转机构型式：液压翻转","2300","T201937370077","2024-10-24","35000.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","铧式犁","单体幅宽35cm及以上,3-4铧翻转犁","郑州市龙丰农业机械装备制造有限公司","液压翻转犁","1LYF-450","单体幅宽:50cm;铧体个数:4x2铧;","犁体数量（个）：4×2；犁体工作幅宽(mm):500；","2300","GZNJ/TJ 2019-246","2024-08-14","39000.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","铧式犁","单体幅宽35cm及以上,3-4铧翻转犁","郑州市龙丰农业机械装备制造有限公司","液压翻转调幅犁","1LYFT-450","单体幅宽:50cm;铧体个数:4x2铧;","犁体数量（个）：4×2；犁体工作幅宽(mm):500；","2300","新2017088","2021-12-31","47000.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","铧式犁","单体幅宽35cm及以上,3-4铧翻转犁","郑州市龙丰农业机械装备制造有限公司","浅翻深松翻转犁（机）","1LS-450","单体幅宽:50cm;铧体个数:4x2铧;","犁体数量（个）：4×2；犁体工作幅宽(mm):500；","2300","GZNJ/TJ 2019-227","2024-08-14","52000.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","铧式犁","单体幅宽35cm及以上,3-4铧翻转犁","郑州市龙丰农业机械装备制造有限公司","液压翻转犁","1LYFT-J360","单体幅宽:45、50、55、60cm;铧体个数:3x2铧;","犁体数量（个）：3×2；犁体工作幅宽(mm):450、500、550、600；","2300","GZNJ/TJ 2019-223","2024-08-14","38500.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","铧式犁","单体幅宽35cm及以上,3-4铧翻转犁","郑州市龙丰农业机械装备制造有限公司","浅翻深松翻转犁（机）","1LS-350","单体幅宽:50cm;铧体个数:3x2铧;","犁体数量（个）：3×2；犁体工作幅宽(mm):500；","2300","GZNJ/TJ 2019-226","2024-08-14","38000.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","铧式犁","单体幅宽35cm及以上,3-4铧翻转犁","郑州市龙丰农业机械装备制造有限公司","液压翻转犁","1LYFT-J460","单体幅宽:45、50、55、60cm;铧体个数:4x2铧;","犁体数量（个）：4×2；犁体工作幅宽(mm):450、500、550、600；","2300","GZNJ/TJ 2019-224","2024-08-14","65800.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","铧式犁","单体幅宽35cm及以上,3-4铧翻转犁","济南义丰农业装备有限公司","翻转铧式犁","1LF-435","单体幅宽:35cm;铧体个数:4+4铧;","型号规格\t/\t1LF-435\n结构型式\t/\t悬挂式液压翻转犁\n工作状态a外形尺寸（长×宽×高）\t㎜\t3260×2100×1450\n工作幅宽\t㎜\t1400\n与拖拉机连接方式\t/\t悬挂式\n翻转机构型式\t/\t液压\n翻转机构油缸型号\t/\t63/30-180\n翻转机构油缸数量\t/\t1\n犁体数量\t/\t4+4\n犁体类型\t/\t铧式犁\n犁体工作幅宽\t㎜\t350\n犁体调幅犁调整幅宽范围\t㎜\t不适用\n犁轮（限深轮/运输轮/尾轮）类型\t/\t限深轮\n犁轮（限深轮/运输轮/尾轮）数量\t/\t1+1\n犁轮（限深轮/运输轮/尾轮）限深轮调节范围\t㎜\t0~250","2300","鲁T2018074","2022-12-31","8500.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，铭牌与样机不符","","","","",""]
["耕整地机械","耕地机械","铧式犁","单体幅宽35cm及以上,3-4铧翻转犁","郑州瑞丰王农业机械有限公司","液压翻转犁","1LFY-335","单体幅宽:35cm;铧体个数:3×2铧;","配套动力范围（kW）：73.5-88.2；外形尺寸（工作状态，长×宽×高)mm：2330×1525×1470；结构质量（kg）:630；犁体数量（个）：6；翻转机构型式：液压式","2300","T202041410080","2025-06-29","9000.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","铧式犁","单体幅宽35cm及以上,3-4铧翻转犁","郑州瑞丰王农业机械有限公司","液压翻转犁","1LFY-435","单体幅宽:35cm;铧体个数:4×2铧;","配套动力范围（kW）：80.9-103；外形尺寸（工作状态，长×宽×高)mm：3100×1980×1570；结构质量（kg）:810；犁体数量（个）：8；翻转机构型式：液压式","2300","T202041410079","2025-06-29","12000.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","铧式犁","单体幅宽35cm及以上,3-4铧翻转犁","济宁神工机械有限公司","液压翻转犁","1LFT-445","单体幅宽:45cm;铧体个数:4铧;","型号规格：1LFT-445；结构型式：双向调幅犁；工作状态外形尺寸：3970*2020*1800mm；与拖拉机联接方式：悬挂式；翻转型式：液压；油缸型号：YD100-125；数量：1个；犁体数量：4+4；类型：栅条式；工作幅宽：不适用；调幅犁调整幅宽范围：350/400/450mm；犁轮类型：橡胶轮；数量：1个；限深轮调节范围：120-330mm；其他油缸型号：不适用；数量：不适用","2300","鲁T2017103","2021-12-31","38000.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","铧式犁","单体幅宽35cm及以上,3-4铧翻转犁","宁晋县保农农牧机械有限公司","液压翻转犁","1LF-427","单体幅宽:27cm;铧体个数:4铧;","外形尺寸：2780×1620×1410mm 机器质量：530kg 配套拖拉机标定功率：51.5~58.8kw\n犁体数量：左4右4  单体幅宽：270mm","2300","冀2016T—160","2020-12-31","8000.00","","非通用类","河北省","评阅不通过","初评员：不通过","专家：不通过，分档不准","","","","",""]
["耕整地机械","耕地机械","铧式犁","单体幅宽35cm及以上,3-4铧翻转犁","宁晋县保农农牧机械有限公司","液压翻转犁","1LF-327","单体幅宽:27cm;铧体个数:3铧;","外形尺寸：2130×1250×1380mm 机器质量：350kg 配套拖拉机标定功率：36.8~44.1kw\n犁体数量：左3右3  单体幅宽：270mm","2300","冀2016T—162","2020-12-31","8000.00","","非通用类","河北省","评阅不通过","初评员：不通过","专家：不通过,单体幅宽不够","","","","",""]
["耕整地机械","耕地机械","铧式犁","单体幅宽35cm及以上,5-6铧翻转犁","郑州市龙丰农业机械装备制造有限公司","液压翻转调幅犁","1LYFT-550","单体幅宽:50cm;铧体个数:5x2铧;","配套动力范围（kW）：132~176；外形尺寸（工作状态，长×宽×高)mm：5620×2270×1750；结构质量（kg）：1680；犁体数量（个）：5×2；翻转机构型式：液压翻转；犁体工作幅宽(mm):500；调幅犁调整幅宽范围：1750mm—2500mm。","3200","新2017089","2021-12-31","71800.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","铧式犁","单体幅宽35cm及以上,5-6铧翻转犁","郑州市龙丰农业机械装备制造有限公司","液压翻转犁","1LYFT-J550","单体幅宽:50cm;铧体个数:5x2铧;","配套动力范围（kW）：132~176；外形尺寸（工作状态，长×宽×高)mm：5620×2270×1750；结构质量（kg）：1680；犁体数量（个）：5×2；翻转机构型式：液压翻转；犁体工作幅宽(mm):500；调幅犁调整幅宽范围：1750mm—2500mm。","3200","GZNJ/TJ 2019-225","2024-08-14","71800.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","铧式犁","单体幅宽35cm及以上,5-6铧翻转犁","天津库恩农业机械有限公司","五铧翻转犁","MULTI-MASTER 153 5T","单体幅宽:45cm;铧体个数:5铧;","结构型式：双向，调幅\n外形尺寸（长x宽x高）：6100x1780x1770mm\n结构质量：1490kg\n配套动力：135~165cm\n与拖拉机配套连接方式：三点悬挂\n翻转机构型式：液压翻转\n犁体数量：主犁10，副犁10\n犁体工作宽幅：360mm，400mm，450mm","3200","T20190606056","2024-12-31","225000.00","","非通用类","天津市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","铧式犁","单体幅宽35cm及以上,5-6铧翻转犁","山东弘泰农业装备有限公司","液压翻转犁","1LT-550","单体幅宽:50cm;铧体个数:5+5铧;","配套动力范围（kW）：150-200；外形尺寸（工作状态，长×宽×高)mm：5500*3100*1800；犁体数量（个）：5＋5；翻转机构型式：液压翻转","3200","T201937370076","2024-10-24","41000.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","铧式犁","单体幅宽35cm及以上,5-6铧翻转犁","济宁神工机械有限公司","液压翻转犁","1LFT-550","单体幅宽:50cm;铧体个数:5铧;","型号规格：1LFT-550；结构型式：双向调幅犁；工作状态外形尺寸：5330*2275*1800mm；与拖拉机联接方式：悬挂式；翻转型式：液压；油缸型号：YD100-240；数量：1个；犁体数量：5+5；类型：栅条式；工作幅宽：不适用；调幅犁调整幅宽范围：350/400/450/500mm；犁轮类型：橡胶轮；数量：1个；限深轮调节范围：120-330mm；其他油缸型号：不适用；数量：不适用","3200","鲁T2017104","2021-12-31","48000.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期，铭牌与机具照片颜色不符","","","","",""]
["耕整地机械","耕地机械","铧式犁","单体幅宽35cm及以上,5-6铧翻转犁","济宁神工机械有限公司","液压翻转犁","1LF-535","单体幅宽:35cm;铧体个数:5铧;","型号规格：1LF-535；结构型式：双向犁；工作状态外形尺寸：3910*1940*1520mm；与拖拉机联接方式：悬挂式；翻转形式：液压；油缸型号：YD70-170；数量：1个；犁体数量：5+5；类型：铧式犁；工作幅宽：350mm；调幅犁调整幅宽范围：不适用；犁轮类型：橡胶轮；数量：1个；限深轮调节范围：120-270mm；其他油缸型号：不适用；数量：不适用","3200","鲁T2017105","2021-12-31","15000.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","旋耕机","单轴1000-1500mm旋耕机","潍坊乐哈哈农业机械装备有限公司","旋耕机","1GQN-125","旋耕机轴数:1个;耕幅:1250mm;","规格型号：1GQN-125,结构质量190kg，耕副：1250mm","300","部20170413","2021-12-31","2100.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书不完整","","","","",""]
["耕整地机械","耕地机械","旋耕机","单轴1000-1500mm旋耕机","潍坊乐哈哈农业机械装备有限公司","旋耕机","1GQN-140","旋耕机轴数:1个;耕幅:1400mm;","规格型号：1GQN-140,结构质量：230kg，耕副宽度：1400mm","300","部20171867","2021-12-31","2400.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书不完整","","","","",""]
["耕整地机械","耕地机械","旋耕机","单轴1000-1500mm旋耕机","南昌中天农机有限公司","旋耕机","1GN-140J","旋耕机轴数:1个;耕幅:1400mm;","1.结构形式:框架式；2.配套拖拉机标定功率:18.4~22.1KW；3.配套拖拉机动力输出轴转速:540R/MIN；4.外形尺寸:(长×宽×高):850×1620×1050MM；5.结构质量:248KG；6.理论作业速度:4.14KM/H；7.幅宽:140CM；8.旋耕深度:旱地12~14CM,水田14~16CM；9.传动方式:中间齿轮传动；10.与拖拉机连接方式:三点悬挂；11.刀辊转速:227R/MIN；12:刀辊最大回转半径:245MM；13.总安装刀数:30把；14.旋耕刀型号:IT245.","300","T201900320719","2024-12-30","4380.00","","通用类","江西省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","旋耕机","单轴1500-2000mm旋耕机","南昌中天农机有限公司","旋耕机","1GQN-165J","旋耕机轴数:1个;耕幅:1650mm;","1.结构形式:框架式；2.配套拖拉机标定功率:29.4~36.8KW；3.配套拖拉机动力输出轴转速:720/540R/MIN；4.外形尺寸:(长×宽×高):1000×1910×1050MM；5.结构质量:367KG；6.理论作业速度:4.57KM/H；7.幅宽:165CM；8.旋耕深度:旱地12~14CM,水田14~16CM；9.传动方式:中间齿轮传动；10.与拖拉机连接方式:三点悬挂；11.刀辊转速:265R/MIN；12:刀辊最大回转半径:245MM；13.总安装刀数:46把；14.旋耕刀型号:IT245.","900","T201900320720","2024-12-30","5420.00","","通用类","江西省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","旋耕机","单轴1500-2000mm旋耕机","南昌中天农机有限公司","旋耕机","1GQN-180J","旋耕机轴数:1个;耕幅:1800mm;","1.结构形式:框架式；2.配套拖拉机标定功率:36.8~44.1KW；3.配套拖拉机动力输出轴转速:720/540R/MIN；4.外形尺寸:(长×宽×高):1000×2060×1050MM；5.结构质量:379KG；6.理论作业速度:4.32KM/H；7.幅宽:180CM；8.旋耕深度:旱地12~14CM,水田14~16CM；9.传动方式:中间齿轮传动；10.与拖拉机连接方式:三点悬挂；11.刀辊转速:265R/MIN；12:刀辊最大回转半径:245MM；13.总安装刀数:50把；14.旋耕刀型号:IT245.","900","T201900320715","2024-12-30","5600.00","","通用类","江西省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","旋耕机","单轴1500-2000mm旋耕机","潍坊乐哈哈农业机械装备有限公司","旋耕机","1GQN-160","旋耕机轴数:1个;耕幅:1600mm;","规格型号：1GQN-160,结构质量：235kg，耕副宽度：1600mm","900","部20170414","2021-12-31","3300.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书不完整","","","","",""]
["耕整地机械","耕地机械","旋耕机","单轴1500-2000mm旋耕机","潍坊农友机械有限公司","旋耕机","1GKN-160","旋耕机轴数:1个;耕幅:1600mm;","结构型式：框架型 ；外形尺寸（工作状态，长×宽×高)mm：830×1780×990；结构质量（kg）：230；工作幅宽(cm)：160；传动方式：中间传动；耕深（cm）：≥12；刀辊总安装刀数(把)：40；旋耕刀型号：IT225;刀轴型式：单轴型。","900","T202037370144","2025-07-06","36000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，期承诺书过","","","","",""]
["耕整地机械","耕地机械","旋耕机","单轴1500-2000mm旋耕机","潍坊农友机械有限公司","旋耕机","1GKN-150","旋耕机轴数:1个;耕幅:1500mm;","结构型式：框架型 ；外形尺寸（工作状态，长×宽×高)mm：830×1680×990；结构质量（kg）：210；工作幅宽(cm)：150；传动方式：中间传动；耕深（cm）：≥12；刀辊总安装刀数(把)：36；旋耕刀型号：IT225;刀轴型式:单轴型。","900","T202037370144","2025-07-06","32000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，期承诺书过","","","","",""]
["耕整地机械","耕地机械","旋耕机","单轴1500-2000mm旋耕机","南昌中天农机有限公司","旋耕机","1GKN-150J","旋耕机轴数:1个;耕幅:1500mm;","1.结构形式:框架式；2.配套拖拉机标定功率:18.4~22.1KW；3.配套拖拉机动力输出轴转速:540R/MIN；4.外形尺寸:(长×宽×高):920×1720×1030MM；5.结构质量:271KG；6.理论作业速度:4.14KM/H；7.幅宽:150CM；8.旋耕深度:旱地12~14CM,水田14~16CM；9.传动方式:中间齿轮传动；10.与拖拉机连接方式:三点悬挂；11.刀辊转速:211R/MIN；12:刀辊最大回转半径:245MM；13.总安装刀数:34把；14.旋耕刀型号:IT245.","900","T201900320721","2024-12-30","4500.00","","通用类","江西省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","旋耕机","单轴1500-2000mm旋耕机","南昌中天农机有限公司","旋耕机","1GKN-160J","旋耕机轴数:1个;耕幅:1600mm;","1.结构形式:框架式；2.配套拖拉机标定功率:22.1~25.7KW；3.配套拖拉机动力输出轴转速:540R/MIN；4.外形尺寸:(长×宽×高):920×1820×1030MM；5.结构质量:283KG；6.理论作业速度:4.32KM/H；7.幅宽:160CM；8.旋耕深度:旱地12~14CM,水田14~16CM；9.传动方式:中间齿轮传动；10.与拖拉机连接方式:三点悬挂；11.刀辊转速:211R/MIN；12:刀辊最大回转半径:245MM；13.总安装刀数:38把；14.旋耕刀型号:IT245.","900","T201900320721","2024-12-30","4900.00","","通用类","江西省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","旋耕机","单轴1500-2000mm旋耕机","泰州樱田农机制造有限公司","旋耕机","1GQ-180","旋耕机轴数:1个;耕幅:1800mm;","配套动力范围（kW） 39.4~40.5；外形尺寸（工作状态，长 ×宽×高)mm：1930x860×1120；结构形式：圆梁式；结构质量（kg）：392；工作幅宽（cm）：180；总安装刀数量(把)：28；旋耕刀型号：专用弧形弯刀；耕深（cm）：10~18；传动机构型式：单侧齿轮传动.","900","苏农机（2019）第（0250）号","2023-12-31","8800.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","旋耕机","单轴1500-2000mm旋耕机","连云港国旋机械有限公司","旋耕机","1GKN-160","旋耕机轴数:单个;耕幅:1600mm;","型号名称\n/\n1GKN-160型旋耕机\n结构型式\n/\n框架型\n整机外形尺寸（长×宽×高）\nmm\n1020×1690×1120\n作业速度范围\nm/s\n0.56～1.39\n工作幅宽\ncm\n160\n耕深\ncm\n≥8\n刀轴型式\n/\n单轴型\n刀轴连接型式\n/\n花键式\n传动型式\n/\n中间传动\n运输方式\n/\n普通型\n变速箱挡位数（变速旋耕机）\n个\n/\n刀辊设计转速\nr/min\n248、258（N动=540）；256、296（N动=720）\n刀辊最大回转半径\nmm\n225\n刀辊总安装刀数\n把\n34\n旋耕刀型号\n/\nIT225\n限深装置型式\n/\n限深板\n镇压型式\n/\n拖板\n配套拖拉机标定功率范围\nkW\n25.7～33.1\n配套拖拉机动力输出轴转速\nr/min\n540、720","900","T202032320111","2025-06-30","4000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期，产品无铭牌","","","","",""]
["耕整地机械","耕地机械","旋耕机","单轴2000-2500mm旋耕机","连云港双亚机械有限公司","反转灭茬机","1JMF-200","旋耕机轴数:1个;耕幅:2000mm;","结构形式：框架式；外形尺寸（mm）：1020×2260×1152、配套功率(kW)：≥62.96、结构质量（kg）：435、工作幅宽(cm)：200、传动方式：侧边齿轮传动、总安装刀数量(把)：50、旋耕刀型号：IT245。 纯工作小时生产率（hm2/h）： 0.42~0.70；耕深 （cm）： ≥72 ；输入轴转数（rpm）： 540、720；刀辊转数（rpm）： 198、264；与拖拉机联接方式： 标准三点悬挂；","1600","苏农机（2016）第（0146）号","2020-12-31","6500.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","旋耕机","单轴2000-2500mm旋耕机","江苏清淮机械有限公司","反转灭茬机","1JMFY-200","旋耕机轴数:1个;耕幅:2000mm;","配套动力(kW):58.8-69.9.作业幅宽(cm):200.与拖拉机挂接方式:标准三点悬挂.结构型式:圆梁式.刀片型号:IT245.刀片数量:50把.结构质量(kg):530.外形尺寸(mm):1380×2270×1260","1600","苏农机（2018）第（0591）号","2022-12-31","6400.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过，名称与归类不符","","","","",""]
["耕整地机械","耕地机械","旋耕机","单轴2000-2500mm旋耕机","江苏清淮机械有限公司","驱动型耙浆平地机","1BPQ-240","旋耕机轴数:1个;耕幅:2400mm;","配套功率（kW):36.8-58.8.作业幅宽（cm):240.连接形式：三点悬挂.作业前进速度（km/h):3-5.整机质量（kg):395.外形尺寸（mm):900×2590×1200","1600","苏农机（2018）第（0592）号","2022-12-31","4800.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过，归类不一致","","","","",""]
["耕整地机械","耕地机械","旋耕机","单轴2000-2500mm旋耕机","连云港国旋机械有限公司","旋耕机","1GKN-200","旋耕机轴数:单个;耕幅:2000mm;","型号名称\n/\n1GKN-200型旋耕机\n结构型式(圆梁式、框架式)\n/\n框架式\n工作状态外形尺寸（长×宽×高）\nmm\n1020×2190×1050\n工作幅宽\ncm\n200\n变速箱挡位数\n/\n/\n传动方式（侧边、中间）\n/\n中间\n旋耕刀型号\n/\nIT245\n总安装刀数\n把\n58\n限深装置型式\n/\n/\n配套拖拉机标定功率\nkW\n58.8-73.5\n动力输出轴转速\nr/min\n540、720","1600","苏农机（2018）第（0264）号","2022-12-31","6000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期，产品无铭牌","","","","",""]
["耕整地机械","耕地机械","旋耕机","单轴2000-2500mm旋耕机","泰州樱田农机制造有限公司","旋耕机","1GQ-200","旋耕机轴数:1个;耕幅:2000mm;","配套动力范围（kW） 40.5~55.125；外形尺寸（工作状态，长 ×宽×高)mm：2160x860×1120；结构形式：圆梁式；结构质量（kg）：426；工作幅宽（cm）：200；总安装刀数量(把)：34；旋耕刀型号：专用弧形弯刀；耕深（cm）：10~18；传动机构型式：单侧齿轮传动.","1600","苏农机（2019）第（0251）号","2023-12-31","9000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","旋耕机","单轴2000-2500mm旋耕机","泰州樱田农机制造有限公司","旋耕机","1GQ-220","旋耕机轴数:1个;耕幅:2200mm;","配套动力范围（kW） 40.5~62.475；外形尺寸（工作状态，长 ×宽×高)mm：2360x860×1120；结构形式：圆梁式；结构质量（kg）：444；工作幅宽（cm）：220;总安装刀数量(把)：37；旋耕刀型号：专用弧形弯刀；耕深（cm）：10~18；传动机构型式：单侧齿轮传动.","1600","苏农机（2019）第（0252）号","2023-12-31","9200.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","旋耕机","单轴2000-2500mm旋耕机","泰州樱田农机制造有限公司","旋耕机","1GQ-240A","旋耕机轴数:1个;耕幅:2400mm;","1GQ-240A    配套动力范围（kW） 51.5~69.825；外形尺寸（工作状态，长 ×宽×高)mm：2560x860×1120；结构形式：圆梁式；结构质量（kg）：465；工作幅宽（cm）：240；总安装刀数量(把)：40；旋耕刀型号：专用弧形弯刀；耕深（cm）：10~18；传动机构型式：单侧齿轮传动.","1600","苏农机（2019）第（0253）号","2023-12-31","9800.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","旋耕机","单轴2000-2500mm旋耕机","南昌中天农机有限公司","旋耕机","1GQQN-200J","旋耕机轴数:1个;耕幅:2000mm;","1.结构形式:框架式；2.配套拖拉机标定功率:44.1~51.5KW；3.配套拖拉机动力输出轴转速:720/540R/MIN；4.外形尺寸:(长×宽×高):1100×2300×1150MM；5.结构质量:414KG；6.理论作业速度:4.75KM/H；7.幅宽:200CM；8.旋耕深度:旱地12~14CM,水田14~16CM；9.传动方式:中间齿轮传动；10.与拖拉机连接方式:三点悬挂；11.刀辊转速:265R/MIN；12:刀辊最大回转半径:245MM；13.总安装刀数:58把；14.旋耕刀型号:IT245.","1600","T201900320714","2024-12-30","7400.00","","通用类","江西省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","旋耕机","单轴2000-2500mm旋耕机","南昌中天农机有限公司","旋耕机","1GQQN-230J","旋耕机轴数:1个;耕幅:2300mm;","1.结构形式:框架式；2.配套拖拉机标定功率:51.5~58.8KW；3.配套拖拉机动力输出轴转速:720/540R/MIN；4.外形尺寸:(长×宽×高):1100×2530×1150MM；5.结构质量:430KG；6.理论作业速度:4.75KM/H；7.幅宽:230CM；8.旋耕深度:旱地12~14CM,水田14~16CM；9.传动方式:中间齿轮传动；10.与拖拉机连接方式:三点悬挂；11.刀辊转速:265R/MIN；12:刀辊最大回转半径:245MM；13.总安装刀数:62把；14.旋耕刀型号:IT245.","1600","T201900320714","2024-12-30","7600.00","","通用类","江西省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","旋耕机","单轴2000-2500mm旋耕机","南昌中天农机有限公司","旋耕机","1GQN-200J","旋耕机轴数:1个;耕幅:2000mm;","1.结构形式:框架式；2.配套拖拉机标定功率:44.1~51.5KW；3.配套拖拉机动力输出轴转速:720/540R/MIN；4.外形尺寸:(长×宽×高):1000×2300×1050MM；5.结构质量:399KG；6.理论作业速度:4.43KM/H；7.幅宽:200CM；8.旋耕深度:旱地12~14CM,水田14~16CM；9.传动方式:中间齿轮传动；10.与拖拉机连接方式:三点悬挂；11.刀辊转速:265R/MIN；12:刀辊最大回转半径:245MM；13.总安装刀数:58把；14.旋耕刀型号:IT245.","1600","T201900320713","2024-12-30","5800.00","","通用类","江西省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","旋耕机","单轴2000-2500mm旋耕机","南昌中天农机有限公司","旋耕机","1GQN-230J","旋耕机轴数:1个;耕幅:2300mm;","1.结构形式:框架式；2.配套拖拉机标定功率:51.5~58.8KW；3.配套拖拉机动力输出轴转速:720/540R/MIN；4.外形尺寸:(长×宽×高):1000×2530×1050MM；5.结构质量:415KG；6.理论作业速度:4.75KM/H；7.幅宽:230CM；8.旋耕深度:旱地12~14CM,水田14~16CM；9.传动方式:中间齿轮传动；10.与拖拉机连接方式:三点悬挂；11.刀辊转速:265R/MIN；12:刀辊最大回转半径:245MM；13.总安装刀数:62把；14.旋耕刀型号:IT245.","1600","T201900320713","2024-12-30","6100.00","","通用类","江西省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","旋耕机","单轴2000-2500mm旋耕机","泰州樱田农机制造有限公司","旋耕机","1GQ-240","旋耕机轴数:1个;耕幅:2400mm;","配套动力范围（kW） 51.5~69.825；外形尺寸（工作状态，长 ×宽×高)mm：2590x1100×1240；结构形式：圆梁式；结构质量（kg）：645；工作幅宽（cm）：240；总安装刀数量(把)：68；旋耕刀型号：专用弧形弯刀；耕深（cm）：10~18；传动机构型式：单侧齿轮传动.","1600","苏农机（2019）第（0254）号","2023-12-31","11800.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","旋耕机","单轴2000-2500mm旋耕机","潍坊乐哈哈农业机械装备有限公司","旋耕机","1GQN-200","旋耕机轴数:1个;耕幅:2000mm;","规格型号：1GQN-200,结构质量：370kg，耕副宽度：2000mm","1600","部20171868","2021-12-31","5500.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书不完整","","","","",""]
["耕整地机械","耕地机械","旋耕机","单轴2000-2500mm旋耕机","石家庄金牛农机制造有限公司","旋耕机","1GKN-200","旋耕机轴数:1个;耕幅:2000mm;","结构型式：单轴框架式 幅宽：200cm","1600","冀2016T—379","2020-12-31","7800.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","旋耕机","单轴2000-2500mm旋耕机","石家庄农业机械股份有限公司","旋耕机","1GQN-200K","旋耕机轴数:单轴个;耕幅:2000mm;","结构型式：单轴框架式\n工作状态外形尺寸（长×宽×高）：1040×2240×1200\tmm\n配套拖拉机标定功率范围：43.6～66.1 kW\n结构质量：\n工作幅宽：200\tcm\n传动方式：中间齿轮传动\t\n刀辊总安装刀数：60\t把\n旋耕刀型号：T245\n作业速度范围：0.56～1.39\tm/s\n耕深：12～16\tcm\n变速箱档位数：/\t个\n刀辊设计转速：267\tr/min\n刀辊最大回转半径：245\tmm\n刀轴连接型式：花键连接","1600","冀2017T—279","2021-12-31","7500.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","旋耕机","单轴2500mm及以上旋耕机","南昌中天农机有限公司","旋耕机","1GQQN-250J","旋耕机轴数:1个;耕幅:2500mm;","结构形式:框架式；2.配套拖拉机标定功率:58.8~73.5KW；3.配套拖拉机动力输出轴转速:720/540R/MIN；4.外形尺寸:(长×宽×高):1100×2800×1150MM；5.结构质量:494KG；6.理论作业速度:4.82KM/H；7.幅宽:250CM；8.旋耕深度:旱地12~14CM,水田14~16CM；9.传动方式:中间齿轮传动；10.与拖拉机连接方式:三点悬挂；11.刀辊转速:265R/MIN；12:刀辊最大回转半径:245MM；13.总安装刀数:66把；14.旋耕刀型号:IT245.","2200","T201900320717","2024-12-30","7900.00","","通用类","江西省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","旋耕机","单轴2500mm及以上旋耕机","南昌中天农机有限公司","旋耕机","1GQQQN-280","旋耕机轴数:1个;耕幅:2800mm;","2结构型式:框架型3整机外形尺寸(长×宽×高):1200×3150×1330mm4作业速度范围:0.56~1.39m/s5工作幅宽:280cm6耕深:旱耕12-14水耕14-16cm7刀轴型式:单轴型8刀轴连接型式:接盘式9传动型式:中间传动10运输方式:普通型11变速箱档位数(变速旋耕机)个:无12刀辊设计转速:326r/min13刀辊最大回转半径:255mm14刀辊总安装刀数:70把15旋耕机刀型号:IT24516限深装置型式:限深板17镇压型式:拖板18配套拖拉机标定功率范围:66.2~73.5kW19配套拖拉机动力输出轴转速:720r/min","2200","T201900320718","2024-12-30","10900.00","","通用类","江西省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","旋耕机","单轴2500mm及以上旋耕机","潍坊嘉利诺农业机械装备有限公司","旋耕机","1GKN-280","旋耕机轴数:1个;耕幅:2800mm;","型式：框架型，结构尺寸（长*宽*高）:1100mm×3000mm×1200mm；工作幅宽：280cm；刀轴型式：单轴型；刀轴连接型式：花键式；传动型式：中间传动；刀棍设计转速：255 r/min ；配套拖拉机动力输出轴转速：720 r/min。","2200","T202037370170","2025-07-06","8600.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，缺鉴定报告","","","","",""]
["耕整地机械","耕地机械","旋耕机","单轴2500mm及以上旋耕机","河北帅旗农业机械制造有限公司","旋耕机","1GQN-300","旋耕机轴数:1个;耕幅:300mm;","耕幅300cm，配套动力132.4-147kw,结构型式框架式，外形尺寸（长×宽×高）1380×3210×1110mm,刀轴型式单轴型，刀轴连接型式接盘式，传动型式中间齿轮传动，运输方式普通型，总安装刀数88把，旋耕刀型号IT245.限深装置型式限深板，镇压形式拖板","2200","T201913130170","2024-12-30","9000.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过，耕幅300MM","","","","",""]
["耕整地机械","耕地机械","旋耕机","单轴2500mm及以上旋耕机","泰州樱田农机制造有限公司","旋耕机","1GQ-280","旋耕机轴数:1个;耕幅:2800mm;","配套动力范围（kW） 51.5~69.825；外形尺寸（工作状态，长 ×宽×高)mm：2990x1100×1240；结构形式：圆梁式；结构质量（kg）：706；工作幅宽（cm）：280；总安装刀数量(把)：80；旋耕刀型号：专用弧形弯刀；耕深（cm）：10~18；传动机构型式：单侧齿轮传动.","2200","苏农机（2019）第（0255）号","2023-12-31","12800.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","旋耕机","单轴2500mm及以上旋耕机","连云港国旋机械有限公司","旋耕机","1GKN-250","旋耕机轴数:单个;耕幅:2500mm;","型号名称\n/\n1GKN-250型旋耕机\n结构型式(圆梁式、框架式)\n/\n框架式\n工作状态外形尺寸（长×宽×高）\nmm\n1040×2740×1210\n工作幅宽\ncm\n250\n变速箱挡位数\n/\n/\n传动方式（侧边、中间）\n/\n中间\n旋耕刀型号\n/\nIT245\n总安装刀数\n把\n66\n限深装置型式\n/\n/\n配套拖拉机标定功率\nkW\n66.2-88.2\n动力输出轴转速\nr/min\n540、720","2200","苏农机（2018）第（0265）号","2022-12-31","7800.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","旋耕机","单轴2500mm及以上旋耕机","连云港国旋机械有限公司","旋耕机","1GKN-300","旋耕机轴数:单个;耕幅:3000mm;","型号名称\n/\n1GKN-300型旋耕机\n结构型式(圆梁式、框架式)\n/\n框架式\n工作状态外形尺寸（长×宽×高）\nmm\n1100×3280×1190\n工作幅宽\ncm\n300\n变速箱挡位数\n/\n/\n传动方式（侧边、中间）\n/\n中间\n旋耕刀型号\n/\nIT245\n总安装刀数\n把\n78\n限深装置型式\n/\n/\n配套拖拉机标定功率\nkW\n80.8-102.9\n动力输出轴转速\nr/min\n540、720","2200","苏农机（2018）第（0266）号","2022-12-31","7800.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","旋耕机","单轴2500mm及以上旋耕机","济宁神工机械有限公司","旋耕机","1GK-260","旋耕机轴数:1个;耕幅:2600mm;","型号名称：1GK-260；结构型式：框架式；工作状态外形尺寸：710*2800*850mm；工作幅宽：260cm；传动方式：侧边（双侧）；变速箱挡位数：1个；旋耕刀型号：IT245；总安装刀数：54把；限深装置形式：限深块；配套拖拉机标定功率：80.9-88.2kw；动力输出轴转速：540/720r/min","2200","鄂2017111","2021-12-31","14800.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","旋耕机","单轴2500mm及以上旋耕机","济宁神工机械有限公司","旋耕机","1GK-300","旋耕机轴数:1个;耕幅:3000mm;","型号名称：1GK-300；结构型式：框架式；工作状态外形尺寸：710*3200*850mm；工作幅宽：300cm；传动方式：侧边（双侧）；变速箱挡位数：1个；旋耕刀型号：IT245；总安装刀数：64把；限深装置型式：/；配套拖拉机标定功率：88.2-95.5kw；动力输出轴转速：540/720r/min","2200","鄂2017112","2021-12-31","16000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","旋耕机","单轴2500mm及以上旋耕机","济宁神工机械有限公司","旋耕机","1GK-350","旋耕机轴数:1个;耕幅:3500mm;","型号名称：1GK-350；结构型式：框架式；工作状态外形尺寸：710*3554*850mm；工作幅宽：350cm；传动方式：侧边（双侧）；变速箱挡位数：1个；旋耕刀型号：IT245；总安装刀数：74把；限深装置型式：/；配套拖拉机标定功率：95.5-103.0kw；动力输出轴转速：540/720r/min","2200","鄂2017113","2021-12-31","19000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","旋耕机","双轴2500mm及以上旋耕机","连云港国旋机械有限公司","双轴旋耕机","1GKM-260","旋耕机轴数:双个;耕幅:2500mm;","型号名称\n/\n1GKM-260型双轴旋耕机\n结构型式\n/\n框架型\n整机外形尺寸（长×宽×高）\nmm\n1500×3020×1120\n作业速度范围\nm/s\n0.56～1.39\n工作幅宽\ncm\n260\n耕深\ncm\n≥8\n刀轴型式\n/\n双轴型\n刀轴连接型式\n/\n接盘式\n传动型式\n/\n前轴:侧边传动；后轴:侧边传动\n运输方式\n/\n普通型\n变速箱挡位数（变速旋耕机）\n个\n/\n刀辊设计转速\nr/min\n前轴:198、265；后轴:320、426\n刀辊最大回转半径\nmm\n前轴:245；后轴:175\n刀辊总安装刀数\n把\n前轴:80；后轴:90\n旋耕刀型号\n/\n前轴:IT245；后轴:IT175\n限深装置型式\n/\n/\n镇压型式\n/\n/\n配套拖拉机标定功率范围\nkW\n102.9～132.3\n配套拖拉机动力输出轴转速\nr/min\n540、720","2900","T202032320112","2025-06-30","11000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期，产品无铭牌","","","","",""]
["耕整地机械","耕地机械","旋耕机","1200-2000mm履带自走式旋耕机","广西玉林市德高机械有限公司","自走履带旋耕机","1GZL120","耕幅:1200mm;形式:履带自走式:是 ;","配备12.13kW的国三标准排放柴油机，型号ZS1105DGⅢ；整机外形尺寸:2500*1350*1700；作业幅宽:1200mm；结构质量:760kg；传动方式:皮带传动；旋耕刀片总数量24把；履带参数：节距72mm，节数38节，履带宽度250mm，轨距620mm","8300","T202045450064","2025-07-08","29800.00","","通用类","广西壮族自治区","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","旋耕机","1200-2000mm履带自走式旋耕机","衡阳市富农机械制造有限公司","履带自走式旋耕机","1GZ-120","耕幅:1200mm;形式:履带自走式:是 ;","1、型号1GZ-120;2、结构形式:履带自走式;3、外形尺寸(长×宽×高)(mm):2420×1310×1350;4、结构质量(kg):500;5、幅宽(cm):120;6、传动方式:侧边链传动;7、刀辊设计转速(r/min):420;8、最大回转半径(mm):175;9、总安装刀数(把):20;10、旋耕刀型号:ⅠT175;11、最小离地间隙(mm):140;12、履带(节距×节数×宽):60mm×50节×150mm;13、轨距(mm):640;14、理论作业速度(km/h):1-4;15、常用作业档:Ⅰ、Ⅱ、Ⅲ;16、最小通过半径:(m):1.75;17、变速箱类型:(3+1)机械变速;18:配套动力:ZH1115G3柴油机:14.7kw:2200r/min","8300","湘20170124030","2021-12-31","44800.00","","通用类","湖南省","评阅不通过","初评员：不通过","专家：不通过，承诺书缺项","","","","",""]
["耕整地机械","耕地机械","深松机","4-5铲深松机","江苏神农农业装备有限公司","深松机","1S-280","振动式:否 ;深松部件个数:4个;","耕幅：280CM","2300","苏农机（2019）第（0358）号","2023-12-31","11000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","深松机","6铲及以上振动式深松机","天津库恩农业机械有限公司","深松机","Cultimer 350T","振动式:是 ;深松部件个数:11个;","外形尺寸（长x宽x高）：3900x3450x1490mm\n结构质量：1890kg\n配套动力：≥128kw\n拖拉机连接方式：三点悬挂\n深松铲：双翼深松铲 11 个\n作业宽幅：3.5m","4900","黑垦鉴2016066","2020-12-31","151000.00","","通用类","天津市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","开沟机","开沟深度50cm以下配套轮式拖拉机开沟机","江苏神农农业装备有限公司","开沟机","1KJ-35","配套轮式拖拉机:是 ;开沟深度:30cm;","沟深：30-40CM","1400","T201932320183","2024-12-30","7000.00","","非通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","开沟机","开沟深度50cm以下配套轮式拖拉机开沟机","江苏神农农业装备有限公司","开沟机","1KJ-35A","配套轮式拖拉机:是 ;开沟深度:30cm;","沟深：30-4CM","1400","T201932320182","2024-12-30","7500.00","","非通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","开沟机","开沟深度50cm以下配套轮式拖拉机开沟机","潍坊潍林农业装备有限公司","开沟机","1KS-45","配套轮式拖拉机:是 ;开沟深度:35～45cm;","1.外形尺寸（长×宽×高）mm: 1250×950×1000(不含万向节)； 2.整机质量(kg): 275； 3.配套动力(kW): 36.8～66.2； 4.配套动力输出轴转速 （r/min ）：540/720/1100； 5.传动方式:中间齿轮传动； 6.开沟深度(cm):35～45； 7. 沟面宽度(cm):35～45；8.开沟刀数量(把): 16；9.开沟沟形：梯矩形;","1400","GZNJ/TJ 2019-352","2024-11-21","6000.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","开沟机","开沟深度50cm及以上配套轮式拖拉机开沟机","潍坊潍林农业装备有限公司","开沟机","1KS-55","配套轮式拖拉机:是 ;开沟深度:50～55cm;","1.外形尺寸（长×宽×高）mm: 1350×1240×1100(不含万向节)； 2.整机质量(kg): 300； 3.配套动力(kW): 36.8～66.2； 4.配套动力输出轴转速 （r/min ）：540/720/1100； 5.传动方式:中间齿轮传动； 6.开沟深度(cm):50～55； 7. 沟面宽度(cm):45～55；8.开沟刀数量(把): 20；9.开沟沟形：梯矩形;","1900","GZNJ/TJ 2019-353","2024-11-21","7000.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW以下微耕机","山东华盛农业药械有限责任公司","微耕机","1WG2.0-60","配套功率:2.0kW;","序号\t    项\t目\t设计值\n1\t型号名称\t1WG2.0-60型微耕机\n2\t结构型式\t前置式\n3\t配套发动型号名称\t160F-1型汽油机\n5\t配套发动标定功率\t2.0kw\n7\t配套发动起动方式\t手拉启动\n8\t配套发动燃油种类\t汽油\n9\t整机外形尺寸（长×宽×高）\t1460×670×830mm\n10\t作业速度\t0.05～0.1m/s\n12\t作业小时生产率\t≥0.02hm2/(h•m)\n13\t单位作业面积燃油消耗量\t≤35kg/hm2\n14\t工作幅宽\t600mm\n15\t刀辊总安装刀数\t18\n16\t旋耕刀型号\tRT165","510","T201937370066","2024-10-24","2600.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW以下微耕机","洛阳精匠机械有限公司","微耕机","1WGQ2.2-50HA","配套功率:2.2kW;","发动机厂家：重庆大江动力设备制造有限公司\n发动机型号：DH98型   汽油发动机,\n功率：2.2Kw、整机外形尺寸（长×宽×高）: 1260mm×520mm×950mm、配套发动机标定转速:3800r/min、启动方式：手拉反冲、工作幅宽:500mm、扶把调整幅度（水平方向）：不可调、扶把调整幅度（垂直方向）:40度、发动机输出传动方式：皮带、刀辊传动方式：链条、刀辊设计转速：225r/min、刀辊最大回转半径：133mm、刀辊总安装刀数：18把、旋耕刀型式：刀盘式、主离合器状态：离心式、主离合器状态：常开","510","T202041410096","2025-06-29","2100.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW以下微耕机","重庆芸析机械制造有限公司","微耕机","1WGFQD2.2-60-1","配套功率:2.2kW;","工作状态外形尺寸（长×宽×高）mm:1185×610×945;\n作业速度m/s:0.05～0.2;\n作业小时生产率hm2/(h·m):≥0.02;\n单位作业面积燃油消耗量kg/hm2:≤35;\n工作幅宽mm:600;","510","T201950500129","2024-09-09","1900.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","四川刚毅科技集团有限公司","微型耕耘机","1WG4.0Q-Z","配套功率:4.0kW;","外形尺寸（长×宽×高)mm：1560×950×900；工作幅宽(cm)：950mm；传动方式（发动机输出）：直联；传动方式（刀辊）：齿轮传动；旋耕刀型号：非标旱地刀；总安装刀数量(把)：24；主离合器型式：摩擦片式。","700","川A19006","2023-12-31","3180.00","","非通用类","四川省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","四川刚毅科技集团有限公司","微耕机","1WG6.3-Z","配套功率:6.3kW;","型 号：1WG6.3-Z微耕机；发动机生产企业：无锡凯奥动力机械有限公司；发动机型号：KMGS450-2；标定功率：6.3KW；标定转速：3600r/min；燃油种类：柴油；排放标准：国三。\n外形尺寸（长×宽×高)mm：1750×1350×900；工作幅宽(cm)1350；传动方式（发动机输出）：直联；传动方式（刀辊）：齿轮传动；旋耕刀型号：非标旱地刀；总安装刀数量(把)：38；主离合器型式：摩擦片式。","700","部20190657","2023-12-31","4180.00","","非通用类","四川省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","四川刚毅科技集团有限公司","微耕机","1WG5.3-Z","配套功率:5.3kW;","型号：1WG5.3-Z微耕机；发动机生产企业：无锡华源凯马发动机有限公司；型号规格：KM186FA；标定功率：5.3KW；标定转速：3000r/min；燃油种类：柴油；排放阶段：国三。 \n配置参数：外形尺寸（长×宽×高)mm：1750×1350×900；工作幅宽(cm)：1350；传动方式（发动机输出）：直联；传动方式（刀辊）：齿轮传动；旋耕刀型号：非标旱地刀；总安装刀数量(把)：38；主离合器型式：摩擦片式。","700","部20190658","2023-12-31","3850.00","","非通用类","四川省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","四川刚毅科技集团有限公司","微耕机","1WG5.7-Z","配套功率:5.7kW;","型号名称：1WG5.7-Z微耕机；外形尺寸（长×宽×高)mm：1750×1350×900；工作幅宽(cm)1350；传动方式（发动机输出）：直联；传动方式（刀辊）：齿轮传动；旋耕刀型号：非标旱地刀；总安装刀数量(把)：38；主离合器型式：摩擦片式。\n发动机生产企业：无锡华源凯马发动机有限公司；发动机型号：KM188F；标定功率：5.7KW；标定转速：3000r/min；燃油种类：柴油；排放标准：国三。","700","部20190656","2023-12-31","3980.00","","非通用类","四川省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","常州科普动力机械有限公司","微耕机","1WG6.3-135FC-ZC","配套功率:6.3kW;","配套发动机标定功率: 6.3KW\n配套发动机燃油种类: 柴油\n作业速度：≥ 0.17m/s\n作业小时生产率：≥0.06hm2/(h·m)\n单位作业面积燃油消耗量：≤30kg/hm2\n工作幅宽： 1350mm\n发动机输出传动方式： 直联\n刀辊传动方式： 齿轮传动\n刀辊最大回转半径： 180mm","700","T201932320179","2024-12-30","5800.00","","非通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过铭牌与机具照片不符","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","常州科普动力机械有限公司","微耕机","1WG4.0-100FQ-ZC","配套功率:4.0kW;","配套发动机标定功率: 4.0KW\n配套发动机燃油种类: 汽油\n作业速度： ≥0.11m/s\n作业小时生产率：≥0.04hm2/(h·m)\n单位作业面积燃油消耗量：≤35kg/hm2\n工作幅宽： 1000mm\n发动机输出传动方式： 直联\n刀辊传动方式： 齿轮传动\n刀辊最大回转半径： 160mm","700","T201932320178","2024-12-30","3500.00","","非通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过铭牌与机具照片不符","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆冠虎科技有限公司","微耕机","1WG4.2-100FQ-ZC","配套功率:4.2kW;","配套动力标定功率：4.2kW,汽油机；配套动力标定转速：3600r/min；外形尺寸（长×宽×高）：1600mm×1010mm×960mm；工作幅度：1000mm；结构质量：70kg；传动方式（发动机输出）：直联式；传动方式（刀辊）：齿轮传动；旋耕刀型号：旱地刀；总安装刀数量：24把；主离合器形式：摩擦片式","700","T201950500208","2024-10-07","3960.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆冠虎科技有限公司","微耕机","1WG4.05-100FC-ZC","配套功率:4.05kW;","配套动力标定功率：4.05kW，国Ⅲ柴油机；配套动力标定转速：3600r/min；外形尺寸（长×宽×高）：1600mm×1010mm×960mm；工作幅度：1000mm；结构质量：80kg；传动方式（发动机输出）：直联式；传动方式（刀辊）：齿轮传动；旋耕刀型号：旱地刀；总安装刀数量：24把；主离合器形式：摩擦片式；主离合器状态：常开。","700","T201950500207","2024-10-07","5980.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆冠虎科技有限公司","微耕机","1WGCZ4.1-105","配套功率:4.1kW;","配套动力标定功率：4.1kW，国Ⅲ柴油机；配套动力标定转速：3600r/min；外形尺寸（长×宽×高）：1610mm×1060mm×1020mm；工作幅度：1050mm；结构质量：105kg；传动方式（发动机输出）：直联式；传动方式（刀辊）：齿轮传动；旋耕刀型号：旱地刀；总安装刀数量：30把；主离合器形式：摩擦片式；主离合器状态：常开。","700","T202050500145","2025-07-13","6150.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆冠虎科技有限公司","微耕机","1WGCZ5.7-135","配套功率:5.7kW;","配套动力标定功率：5.7kW,国Ⅲ柴油机；配套动力标定转速：3000r/min；外形尺寸（长×宽×高）：1610mm×1360mm×1050mm；工作幅度：1350mm；结构质量：124kg；传动方式（发动机输出）：直联式；传动方式（刀辊）：齿轮传动；旋耕刀型号：旱地刀；总安装刀数量：38把；主离合器形式：摩擦片式；主离合器状态：常开。","700","T202050500146","2025-07-13","6360.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆冠虎科技有限公司","微耕机","1WGCZ6.2-135","配套功率:6.2kW;","配套动力标定功率：6.2kW，国Ⅲ柴油机；配套动力标定转速：3000r/min；外形尺寸（长×宽×高）：1750mm×1360mm×1050mm；工作幅度：1350mm；结构质量：126kg；传动方式（发动机输出）：直联式；传动方式（刀辊）：齿轮传动；旋耕刀型号：旱地刀；总安装刀数量：38把；主离合器形式：摩擦片式；主离合器状态：常开。","700","T202050500148","2025-07-13","6400.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆冠虎科技有限公司","微耕机","1WGQZ5.4-105","配套功率:5.4kW;","配套动力标定功率：5.4kW，汽油机；配套动力标定转速：3600r/min；外形尺寸（长×宽×高）：1730mm×1060mm×1050mm；工作幅度：1050mm；传动方式（发动机输出）：直联式；传动方式（刀辊）：齿轮传动；旋耕刀型号：Ⅱ型旱地耕刀；总安装刀数量：30把；主离合器形式：摩擦片式,主离合器状态：常开。","700","T202050500147","2025-07-13","4480.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆市冠腾机械有限公司","微耕机","1WG4.1-105FC-ZC","配套功率:4.1kW;","配套动力标定功率：4.1kW，国Ⅲ柴油机；配套动力标定转速：3600r/min；外形尺寸（长×宽×高）：1750mm×1050mm×1000mm；工作幅度：1050mm；结构质量：105kg；传动方式（发动机输出）：直联式；传动方式（刀辊）：齿轮传动；旋耕刀型号：旱地刀；总安装刀数量：30把；主离合器形式：摩擦片式；主离合器状态：常开。","700","T201950500203","2024-10-07","6080.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆市冠腾机械有限公司","微耕机","1WGQZ4.0-100","配套功率:4.0kW;","配套动力标定功率：4.0kW，汽油机；配套动力标定转速：3600r/min；外形尺寸（长×宽×高）：1550mm×1010mm×1000mm；工作幅度：1000mm；传动方式（发动机输出）：直联式；传动方式（刀辊）：齿轮传动；旋耕刀型号：Ⅱ型旱地耕刀；总安装刀数量：24把；主离合器形式：摩擦片式,主离合器状态：常开。","700","T202050500130","2025-06-21","3660.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆市冠腾机械有限公司","微耕机","1WGQZ5.4-105","配套功率:5.4kW;","配套动力标定功率：5.4kW，汽油机；配套动力标定转速：3600r/min；外形尺寸（长×宽×高）：1660mm×1060mm×1030mm；工作幅度：1050mm；传动方式（发动机输出）：直联式；传动方式（刀辊）：齿轮传动；旋耕刀型号：Ⅱ型旱地耕刀；总安装刀数量：30把；主离合器形式：摩擦片式,主离合器状态：常开。","700","T202050500119","2025-06-21","4680.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆市冠腾机械有限公司","微耕机","1WGCZ6.3-135","配套功率:6.3kW;","配套动力标定功率：6.3kW，柴油机；配套动力标定转速：3600r/min；外形尺寸（长×宽×高）：1700mm×1360mm×1030mm；工作幅度：1350mm；传动方式（发动机输出）：直联式；传动方式（刀辊）：齿轮传动；旋耕刀型号：Ⅱ型旱地耕刀；总安装刀数量：38把；主离合器形式：摩擦片式,主离合器状态：常开。","700","T202050500127","2025-06-21","6160.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆市冠腾机械有限公司","微耕机","1WGCZ4.0-105","配套功率:4.0kW;","配套动力标定功率：4.0kW，柴油机；配套动力标定转速：3600r/min；外形尺寸（长×宽×高）：1590mm×1060mm×960mm；工作幅度：1050mm；传动方式（发动机输出）：直联式；传动方式（刀辊）：齿轮传动；旋耕刀型号：Ⅱ型旱地耕刀；总安装刀数量：30把；主离合器形式：摩擦片式,主离合器状态：常开。","700","T202050500129","2025-06-21","6060.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆市冠腾机械有限公司","微耕机","1WGCZ4.05-100","配套功率:4.05kW;","配套动力标定功率：4.05kW，柴油机；配套动力标定转速：3600r/min；外形尺寸（长×宽×高）：1560mm×1010mm×960mm；工作幅度：1000mm；传动方式（发动机输出）：直联式；传动方式（刀辊）：齿轮传动；旋耕刀型号：Ⅱ型旱地耕刀；总安装刀数量：30把；主离合器形式：摩擦片式,主离合器状态：常开。","700","T202050500128","2025-06-21","5980.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆市冠腾机械有限公司","微耕机","1WG4.05-100FC-ZC","配套功率:4.05kW;","配套动力标定功率：4.05kW，国Ⅲ柴油机；配套动力标定转速：3600r/min；外形尺寸（长×宽×高）：1560mm×1010mm×960mm；工作幅度：1000mm；结构质量：80kg；传动方式（发动机输出）：直联式；传动方式（刀辊）：齿轮传动；旋耕刀型号：旱地刀；总安装刀数量：24把；主离合器形式：摩擦片式；主离合器状态：常开。","700","T201950500204","2024-10-07","5980.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆尚翔机电有限公司","微耕机","1WGQZ4.0-95","配套功率:4.0kW;","外形尺寸（长×宽×高)mm：640×960×960；配套动力:汽油机；标定功率:4.0kW；标定转速:3600r/min；工作幅宽(cm)：95；结构质量（kg）：90；作业速度:0.1-0.3m/s；作业小时生产率:≥0.04hm²/(h•m)；耕深:≥10cm；传动方式（发动机输出）：直联式；传动方式（刀辊）：齿轮传动；旋耕刀型号：旱地刀；总安装刀数量(把)：24；主离合器型式：摩擦片式。","700","T201950500200","2024-10-07","2680.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆尚翔机电有限公司","微耕机","1WGQZ4.0-40A","配套功率:4.0kW;","外形尺寸（长×宽×高)mm：1280×510×830；配套动力:汽油机；标定功率:4.0kW；标定转速:3600r/min；工作幅宽(cm)：40；结构质量（kg）：30；作业速度:0.05-0.2m/s；作业小时生产率:≥0.02hm²/(h•m)；耕深:≥10cm；传动方式（发动机输出）：直联式；传动方式（刀辊）：蜗轮蜗杆传动；旋耕刀型号：旱地刀；总安装刀数量(把)：12；主离合器型式：离心式。","700","T201950500199","2024-10-07","3080.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆尚翔机电有限公司","微耕机","1WGCZ4.05-95","配套功率:4.05kW;","外形尺寸（长×宽×高)mm： 1640×960×960；配套动力:柴油机；标定功率:4.05kW；标定转速:3600r/min；工作幅宽(cm)：95；结构质量（kg）：100；作业速度:0.1-0.3m/s；作业小时生产率:≥0.04hm²/(h•m)；耕深:≥10cm；传动方式（发动机输出）：直联式；传动方式（刀辊）：齿轮传动；旋耕刀型号：旱地刀；总安装刀数量(把)：24；主离合器型式：摩擦片式。","700","T201950500202","2024-10-07","5030.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆尚翔机电有限公司","微耕机","1WGCZ4.05-90","配套功率:4.05kW;","外形尺寸（长×宽×高)mm：1570×930×950；配套动力:柴油机；标定功率:4.05kW；标定转速:3600r/min；工作幅宽(cm)：90；结构质量（kg）：100；作业速度:0.1-0.3m/s；作业小时生产率:≥0.04hm²/(h•m)；耕深:≥10cm；传动方式（发动机输出）：直联式；传动方式（刀辊）：齿轮传动；旋耕刀型号：旱地刀；总安装刀数量(把)：24；主离合器型式：摩擦片式。","700","T201950500201","2024-10-07","5080.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆嘉木机械有限公司","微耕机","1WG4.0-100FQ-D","配套功率:4.0kW;","配套发动机标定功率：4.0KW，配套发动机标定转速：3600r/min，配套发动机燃油种类：汽油，整机外形尺寸（长×宽×高）mm：1450×1010×950，工作幅宽:1000mm，发动机输出传动方式：皮带传动，旋耕刀型式:旱地刀，主离合器型式：张紧轮式。","700","T201950500270","2024-12-25","2880.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆嘉木机械有限公司","微耕机","1WG4.0-105FQ-Z","配套功率:4.0kW;","配套发动机标定功率：4.0KW，配套发动机标定转速：3600r/min，配套发动机燃油种类：汽油，整机外形尺寸（长×宽×高）mm：1600×1060×950，工作幅宽：1050mm，发动机输出传动方式：直联，旋耕刀型式：旱地刀，主离合器型式：摩擦片式。","700","T201950500271","2024-12-25","2980.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆嘉木机械有限公司","微耕机","1WG4.05-105FC-ZC","配套功率:4.05kW;","配套发动机标定功率4.05KW，配套发动机标定转速3600r/min，整机外形尺寸（长×宽×高）mm：1610×1060×950，工作幅宽1050mm，发动机输出传动方式：直联，旋耕刀型式：旱地刀，主离合器型式：摩擦片式。","700","T201950500272","2024-12-25","3200.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","广西玉林市德高机械有限公司","前置微耕机","1WG4.0-60","配套功率:4.0kW;","外形尺寸:1800*650*1080；耕宽:600mm；结构质量:70kg；传动方式:皮带传动；旋耕刀型号:PIT160；旋耕刀片总数量18把；刀辊最大回转半径160mm；主离合器型式:摩擦片式；结构形式:前置式.","700","TJ2018025","2022-12-31","3200.00","","非通用类","广西壮族自治区","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","广西玉林市德高机械有限公司","前置微耕机","1WG7.5-100","配套功率:7.5kW;","外形尺寸:2030*1050*1200；耕宽:1000mm；结构质量:365kg；传动方式:皮带传动；旋耕刀型号:IIIS180；旋耕刀片总数量32把；刀辊最大回转半径160mm；主离合器型式:摩擦片式；结构形式:前置式.","700","TJ2018026","2022-12-31","13800.00","","非通用类","广西壮族自治区","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","广西玉林市德高机械有限公司","前置微耕机","1WG5.9-80","配套功率:5.9kW;","外形尺寸:1850*850*1040；耕宽:800mm；结构质量:150kg；传动方式:皮带传动；旋耕刀型号:PIT180；旋耕刀片总数量24把；刀辊最大回转半径180mm；主离合器型式:摩擦片式；结构形式:前置式.","700","TJ2018018","2022-12-31","3800.00","","非通用类","广西壮族自治区","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆市美琪工业制造有限公司","微耕机","1WG4.0-100FQ-ZC","配套功率:4.0kW;","配套发动机:170F汽油机；额定功率:4.0KW；外形尺寸(MM):1540×1030×1030；结构形式：手持式；作业速度：m/s0.1～0.3；结构质量:70KG；传动方式:齿轮传动；连接方式:直联；旋耕刀型号:旱地刀；总安装刀数:24把；作业小时生产率:≥0.04HM2/(H·M)；单位作业面积燃油消耗量:≤35KG/HM2；耕宽1000MM。","700","T202050500017","2025-03-11","4100.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆芸析机械制造有限公司","微耕机","1WGFQD4.0-60-1","配套功率:4.0kW;","工作状态外形尺寸（长×宽×高）mm:1300×640×950;\n作业速度m/s:0.05～0.2;\n作业小时生产率hm2/(h·m):≥0.02;\n单位作业面积燃油消耗量kg/hm2:≤35;\n工作幅宽mm:600;","700","T202050500037","2025-03-11","1950.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆芸析机械制造有限公司","微耕机","1WG4.0-90FQ-ZCS","配套功率:4.0kW;","工作状态外形尺寸（长×宽×高）mm:1600×910×940;\n作业速度m/s:0.1～0.3;\n作业小时生产率hm2/(h·m):≥0.04;\n单位作业面积燃油消耗量kg/hm2:≤35;\n工作幅宽mm:900;\n设计转速r/min:140","700","T202050500023","2025-03-11","2200.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆源顺进机械制造有限公司","微耕机","1WG6.3-135FC-ZC","配套功率:6.3kW;","配套发动机标定功率：6.3KW、标定转速：3600r/min、起动方式：手拉起动、燃油种类：柴油、工作幅宽1350mm","700","T201950500232","2024-11-12","4500.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，推广鉴定报告不规范","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","洛阳精匠机械有限公司","微耕机","1WGQ4-90B","配套功率:4kW;","发动机厂家：隆鑫通用动力股份有限公司     发动机型号：LC1P70F-3型  汽油发动机   功率：4Kw、整机外形尺寸（长×宽×高）: 1350mm×910mm×880mm、配套发动机标定转速:3600r/min、启动方式：手拉反冲、工作幅宽: 900mm、扶把调整幅度（水平方向）：90度、扶把调整幅度（垂直方向）:75度、发动机输出传动方式：齿轮、刀辊传动方式：齿轮、刀辊设计转速：225r/min、刀辊最大回转半径：150mm、刀辊总安装刀数：24把、旋耕刀型式：刀盘式、主离合器状态：离心式、主离合器状态：常开","700","T202041410097","2025-06-29","3100.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆艾铭玛机械制造有限公司","微耕机","1WG4.0-90FQ-DLA","配套功率:4.0kW;","外形尺寸（长×宽×高)mm：1550×900×900；工作幅宽(cm)90；结构质量（kg）：70；传动方式（发动机输出）：皮带传动；发动机功率：4.0KW；传动方式（刀辊）：链条传动；旋耕刀型号：II型旱地刀；总安装刀数量(把)：24；主离合器型式：张紧轮式。","700","T201950500245","2024-11-12","2850.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆铭宸机械制造有限公司","微耕机","1WGCZ4.0-95","配套功率:4.05kW;","项目\t单位\t设计值\n型号名称\t/\t1WGCZ4.0-95 微耕机\n结构型式\t/\t手持式\n配套发动机标定功率\tkW\t4.05\n配套发动机标定转速\tr/min\t3600\n配套发动机起动方式\t/\t手拉起动\n配套发动机燃油种类\t/\t柴油\n整机外形尺寸（长×宽×高）\tmm\t1500×960×930\n作业速度\tm/s\t0.1～0.3\n扶把振动\tm/s2\t≤50\n作业小时生产率\thm2/(h·m)\t≥0.04\n单位作业面积燃油消耗量\tkg/hm2\t≤30\n工作幅宽\tmm\t950\n发动机输出传动方式\t/\t直联\n刀辊传动方式\t/\t齿轮传动\n扶把调整幅度（水平方向）\t（º）\t0\n扶把调整幅度（垂直方向）\t（º）\t125\n刀辊设计转速\tr/min\t快挡：146；慢挡：90\n刀辊最大回转半径\tmm\t160\n刀辊总安装刀数\t/\t24\n旋耕刀型式\t/\t防缠刀\n主离合器型式\t/\t摩擦片式\n主离合器状态\t/\t常开","700","T202050500121","2025-06-21","4000.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆铭宸机械制造有限公司","微耕机","1WGCZ5.3-106","配套功率:5.3kW;","项目\t单位\t设计值\n型号名称\t/\t1WGCZ5.3-106 微耕机\n结构型式\t/\t手持式\n配套发动机标定功率\tkW\t5.3\n配套发动机标定转速\tr/min\t3000\n配套发动机起动方式\t/\t手拉起动\n配套发动机燃油种类\t/\t柴油\n整机外形尺寸（长×宽×高）\tmm\t1730×1070×1030\n作业速度\tm/s\t0.1～0.3\n扶把振动\tm/s2\t≤50\n作业小时生产率\thm2/(h·m)\t≥0.04\n单位作业面积燃油消耗量\tkg/hm2\t≤30\n工作幅宽\tmm\t1060\n发动机输出传动方式\t/\t直联\n刀辊传动方式\t/\t齿轮传动\n扶把调整幅度（水平方向）\t（º）\t0\n扶把调整幅度（垂直方向）\t（º）\t120\n刀辊设计转速\tr/min\t快挡：134；慢挡：76\n刀辊最大回转半径\tmm\t190\n刀辊总安装刀数\t/\t24\n旋耕刀型式\t/\t防缠刀\n主离合器型式\t/\t摩擦片式\n主离合器状态\t/\t常开","700","T202050500120","2025-06-21","4400.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆铭宸机械制造有限公司","微耕机","1WGCZ4.1-106","配套功率:4.1kW;","项目\t单位\t设计值\n型号名称\t/\t1WGCZ4.1-106 微耕机\n结构型式\t/\t手持式\n配套发动机标定功率\tkW\t4.1\n配套发动机标定转速\tr/min\t3600\n配套发动机起动方式\t/\t手拉起动\n配套发动机燃油种类\t/\t柴油\n整机外形尺寸（长×宽×高）\tmm\t1660×1070×1000\n作业速度\tm/s\t0.1～0.3\n扶把振动\tm/s2\t≤50\n作业小时生产率\thm2/(h·m)\t≥0.04\n单位作业面积燃油消耗量\tkg/hm2\t≤30\n工作幅宽\tmm\t1060\n发动机输出传动方式\t/\t直联\n刀辊传动方式\t/\t齿轮传动\n扶把调整幅度（水平方向）\t（º）\t0\n扶把调整幅度（垂直方向）\t（º）\t85\n刀辊设计转速\tr/min\t快挡：145；慢挡：90\n刀辊最大回转半径\tmm\t190\n刀辊总安装刀数\t/\t24\n旋耕刀型式\t/\t防缠刀\n主离合器型式\t/\t摩擦片式\n主离合器状态\t/\t常开","700","T202050500123","2025-06-21","4200.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆铭宸机械制造有限公司","微耕机","1WGCZ6.3-106","配套功率:6.3kW;","项目\t单位\t设计值\n型号名称\t/\t1WGCZ6.3-106 微耕机\n结构型式\t/\t手持式\n配套发动机标定功率\tkW\t6.3\n配套发动机标定转速\tr/min\t3600\n配套发动机起动方式\t/\t手拉起动\n配套发动机燃油种类\t/\t柴油\n整机外形尺寸（长×宽×高）\tmm\t1730×1070×1015\n作业速度\tm/s\t0.1～0.3\n扶把振动\tm/s2\t≤30\n作业小时生产率\thm2/(h·m)\t≥0.04\n单位作业面积燃油消耗量\tkg/hm2\t≤30\n工作幅宽\tmm\t1060\n发动机输出传动方式\t/\t直联\n刀辊传动方式\t/\t齿轮传动\n扶把调整幅度（水平方向）\t（º）\t0\n扶把调整幅度（垂直方向）\t（º）\t120\n刀辊设计转速\tr/min\t快挡：135；慢挡：78\n刀辊最大回转半径\tmm\t190\n刀辊总安装刀数\t/\t24\n旋耕刀型式\t/\t防缠刀\n主离合器型式\t/\t摩擦片式\n主离合器状态\t/\t常开","700","T202050500122","2025-06-21","4500.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆铭宸机械制造有限公司","微耕机","1WG4.0-95FQ-D","配套功率:4.0kW;","项目\t单位\t设计值\n型号名称\t/\t1WG4.0-95FQ-D微耕机\n结构型式\t/\t手持式\n配套发动机标定功率\tkW\t4\n配套发动机标定转速\tr/min\t3600\n配套发动机起动方式\t/\t手拉起动\n配套发动机燃油种类\t/\t汽油\n整机外形尺寸（长×宽×高）\tmm\t1500×960×850\n作业速度\tm/s\t0.1～0.3\n扶把振动\tm/s2\t≤50\n作业小时生产率\thm2/(h·m)\t≥0.04\n单位作业面积燃油消耗量\tkg/hm2\t≤35\n工作幅宽\tmm\t950\n发动机输出传动方式\t/\t皮带传动\n刀辊传动方式\t/\t链条传动\n扶把调整幅度（水平方向）\t（º）\t0\n扶把调整幅度（垂直方向）\t（º）\t200\n刀辊设计转速\tr/min\t快挡：140；慢挡：100\n刀辊最大回转半径\tmm\t180\n刀辊总安装刀数\t/\t24\n旋耕刀型式\t/\t旱地刀\n主离合器型式\t/\t张紧轮式\n主离合器状态\t/\t常开","700","T202050500022","2025-03-11","3350.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆铭宸机械制造有限公司","微耕机","1WG4.0-95FQ-ZCA","配套功率:4.0kW;","项目\t单位\t设计值\n型号名称\t/\t1WG4.0-95FQ-ZCA微耕机\n结构型式\t/\t手持式\n配套发动机标定功率\tkW\t4\n配套发动机标定转速\tr/min\t3600\n配套发动机起动方式\t/\t手拉起动\n配套发动机燃油种类\t/\t汽油\n整机外形尺寸（长×宽×高）\tmm\t1560×960×950\n作业速度\tm/s\t0.1～0.3\n扶把振动\tm/s2\t≤50\n作业小时生产率\thm2/(h·m)\t≥0.04\n单位作业面积燃油消耗量\tkg/hm2\t≤35\n工作幅宽\tmm\t950\n发动机输出传动方式\t/\t直联\n刀辊传动方式\t/\t齿轮传动\n扶把调整幅度（水平方向）\t（º）\t0\n扶把调整幅度（垂直方向）\t（º）\t210\n刀辊设计转速\tr/min\t140\n刀辊最大回转半径\tmm\t180\n刀辊总安装刀数\t/\t24\n旋耕刀型式\t/\t旱地刀\n主离合器型式\t/\t摩擦片式\n主离合器状态\t/\t常开","700","T202050500021","2025-03-11","3420.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆渝奥农业机械有限公司","微耕机","1WG4.05-90FC-ZC","配套功率:4.05kW;","1  型号名称：1WG4.05-90FC-ZC微耕机；2 结构型式:手持式; 3 配套发动机标定功率：4.05(KW); 4 配套发动机标定转速： 3600r/min  ；5  配套发动机起动方式：手拉起动 ；6  配套发动机燃油种类：柴油；  7 整机外形尺寸（长×宽×高）：1500×910×980（mm）  ；8  作业速度：0.1～0.3（m/s）；9 扶把振动：≤50（m/s2）； 10 作业小时生产率：≥0.04hm2/(h·m)；11 单位作业面积燃油消耗量：≤30kg/hm2；12  工作幅宽：900mm；13 发动机输出传动方式：直联；14 刀辊传动方式：齿轮传动；15 扶把水平方向调整幅度：0（º）；16 扶把垂直方向调整幅度：150（º）；17  刀辊设计转速：快档：125r/min；慢档：85r/min；18 刀辊最大回转半径：180mm; 19  刀辊总安装刀数:24把； 20 旋耕刀型式：旱地刀 ；21  主离合器型式：摩擦片式； 22  主离合器状态：常开； 23  水田轮结构型式：叶片式； 24  水田轮直径：360mm","700","渝2019147","2023-12-31","2340.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆渝奥农业机械有限公司","微耕机","1WG5.3-135FC-ZC","配套功率:5.3kW;","1  型号名称：1WG5.3-135FC-ZC微耕机；2 结构型式:手持式; 3 配套发动机标定功率：5.3(KW); 4 配套发动机标定转速： 3000r/min  ；5  配套发动机起动方式：手拉起动 ；6  配套发动机燃油种类：柴油；  7 整机外形尺寸（长×宽×高）：1750×1360×10200（mm）  ；8  作业速度：0.1～0.3（m/s）；9 扶把振动：≤50（m/s2）； 10 作业小时生产率：≥0.04hm2/(h·m)；11 单位作业面积燃油消耗量：≤30kg/hm2；12  工作幅宽：1350mm；13 发动机输出传动方式：直联；14 刀辊传动方式：齿轮传动；15 扶把水平方向调整幅度：0（º）；16 扶把垂直方向调整幅度：120（º）；17  刀辊设计转速：快档：120r/min；慢档：100r/min；18 刀辊最大回转半径：180mm; 19  刀辊总安装刀数:38把； 20 旋耕刀型式：旱地刀 ；21  主离合器型式：摩擦片式； 22  主离合器状态：常开； 23  水田轮结构型式：叶片式； 24  水田轮直径：375mm","700","渝2019149","2023-12-31","2340.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆渝奥农业机械有限公司","微耕机","1WG4.0-100FQ-ZC","配套功率:4.0kW;","1 型号名称:1WG4.0-100FQ-ZC微耕机； 2 结构型式：手持式； 3 配套发动机标定功率：4.0KW; 4 配套发动机标定转速：3600r/min； 5 配套发动机起动方式：手拉起动； 6  配套发动机燃油种类：汽油； 7  整机外形尺寸（长×宽×高）：1475×1010×980（mm）；8 作业速度：0.1～0.3（m/s）；9 扶把振动：≤50m/s2；10 作业小时生产率：≥0.04hm2/(h·m)；11 单位作业面积燃油消耗量：≤35kg/hm2；12 工作幅宽：1000mm； 13 发动机输出传动方式：直联；14 刀辊传动方式：齿轮传动；15 扶把水平方向调整幅度：0（º）；16 扶把垂直方向调整幅度：150（º）；17 刀辊设计转速：快档：125r/min；慢档：85r/min；18 刀辊最大回转半径： 180mm； 19  刀辊总安装刀数：24；20 旋耕刀型式：旱地刀；21 主离合器型式：摩擦片式；22  主离合器状态：常开；23  水田轮结构型式：叶片式；24  水田轮直径：360mm","700","渝2019150","2023-12-31","2334.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆渝奥农业机械有限公司","微耕机","1WG4.0-90FQ-ZCA","配套功率:4.0kW;","1 型号名称:1WG4.0-90FQ-ZCA微耕机； 2 结构型式：手持式； 3 配套发动机标定功率：4.0KW; 4 配套发动机标定转速：3600r/min； 5 配套发动机起动方式：手拉起动； 6  配套发动机燃油种类：汽油； 7 整机外形尺寸（长×宽×高）：1475×910×880（mm）；8 作业速度：0.1～0.3（m/s）；9 扶把振动：≤50m/s2；10 作业小时生产率：≥0.04hm2/(h·m)；11 单位作业面积燃油消耗量：≤35kg/hm2；12 工作幅宽：900mm； 13 发动机输出传动方式：直联；14 刀辊传动方式：齿轮传动；15 扶把水平方向调整幅度：0（º）；16 扶把垂直方向调整幅度：140（º）；17 刀辊设计转速：快档：150r/min；18 刀辊最大回转半径： 180mm； 19  刀辊总安装刀数：24；20 旋耕刀型式：旱地刀；21 主离合器型式：离心式；22  主离合器状态：常开；23 水田轮结构型式：叶片式；24 水田轮直径：360mm","700","渝2019148","2023-12-31","2334.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆渝奥农业机械有限公司","微耕机","1WGQZ4.0-90A","配套功率:4.0kW;","1型号名称:1WGCZ4.0-90A微耕机;2结构型式:手持式;3配套发动机型号名称:AH170F/P汽油机;4配套发动机生产企业:;重庆奥虎机电制造有限公司5配套发动机标定功率:4.0kW;6配套发动机标定转速:3600r/min;7配套发动机起动方式:手拉起动;8配套发动机燃油种类:汽油;9整机外形尺寸（长×宽×高）:1450×920×950mm;10作业速度:0.1～0.3m/s;11扶把振动:≤50m/s2;12作业小时生产率：≥0.04hm2/(h·m)；13单位作业面积燃油消耗量：≤35；14工作幅宽：900；15发动机输出传动方式：直联；16刀辊传动方式：齿轮传动；17扶把调整幅度（水平方向）：0（º）；18扶把调整幅度（垂直方向）：190（º）；19刀辊设计转速：150r/min；20刀辊最大回转半径：160mm；21刀辊总安装刀数:24;22旋耕刀型号:旱地刀;23主离合器型式:摩擦片式;24主离合器状态:常开。","700","T202050500063","2025-05-10","2367.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆渝奥农业机械有限公司","微耕机","1WGCZ4.1-102","配套功率:4.1kW;","1型号名称:1WGCZ4.1-102微耕机;2结构型式:手持式;3配套发动机型号名称:KAGS350柴油机;4配套发动机生产企业:;无锡凯奥动力机械有限公司；5配套发动机标定功率:4.1kW;6配套发动机标定转速:3600r/min;7配套发动机起动方式:手拉起动;8配套发动机燃油种类:柴油;9整机外形尺寸（长×宽×高）:1770×1030×1020mm;10作业速度:0.1～0.3m/s;11扶把振动:≤50m/s2;12作业小时生产率：≥0.04hm2/(h·m)；13单位作业面积燃油消耗量：≤30；14工作幅宽：1020；15发动机输出传动方式：直联；16刀辊传动方式：齿轮传动；17扶把调整幅度（水平方向）：0（º）；18扶把调整幅度（垂直方向）：95（º）；19刀辊设计转速：快档：120r/min；慢档：70r/min；20刀辊最大回转半径：180mm；21刀辊总安装刀数:24;22旋耕刀型号:旱地刀;23主离合器型式:摩擦片式;24主离合器状态:常开。","700","T202050500062","2025-05-10","3000.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆渝奥农业机械有限公司","微耕机","1WGCZ4.05-90","配套功率:4.05kW;","1型号名称:1WGCZ4.05-90微耕机;2结构型式:手持式;3配套发动机型号名称:KM173FAD柴油机;4配套发动机生产企业:无锡华源凯马发动机有限公司;5配套发动机标定功率:4.05kW;6配套发动机标定转速:3600r/min;7配套发动机起动方式:手拉起动;8配套发动机燃油种类:柴油;9整机外形尺寸（长×宽×高）:1450×920×950mm;10作业速度:0.1～0.3m/s;11扶把振动:≤50m/s2;12作业小时生产率：≥0.04hm2/(h·m)；13单位作业面积燃油消耗量：≤30；14工作幅宽：900；15发动机输出传动方式：直联；16刀辊传动方式：齿轮传动；17扶把调整幅度（水平方向）：0（º）；18扶把调整幅度（垂直方向）：190（º）；19刀辊设计转速：130r/min；20刀辊最大回转半径：160mm；21刀辊总安装刀数:24;22旋耕刀型号:旱地刀;23主离合器型式:摩擦片式;24主离合器状态:常开.","700","T202050500060","2025-05-10","3000.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆渝奥农业机械有限公司","微耕机","1WG4.0-60FQ-DL","配套功率:4.0kW;","1型号名称:1WG4.0-60FQ-DL微耕机;2结构型式:手持式;3配套发动机型号名称:AH170F/P汽油机;4配套发动机生产企业:;重庆奥虎机电制造有限公司5配套发动机标定功率:4.0kW;6配套发动机标定转速:3600r/min;7配套发动机起动方式:手拉起动;8配套发动机燃油种类:汽油;9整机外形尺寸（长×宽×高）:1360×700×880；10作业速度:0.05～0.2m/s；11扶把振动:≤50m/s2;12作业小时生产率：≥0.02hm2/(h·m)；13单位作业面积燃油消耗量：≤35；14工作幅宽：600；15发动机输出传动方式：皮带传动；16刀辊传动方式：链条传动；17扶把调整幅度（水平方向）：0（º）；18扶把调整幅度（垂直方向）：50（º）；19刀辊设计转速：340r/min；20刀辊最大回转半径：180mm；21刀辊总安装刀数:24;22旋耕刀型号:旱地刀;3主离合器型式:摩擦片式;24主离合器状态:常开","700","T202050500061","2025-05-10","2367.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆美多盈机械有限公司","微耕机","1WG4.0-75FQ-DC","配套功率:4.0kW;","结构型式：手持式；配套发动机标定功率kW：4.0；配套发动机标定转速r/min：3600；配套发动机起动方式：手拉起动；配套发动机燃油种类：汽油；整机外形尺寸（长×宽×高）mm：1500×760×850；作业速度m/s：0.1～0.3；工作幅宽mm：750；发动机输出传动方式：皮带传动；刀辊传动方式：齿轮传动；刀辊总安装刀数：18把；旋耕刀型式：旱地刀；主离合器型式：张紧轮式；","700","T201950500128","2024-09-09","2800.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆美多盈机械有限公司","微耕机","1WG4.0-95FQ-ZC","配套功率:4.0kW;","结构型式：手持式；配套发动机标定功率kW：4.0；配套发动机标定转速r/min：3600；配套发动机起动方式：手拉起动；配套发动机燃油种类：汽油；整机外形尺寸（长×宽×高）mm：1600×960×1000；作业速度m/s：0.1～0.3；工作幅宽mm：950；发动机输出传动方式：直联；刀辊传动方式：齿轮传动；刀辊总安装刀数：24把；旋耕刀型式：旱地刀；主离合器型式：摩擦片式；主离合器状态：常开；","700","T201950500124","2024-09-09","2800.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆美多盈机械有限公司","微耕机","1WG6.3-135FC-ZC","配套功率:6.3kW;","结构型式：手持式；配套发动机标定功率kW：6.3；配套发动机标定转速r/min：3600；配套发动机起动方式：手拉起动；配套发动机燃油种类：柴油；工作状态外形尺寸（长×宽×高）mm：1640×1360×980；作业速度m/s：0.1～0.3；工作幅宽mm：1350；发动机输出传动方式：直联；刀辊传动方式：齿轮传动；刀辊总安装刀数：38把；旋耕刀型号：旱地刀；主离合器型式：摩擦片式；主离合器状态：常开；","700","T201950500125","2024-09-09","3000.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆美多盈机械有限公司","微耕机","1WG5.3-135FC-ZC","配套功率:5.3kW;","结构型式：手持式；配套发动机标定功率kW：5.3；配套发动机标定转速r/min：3000；配套发动机起动方式：手拉起动；配套发动机燃油种类：柴油；整机外形尺寸（长×宽×高）mm：1640×1360×980；作业速度m/s：0.1～0.3；工作幅宽mm：1350；发动机输出传动方式：直联；刀辊传动方式：齿轮传动；刀辊总安装刀数：38把；旋耕刀型式：旱地刀；主离合器型式：摩擦片式；主离合器状态：常开；","700","T201950500127","2024-09-09","3000.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["耕整地机械","耕地机械","微耕机","功率4kW及以上微耕机","重庆美多盈机械有限公司","微耕机","1WG4.1-105FC-ZC","配套功率:4.1kW;","结构型式：手持式；配套发动机标定功率kW：4.1；配套发动机标定转速r/min；3600；配套发动机起动方式：手拉起动；配套发动机燃油种类：柴油；整机外形尺寸（长×宽×高）mm：1620×1060×980；作业速度m/s：0.1～0.3；工作幅宽mm：1050；发动机输出传动方式：直联；刀辊传动方式：齿轮传动；刀辊总安装刀数：32把；旋耕刀型式：旱地刀；主离合器型式：摩擦片式；主离合器状态：常开；","700","T201950500126","2024-09-09","3000.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["种植施肥机械","播种机械","条播机","7-11行条播机","任丘市超鹰农机有限公司","小麦施肥播种机","2BXF-9","播种行数:9行;","2BXF-9小麦施肥播种机，机械式、悬挂式结构型式，13.2～29.4kW配套动力，整机外形尺寸（长×宽×高）：1930×1850×1180mm，1.1～1.7m/s作业速度范围，0.5～0.7hm2/h作业小时生产率，工作幅宽135cm，行距15cm，工作行数9行，9个槽轮式（非金属材料）排肥器，9个槽轮式（非金属材料）排种器，9个双圆盘式排种开沟器，9个双圆盘式排肥开沟器，20～50mm排肥/种开沟器深度调节范围，种/肥箱容积75/75L，排量调节方式：种：档位+螺纹 肥：螺纹，播种部分传动方式：轴+链条传动，310mm直径滚笼式地轮，0～50mm地轮高度调节范围,刮板式覆土器，轮式镇压器","670","T201913130262","2024-12-30","3200.00","","非通用类","河北省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期，铭牌放置不明确","","","","",""]
["种植施肥机械","播种机械","条播机","12-18行条播机","任丘市超鹰农机有限公司","小麦施肥播种机","2BXF-16","播种行数:16行;","2BXF-16小麦施肥播种机，机械式、悬挂式结构型式，36.8～58.8kW配套动力，整机外形尺寸（长×宽×高）：1930×2780×1180mm，1.1～1.7m/s作业速度范围，1～1.2hm2/h作业小时生产率，工作幅宽240cm，行距15cm，工作行数16行，16个槽轮式（非金属材料）排肥器，16个槽轮式（非金属材料）排种器，16个双圆盘式排种开沟器，16个双圆盘式排肥开沟器，20～50mm排肥/种开沟器深度调节范围，种/肥箱容积125/125L，排量调节方式：种：档位+螺纹 肥：螺纹，播种部分传动方式：轴+链条传动，310mm直径滚笼式地轮，0～50mm地轮高度调节范围,刮板式覆土器，轮式镇压器。","890","T201913130263","2024-12-30","5700.00","","非通用类","河北省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["种植施肥机械","播种机械","条播机","12-18行条播机","任丘市超鹰农机有限公司","小麦施肥播种机","2BXF-14","播种行数:14行;","2BXF-14小麦施肥播种机，机械式、悬挂式结构型式，22～36.8kW配套动力，整机外形尺寸（长×宽×高）：1930×2580×1180mm，1.1～1.7m/s作业速度范围，0.8～1hm2/h作业小时生产率，工作幅宽210cm，行距15cm，工作行数14行，14个槽轮式（非金属材料）排肥器，14个槽轮式（非金属材料）排种器，14个双圆盘式排种开沟器，14个双圆盘式排肥开沟器，20～50mm排肥/种开沟器深度调节范围，种/肥箱容积115/115L，排量调节方式：种：档位+螺纹 肥：螺纹，播种部分传动方式：轴+链条传动，310mm直径滚笼式地轮，0～50mm地轮高度调节范围,刮板式覆土器，轮式镇压器。","890","T201913130263","2024-12-30","4750.00","","非通用类","河北省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["种植施肥机械","播种机械","条播机","12-18行条播机","任丘市超鹰农机有限公司","小麦施肥播种机","2BXF-12","播种行数:12行;","2BXF-12小麦施肥播种机，机械式、悬挂式结构型式，22～36.8kW配套动力，整机外形尺寸（长×宽×高）：1930×2180×1180mm，1.1～1.7m/s作业速度范围，0.7～0.8hm2/h作业小时生产率，工作幅宽180cm，行距15cm，工作行数12行，12个槽轮式（非金属材料）排肥器，12个槽轮式（非金属材料）排种器，12个双圆盘式排种开沟器，12个双圆盘式排肥开沟器，20～50mm排肥/种开沟器深度调节范围，种/肥箱容积95/95L，排量调节方式：种：档位+螺纹 肥：螺纹，播种部分传动方式：轴+链条传动，310mm直径滚笼式地轮，0～50mm地轮高度调节范围,刮板式覆土器，轮式镇压器","890","T201913130262","2024-12-30","4100.00","","非通用类","河北省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["种植施肥机械","播种机械","条播机","19-24行条播机","石家庄农业机械股份有限公司","施肥播种机","2BFX-24","播种行数:24行;","配套动力范围\t55～74\tkW\n外形尺寸（长×宽×高）\t2320×3900×1445\tmm\n结构质量\t1080\tkg\n行距\t15\tcm\n工作行数\t24\t行\n工作幅宽\t360\tcm\n传动机构形式\t链传动\t\n排种器型式\t铁制外槽轮\t\n排种器数量\t24\t个\n排肥器型式\t外槽轮\t\n排肥器数量\t24\t个\n开沟器型式\t双轴承双圆盘式\t\n地轮型式\t橡胶充气轮胎\t\n地轮直径\t68\tcm\n覆土器型式：覆土环\n与配套拖拉机联接方式\t三点悬挂","4400","冀2018T—267（续）","2022-12-31","30000.00","","非通用类","河北省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["种植施肥机械","播种机械","条播机","25行及以上条播机","石家庄农业机械股份有限公司","施肥播种机","2BF-36","播种行数:36行;","结构型式：机械式、牵引式\n配套动力范围：55.1～132.3\tkW\n外形尺寸（长×宽×高）\t4120×7460×2500\tmm\n作业速度范围：1.67-2.78m/s\n作业小时生产率：3.24-5.4hm2/h\n工作幅宽\t540\tcm\n行距\t15\tcm\n工作行数\t36\t行\n排种器型式\t槽轮式、金属材料\n排种器数量\t36\t个\n排肥器型式\t槽轮式、金属材料\t\n排肥器数量\t36\t个\n排种开沟器型式：双圆盘式\n排种开沟器数量  36个\n排种开沟器深度调节范围：30-80mm\n排肥开沟器型式：双圆盘式\n排肥开沟器数量  36个\n排肥开沟器深度调节范围：30-80mm\n种/肥箱容积\t920/850\tL\n排量调节方式：手柄调节\n结构质量\t2250\tkg\n排种部分传动方式：\t链传动\t\n地轮型式\t充气轮胎\n地轮直径\tφ900mm\n覆土器型式\t覆土环\n镇压器型式\t覆土环","6600","T201913130257","2024-12-30","52000.00","","非通用类","河北省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["种植施肥机械","播种机械","免耕播种机","2-3行免耕穴播机","宁津县奥华农业机械有限公司","玉米免耕施肥播种机","2BMYF-3","播种行数:3行;播种形式:免耕穴播 ;","外形尺寸（长*宽*高）（mm)：1700*1720*1200mm；结构质量kg:280kg;行距mm:450-650;工作行数：3行；工作幅宽mm:1350-1950；排种器型式：勺盘式，金属材料；排种器数量：3个 ；排肥器型式：外槽轮式；排肥器数量：3个；地轮型式：橡胶轮；地轮直径mm：370mm；传动机构型式：传动轴；开沟器型式：尖铲式；配套动力范围：14.7-29.4kW","900","T201937370008","2024-08-08","3800.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过,承诺书过期。","","","","",""]
["种植施肥机械","播种机械","免耕播种机","2-3行免耕穴播机","宁津县奥华农业机械有限公司","玉米免耕施肥播种机","2BMYF-2","播种行数:2行;播种形式:免耕穴播 ;","外形尺寸（长*宽*高）（mm)：1720*1200*1200mm；结构质量kg:180kg;行距mm:450-700;工作行数：2行；工作幅宽mm:900-1400；排种器型式：勺盘式，金属材料；排种器数量：2个 ；排肥器型式：外槽轮式；排肥器数量：2个；地轮型式：橡胶轮；地轮直径370mm；传动机构型式：传动轴；开沟器型式：尖铲式；配套动力范围：14.7-29.4kW","900","T201937370008","2024-08-08","3200.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期。","","","","",""]
["种植施肥机械","播种机械","免耕播种机","4-5行免耕穴播机","宁津县奥华农业机械有限公司","玉米免耕施肥播种机","2BMYF-4","播种行数:4行;播种形式:免耕穴播 ;","外形尺寸（长*宽*高）（mm)：1760*2460*1210mm；结构质量kg:370kg;行距mm:500-680;工作行数：4行；工作幅宽mm:2000-2720；排种器型式：勺盘式，金属材料；排种器数量：4个 ；排肥器型式：外槽轮式；排肥器数量：4个；地轮型式：橡胶轮；地轮直径mm：370mm；传动机构型式：传动轴；开沟器型式：尖铲式；配套动力范围：29.4-95.6kW","1600","T201900370165","2024-11-28","5800.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期。","","","","",""]
["种植施肥机械","播种机械","免耕播种机","2-3行免耕精量穴播机","吉林省隆博农业发展有限公司","免耕指夹式精量施肥播种机","2BMZF-2","播种行数:2行;播种形式:免耕精量穴播 ;","型号名称:2BMZF-2型；结构型式:机械式、牵引式；配套动力范围:37-48kW；整机外形尺寸（mm）:3200*2000*1600；作业速度范围:6-8km/h；作业小时生产率:0.5-1.2hm^2/h；行距:400mm-700mm（可调）；工作行数:2；作业幅宽:800mm-1400mm；排种器型式:  指夹式；排种器数量:2；排种器驱动方式:链条；排肥器型式:双搅龙；排肥器数量:2；排肥器驱动方式:链条；种/肥箱容积:65L/200L；种/肥排量调节方式:链轮；传动机构型式:上置链条传动；开沟器型式:双圆盘；开沟器数量:2；开沟器深度调节范围:30mm-100mm；地轮型式:胶轮；地轮直径:700mm；覆土器型式:V型设置窄空心橡胶轮；镇压器型式:V型设置窄空心橡胶轮。","1000","T202022220073","2025-05-28","35000.00","","通用类","吉林省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["种植施肥机械","播种机械","免耕播种机","2-3行免耕精量穴播机","灵璧县泰顺机械有限公司","免耕指夹式精量施肥播种机","2BMZF-2","播种行数:2行;播种形式:免耕精量穴播 ;","型号;2BMZF-2、结构型式;牵引式、配套动力范围;22~37(kw)、工作状态外形尺寸;3080*2080*1480(mm)、作业速度范围;6~8(km/h)、作业小时生产率;0.6~0.8(km2/h)、行距;600(mm)、工作行数;2行、工作幅宽;1.2m,、排钟器型式;指夹式、排种器数量;2个、排种器驱动方式;充气橡胶地轮、排肥器型式;前;搅龙式、后;外槽轮式、排肥器;前2个、后2个、排肥器驱动方式;充气橡胶地轮、种肥箱容积;90/210(L)、排量调节方式;前排肥;链轮组合调节;排种;链轮组合调节、传动机构型式;链轮链条、开沟器;型式;豁口单圆盘切刀式、数量;2个、深度调节范围30~100(mm)、地轮;型式;充气橡胶轮、直径;700(mm)、破茬清垄工作部件型式;除茬圆盘刀+拨草轮、破土器型式;铁轮毂橡胶轮、镇压器型式;V型对置窄橡胶轮","1000","2019TJ253","2023-12-31","28000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["种植施肥机械","播种机械","免耕播种机","4-5行免耕精量穴播机","吉林省隆博农业发展有限公司","免耕指夹式精量施肥播种机","2BMZF-5","播种行数:5行;播种形式:免耕精量穴播 ;","型号名称:2BMZF-5型；结构型式:机械式、牵引式；配套动力范围:≥48kW；整机外形尺寸（mm）:3760*4660*1850；作业速度范围:6-8km/h；作业小时生产率:1.5-3hm^2/h；行距:500mm-750mm（可调）；工作行数:5；作业幅宽:2500mm-3750mm；排种器型式:  指夹式；排种器数量:5；排种器驱动方式:链条；排肥器型式:双搅龙；排肥器数量:5；排肥器驱动方式:链条；种/肥箱容积:163L/500L；种/肥排量调节方式:链轮；传动机构型式:上置链条传动；开沟器型式:双圆盘；开沟器数量:5；开沟器深度调节范围:30mm-100mm；地轮型式:胶轮；地轮直径:700mm；覆土器型式:V型设置窄空心橡胶轮；镇压器型式:V型设置窄空心橡胶轮。","1600","T202000220141","2025-07-05","100000.00","","通用类","吉林省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["种植施肥机械","播种机械","水稻直播机","8行及以上水稻精量穴播机","泰州樱田农机制造有限公司","水稻精量穴播机","2BD-830","播种行数:8行;播种形式:播量可调,穴直播 ;","配套动力范围（kW）：≥8kW(配高速乘座式插秧机)；外形尺寸（工作状态，长 ×宽×高)mm：2560x800×1700；结构质量（kg）：126；行距 （cm）：30；；工作行数：8；工作幅宽（cm）：240；传动机构型式：中间轴传动；排种器型式：轮槽式；排种器数量：8；种子箱容积：8x5L。","8400","苏农机（2018）第（0267）号","2022-12-31","31000.00","","非通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["种植施肥机械","播种机械","水稻直播机","8行及以上水稻精量穴播机","泰州樱田农机制造有限公司","水稻精量穴播机","2BD-1025","播种行数:10行;播种形式:播量可调,穴直播 ;","配套动力范围（kW）：≥8kW(配高速乘座式插秧机)；外形尺寸（工作状态，长 ×宽×高)mm：2660x800×1700；结构质量（kg）：134；行距 （cm）：25；；工作行数：10；工作幅宽（cm）：250；传动机构型式：中间轴传动；排种器型式：轮槽式；排种器数量：10；种子箱容积：10x10L。","8400","苏农机（2018）第（0330）号","2022-12-31","32000.00","","非通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过","","","","",""]
["种植施肥机械","播种机械","精量播种机","2-3行精量播种机","河北峥嵘农机有限公司","玉米施肥精量播种机","2BYCF-2","播种行数:2行;是否精量播种:否 ;","结构型式：机械式、悬挂式整机外形尺寸（长*宽*高）mm:1720*1260*1180 配套动力范围KW：11-22 工作幅宽cm:160  行距cm:80    行数：2排种器型式：勺轮式（金属材料）排种器数量：2个排肥器型式：外槽轮式排肥器数量：2个","930","T201913130203","2024-12-30","3300.00","","非通用类","河北省","评阅不通过","初评员：不通过","专家：不通过，非精量播种机","","","","",""]
["种植施肥机械","播种机械","精量播种机","2-3行精量播种机","河北峥嵘农机有限公司","玉米施肥精量播种机","2BYCF-3","播种行数:3行;是否精量播种:否 ;","结构型式：机械式、悬挂式整机外形尺寸（长*宽*高）mm:1720*1700*1180 配套动力范围KW：11-33 工作幅宽cm:180  行距cm:60    行数：3排种器型式：勺轮式（金属材料）排种器数量：3个排肥器型式：外槽轮式排肥器数量：3个","930","T201913130202","2024-12-30","4500.00","","非通用类","河北省","评阅不通过","初评员：不通过","专家：不通过，非精量播种机，投档范围不对","","","","",""]
["种植施肥机械","播种机械","精量播种机","2-3行精量播种机","任丘市喜洋洋农业机械有限公司","玉米施肥播种机","2BYCF-3","播种行数:3行;是否精量播种:否 ;","1结构型式：机械式、悬挂式； 2.)外形尺寸（长×宽×高）： 1510mm×1750mm×11mm；      3)行数：3行； 4)行距：500mm～650mm；   5)工作幅宽：1.20m～1.80m；  6)排种器形式：仓转舀勺联体式；        7)传动机构形式：轴传动+链传动；8)开沟器形式：铲式","930","T202013130001","2025-02-27","3850.00","","非通用类","河北省","评阅不通过","初评员：不通过","专家：不通过，铭牌放置不明确","","","","",""]
["种植施肥机械","播种机械","精量播种机","2-3行精量播种机","任丘市超鹰农机有限公司","玉米免耕精量播种机","2BYZF-3","播种行数:3行;是否精量播种:是 ;","型号2BYZF-3，机械式；悬挂式结构形式，配套动力13.2～22kw，工作状态外形尺寸（长×宽×高）1640mm×1650mm×980mm，作业速度范围4～6km/h，作业小时生产率0.2～0.5hm2/h,行距400～650mm,工作行数3行，工作宽幅1.2～1.95m，排种/肥器型式指夹式/外槽轮式数量3/3个驱动方式地轮驱动，种/肥箱容积9×3个/103L，排量调节方式种：档位 肥：螺纹，传动机构型式轴、链条传动，开沟器型式锄铲式数量种：3个肥：3个，深度调节范围0～100mm，地轮型式实心胶地轮直径380mm高度调节范围0～100mm,覆土器型式双圆盘式，镇压器型式实心橡胶轮。","930","冀2018T-103（续）","2022-12-31","3800.00","","非通用类","河北省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["种植施肥机械","播种机械","精量播种机","2-3行精量播种机","任丘市超鹰农机有限公司","玉米免耕精量播种机","2BYZF-2","播种行数:2行;是否精量播种:是 ;","型号2BYZF-2，机械式；悬挂式结构形式，配套动力11～22kw，工作状态外形尺寸（长×宽×高）1640mm×1230mm×980mm，作业速度范围4～6km/h，作业小时生产率0.2~0.5hm2/h,行距400～900mm,工作行数2行，工作宽幅0.8～1.8m，排种/肥器型式指夹式/外槽轮式数量2/2个驱动方式地轮驱动，种/肥箱容积9×2个/75L,排量调节方式种：档位 肥：螺纹，传动机构型式轴、链条传动，开沟器型式锄铲式数量种：2个肥：2个，深度调节范围0～100mm，地轮型式实心胶地轮直径380mm高度调节范围0～100mm,覆土器型式双圆盘式，镇压器型式实心橡胶轮。","930","冀2018T-102（续）","2022-12-31","3200.00","","非通用类","河北省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["种植施肥机械","播种机械","精量播种机","4-5行精量播种机","河北峥嵘农机有限公司","玉米施肥精量播种机","2BYCFB-5","播种行数:5行;是否精量播种:否 ;","结构型式：机械式、悬挂式整机外形尺寸（长*宽*高）mm:1630*2850*1170 配套动力范围KW：36.8-73.5    工作幅宽cm:250-300   行距cm:50-60    行数：5排种器型式：勺轮式（金属材料）排种器数量：5个排肥器型式：外槽轮式排肥器数量：5个","2200","T201900140433","2024-12-30","9100.00","","非通用类","河北省","评阅不通过","初评员：不通过","专家：不通过，非精量播种机","","","","",""]
["种植施肥机械","播种机械","精量播种机","4-5行精量播种机","河北峥嵘农机有限公司","玉米施肥精量播种机","2BYCFB-4","播种行数:4行;是否精量播种:否 ;","结构型式：机械式、悬挂式整机外形尺寸（长*宽*高）mm:1630*2310*1170 配套动力范围KW：22-51.5  工作幅宽cm:200-240   行距cm:50-60    行数：4排种器型式：勺轮式（金属材料）排种器数量：4个排肥器型式：外槽轮式排肥器数量：4个","2200","T201900140433","2024-12-30","8100.00","","非通用类","河北省","评阅不通过","初评员：不通过","专家：不通过，非精量播种机","","","","",""]
["种植施肥机械","播种机械","精量播种机","4-5行精量播种机","保定市鑫飞达农机装备有限公司","气吸式精量播种机","2BYQL-4","播种行数:4行;是否精量播种:是 ;","\"结构尺寸（长*宽*高mm）： 1650*2290*990  整机质量（kg）： 300  \n配套动力（kw）： 25.7-36.8  行距（cm）： 50-60  \n工作幅宽（cm）： 200-240  排种器（形式/数量）： 垂直圆盘气吸式/4个  \n排肥器（形式/数量）： 外槽轮/4个  传动机构形式： 轴传动与齿轮传动  \n开沟器形式： 锄铲式  地轮（形式/直径）： 胶轮/40cm  \n风机叶轮直径/质量/工作转速： 355mm/3.5kg/3200-3500r/min  排种器形式： 精量播种器  \n播种行数（行）： 4 \n\"","2200","冀2018T-136（续）","2022-12-31","11500.00","","非通用类","河北省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["种植施肥机械","播种机械","精量播种机","4-5行精量播种机","任丘市超鹰农机有限公司","玉米免耕精量播种机","2BYZF-4","播种行数:4行;是否精量播种:是 ;","型号2BYZF-4，机械式；悬挂式结构形式，配套动力22～36.8kw，工作状态外形尺寸（长×宽×高）1640mm×2260mm×1110mm，作业速度范围4～6km/h，作业小时生产率0.3～0.6hm2/h,行距400～650mm,工作行数4行，工作宽幅1.6～2.6m，排种/肥器型式指夹式/外槽轮式数量4/4个驱动方式地轮驱动，种/肥箱容积9×4个/152L，排量调节方式种：档位 肥：螺纹，传动机构型式轴、链条传动，开沟器型式锄铲式数量种：4个肥：4个，深度调节范围0～100mm，地轮型式实心胶地轮直径380mm高度调节范围0～100mm,覆土器型式双圆盘式，镇压器型式实心橡胶轮。","2200","冀2018T-104（续）","2022-12-31","7600.00","","非通用类","河北省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["种植施肥机械","播种机械","精量播种机","4-5行精量播种机","任丘市超鹰农机有限公司","玉米免耕精量播种机","2BYZF-5","播种行数:5行;是否精量播种:是 ;","型号2BYZF-5，机械式；悬挂式结构形式，配套动力36.8～73.5kw，工作状态外形尺寸（ 长×宽×高）1830mm×2760mm×1150mm，作业速度范围4～6km/h，作业小时生产率0.4～1.0hm2/h,行距400～600mm,工作行数5行，工作宽幅2.0～3.0m，排种/肥器型式指夹式/外槽轮式数量5/5个驱动方式地轮驱动，种/肥箱容积9×5个/174L，排量调节方式种：档位 肥：螺纹，传动机构型式轴、链条传动，开沟器型式锄铲式数量种：5个肥：5个，深度调节范围0～100mm，地轮型式实心胶地轮直径380mm高度调节范围0～100mm,覆土器型式双圆盘式，镇压器型式实心橡胶轮。","2200","冀2018T-105（续）","2022-12-31","8500.00","","非通用类","河北省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期；铭牌放置不明确","","","","",""]
["种植施肥机械","播种机械","精量播种机","4-5行精量播种机","石家庄农业机械股份有限公司","气吸精量播种机","2BQ-4","播种行数:4行;是否精量播种:是 ;","结构形式：悬挂式、气力式\n配套动力;22.1-36.8kw\n外形尺寸（长×宽×高）\t1550×2730×1550\tmm\n作业速度范围;1.11-1.67m/s\n作业小时生产率：0.8-1.44hm2/h\n工作幅宽\t200～240\tcm\n行距\t50～60\tcm\n工作行数\t4\t行\n排种器形式\t气力式\t金属材料\n排种器数量\t4\t个\n排肥器形式\t槽轮式\t金属材料\n排肥器数量\t4\t个\n排种开沟器形式：滑刀式\t\n排种开沟器数量：4个\n排种开沟器深度调节范围：20-60cm\n排肥开沟器形式：铲式\t\n排肥开沟器数量：4个\n排肥开沟器深度调节范围：30-80\n种/肥箱容积：种11*4，肥70*2L\n排量调节方式：种：更换气吸盘、肥：螺纹调节\n排种部分传动方式：\t链传动＋轴传动\t\n地轮型式：\t充气轮胎\t\n地轮直径：\tφ550\tmm\n风机型式：离心式\n覆土器型式：刮板式\n镇压器型式：圆锥组合镇压轮","2200","T201913130258","2024-12-30","9900.00","","非通用类","河北省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["种植施肥机械","播种机械","精量播种机","4-5行精量播种机","河北江天农业机械有限公司","多层施肥播种机","2BYF-4","播种行数:4行;是否精量播种:是 ;","结构型式:机械悬挂式.配套动力范围(kW):29.4~44.1.工作状态外形尺寸(长X宽X高,mm)1920×2300×1150.作业速度范围(km/h):3~5.作业小时生产率(hm2/h):0.4~0.6.行距(mm):500~600.工作行数(行):4.工作幅宽(m):2.0~2.4.排种/排肥型式:勺轮/外槽轮,数量(个):4/4,驱动方式:地轮驱动.种/肥箱容积(L):7X4/140.排量调节方式:排种:机械式;排肥:手动螺旋.传动结构型式:轴传动(地轮驱动).开沟器型式:锄铲式;数量(个):播种4;施肥4;深度调节范围(mm):0~120.地轮型式:实心橡胶轮;直径(mm):φ390;高度调节范围(mm):0~130.覆土器型式:板式.镇压器型式:地轮.","2200","冀2017T—085","2021-12-31","7400.00","","非通用类","河北省","评阅不通过","初评员：不通过","专家：不通过，非精量播种机","","","","",""]
["种植施肥机械","播种机械","精量播种机","6-10行精量播种机","河北峥嵘农机有限公司","玉米施肥精量播种机","2BYCFB-6","播种行数:6行;是否精量播种:否 ;","结构型式：机械式、悬挂式整机外形尺寸（长*宽*高）mm:1630*3450*1170 配套动力范围KW：36.8-73.5    工作幅宽cm:300-360   行距cm:50-60    行数：6 排种器型式：勺轮式（金属材料）排种器数量：6个排肥器型式：外槽轮式排肥器数量：6个","3900","T201900140433","2024-12-30","14100.00","","非通用类","河北省","评阅不通过","初评员：不通过","专家：不通过，非精量播种机","","","","",""]
["种植施肥机械","播种机械","精量播种机","6-10行精量播种机","天津库恩农业机械有限公司","精量点播机","MAXIMA 2M-6","播种行数:6行;是否精量播种:是 ;","外形尺寸（长x宽x高）：2160x4400x1910mm\n结构质量：1650kg\n行距：50~70cm\n工作行数：6\n工作宽幅：300~420cm\n排种器：气吸式，6个","3900","黑垦鉴2016059","2020-12-31","360000.00","","非通用类","天津市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["种植施肥机械","播种机械","精量播种机","6-10行精量播种机","天津库恩农业机械有限公司","精量点播机","MAXIMA 2M-9","播种行数:9行;是否精量播种:是 ;","外形尺寸（长x宽x高）：2000x7000x2000mm\n结构质量：2300kg\n行距：50~70cm\n工作行数：9\n工作宽幅：450-630cm\n排种器：气吸式，9个","3900","黑垦鉴2016060","2020-12-31","410000.00","","非通用类","天津市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["种植施肥机械","播种机械","精量播种机","6-10行精量播种机","任丘市超鹰农机有限公司","玉米免耕精量播种机","2BYZF-6","播种行数:6行;是否精量播种:是 ;","型号2BYZF-6，机械式；悬挂式结构形式，配套动力36.8～73.5kw，工作状态外形尺寸（ 长×宽×高）1830mm×3380mm×1150mm，作业速度范围4～6km/h，作业小时生产率1.0～2.0hm2/h,行距400～600mm,工作行数6行，工作宽幅2.4～3.6m，排种/肥器型式指夹式/外槽轮式数量6/6个驱动方式地轮驱动，种/肥箱容积9×6个/110×2个L，排量调节方式种：档位 肥：螺纹，传动机构型式轴、链条传动，开沟器型式锄铲式数量种：6个肥：6个，深度调节范围0～100mm，地轮型式实心胶地轮直径380mm高度调节范围0～100mm,覆土器型式双圆盘式，镇压器型式实心橡胶轮。","3900","冀2018T-106（续）","2022-12-31","14000.00","","非通用类","河北省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期，铭牌放置不明确","","","","",""]
["种植施肥机械","育苗机械设备","秧盘播种成套设备（含床土处理）","生产率500(盘/h)及以上秧盘播种成套设备","大安市祥和农业机械制造有限公司","水稻秧盘播种机","2BYP-14/17","含铺底土、播种、洒水、覆土功能:是 ;生产率:/盘/h;","配套动力:铺土电机120w,覆土电机120w,播种电机60w","3100","T201922220069","2024-12-15","10400.00","","非通用类","吉林省","评阅不通过","初评员：不通过","专家：不通过，铭牌与机器不配套","","","","",""]
["种植施肥机械","育苗机械设备","秧盘播种成套设备（含床土处理）","生产率500(盘/h)及以上秧盘播种成套设备","黑龙江农垦依民机械制造有限公司","水稻育秧播种机","2BP-800","含铺底土、播种、洒水、覆土功能:是 ;生产率:1000盘/h;","产品型号名称 / 2BP-800 水稻育秧播种机\n2 作业状态整机外型尺寸(长×宽×高) cm 484×53×109\n3 小时生产率 盘/h 800～1000\n4 结构型式 / 固定式\n5 铺土\n铺土器形式 / 胶带 板刷式\n铺土箱容积 L 40\n6 播种\n排种器形式 / 铝轮 滚刷式\n播种量调节档位数量 个 无极调速\n铺土箱容积 L 40\n7 覆土\n覆土箱形式 / 胶带毛刷式（或铁板）\n覆土箱容积 L 55\n8 输送传动型式 / 调速电机驱动 链条传动\n9 覆土平整方式 / 板刷式\n10 作业流程 / 送盘、铺土、播种、覆土\n11 配套动力功率 kW 0.26\n12 配套动力类型 / 交流电机","3100","T201923230148","2024-10-07","8500.00","","非通用类","黑龙江","评阅不通过","初评员：不通过","专家：不通过，铭牌不规范，缺少生产日期、编号等","","","","",""]
["种植施肥机械","育苗机械设备","秧盘播种成套设备（含床土处理）","生产率500(盘/h)及以上秧盘播种成套设备","黑龙江农垦依民机械制造有限公司","电动育秧成套设备","2BP-840","含铺底土、播种、洒水、覆土功能:是 ;生产率:1000盘/h;","作业状态整机外型尺寸(长×宽×高) cm 103×70×66 3 小时生产率 盘/h 800～1000 4 结构型式 / 行走式 5 铺土 铺土器形式 / 胶带 板刷 铺土箱容积 L 44 6 播种 排种器形式 / 槽轮 滚刷 板刷 播种量调节档位数量 个 1-60 播种箱容积 L 6 7 覆土 覆土箱形式 / 胶带 板刷 挡板 覆土箱容积 L 44 8 覆土平整方式 / 调整板 9 输送传动型式 / 链轮 链条 10 作业流程 / 播肥铺土、播种覆土、浇水 11 配套动力功率 W 540 12 配套动力类型 / 直流电机 锂电","3100","T201923230270","2024-12-29","7800.00","","非通用类","黑龙江","评阅不通过","初评员：不通过","专家：不通过，名牌与机器不配套。","","","","",""]
["种植施肥机械","育苗机械设备","秧盘播种成套设备（含床土处理）","生产率500(盘/h)及以上秧盘播种成套设备","黑龙江农垦依民机械制造有限公司","水稻育秧摆盘机","2BP-1000","含铺底土、播种、洒水、覆土功能:是 ;生产率:1200盘/h;","作业状态整机外型尺寸(长×宽×高) cm 238×77.4×106 3 小时生产率 盘/h 1000～1200 4 结构型式 / 行走式 5 铺土 铺土器形式 / 胶带 板刷调整板 铺土箱容积 L 48 6 播种 排种器形式 / 槽轮 滚刷 板刷 播种量调节档位数量 个 1-60 播种箱容积 L 19 7 覆土 覆土箱形式 / 胶带 板刷 挡板 覆土箱容积 L 34 8 输送传动型式 / 齿轮 链轮 链条 9 作业流程 / 行走送盘 播肥铺土、播种覆土、 浇水 10 配套动力功率 W 290 11 配套动力类型 / 直流电机 锂电","3100","T201923230279","2024-12-29","8900.00","","非通用类","黑龙江","评阅不通过","初评员：不通过","专家：不通过，名牌与机器不配套。","","","","",""]
["种植施肥机械","育苗机械设备","秧盘播种成套设备（含床土处理）","生产率500(盘/h)及以上秧盘播种成套设备","黑龙江农垦依民机械制造有限公司","电动育秧成套设备","2BP-1120","含铺底土、播种、洒水、覆土功能:是 ;生产率:1200盘/h;","作业状态整机外型尺寸(长×宽×高) cm 131×70×66 3 小时生产率 盘/h 1000～1200 4 结构型式 / 行走式 5 铺土 铺土器形式 / 胶带 板刷 铺土箱容积 L 58 6 播种 排种器形式 / 槽轮 滚刷 板刷 播种量调节档位数量 个 1-60 播种箱容积 L 8 7 覆土 覆土箱形式 / 胶带 板刷 挡板 覆土箱容积 L 58 8 输送传动型式 / 链轮 链条 9 作业流程 / 播肥铺土、播种覆土、浇水 10 配套动力功率 W 540 11 配套动力类型 / 直流电机 锂电","3100","T201923230271","2024-12-29","8800.00","","非通用类","黑龙江","评阅不通过","初评员：不通过","专家：不通过，名牌与机器不配套","","","","",""]
["种植施肥机械","栽植机械","水稻插秧机","6行及以上手扶步进式水稻插秧机","南通富来威农业装备有限公司","机动插秧机","2ZF-6AKE","形式:手扶步进式 ;行数:6行;","行数:6行；手扶式；穴距(mm):120、140、160、180、210；行距(mm):250(中央300）；结构质量(kg):190；插秧深度(mm):4-40；插植臂型式:曲柄摇杆式；配套发动机:雅马哈MZ175B8EA0；标定功率:3.3KW","5800","T201932320191","2024-12-30","23000.00","","非通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["种植施肥机械","栽植机械","水稻插秧机","4行四轮乘坐式水稻插秧机","苏州久富农业机械有限公司","乘坐式高速插秧机","2ZG-5G(G5G)","形式:四轮乘坐式 ;行数:5行;","结构型式：高速乘坐式；整机外形尺寸(长×宽高)：2886×1888×1570mm；作业速度：0～1.33m/s；作业小时生产率：0.08～0.29hm2/h；单位作业量燃油消耗量：1.7∽2.4kg/hm2；工作行数：5行；行距：300mm；穴距调节机构型式：手柄调节；穴距调节档位数量：5个；穴距：120、140、160、180、210（100、240选配）mm；插秧深度：10～35mm；移距：20、17.5、15.5、14（12.7、10.7选配）mm；取秧深度：10～20mm；插秧频次：最低150、最高670穴/分；\n变速方式：机械变速；行走轮结构型式(前、后)：宽幅防爆轮胎、粗轮毂橡胶轮胎；行走轮直径（前、后）：Φ600、Φ850mm；平衡机构型式：机械式；插植臂型式：旋转式；","12400","T201932320192","2024-12-30","58000.00","","非通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["种植施肥机械","栽植机械","水稻插秧机","6-7行四轮乘坐式水稻插秧机","苏州久富农业机械有限公司","乘坐式高速插秧机","2ZG-7GS(G7SG)","形式:四轮乘坐式 ;行数:7行;","结构型式：高速乘坐式；整机外形尺寸(长×宽高)：2886×2488×1570mm；作业速度：0～0.66m/s；作业小时生产率：0.08～0.20hm2/h；单位作业量燃油消耗量：1.7∽2.4kg/hm2；工作行数：7行；行距：300mm；穴距调节机构型式：手柄调节；穴距调节档位数量：5个；穴距：120、140、160、180、210（100、240选配）mm；插秧深度：10～35mm；移距：20、17.5、15.5、14（12.7、10.7选配）mm；取秧深度：10～21mm；插秧频次：最低110、最高330穴/分；\n变速方式：机械变速；行走轮结构型式(前、后)：宽幅防爆轮胎、粗轮毂橡胶轮胎；行走轮直径（前、后）：Φ600、Φ850mm；平衡机构型式：电子式；插植臂型式：曲柄摇杆式；","28400","T201932320193","2024-12-30","88000.00","","非通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["种植施肥机械","栽植机械","水稻插秧机","6-7行四轮乘坐式水稻插秧机","潍坊久瑞田农业装备有限公司","高速乘坐式插秧机","2ZGQ-6","形式:四轮乘坐式 ;行数:6行;","结构型式：高速乘坐式；整机外形尺寸（长×宽×高）mm：3500×2080×2560；工作行数（行）：6；行距（mm）：300；穴距（mm）：110、130、150、160、180、210；变速方式：前：无内胎橡胶车轮；后：无内胎橡胶凸爪高耳车轮；行走轮直径（前、后）（mm）：前：φ650；后：φ950；平衡机构型式：电子液压平衡；插植臂型式：旋转式","28400","GZNJ/TJ 2019-430","2025-03-16","97500.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["种植施肥机械","栽植机械","水稻插秧机","6-7行四轮乘坐式水稻插秧机","江苏隆庆机械有限公司","乘坐式高速插秧机","2ZG-6D","形式:四轮乘坐式 ;行数:6行;","型号名称:2ZG-6D乘坐式高速插秧机,结构型式:高速乘坐式,发动机额定功率:14.7KW,发动机额定转速:3600k/min,工作行数:6行,穴距调节机构型式:齿轮调节,穴距调节档位数量:7个,行距:300mm","28400","鄂2019270","2024-07-17","98800.00","","非通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期。","","","","",""]
["种植施肥机械","栽植机械","水稻插秧机","8行及以上四轮乘坐式水稻插秧机","潍坊久瑞田农业装备有限公司","高速乘坐式插秧机","2ZGQ-8","形式:四轮乘坐式 ;行数:8行;","结构型式： 高速乘坐式；整机外形尺寸（长×宽×高）（mm）;3500×2240×2550;工作行数(行）：8；行距（mm）；250；穴距（mm）：110、130、150、160、180、210","38600","GZNJ/TJ 2019-431","2025-03-16","135000.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["种植施肥机械","栽植机械","水稻插秧机","8行及以上四轮乘坐式水稻插秧机","潍坊久瑞田农业装备有限公司","高速乘坐式插秧机","2ZGC-8KZ","形式:四轮乘坐式 ;行数:8行;","结构型式:高速乘坐式；整机外形尺寸（长×宽×高）（mm）：3500×2360×2560；工作行数（行）：8；行距（mm）：窄：170；宽：330；穴距（mm）：110、120、140、160、190、210","38600","GZNJ/TJ 2019-432","2025-03-16","135000.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["种植施肥机械","施肥机械","施肥机","水稻侧深施肥装置(配套6行及以上乘坐式水稻插秧机或水稻精量穴播机)","苏州久富农业机械有限公司","水稻侧深施肥机","2FH-1.8C（6F2）","行数:6行;定位、定量深施,与高速插秧机或水稻精量穴播机配套同步作业.配置强制施肥装置、漏施堵塞报警装置、插秧施:是 ;","规格型号：2FH-1.8C（6F2）；行数：6行；配套动力形式：步进减速电机+鼓风机；动力传输方式：链条传动；主机体尺寸（长×宽×高）：（530×370×650）×2个mm；肥料排出方式：外槽轮；施肥量调节方式：旋钮调节+车速传感器；施肥量范围：150～900kg/h㎡；施肥深度：50±10mm；施肥位置：侧40±10mm；肥箱容积：2×40L（80L）L；防堵塞、漏施或报警装置：有；离合器形式：电子式单侧离合；输送装置形式：管路风送式；配置有强制施肥装置：有；","6500","T202032320125","2025-07-09","24800.00","","非通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["种植施肥机械","施肥机械","施肥机","水稻侧深施肥装置(配套6行及以上乘坐式水稻插秧机或水稻精量穴播机)","苏州久富农业机械有限公司","水稻侧深施肥机","2FH-2.4C（8F2）","行数:8行;定位、定量深施,与高速插秧机或水稻精量穴播机配套同步作业.配置强制施肥装置、漏施堵塞报警装置、插秧施:是 ;","规格型号：2FH-2.4C（8F2）；行数：8行；配套动力形式：步进减速电机+鼓风机；动力传输方式：链条传动；主机体尺寸（长×宽×高）：（530×370×650）×2个mm；肥料排出方式：外槽轮；施肥量调节方式：旋钮调节+车速传感器；施肥量范围：150～900kg/h㎡；施肥深度：50±10mm；施肥位置：侧40±10mm；肥箱容积：2×40L（80L）L；防堵塞、漏施或报警装置：有；离合器形式：电子式单侧离合；输送装置形式：管路风送式；配置有强制施肥装置：有；","6500","T202032320126","2025-07-09","24800.00","","非通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","中耕机械","田园管理机","功率4kW以下田园管理机","山东乐佳佳机电科技有限公司","田园管理机","3TGQ-2A","配套功率:2.2kW;","型号名称\t3TGQ-2A型田园管理机\t\n结构型式\t/\t单轴；轮式\t\n外形尺寸(长×宽×高)\tmm\t1200X600X950\t\n扶把水平调整\t/\t不可调\t\n扶把上下调整\t/\t不可调\t\n发动机输出传动方式\t/\t皮带传动\t\n主离合器型式\t/\t张紧式\t\n主离合器状态\t/\t常开\t\n标定（额定）功率\tkW\t2.2\t\n标定（额定）转速\tr/min\t3600\t\n配套锄草装置型式\t/\t锄草轮\t\n配套锄草装置最大工作宽度\tmm\t280\t\n配套起垄装置型式\t/\t绞龙+仿形器\n配套起垄装置起垄数量      /       1\t\n配套起垄装置最大工作起垄高度\tmm\t200","510","T202037370014","2025-07-06","1900.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","中耕机械","田园管理机","功率4kW以下田园管理机","山东乐佳佳机电科技有限公司","田园管理机","3TGQ-2C","配套功率:2.2kW;","型号名称\t3TGQ-2C型田园管理机\t\n结构型式\t/\t单轴；轮式\t\n外形尺寸(长×宽×高)\tmm\t1330X600X850\t\n扶把水平调整\t/\t不可调\t\n扶把上下调整\t/\t不可调\t\n发动机输出传动方式\t/\t皮带传动\t\n主离合器型式\t/\t张紧式\t\n主离合器状态\t/\t常开\t\n标定（额定）功率\tkW\t2.2\t\n标定（额定）转速\tr/min\t3600\t\n配套锄草装置型式\t/\t锄草轮\t\n配套锄草装置最大工作宽度\tmm\t280\t\n配套起垄装置型式\t/\t绞龙+仿形器\n配套起垄装置起垄数量      /       1\t\n配套起垄装置最大工作起垄高度\tmm\t200","510","T202037370012","2025-07-06","1900.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","中耕机械","田园管理机","功率4kW及以上田园管理机","潍坊昊杰机械有限公司","田园管理机","3TGQ-4","配套功率:4.0kW;","标定功率：4.0kw.额定转速：3600r/min","710","T201937370051","2024-10-24","3200.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","中耕机械","田园管理机","功率4kW及以上田园管理机","莱州奥伦农业机械有限公司","田园管理机","3TGQ-4D","配套功率:4kW;","结构型式：双轴；轮式、外形尺寸（长×宽×高）：1900×640×950mm、主离合器形式：涨紧式、主离合器状态：常开、配套开沟装置型式：旋刀式、配套培土装置型式：旋刀式、配套开沟装置最大工作宽度：270mm、配套培土装置最大工作宽度：270mm、培土刀总安装刀数：10片、发动机输出传动方式：三角带","710","T202037370026","2025-07-06","4800.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","中耕机械","田园管理机","功率4kW及以上田园管理机","费县华源农业装备工贸有限公司","田园管理机","3TG-6","配套功率:6.3kW;","结构型式：双轴/轮式；外形尺寸：1720*720*940mm；扶把水平可调整：扶把上下可调整；发动机输出传动方式：皮带传动；主离合器型式：涨紧轮式，主离合器常开状态；标定功率6.3KW;标定转速3600r/min；配套培土装置型式：旋刀式；培土装置最大工作宽度300mm：配套开沟装置型式：旋刀式；开沟装置最大工作宽度300mm。","710","T201937370184","2024-12-23","6800.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","中耕机械","田园管理机","功率4kW及以上田园管理机","费县华源农业装备工贸有限公司","田园管理机","3TG-6H","配套功率:6.3kW;","结构型式：双轴/轮式；外形尺寸：1950*550*1060mm；扶把水平可调整：扶把上下可调整；发动机输出传动方式：皮带传动；主离合器型式：涨紧轮式，主离合器常开状态；标定功率6.3KW;标定转速3600r/min；配套培土装置型式：旋刀式；培土装置最大工作宽度300mm：配套开沟装置型式：旋刀式；开沟装置最大工作宽度300mm。","710","T201937370186","2024-12-23","6900.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","中耕机械","田园管理机","功率4kW及以上田园管理机","费县华源农业装备工贸有限公司","田园管理机","3TG-6Z","配套功率:6.3kW;","结构型式：双轴/轮式；外形尺寸：1550*700*940mm；扶把水平可调整：扶把上下可调整；发动机输出传动方式：齿轮传动；主离合器型式：摩擦片式，主离合器常开状态；标定功率6.3KW;标定转速3600r/min；配套培土装置型式：旋刀式；培土装置最大工作宽度300mm：配套开沟装置型式：旋刀式；开沟装置最大工作宽度300mm。","710","T201937370185","2024-12-23","6980.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：不通过","","","","",""]
["田间管理机械","中耕机械","田园管理机","功率4kW及以上田园管理机","费县华源农业装备工贸有限公司","田园管理机","3TGQ-5","配套功率:5.2kW;","结构型式：双轴/轮式；外形尺寸：1720*700*940mm；扶把水平可调整：扶把上下可调整；发动机输出传动方式：皮带传动；主离合器型式：涨紧轮式，主离合器常开状态；标定功率5.2KW;标定转速3600r/min；配套培土装置型式：旋刀式；培土装置最大工作宽度300mm：配套开沟装置型式：旋刀式；开沟装置最大工作宽度300mm：","710","T201937370180","2024-12-23","4580.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","中耕机械","田园管理机","功率4kW及以上田园管理机","费县华源农业装备工贸有限公司","田园管理机","3TGQ-5H","配套功率:5.2kW;","结构型式：双轴/轮式；外形尺寸：1860*530*940mm；扶把水平可调整：扶把上下可调整；发动机输出传动方式：皮带传动；主离合器型式：涨紧轮式，主离合器常开状态；标定功率5.2KW;标定转速3600r/min；配套培土装置型式：旋刀式；培土装置最大工作宽度300mm：配套开沟装置型式：旋刀式；开沟装置最大工作宽度300mm。","710","T201937370182","2024-12-23","4800.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","中耕机械","田园管理机","功率4kW及以上田园管理机","费县华源农业装备工贸有限公司","田园管理机","3TGQ-5Z","配套功率:5.2kW;","结构型式：双轴/轮式；外形尺寸：1490*700*940mm；扶把水平可调整：扶把上下可调整；发动机输出传动方式：齿轮传动；主离合器型式：摩擦片式，主离合器常开状态；标定功率5.2KW;标定转速3600r/min；配套培土装置型式：旋刀式；培土装置最大工作宽度300mm：配套开沟装置型式：旋刀式；开沟装置最大工作宽度300mm：","710","T201937370183","2024-12-23","5200.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","中耕机械","田园管理机","功率4kW及以上田园管理机","费县华源农业装备工贸有限公司","田园管理机","3TGQ-4A","配套功率:4.0kW;","结构型式：双轴/轮式；外形尺寸：1490*700*940mm；扶把水平可调整：扶把上下可调整；发动机输出传动方式：皮带传动；主离合器型式：涨紧轮式，主离合器常开状态；标定功率4.0KW;标定转速3600r/min；配套培土装置型式：旋刀式；培土装置最大工作宽度300mm：配套开沟装置型式：旋刀式；开沟装置最大工作宽度300mm。","710","T201937370162","2024-12-23","3280.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","中耕机械","田园管理机","功率4kW及以上田园管理机","费县华源农业装备工贸有限公司","田园管理机","3TGQ-4H","配套功率:4.0kW;","结构型式：双轴/轮式；外形尺寸：1900*550*940mm；扶把水平可调整：扶把上下可调整；发动机输出传动方式：皮带传动；主离合器型式：涨紧轮式，主离合器常开状态；标定功率4.0KW;标定转速3600r/min；配套培土装置型式：旋刀式；培土装置最大工作宽度300mm：配套开沟装置型式：旋刀式；开沟装置最大工作宽度300mm。","710","T201937370181","2024-12-23","3280.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","中耕机械","田园管理机","功率4kW及以上田园管理机","费县华源农业装备工贸有限公司","田园管理机","3TGQ-4Z","配套功率:4.0kW;","结构型式：双轴/轮式；外形尺寸：1490*700*940mm；扶把水平可调整：扶把上下可调整；发动机输出传动方式：齿轮传动；主离合器型式：摩擦片式，主离合器常开状态；标定功率4.0KW;标定转速3600r/min；配套培土装置型式：旋刀式；培土装置最大工作宽度300mm：配套开沟装置型式：旋刀式；开沟装置最大工作宽度300mm。","710","T201937370187","2024-12-23","3500.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","中耕机械","田园管理机","功率4kW及以上田园管理机","山东华盛农业药械有限责任公司","田园管理机","3TGQ-4","配套功率:4.0kW;","序号\t项目\t设计值\n1\t型号名称\t3TGQ-4型田园管理机\n2\t结构型式\t双轴；轮式\n3\t外形尺寸(长×宽×高)\t1160×640×870mm\n4\t扶把水平调整（可调/不可调）\t可调\n5\t扶把上下调整（可调/不可调）\t可调\n6\t发动机输出传动方式\t皮带传动\n7\t主离合器型式\t涨紧式\n8\t主离合器状态\t常开\n9\t标定（额定）功率\t4.0kW\n10\t标定（额定）转速\t3600r/min\n11\t配套培土装置型式\t旋刀式\n12\t配套培土装置最大工作宽度\t300mm\n13\t配套开沟装置型式\t旋刀式\n14\t配套开沟装置最大工作宽度\t240mm","710","T201937370067","2024-10-24","3600.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","中耕机械","田园管理机","功率4kW及以上田园管理机","潍坊沃富机械有限公司","田园管理机","3TG-6","配套功率:6.3kW;","外形尺寸：1800x640x1150，结构型式：双轴.轮式。发动机输出传动方式：皮带传动。主离合器型式：张紧轮。主离合器状态：常开。标定功率：6.3KW。标定转速：3600r/min。配套开沟装置型式；驱动刀轮式。配套开沟装置最大开沟宽度：140mm。配套培土装置型式：驱动刀轮式。配套培土装置最大工作宽度：140mm。","710","T202037370051","2025-07-06","4600.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","中耕机械","田园管理机","功率4kW及以上田园管理机","山东乐佳佳机电科技有限公司","田园管理机","3TGQ-4D","配套功率:4.0kW;","产品名称\t3TGQ-4D型田园管理机\t\n结构型式\t/\t双轴；轮式\t\n外形尺寸(长×宽×高)\tmm\t1550×740×950\t\n扶把水平调整\t/\t可调\t\n扶把上下调整\t/\t可调\t\n发动机输出传动方式\t/\t齿轮传动\t\n主离合器型式\t/\t摩擦片\t\n主离合器状态\t/\t常开\t\n标定（额定）功率\tkW\t4.0\t\n标定（额定）转速\tr/min\t3600\t\n配套锄草装置型式\t/\t锄草轮\t\n配套锄草装置最大工作宽度\tmm\t700\t\n配套开沟装置型式\t/\t旋刀式\t\n配套开沟装置最大工作宽度\tmm\t250","710","T202037370018","2025-07-06","2800.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","中耕机械","田园管理机","功率4kW及以上田园管理机","山东乐佳佳机电科技有限公司","田园管理机","3TGQ-4.5A","配套功率:4.5kW;","型号名称\t/\t3TGQ-4.5A型田园管理机\t\n结构型式\t/\t双轴；轮式\t\n外形尺寸(长×宽×高)\tmm\t1600×740×950\t\n扶把水平调整\t/\t可调\t\n扶把上下调整\t/\t可调\t\n发动机输出传动方式\t/\t齿轮传动\t\n主离合器型式\t/\t摩擦片\t\n主离合器状态\t/\t常开\t\n标定（额定）功率\tkW\t4.5\t\n标定（额定）转速\tr/min\t3600\t\n配套锄草装置型式\t/\t锄草轮\t\n配套锄草装置最大工作宽度\tmm\t700\t\n配套开沟装置型式\t/\t旋刀式\t\n配套开沟装置最大工作宽度\tmm\t250","710","T202037370008","2025-07-06","3200.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","中耕机械","田园管理机","功率4kW及以上田园管理机","山东乐佳佳机电科技有限公司","田园管理机","3TGQ-4C","配套功率:4.0kW;","型号名称\t/\t3TGQ-4C型田园管理机\t\n结构型式\t/\t双轴；轮式\t\n外形尺寸(长×宽×高)\tmm\t1530×740×980\t\n扶把水平调整\t/\t可调\t\n扶把上下调整\t/\t可调\t\n发动机输出传动方式\t/\t皮带传动\t\n主离合器型式\t/\t张紧式\t\n主离合器状态\t/\t常开\t\n标定（额定）功率\tkW\t4.0\t\n标定（额定）转速\tr/min\t3600\t\n配套锄草装置最大工作宽度\tmm\t700\t\n配套开沟装置型式\t/\t旋刀式\t\n配套开沟装置最大工作宽度\tmm\t250","710","T202037370015","2025-07-06","2800.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","中耕机械","田园管理机","功率4kW及以上田园管理机","山东乐佳佳机电科技有限公司","田园管理机","3TGQ-4.5C","配套功率:4.5kW;","型号名称\t/\t3TGQ-4.5C型田园管理机\t\n结构型式\t/\t双轴；轮式\t\n外形尺寸(长×宽×高)\tmm\t1600×740×950\t\n扶把水平调整\t/\t可调\t\n扶把上下调整\t/\t可调\t\n发动机输出传动方式\t/\t皮带传动\t\n主离合器型式\t/\t张紧式\t\n主离合器状态\t/\t常开\t\n标定（额定）功率\tkW\t4.5\t\n标定（额定）转速\tr/min\t3600\t\n配套锄草装置型式\t/\t锄草轮\t\n配套锄草装置最大工作宽度\tmm\t700\t\n配套开沟装置型式\t/\t旋刀式\t\n配套开沟装置最大工作宽度\tmm\t250","710","T202037370009","2025-07-06","3200.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","中耕机械","田园管理机","功率4kW及以上田园管理机","山东乐佳佳机电科技有限公司","田园管理机","3TGQ-4E","配套功率:4.0kW;","产品名称\t3TGQ-4E型田园管理机\t\n结构型式\t/\t单轴；轮式\t\n外形尺寸(长×宽×高)\tmm\t1500X660X950\t\n扶把水平调整\t/\t可调\t\n扶把上下调整\t/\t可调\t\n发动机输出传动方式\t/\t皮带传动\t\n主离合器型式\t/\t张紧式\t\n主离合器状态\t/\t常开\t\n标定（额定）功率\tkW\t4.0\t\n标定（额定）转速\tr/min\t3600\t\n配套锄草装置型式\t/\t锄草轮\t\n配套锄草装置最大工作宽度\tmm\t740\t\n配套起垄装置型式\t/\t绞龙+仿形器\n配套起垄装置起垄数量      /       1\t\n配套起垄装置最大工作起垄高度\tmm\t240","710","T202037370016","2025-07-06","2400.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","中耕机械","田园管理机","功率4kW及以上田园管理机","山东乐佳佳机电科技有限公司","田园管理机","3TGQ-4G","配套功率:4.0kW;","产品型号名称\t/\t3TGQ-4G型田园管理机\t\n结构型式\t/\t单轴；履带\t\n外形尺寸(长×宽×高)\tmm\t1620×600×950\t\n扶把水平调整\t/\t不可调\t\n扶把上下调整\t/\t不可调\t\n发动机输出传动方式\t/\t皮带传动\t\n主离合器型式\t/\t离心式\t\n主离合器状态\t/\t常开\t\n标定（额定）功率\tkW\t4.0\t\n标定（额定）转速\tr/min\t3600\t\n配套锄草装置型式\t/\t锄铲式\t\n配套锄草装置最大工作宽度\tmm\t400\t\n配套施肥装置排肥器型式\t/\t外槽轮\t\n配套施肥装置施肥行数\t/\t1\t\n配套施肥装置施肥开沟器型式\t/\t尖铲式","710","T202037370013","2025-07-06","2400.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","中耕机械","田园管理机","功率4kW及以上田园管理机","山东乐佳佳机电科技有限公司","田园管理机","3TGQ-4A","配套功率:4.0kW;","型号名称\t3TGQ-4A型田园管理机\t\n结构型式\t/\t单轴；轮式\t\n外形尺寸(长×宽×高)\tmm\t1460X700X950\t\n扶把水平调整\t/\t可调\t\n扶把上下调整\t/\t可调\t\n发动机输出传动方式\t/\t齿轮传动\t\n主离合器型式\t/\t摩擦片\t\n主离合器状态\t/\t常开\t\n标定（额定）功率\tkW\t4.0\t\n标定（额定）转速\tr/min\t3600\t\n配套锄草装置型式\t/\t锄草轮\t\n配套锄草装置最大工作宽度\tmm\t720\t\n配套起垄装置型式\t/\t绞龙+仿形器\n配套起垄装置起垄数量      /       1\t\n配套起垄装置最大工作起垄高度\tmm\t240","710","T202037370017","2025-07-06","2400.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","中耕机械","田园管理机","功率4kW及以上田园管理机","重庆美多盈机械有限公司","田园管理机","3TG-6","配套功率:6.2kW;","型号名称：3TG-6型田园管理机；结构型式：双轴轮式：外形尺寸(长×宽×高)mm：1900×1100×1060；扶把水平调整：可调；扶把上下调整：可调；发动机输出传动方式：直联；主离合器型式：摩擦片式；主离合器状态：常开；标定功率kW：6.2；标定转速r/min：3000；燃油种类：柴油；配套锄草装置型式：轮式；配套锄草装置最大工作宽度mm：890；配套开沟装置型式：刀片式；配套开沟装置最大工作宽度mm：470；","710","T201950500123","2024-09-09","3200.00","","非通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","植保机械","喷杆喷雾机","12m以下悬挂及牵引式喷杆喷雾机","邯郸市升华机械制造有限公司","喷杆式喷雾机","3WSH100型悬挂式喷杆喷雾机","形式:悬挂及牵引式:是 ;喷杆长度:8m;","1、规格型号：3WSH100；2、结构型式：悬挂式；3、运输状态外形尺寸(长×宽×高)mm：1950×880×1150；4、药箱容量L：400；5、喷杆作业(整机作业)常用工作压力mpa：0.3-0.5；6、喷杆喷幅M：8；7、配套泵名称：隔膜泵；8、配套泵工作压力mpa：2.5；9、配套泵流量L/min：45-48；10、配套泵转速r/min：550；11、配套喷头型式：扇形防滴喷头；12、配套喷头数量(个):16；13、配套喷头喷量（单个）L/min：1.6-1.8；","730","2010041401000041","2022-11-05","5200.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","植保机械","喷杆喷雾机","12-18m悬挂及牵引式喷杆喷雾机","邯郸市升华机械制造有限公司","喷杆式喷雾机","3WSH200A型悬挂式喷杆喷雾机","形式:悬挂及牵引式:是 ;喷杆长度:14m;","1、规格型号：3WSH200A；2、结构型式：悬挂式；3、运输状态外形尺寸(长×宽×高)mm：2860×2540×1950；4、药箱容量L：1000；5、喷杆作业(整机作业)常用工作压力mpa：0.3-0.5；6、喷杆喷幅M：14；7、配套泵名称：隔膜泵；8、配套泵工作压力mpa：3.0；9、配套泵流量L/min：70-80；10、配套泵转速r/min：550；11、配套喷头型式：扇形防滴喷头；12、配套喷头数量(个):28；13、配套喷头喷量（单个）L/min：1.6-1.8；","1650","2010041401000041","2022-11-05","17000.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","植保机械","喷杆喷雾机","18m及以上悬挂及牵引式喷杆喷雾机","邯郸市升华机械制造有限公司","喷杆式喷雾机","3WSH200C型悬挂式喷杆喷雾机","形式:悬挂及牵引式:是 ;喷杆长度:21m;","1、规格型号：3WSH200C；2、结构型式：悬挂式；3、运输状态外形尺寸(长×宽×高)mm：4000×2380×2460；4、药箱容量L：1200；5、喷杆作业(整机作业)常用工作压力mpa：0.3-0.5；6、喷杆喷幅M：21；7、配套泵名称：隔膜泵；8、配套泵工作压力mpa：2.0；9、配套泵流量L/min：163-170；10、配套泵转速r/min：550；11、配套喷头型式：扇形防滴喷头；12、配套喷头数量(个):42；13、配套喷头喷量（单个）L/min：1.6-1.8；","6300","2010041401000041","2022-11-05","46800.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","植保机械","喷杆喷雾机","18m及以上悬挂及牵引式喷杆喷雾机","邯郸市升华机械制造有限公司","喷杆式喷雾机","3WSH200D型悬挂式喷杆喷雾机","形式:悬挂及牵引式:是 ;喷杆长度:25m;","1、规格型号：3WSH200D；2、结构型式：悬挂式；3、运输状态外形尺寸(长×宽×高)mm：3050×5000×2300；4、药箱容量L：2000；5、喷杆作业(整机作业)常用工作压力mpa：0.3-0.5；6、喷杆喷幅M：25；7、配套泵名称：隔膜泵；8、配套泵工作压力mpa：2.0；9、配套泵流量L/min：163-170；10、配套泵转速r/min：550；11、配套喷头型式：扇形防滴喷头；12、配套喷头数量(个):50；13、配套喷头喷量（单个）L/min：1.6-1.8；","6300","2010041401000041","2022-11-05","52000.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","植保机械","喷杆喷雾机","18m及以上悬挂及牵引式喷杆喷雾机","邯郸市升华机械制造有限公司","喷杆式喷雾机","3WSH300型牵引式喷杆喷雾机","形式:悬挂及牵引式:是 ;喷杆长度:18m;","1、规格型号：3WSH300；2、结构型式：牵引式；3、运输状态外形尺寸(长×宽×高)mm：4410×2300×2220；4、药箱容量L：3000；5、喷杆作业(整机作业)常用工作压力mpa：0.3-0.5；6、喷杆喷幅M：18；7、配套泵名称：隔膜泵；8、配套泵工作压力mpa：2.0；9、配套泵流量L/min：160-170；10、配套泵转速r/min：550；11、配套喷头型式：扇形防滴喷头；12、配套喷头数量(个):36；13、配套喷头喷量（单个）L/min：1.6-1.8；","6300","2010041401000041","2022-11-05","56000.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","植保机械","喷杆喷雾机","18m及以上悬挂及牵引式喷杆喷雾机","邯郸市升华机械制造有限公司","喷杆式喷雾机","3W-1200VRT型悬挂式变量喷杆喷雾机","形式:悬挂及牵引式:是 ;喷杆长度:18m;","1、规格型号：3W-1200VRT；2、结构型式：悬挂式；3、运输状态外形尺寸(长×宽×高)mm：3010×3200×1900；4、药箱容量L：1200；5、喷杆作业(整机作业)常用工作压力mpa：0.3-0.5；6、喷杆喷幅M：18；7、配套泵名称：隔膜泵；8、配套泵工作压力mpa：2.0；9、配套泵流量L/min：130；10、配套泵转速r/min：550；11、配套喷头型式：扇形防滴喷头；12、配套喷头数量(个):37；13、配套喷头雾锥角（度）：110；14、配套喷头喷量（单个）L/min：1.6-1.8；15、配套喷头间隔(mm):500;","6300","2010041401000041","2022-11-05","49800.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","植保机械","喷杆喷雾机","18m及以上悬挂及牵引式喷杆喷雾机","邯郸市升华机械制造有限公司","喷杆式喷雾机","3W-1800VRT型悬挂式变量喷杆喷雾机","形式:悬挂及牵引式:是 ;喷杆长度:21m;","1、规格型号：3W-1800VRT；2、结构型式：悬挂式；3、运输状态外形尺寸(长×宽×高)mm：3560×4190×2190；4、药箱容量L：1800；5、喷杆作业(整机作业)常用工作压力mpa：0.3-0.5；6、喷杆喷幅M：21；7、配套泵名称：隔膜泵；8、配套泵工作压力mpa：2.0；9、配套泵流量L/min：163；10、配套泵转速r/min：550；11、配套喷头型式：扇形防滴喷头；12、配套喷头数量(个):42；13、配套喷头雾锥角（度）：110；14、配套喷头喷量（单个）L/min：1.6-1.8；15、配套喷头间隔(mm):500;","6300","2010041401000041","2022-11-05","58600.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","植保机械","喷杆喷雾机","18-50马力自走式喷杆喷雾机(两轮驱动)","华创机器人制造有限公司","自走式喷杆喷雾机","3WZP-600A","功率:24马力;形式:自走式,两驱:是 ;药箱容积:600L;离地间隙:0.3m;喷杆长度:7m;","规格型号：3WZP-600A；型式:自走式,两轮驱动，两轮转向；工作状态外形尺寸mm:3050×7000×2250；药箱容量L:600；喷杆长度mm:7000；喷头型式:扇形雾防滴喷头；喷杆升降机构型式:手动升降；喷杆折叠机构型式:液压折叠；配套泵型式:柱塞泵；配套泵流量l/min:45；离合器型式(自走式):摩擦式离合器；制动器型式(自走式):鼓式制动；驱动方式(自走式):前轮驱动；驾驶室(自走式):无；前/后最大轮距 (自走式)：1280/1280；轴距(自走式)mm:1530；前/后轮胎规格(自走式)前轮外径mm:900；前/后轮胎规格(自走式)前轮胎宽mm:120；前/后轮胎规格(自走式)后轮外径mm:900；前/后轮胎规格(自走式)后轮胎宽mm：120；前/后轮胎规格(自走式)前/后轮胎型式:橡胶充气轮胎;离地间隙mm：300；","14400","部20170820","2021-12-31","93000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","植保机械","喷杆喷雾机","18-50马力自走式喷杆喷雾机","青州泰达机械有限公司","自走式喷杆喷雾机","3WPZ-500A","功率:36.04马力;形式:自走式:是 ;四轮驱动,四轮转向:是 ;药箱容积:500L;离地间隙:1.015m;喷杆长度:10.6m;","产品名称：自走式喷杆喷雾机；规格型号：3WPZ-500A；型式：自走式；外形尺寸（长×宽×高）：工作状态3700×10790×2900mm，运输状态4500×1820×2900mm；药液箱容量：500L；喷杆作业常用工作压力：0.3-0.5MPa；喷头型式：扇形；喷杆长度：10.6m；配套动力：名称：柴油机发动机，结构型式：三缸四冲程水冷，标定功率/转速：26.5kw/2400（r/min）；配套泵：型式：隔膜泵，工作压力：1-3MPa，流量：70-100L/min；离地间隙：101.5cm；轴距：206cm，前/后最大轮距：150/150cm；驱动方式：四轮驱动；转向方式：四轮转向。","15500","鲁T2017028","2021-12-31","52000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","植保机械","喷杆喷雾机","18-50马力自走式喷杆喷雾机","华创机器人制造有限公司","自走式喷杆喷雾机","3WZP-600B","功率:24马力;形式:自走式:是 ;四轮驱动,四轮转向:是 ;药箱容积:600L;离地间隙:1.1m;喷杆长度:9.83m;","规格型号：3WZP-600B；型式:自走式,四轮驱动，四轮转向；外形尺寸(工作状态)mm:4000×9830×2880；药箱容量L:600；喷头型式:扇形雾防滴喷头；喷杆升降机构型式:电动升降；喷杆折叠机构型式:电动折叠；喷杆(喷杆长度)mm:9830；配套泵型式:三缸柱塞泵;配套泵流量l/min:52；离地间隙mm:1100；轴距(自走式)mm:1990；前/后最大轮距 (自走式)mm:1620/1620；","15500","部20180194","2022-12-31","93000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","植保机械","喷杆喷雾机","18-50马力自走式喷杆喷雾机","华创机器人制造有限公司","自走式喷杆喷雾机","3WZP-500A","功率:24马力;形式:自走式:是 ;四轮驱动,四轮转向:是 ;药箱容积:500L;离地间隙:/m;喷杆长度:10.5m;","规格型号：3WZP-500A；型式：自走式,四轮驱动，四轮转向；运输状态外形尺寸(长×宽×高)mm：3980×1770×2425;药箱容量L:500;喷杆喷幅m:10.5;配套泵名称:三缸柱塞泵;配套泵流量l/min:40;配套喷头型式:扇形雾喷头;配套喷头数量:22个；配套喷头雾锥角：110度；配套喷头喷量(单个)l/min：0.6；配套喷头间隔mm：500（中间）、170（两端）;","15500","部20170029","2021-12-31","91000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","植保机械","喷杆喷雾机","18-50马力自走式喷杆喷雾机","华创机器人制造有限公司","自走式喷杆喷雾机","3WZP-500B","功率:24马力;形式:自走式:是 ;四轮驱动,四轮转向:是 ;药箱容积:500L;离地间隙:1.09m;喷杆长度:9.84m;","规格型号：3WZP-500B；型式:自走式、四轮驱动，四轮转向；工作状态外形尺寸mm:3630×9840×2750；药箱容量L:500；喷头型式:扇形雾防滴喷头；喷杆升降机构型式:电动升降；喷杆折叠机构型式:电动折叠；喷杆长度mm:9840；配套泵型式:配套泵型式；配套泵流量l/min:21-34；离地间隙mm:1090；轴距mm(自走式):1320；前/后最大轮距 mm(自走式):1720/1720；前/后轮胎规格(自走式)前轮外径mm:900；前/后轮胎规格(自走式)前轮胎宽mm:120；前/后轮胎规格(自走式)后轮外径mm:900；前/后轮胎规格(自走式)后轮胎宽mm:120；前/后轮胎规格(自走式)前/后轮胎型式:橡胶充气轮胎；制动器型式(自走式):盘式制动；离合器型式(自走式):摩擦式离合器；","15500","部20170821","2021-12-31","91000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","植保机械","喷杆喷雾机","18-50马力自走式喷杆喷雾机","曲阜汇富机械制造有限公司","喷杆式喷雾机","3WPZ-700型自走式喷杆喷雾机","功率:50马力;形式:自走式:是 ;四轮驱动,四轮转向:是 ;药箱容积:700L;离地间隙:/m;喷杆长度:10.65m;","功率：50马力（36.8kW）结构形式：自走式；驱动形式：四轮驱动；转向形式：四轮转向；外形尺寸（长x宽x高）mm：4650x1680x2550；药箱额定容量：700L；喷杆长度：10650mm；配套泵名称：隔膜泵；配套泵流量：60L/min；","15500","2018281401000070","2024-01-01","51680.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，离地间隙未标明","","","","",""]
["田间管理机械","植保机械","喷杆喷雾机","18-50马力自走式喷杆喷雾机","常州尊隆内燃机配件有限公司","履带自走式喷杆喷雾机","ZL3WP-245","功率:14.7/kw马力;形式:自走式:是 ;四轮驱动,四轮转向:是 ;药箱容积:245L;离地间隙:0.14m;喷杆长度:12m;","18马力≤功率<50马力；形式:自走式,四轮驱动、四轮转向产品归档配置和技术参数形式是履带自走式,药箱容量是245L,喷杆作业常用工作压力0.2MPA到0.4MPA,喷头形式是扇形,折叠机构是上下折叠,喷杆长度是12米,配套动力是单缸水冷卧式柴油机,标定功率14,7KW,配套泵形式是三缸柱塞泵,工作压力是2.1MPA到4.0MPA,流量是301/MIN,离地间隙是145MM,轴距是760MM,制动器型式是鼓式,离合器形式是摩擦片,驱动方式两轮驱动自走式.","15500","苏农机（2017）第（0033）号","2021-12-31","86800.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过，承诺书不完整。","","","","",""]
["田间管理机械","植保机械","喷杆喷雾机","18-50马力自走式喷杆喷雾机","青州江隆机械有限公司","自走式喷杆喷雾机","3WPZ-700A","功率:48.96马力;形式:自走式:是 ;四轮驱动,四轮转向:是 ;药箱容积:700L;离地间隙:0.95m;喷杆长度:10.4m;","型式：自走式；规格型号：3WPZ-700A；工作状态外形尺寸(mm)：4200*10400*2960；运输状态外形尺寸(mm)：4600*1780*2960；药箱容量（L）：700；喷杆作业（整机作业）常用工作压力（MPa）：0.3-0.5；喷头型式：扇形雾防滴喷头；喷杆升降机构型式：液压升降；喷杆折叠机构型式：液压折叠；喷杆长度（mm）：10400；配套动力名称、结构型式：四缸水冷四冲程柴油机；配套动力标定功率/转速（kW/r/min）：36/2400；配套泵型式：隔膜泵；配套泵工作压力（MPa）：0-2.5；配套泵流量（L/min）：60；离地间隙（mm）：950；轴距（mm）：2320；前/后最大轮距(mm)：1510/1510；前轮外径（mm）：930；前轮胎宽（mm）：100；后轮外径（mm）：930；后轮胎宽（mm）：100；前/后轮胎型式：充气轮胎；制动器型式：鼓式；离合器型式：摩擦片式；驱动方式：四轮驱动（四轮转向）；驾驶室：无","15500","部20181020","2022-12-31","52000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","植保机械","喷杆喷雾机","18-50马力自走式喷杆喷雾机","青州市禾田农业装备有限公司","自走式喷杆喷雾机","3WPZ-700A","功率:50马力;形式:自走式:是 ;四轮驱动,四轮转向:是 ;药箱容积:700L;离地间隙:0.98m;喷杆长度:10.16m;","功率：50马力(36.8kw) 形式：自走式，四轮驱动、四轮转向 外形尺寸(mm)工作状态4100×10160×2350运输状态4400×1845×2350 配套泵：齿轮泵 喷杆：液压升降、液压折叠        药箱容积：700L   离地间隙：980(mm)    喷杆长度：10160(mm)","15500","部20180351","2022-12-31","51600.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","植保机械","喷杆喷雾机","50-100马力自走式喷杆喷雾机","青州泰达机械有限公司","喷杆式喷雾机","3WPZ-1600型自走式喷杆喷雾机","功率:50.05马力;形式:自走式:是 ;四轮驱动,四轮转向:是 ;药箱容积:1600L;离地间隙:1.0m;喷杆长度:16.7m;","品目：喷杆喷雾机；型号规格：3WPZ-1600;结构型式：自走式；外形尺寸（mm）：5670×2860×2940;工作压力（Mpa）：0.3-0.5；驱动型式：四轮驱动；转向型式：四轮转向；喷杆长度（mm）：16700；喷杆折叠型式：液压折叠；喷杆升降型式：液压升降；最小离地间隙（mm）：1000；驾驶室型式：无；轴距（mm）：2750；前最大轮距（mm）：2350；后最大轮距（mm）：2350；前轮外径（mm）：1000；前轮胎宽（mm）：200；前轮轮胎型式：充气橡胶轮胎；后轮外径（mm）：1000；后轮胎宽（mm）：200；后轮轮胎型式：充气橡胶轮胎；限压安全装置结构型式：弹簧式；限压安全装置限定压力（Mpa）：≤0.6;配套动力名称：柴油机；配套动力结构型式：四缸水冷四冲程；配套动力标定功率（kW）：74；配套动力标定转速（r/min）：2400；液泵结构型式：隔膜泵；液泵额定压力（Mpa）：2.5；液泵额定流量（L/min）：160-180；药箱材质：塑料；药箱容积（L）：1600；喷杆材质：不锈钢；喷射部件最高允许工作压力（Mpa）：2.76；承压软管允许最大工作压力：2.76(400psi)；蓄电池类型：免维护铅酸蓄电池；蓄电池容量（Ah）：40；蓄电池标称电压（V）：12x2（串联）。","18600","2015041401000121","2020-12-16","62000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","植保机械","喷杆喷雾机","50-100马力自走式喷杆喷雾机","青州泰达机械有限公司","喷杆式喷雾机","3WPZ-1000AD型自走式喷杆喷雾机","功率:100.64马力;形式:自走式:是 ;四轮驱动,四轮转向:是 ;药箱容积:1000L;离地间隙:0.95m;喷杆长度:18.5m;","品目：喷杆喷雾机；型号规格：3WPZ-1000AD;结构型式：自走式；外形尺寸（mm）：4950x2400x3045;工作压力（Mpa）：0.3-0.5；驱动型式：四轮驱动；转向型式：四轮转向；喷杆长度（mm）：18500；喷杆折叠型式：液压折叠；喷杆升降型式：液压升降；最小离地间隙（mm）：950；驾驶室型式：无；轴距（mm）：2720；前最大轮距（mm）：1820；后最大轮距（mm）：1820；前轮外径（mm）：930；前轮胎宽（mm）：120；前轮轮胎型式：充气橡胶轮胎；后轮外径（mm）：930；后轮胎宽（mm）：120；后轮轮胎型式：充气橡胶轮胎；限压安全装置结构型式：弹簧式；限压安全装置限定压力（Mpa）：≤0.6;配套动力名称：柴油机；配套动力结构型式：四缸水冷四冲程；配套动力标定功率（kW）：74；配套动力标定转速（r/min）：2400；液泵结构型式：隔膜泵；液泵额定压力（Mpa）：3.0；液泵额定流量（L/min）：100；药箱材质：塑料；药箱容积（L）：1000；喷杆材质：不锈钢+塑料；喷射部件最高允许工作压力（Mpa）：4.0；蓄电池类型：免维护铅酸蓄电池；蓄电池容量（Ah）：60；蓄电池标称电压（V）：12x2（串联）。","18600","2018281401000013","2023-03-04","65000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","植保机械","喷杆喷雾机","50-100马力自走式喷杆喷雾机","邯郸市升华机械制造有限公司","喷杆式喷雾机","3WSHZ2000-21型自走式喷杆喷雾机","功率:90马力;形式:自走式:是 ;四轮驱动,四轮转向:是 ;药箱容积:2000L;离地间隙:1.6m;喷杆长度:21m;","1、规格型号：3WSHZ2000-21；2、结构型式：自走式；3、运输状态外形尺寸(长×宽×高)mm：6400×3110×3280；4、整机工作压力mpa：0.3-0.5；5、整机喷杆展开宽度M：21；6、限压安全装置结构形式：微启式安全阀；7、限压安全装置限定压力Mpa：0.6；8、配套动力名称：柴油机；9、配套动力结构形式：四缸立式四冲程水冷循环式；10、配套动力标定功率KW：66.2；11、配套动力标定转速r/min：2300；12、液泵结构形式：隔膜泵；13、液泵额定压力Mpa:2.0；14、液泵额定流量L/min：163；15、药箱材质：不锈钢；16、药箱容积L：2000；17、喷射部件喷杆材质：不锈钢；18、喷射部件最高允许工作压力Mpa：3；19、蓄电池类型：铅酸蓄电池；20、蓄电池容量Ah：60；21、蓄电池标称电压V：12。","18600","2010041401000041","2022-11-05","148000.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","植保机械","喷杆喷雾机","50-100马力自走式喷杆喷雾机","邯郸市升华机械制造有限公司","喷杆式喷雾机","3WSHZ600-12型自走式喷杆喷雾机","功率:55马力;形式:自走式:是 ;四轮驱动,四轮转向:是 ;药箱容积:600L;离地间隙:1.6m;喷杆长度:12m;","1、规格型号：3WSHZ600-12；2、结构型式：自走式；3、运输状态外形尺寸(长×宽×高)mm：4600×2300×3270；4、整机工作压力mpa：0.3-0.5；5、整机喷杆展开宽度M：12；6、限压安全装置结构形式：微启式安全阀；7、限压安全装置限定压力Mpa：0.6；8、配套动力名称：柴油机；9、配套动力结构形式：四缸立式四冲程水冷循环式；10、配套动力标定功率KW：40.4；11、配套动力标定转速r/min：2400；12、液泵结构形式：隔膜泵；13、液泵额定压力Mpa:2.0；14、液泵额定流量L/min：65.5；15、药箱材质：不锈钢；16、药箱容积L：600；17、喷射部件喷杆材质：不锈钢；18、喷射部件最高允许工作压力Mpa：3；19、蓄电池类型：铅酸蓄电池；20、蓄电池容量Ah：60；21、蓄电池标称电压V：12。","18600","2010041401000041","2022-11-05","98000.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","植保机械","喷杆喷雾机","50-100马力自走式喷杆喷雾机","华创机器人制造有限公司","自走式喷杆喷雾机","3WZP-1300A","功率:50马力;形式:自走式:是 ;四轮驱动,四轮转向:是 ;药箱容积:1300L;离地间隙:0.62m;喷杆长度:10.199999999999999m;","规格型号：3WZP-1300A；型 式：自走式,四轮驱动，四轮转向；工作状态外形尺寸mm：6230×10200×2590;药箱容量L:1300;喷头型式:扇形，雾锥角110°;喷杆升降机构型式:自动式液压缸;喷杆折叠机构型式:电动液压推杆;喷杆喷杆长度m:10.199999999999999；配套泵型式:齿轮式高压喷雾泵;配套泵流量l/min:60;离地间隙m:0.62;轴距(自走式)m:2.7;","18600","鄂2018008","2022-12-31","103000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","植保机械","喷杆喷雾机","50-100马力自走式喷杆喷雾机","华创机器人制造有限公司","自走式喷杆喷雾机","3WZP-800B","功率:50马力;形式:自走式:是 ;四轮驱动,四轮转向:是 ;药箱容积:800L;离地间隙:1.01m;喷杆长度:11.94m;","规格型号：3WZP-800B；型式：自走式,四轮驱动，四轮转向；外形尺寸mm(工作状态)：4700×11940×2880；药箱容量L:800；喷头型式:扇形雾防滴喷头；喷杆升降机构型式:液压升降；喷杆折叠机构型式:液压折叠；喷杆(喷杆长度)mm:11940；配套泵型式:齿轮泵；配套泵流量l/min:60；离地间隙mm:1010；轴距(自走式)mm:2320；","18600","部20180195","2022-12-31","101000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过","","","","",""]
["田间管理机械","植保机械","喷杆喷雾机","50-100马力自走式喷杆喷雾机","青州爱科机械科技有限公司","喷杆式喷雾机","3WPZ-1500A型自走式喷杆喷雾机","功率:50马力;形式:自走式:是 ;四轮驱动,四轮转向:是 ;药箱容积:1500L;离地间隙:1m;喷杆长度:18.4m;","产品品目：喷杆喷雾机；驱动型式：四轮驱动；转向型式：四轮转向；结构型式：自走式；柴油机功率:36.8kW/2500r/min；整机尺寸(mm)4900×2400×2650;喷杆长度:18400mm;工作压力(MPa):0.3~0.6;药箱容积:1500L,配套泵:齿轮式高压喷射泵(流量:60L/min)","18600","2015041401000069","2024-06-02","65000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过","","","","",""]
["田间管理机械","植保机械","喷杆喷雾机","100马力及以上自走式喷杆喷雾机(两轮驱动)","青州市东禾农业科技有限公司","喷杆式喷雾机","3WPZ-2000G型自走式喷杆喷雾机","功率:100马力;形式:自走式,两驱:是 ;药箱容积:2000L;离地间隙:/m;喷杆长度:16m;","功率：100马力(74kw)     形式：自走式，四轮驱动、四轮转向    外形尺寸(mm)4700×2900×2700     配套泵：隔膜泵 喷杆：液压升降、液压折叠      药箱容积：2000L    喷杆长度：16m","39000","2019281401000003","2024-04-01","130000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","植保机械","喷杆喷雾机","100马力及以上自走式喷杆喷雾机","青州泰达机械有限公司","喷杆式喷雾机","3WPZ-1600G型自走式喷杆喷雾机","功率:100.64马力;形式:自走式:是 ;四轮驱动,四轮转向:是 ;药箱容积:1600L;离地间隙:1.5m;喷杆长度:18.34m;","品目：喷杆喷雾机；型号规格：3WPZ-1600G;结构型式：自走式；外形尺寸（mm）：5200x3100x3750;工作压力（Mpa）：0.3-0.5；驱动型式：四轮驱动；转向型式：四轮转向；喷杆长度（mm）：18340；喷杆折叠型式：液压折叠；喷杆升降型式：液压升降；最小离地间隙（mm）：1500；驾驶室型式：无；轴距（mm）：2720；前最大轮距（mm）：2600；后最大轮距（mm）：2600；前轮外径（mm）：1200；前轮胎宽（mm）：180；前轮轮胎型式：充气橡胶轮胎；后轮外径（mm）：1200；后轮胎宽（mm）：180；后轮轮胎型式：充气橡胶轮胎；限压安全装置结构型式：弹簧式；限压安全装置限定压力（Mpa）：≤0.6;配套动力名称：柴油机；配套动力结构型式：四缸水冷四冲程；配套动力标定功率（kW）：74；配套动力标定转速（r/min）：2400；液泵结构型式：隔膜泵；液泵额定压力（Mpa）：2.5；液泵额定流量（L/min）：160-180；药箱材质：塑料；药箱容积（L）：1600；喷杆材质：不锈钢；喷射部件最高允许工作压力（Mpa）：4.0；蓄电池类型：免维护铅酸蓄电池；蓄电池容量（Ah）：60；蓄电池标称电压（V）：12x2（串联）。","40100","2018281401000013","2023-03-04","135000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","植保机械","喷杆喷雾机","100马力及以上自走式喷杆喷雾机","青州泰达机械有限公司","喷杆式喷雾机","3WPZ-2000AD型自走式喷杆喷雾机","功率:100.64马力;形式:自走式:是 ;四轮驱动,四轮转向:是 ;药箱容积:2000L;离地间隙:1.15m;喷杆长度:18.34m;","品目：喷杆喷雾机；型号规格：3WPZ-2000AD;结构型式：自走式；外形尺寸（mm）：5300x2820x3350;工作压力（Mpa）：0.3-0.5；驱动型式：四轮驱动；转向型式：四轮转向；喷杆长度（mm）：18340；喷杆折叠型式：液压折叠；喷杆升降型式：液压升降；最小离地间隙（mm）：1150；驾驶室型式：无；轴距（mm）：2310；前最大轮距（mm）：2280；后最大轮距（mm）：2280；前轮外径（mm）：1060；前轮胎宽（mm）：230；前轮轮胎型式：充气橡胶轮胎；后轮外径（mm）：1060；后轮胎宽（mm）：230；后轮轮胎型式：充气橡胶轮胎；限压安全装置结构型式：弹簧式；限压安全装置限定压力（Mpa）：≤0.6;配套动力名称：柴油机；配套动力结构型式：四缸水冷四冲程；配套动力标定功率（kW）：74；配套动力标定转速（r/min）：2400；液泵结构型式：隔膜泵；液泵额定压力（Mpa）：2.5；液泵额定流量（L/min）：280；药箱材质：塑料；药箱容积（L）：1000x2；喷杆材质：不锈钢；喷射部件最高允许工作压力（Mpa）：16；蓄电池类型：免维护铅酸蓄电池；蓄电池容量（Ah）：60；蓄电池标称电压（V）：12x2（串联）。","40100","2018281401000013","2023-03-04","135000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","植保机械","喷杆喷雾机","100马力及以上自走式喷杆喷雾机","青州泰达机械有限公司","喷杆式喷雾机","3WPZ-2000G型自走式喷杆喷雾机","功率:100.64马力;形式:自走式:是 ;四轮驱动,四轮转向:是 ;药箱容积:2000L;离地间隙:1.72m;喷杆长度:18.34m;","品目：喷杆喷雾机；型号规格：3WPZ-2000G;结构型式：自走式；外形尺寸（mm）：5800x2940x4000;工作压力（Mpa）：0.3-0.5；驱动型式：四轮驱动；转向型式：四轮转向；喷杆长度（mm）：18340；喷杆折叠型式：液压折叠；喷杆升降型式：液压升降；最小离地间隙（mm）：1720；驾驶室型式：无；轴距（mm）：2300；前最大轮距（mm）：2600；后最大轮距（mm）：2600；前轮外径（mm）：1180；前轮胎宽（mm）：180；前轮轮胎型式：充气橡胶轮胎；后轮外径（mm）：1180；后轮胎宽（mm）：180；后轮轮胎型式：充气橡胶轮胎；限压安全装置结构型式：弹簧式；限压安全装置限定压力（Mpa）：≤0.6;配套动力名称：柴油机；配套动力结构型式：四缸水冷四冲程；配套动力标定功率（kW）：74；配套动力标定转速（r/min）：2400；液泵结构型式：隔膜泵；液泵额定压力（Mpa）：2.5；液泵额定流量（L/min）：280；药箱材质：塑料；药箱容积（L）：1000x2；喷杆材质：不锈钢；喷射部件最高允许工作压力（Mpa）：16；蓄电池类型：免维护铅酸蓄电池；蓄电池容量（Ah）：60；蓄电池标称电压（V）：12x2（串联）。","40100","2018281401000013","2023-03-04","135000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","植保机械","喷杆喷雾机","100马力及以上自走式喷杆喷雾机","青州泰达机械有限公司","喷杆式喷雾机","3WPZ-3000AD型自走式喷杆喷雾机","功率:100.64马力;形式:自走式:是 ;四轮驱动,四轮转向:是 ;药箱容积:3000L;离地间隙:1.02m;喷杆长度:18.34m;","品目：喷杆喷雾机；型号规格：3WPZ-3000AD;结构型式：自走式；外形尺寸（mm）：5200x2800x3280;工作压力（Mpa）：0.3-0.5；驱动型式：四轮驱动；转向型式：四轮转向；喷杆长度（mm）：18340；喷杆折叠型式：液压折叠；喷杆升降型式：液压升降；最小离地间隙（mm）：1020；驾驶室型式：无；轴距（mm）：2310；前最大轮距（mm）：2280；后最大轮距（mm）：2280；前轮外径（mm）：1060；前轮胎宽（mm）：230；前轮轮胎型式：充气橡胶轮胎；后轮外径（mm）：1060；后轮胎宽（mm）：230；后轮轮胎型式：充气橡胶轮胎；限压安全装置结构型式：弹簧式；限压安全装置限定压力（Mpa）：≤0.6;配套动力名称：柴油机；配套动力结构型式：四缸水冷四冲程；配套动力标定功率（kW）：74；配套动力标定转速（r/min）：2400；液泵结构型式：隔膜泵；液泵额定压力（Mpa）：2.5；液泵额定流量（L/min）：280；药箱材质：塑料；药箱容积（L）：1500x2；喷杆材质：不锈钢；喷射部件最高允许工作压力（Mpa）：16；蓄电池类型：免维护铅酸蓄电池；蓄电池容量（Ah）：60；蓄电池标称电压（V）：12x2（串联）。","40100","2018281401000013","2023-03-04","135000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","植保机械","喷杆喷雾机","100马力及以上自走式喷杆喷雾机","青州泰达机械有限公司","喷杆式喷雾机","3WPZ-3000C型自走式喷杆喷雾机","功率:100.64马力;形式:自走式:是 ;四轮驱动,四轮转向:是 ;药箱容积:3000L;离地间隙:1.05m;喷杆长度:18.34m;","品目：喷杆喷雾机；型号规格：3WPZ-3000C;结构型式：自走式；外形尺寸（mm）：5640x2750x3300;工作压力（Mpa）：0.3-0.5；驱动型式：四轮驱动；转向型式：四轮转向；喷杆长度（mm）：18340；喷杆折叠型式：液压折叠；喷杆升降型式：液压升降；最小离地间隙（mm）：1050；驾驶室型式：密封式；轴距（mm）：2310；前最大轮距（mm）：2280；后最大轮距（mm）：2280；前轮外径（mm）：1060；前轮胎宽（mm）：230；前轮轮胎型式：充气橡胶轮胎；后轮外径（mm）：1060；后轮胎宽（mm）：230；后轮轮胎型式：充气橡胶轮胎；限压安全装置结构型式：弹簧式；限压安全装置限定压力（Mpa）：≤0.6;配套动力名称：柴油机；配套动力结构型式：四缸水冷四冲程；配套动力标定功率（kW）：74；配套动力标定转速（r/min）：2400；液泵结构型式：隔膜泵；液泵额定压力（Mpa）：2.5；液泵额定流量（L/min）：280；药箱材质：塑料；药箱容积（L）：1500x2；喷杆材质：不锈钢；喷射部件最高允许工作压力（Mpa）：16；蓄电池类型：免维护铅酸蓄电池；蓄电池容量（Ah）：60；蓄电池标称电压（V）：12x2（串联）。","40100","2018281401000013","2023-03-04","135000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","植保机械","喷杆喷雾机","100马力及以上自走式喷杆喷雾机","青州爱科机械科技有限公司","喷杆式喷雾机","3WPZ-4500-4型自走式喷杆喷雾机","功率:100马力;形式:自走式:是 ;四轮驱动,四轮转向:是 ;药箱容积:1500*3L;离地间隙:1m;喷杆长度:18.4m;","产品品目：喷杆喷雾机；驱动型式：四轮驱动；转向型式：四轮转向；结构型式：自走式；柴油机功率:74kW/2400r/min；整机尺寸(mm)5800×2500×2700;喷杆长度:18400mm;工作压力(MPa):0.3~0.6;药箱容积:1500×3L,配套泵:隔膜泵(流量:280L/min)","40100","2015041401000069","2024-06-02","165000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","植保机械","喷杆喷雾机","100马力及以上自走式喷杆喷雾机","青州爱科机械科技有限公司","喷杆式喷雾机","3WPZ-1500B型自走式喷杆喷雾机","功率:100马力;形式:自走式:是 ;四轮驱动,四轮转向:是 ;药箱容积:1500L;离地间隙:1m;喷杆长度:18.4m;","产品品目：喷杆喷雾机；驱动型式：四轮驱动；转向型式：四轮转向；结构型式：自走式；柴油机功率:74kW/2400r/min；整机尺寸(mm)5020×2300×2650;喷杆长度:18400mm;工作压力(MPa):0.3~0.6;药箱容积:1500L,配套泵:齿轮式高压喷射泵(流量:60L/min)","40100","2015041401000069","2024-06-02","160000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","植保机械","喷杆喷雾机","100马力及以上自走式喷杆喷雾机","华创机器人制造有限公司","自走式喷杆喷雾机","3WZP-2000A","功率:125马力;形式:自走式:是 ;四轮驱动,四轮转向:是 ;药箱容积:2000L;离地间隙:/m;喷杆长度:18m;","规格型号：3WZP-2000A；型式：自走式、四轮驱动、四轮转向；运输状态外形尺寸(长×宽×高)mm：7310×3360×3750；药箱容量L:2000；喷杆喷幅m：18；配套泵名称：隔膜泵；配套泵流量l/min：215；配套喷头型式：扇形雾喷头；配套喷头数量：36个；配套喷头雾锥角度:110；配套喷头喷量(单个)l/min：1.2左右；配套喷头间隔mm：500;","40100","部20160580","2020-12-31","168000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","植保机械","喷杆喷雾机","100马力及以上自走式喷杆喷雾机","华创机器人制造有限公司","自走式喷杆喷雾机","3WZP-4000A","功率:270马力;形式:自走式:是 ;四轮驱动,四轮转向:是 ;药箱容积:4000L;离地间隙:/m;喷杆长度:28m;","规格型号：3WZP-4000A；型式:自走式、四轮驱动、四轮转向；运输状态外形尺寸(长×宽×高)mm：8160×3740×3800；药箱容量L:4000；喷杆喷幅m:28；配套泵名称：离心泵；配套泵流量l/min：167～784；配套喷头型式：扇形雾喷头；配套喷头数量：56个；配套喷头雾锥角：110度；配套喷头喷量(单个)l/min：1.8（红）、2.4（棕）、2.7（灰）；配套喷头间隔mm：500；","40100","部20160581","2020-12-31","182000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","植保机械","喷杆喷雾机","100马力及以上自走式喷杆喷雾机","青州江隆机械有限公司","喷杆式喷雾机","3WPZ-1600G型自走式喷杆喷雾机","功率:100.64马力;形式:自走式:是 ;四轮驱动,四轮转向:是 ;药箱容积:1600L;离地间隙:1.5m;喷杆长度:18.34m;","品目：喷杆喷雾机；型号规格：3WPZ-1600G;结构型式：自走式；外形尺寸（mm）：5200x3100x3750;工作压力（Mpa）：0.3-0.5；驱动型式：四轮驱动；转向型式：四轮转向；喷杆长度（mm）：18340；喷杆折叠型式：液压折叠；喷杆升降型式：液压升降；最小离地间隙（mm）：1500；驾驶室型式：无；轴距（mm）：2720；前最大轮距（mm）：2600；后最大轮距（mm）：2600；前轮外径（mm）：1200；前轮胎宽（mm）：180；前轮轮胎型式：充气橡胶轮胎；后轮外径（mm）：1200；后轮胎宽（mm）：180；后轮轮胎型式：充气橡胶轮胎；限压安全装置结构型式：弹簧式；限压安全装置限定压力（Mpa）：≤0.6;配套动力名称：柴油机；配套动力结构型式：四缸水冷四冲程；配套动力标定功率（kW）：74；配套动力标定转速（r/min）：2400；液泵结构型式：隔膜泵；液泵额定压力（Mpa）：2.5；液泵额定流量（L/min）：160-180；药箱材质：塑料；药箱容积（L）：1600；喷杆材质：不锈钢；喷射部件最高允许工作压力（Mpa）：4.0；蓄电池类型：免维护铅酸蓄电池；蓄电池容量（Ah）：60；蓄电池标称电压（V）：12x2（串联）。","40100","2018281401000011","2023-02-26","135000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","植保机械","喷杆喷雾机","100马力及以上自走式喷杆喷雾机","青州江隆机械有限公司","喷杆式喷雾机","3WPZ-2000AD型自走式喷杆喷雾机","功率:100.64马力;形式:自走式:是 ;四轮驱动,四轮转向:是 ;药箱容积:2000L;离地间隙:1.15m;喷杆长度:18.34m;","品目：喷杆喷雾机；型号规格：3WPZ-2000AD;结构型式：自走式；外形尺寸（mm）：5300x2820x3350;工作压力（Mpa）：0.3-0.5；驱动型式：四轮驱动；转向型式：四轮转向；喷杆长度（mm）：18340；喷杆折叠型式：液压折叠；喷杆升降型式：液压升降；最小离地间隙（mm）：1150；驾驶室型式：无；轴距（mm）：2310；前最大轮距（mm）：2280；后最大轮距（mm）：2280；前轮外径（mm）：1060；前轮胎宽（mm）：230；前轮轮胎型式：充气橡胶轮胎；后轮外径（mm）：1060；后轮胎宽（mm）：230；后轮轮胎型式：充气橡胶轮胎；限压安全装置结构型式：弹簧式；限压安全装置限定压力（Mpa）：≤0.6;配套动力名称：柴油机；配套动力结构型式：四缸水冷四冲程；配套动力标定功率（kW）：74；配套动力标定转速（r/min）：2400；液泵结构型式：隔膜泵；液泵额定压力（Mpa）：2.5；液泵额定流量（L/min）：280；药箱材质：塑料；药箱容积（L）：1000x2；喷杆材质：不锈钢；喷射部件最高允许工作压力（Mpa）：16；蓄电池类型：免维护铅酸蓄电池；蓄电池容量（Ah）：60；蓄电池标称电压（V）：12x2（串联）。","40100","2018281401000011","2023-02-26","135000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","植保机械","喷杆喷雾机","100马力及以上自走式喷杆喷雾机","青州江隆机械有限公司","喷杆式喷雾机","3WPZ-2000G型自走式喷杆喷雾机","功率:100.64马力;形式:自走式:是 ;四轮驱动,四轮转向:是 ;药箱容积:2000L;离地间隙:1.72m;喷杆长度:18.34m;","品目：喷杆喷雾机；型号规格：3WPZ-2000G;结构型式：自走式；外形尺寸（mm）：5800x2940x4000;工作压力（Mpa）：0.3-0.5；驱动型式：四轮驱动；转向型式：四轮转向；喷杆长度（mm）：18340；喷杆折叠型式：液压折叠；喷杆升降型式：液压升降；最小离地间隙（mm）：1720；驾驶室型式：无；轴距（mm）：2300；前最大轮距（mm）：2600；后最大轮距（mm）：2600；前轮外径（mm）：1180；前轮胎宽（mm）：180；前轮轮胎型式：充气橡胶轮胎；后轮外径（mm）：1180；后轮胎宽（mm）：180；后轮轮胎型式：充气橡胶轮胎；限压安全装置结构型式：弹簧式；限压安全装置限定压力（Mpa）：≤0.6;配套动力名称：柴油机；配套动力结构型式：四缸水冷四冲程；配套动力标定功率（kW）：74；配套动力标定转速（r/min）：2400；液泵结构型式：隔膜泵；液泵额定压力（Mpa）：2.5；液泵额定流量（L/min）：280；药箱材质：塑料；药箱容积（L）：1000x2；喷杆材质：不锈钢；喷射部件最高允许工作压力（Mpa）：16；蓄电池类型：免维护铅酸蓄电池；蓄电池容量（Ah）：60；蓄电池标称电压（V）：12x2（串联）。","40100","2018281401000011","2023-02-26","135000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过","","","","",""]
["田间管理机械","植保机械","喷杆喷雾机","100马力及以上自走式喷杆喷雾机","青州江隆机械有限公司","喷杆式喷雾机","3WPZ-3000AD型自走式喷杆喷雾机","功率:100.64马力;形式:自走式:是 ;四轮驱动,四轮转向:是 ;药箱容积:3000L;离地间隙:1.02m;喷杆长度:18.34m;","品目：喷杆喷雾机；型号规格：3WPZ-3000AD;结构型式：自走式；外形尺寸（mm）：5200x2800x3280;工作压力（Mpa）：0.3-0.5；驱动型式：四轮驱动；转向型式：四轮转向；喷杆长度（mm）：18340；喷杆折叠型式：液压折叠；喷杆升降型式：液压升降；最小离地间隙（mm）：1020；驾驶室型式：无；轴距（mm）：2310；前最大轮距（mm）：2280；后最大轮距（mm）：2280；前轮外径（mm）：1060；前轮胎宽（mm）：230；前轮轮胎型式：充气橡胶轮胎；后轮外径（mm）：1060；后轮胎宽（mm）：230；后轮轮胎型式：充气橡胶轮胎；限压安全装置结构型式：弹簧式；限压安全装置限定压力（Mpa）：≤0.6;配套动力名称：柴油机；配套动力结构型式：四缸水冷四冲程；配套动力标定功率（kW）：74；配套动力标定转速（r/min）：2400；液泵结构型式：隔膜泵；液泵额定压力（Mpa）：2.5；液泵额定流量（L/min）：280；药箱材质：塑料；药箱容积（L）：1500x2；喷杆材质：不锈钢；喷射部件最高允许工作压力（Mpa）：16；蓄电池类型：免维护铅酸蓄电池；蓄电池容量（Ah）：60；蓄电池标称电压（V）：12x2（串联）。","40100","2018281401000011","2023-02-26","135000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","植保机械","喷杆喷雾机","100马力及以上自走式喷杆喷雾机","青州江隆机械有限公司","喷杆式喷雾机","3WPZ-3000C型自走式喷杆喷雾机","功率:100.64马力;形式:自走式:是 ;四轮驱动,四轮转向:是 ;药箱容积:3000L;离地间隙:1.05m;喷杆长度:18.34m;","品目：喷杆喷雾机；型号规格：3WPZ-3000C;结构型式：自走式；外形尺寸（mm）：5640x2750x3300;工作压力（Mpa）：0.3-0.5；驱动型式：四轮驱动；转向型式：四轮转向；喷杆长度（mm）：18340；喷杆折叠型式：液压折叠；喷杆升降型式：液压升降；最小离地间隙（mm）：1050；驾驶室型式：密封式；轴距（mm）：2310；前最大轮距（mm）：2280；后最大轮距（mm）：2280；前轮外径（mm）：1060；前轮胎宽（mm）：230；前轮轮胎型式：充气橡胶轮胎；后轮外径（mm）：1060；后轮胎宽（mm）：230；后轮轮胎型式：充气橡胶轮胎；限压安全装置结构型式：弹簧式；限压安全装置限定压力（Mpa）：≤0.6;配套动力名称：柴油机；配套动力结构型式：四缸水冷四冲程；配套动力标定功率（kW）：74；配套动力标定转速（r/min）：2400；液泵结构型式：隔膜泵；液泵额定压力（Mpa）：2.5；液泵额定流量（L/min）：280；药箱材质：塑料；药箱容积（L）：1500x2；喷杆材质：不锈钢；喷射部件最高允许工作压力（Mpa）：16；蓄电池类型：免维护铅酸蓄电池；蓄电池容量（Ah）：60；蓄电池标称电压（V）：12x2（串联）。","40100","2018281401000011","2023-02-26","135000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","植保机械","喷杆喷雾机","100马力及以上自走式喷杆喷雾机","山东中农嘉禾机械科技有限公司","喷杆式喷雾机","3WPZ-3000型自走式喷杆喷雾机","功率:100马力;形式:自走式:是 ;四轮驱动,四轮转向:是 ;药箱容积:(1500×2)L;离地间隙:1.13m;喷杆长度:18m;","功率：100马力（74kW);形式：自走式、四轮驱动、四轮转向。离地间隙：1.13m;药箱容积：1500L×2，喷杆长度：18m；工作压力（MPa)：0.2~0.4；整机尺寸（mm）5460×2850×2930,配套泵：隔膜泵（流量：280L/min),","40100","2019041401000010","2024-01-29","138000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","植保机械","喷杆喷雾机","100马力及以上自走式喷杆喷雾机","青州市禾田农业装备有限公司","喷杆式喷雾机","3WPZ-1000型自走式喷杆喷雾机","功率:100马力;形式:自走式:是 ;四轮驱动,四轮转向:是 ;药箱容积:1000L;离地间隙:0.93m;喷杆长度:19m;","功率：100马力(74kw)      形式：自走式，四轮驱动、四轮转向       外形尺寸(mm)：4500×2000×2400       配套泵：齿轮泵       喷杆：液压升降、液压折叠      最小离地间隙：930(mm)      喷杆长度：190000(mm)      药箱容积：1000L","40100","2018281401000003","2023-02-11","133600.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","植保机械","喷杆喷雾机","100马力及以上自走式喷杆喷雾机","青州市禾田农业装备有限公司","喷杆式喷雾机","3WPZ-2800型自走式喷杆喷雾机","功率:100马力;形式:自走式:是 ;四轮驱动,四轮转向:是 ;药箱容积:2800L;离地间隙:1.05m;喷杆长度:20m;","功率：100马力(74kw) 形式：自走式，四轮驱动、四轮转向 外形尺寸(mm)5400×2900×2900配套泵：隔膜泵 喷杆：液压升降、液压折叠  喷杆长度：20000(mm)     最小离地间隙：1050(mm)     药箱容积：2800L","40100","2018281401000003","2023-02-11","133700.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","植保机械","喷杆喷雾机","100马力及以上自走式喷杆喷雾机","青州市奥林工程机械有限公司","喷杆式喷雾机","3WPZ-4500-4型自走式喷杆喷雾机","功率:100马力;形式:自走式:是 ;四轮驱动,四轮转向:是 ;药箱容积:1500*3L;离地间隙:910m;喷杆长度:18.4m;","产品品目：喷杆喷雾机；驱动型式：四轮驱动；转向型式：四轮转向；结构型式：自走式；柴油机功率:74kW/2400r/min；整机尺寸(mm)5800×2500×2700;喷杆长度:18400mm;工作压力(MPa):0.3~0.6;药箱容积:1500×3L,配套泵:隔膜泵(流量:280L/min)","40100","2019041401000006","2024-01-24","160000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","植保机械","风送喷雾机","药箱容积≥300L;喷幅半径≥20m自走式","昆明鸿溪机电有限公司","风送式喷雾机","3WFZL-380A型自走式风送喷雾机","形式:自走式 ;药箱容积:380L;喷幅半径:35m;","整机结构型式：自走式；药箱容积：380L；喷幅半径：35m","6000","2018281401000048","2023-07-30","20000.00","","非通用类","云南省","评阅不通过","初评员：不通过","专家：不通过，铭牌与机型不对应","","","","",""]
["田间管理机械","修剪机械","茶树修剪机","单人手提式茶树修剪机","金华九奇机械有限公司","电动茶树修剪机","3CXD-600S","作业幅宽:0.6m;形式:单人 ;自带动力:是 ;","结构形式:单人背负式;蓄电池类型:锂电池;蓄电池额定容量:20Ah;蓄电池额定电压:24V;作业幅宽:600mm","240","T201933330092","2024-12-25","2000.00","","非通用类","浙江省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["田间管理机械","修剪机械","茶树修剪机","双人平行式茶树修剪机","金华九奇机械有限公司","双人修剪机","3CXP-1100","作业幅宽:1.1m;形式:双人 ;自带动力:是 ;","工作幅宽:1100mm;切割形式:刀片往复式;动力型号:TU43;发动机额定功率:1.3kW;发动机额定转速:6500r/min;操作人员2个","1600","T201933330093","2024-12-25","6500.00","","非通用类","浙江省","评阅不通过","初评员：不通过","专家：不通过，承诺书过期","","","","",""]
["收获机械","谷物收获机械","自走轮式谷物联合收割机","7kg/s及以上自走轮式谷物联合收割机","洛阳中收机械装备有限公司","自走轮式谷物联合收割机","4LZ-8B2","形式:自走轮式 ;全喂入:是 ;喂入量:8kg/s;","结构型式(轮式自走式)：全喂入；工作状态外形尺寸长×宽×高（mm）：7160×3100×3420；结构质量（kg）：5800；割台宽度（mm）：2750；割刀型式 ：II型；拨禾轮型式：偏心弹齿式；脱粒机构布置方式：切流+横轴流；凹板筛型式：栅格式；复脱器型式：风扇复脱抛扔式；变速箱类型：机械变速+液压无极变速式；驱动方式：4×2；制动器型式：钳盘式；驱动桥型式：机械驱动；驾驶室类型：普通式；卸粮方式：机械；轮胎规格 ：导向轮10.0/75-15.3；驱动轮：15-24。","29300","T201900410029","2024-10-22","135000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","谷物收获机械","自走轮式谷物联合收割机","7kg/s及以上自走轮式谷物联合收割机","洛阳中收机械装备有限公司","自走轮式谷物联合收割机","4LZ-9B","形式:自走轮式 ;全喂入:是 ;喂入量:9kg/s;","结构型式(轮式自走式)：全喂入；工作状态外形尺寸长×宽×高（mm）：7160×3200×3420；结构质量（kg）：5850；割台宽度（mm）：2960；割刀型式 ：II型；拨禾轮型式：偏心弹齿式；脱粒机构布置方式：切流+横轴流；凹板筛型式：栅格式；复脱器型式：风扇复脱抛扔式；变速箱类型：机械变速+液压无极变速式；驱动方式：4×2；制动器型式：钳盘式；驱动桥型式：机械驱动；驾驶室类型：普通式；卸粮方式：机械；轮胎规格 ：导向轮10.0/75-15.3；驱动轮：15-24。","29300","T201900410030","2024-10-22","145000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","谷物收获机械","自走履带式谷物联合收割机（全喂入）","4kg/s及以上自走履带式谷物联合收割机(全喂入)","湖州思达机械制造有限公司","全喂入联合收割机","4LZ-5.0Z","形式:自走履带式 ;全喂入:是 ;喂入量:5kg/s;","73.5kw发动机，21000mm割台，无级变速行走，90*51*450履带，纵向轴流钉齿脱粒滚筒，","26700","T201900340838","2024-12-30","108000.00","","通用类","浙江省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","玉米收获机械","自走式玉米收获机","2行摘穗剥皮型自走式玉米收获机","潍坊久瑞田农业装备有限公司","自走式玉米收获机","4YZP-2","收获行数:2行;工作幅宽:1.39m;形式:自走式(摘穗剥皮型):是 ;","型号名称：4YZP-2型自走式玉米收获机；结构型式：轮式、摘穗、剥皮、粉碎还田；整机外形尺寸(长×宽×高)mm：5200×1890×2530；工作行数（行）：2；行距（mm）：680；工作幅宽（mm）：1390；最大通过高度（mm）：2400；作业速度（km/h）：2.0～4.0；摘穗机构型式：辊式；秸秆粉碎还田机构工作幅宽（mm）：1080；秸秆粉碎还田机构型式：辊刀式。","21300","鄂2019432","2024-11-15","73500.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","玉米收获机械","自走式玉米收获机","2行摘穗剥皮型自走式玉米收获机","山东瑞泽重工有限公司","自走式玉米收获机","4YZP-2","收获行数:2行;工作幅宽:1.55m;形式:自走式(摘穗剥皮型):是 ;","收获行数：2行  工作幅宽：1.55m  行距：680mm 形式：自走式摘穗剥皮型","21300","部20171857","2021-12-31","80000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","玉米收获机械","自走式玉米收获机","3行摘穗剥皮型自走式玉米收获机","山东瑞泽重工有限公司","自走式玉米收获机","4YZB-3","收获行数:3行;工作幅宽:1.86m;形式:自走式(摘穗剥皮型):是 ;","收获行数：三行 工作幅宽：1860mm 工作行距：580mm 形式：自走式摘穗剥皮型","37700","部20171553","2021-12-31","130000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","玉米收获机械","自走式玉米收获机","3行摘穗剥皮型自走式玉米收获机","洛阳中收机械装备有限公司","自走式玉米收获机","4YZ-3D2","收获行数:3行;工作幅宽:1.75m;形式:自走式(摘穗剥皮型):是 ;","结构型式（自走式）:摘穗剥皮型；工作状态外形尺寸长×宽×高（mm）：6700×2360×3355；结构质量（kg）：6400；工作行数：3；适应行距范围（mm）：580、550；果穗升运器布置位置：中置；果穗升运器结构型式：刮板式；摘穗机构型式：摘穗辊式；剥皮机型式：旋转对辊式；剥皮辊数量（个）：16；秸秆粉碎还田机构型式：甩刀式；工作幅宽（mm）：1700；位置:中置；驱动方式：4x2；制动器型式：前钳盘式后鼓式；驱动桥型式：机械驱动；轮胎规格 ：导向轮轮胎规格10.0-15；驱动轮13.6-24。","37700","T202000410089","2025-03-31","145000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","玉米收获机械","自走式玉米收获机","3行摘穗剥皮型自走式玉米收获机","长春继鑫农业装备有限公司","自走履带式玉米收获机","4YZL-3F","收获行数:3行;工作幅宽:1.8m;形式:自走式(摘穗剥皮型):是 ;","型号名称：4YZL-3F自走履带式玉米收获机；结构型式：履带式、摘穗、剥皮、秸秆还田；配套发动机型号规格：4G33TC；配套发动机生产企业：常柴股份有限公司；配套发动机结构型式：直列式L4柴油机；配套发动机额定功率：74.5kW；配套发动机额定转速：2400r/min；整机外形尺寸（长X宽X高）：5850mmX2150mmX2500mm；工作行数：3行；行距：600mm；工作幅宽：1800mm；最小离地间隙：290mm；作业速度：1.7-5km/h；作业小时生产率：0.28—0.52h㎡/h；单位面积燃油消耗量：≤45kg/h㎡；果穗升运器布置位置：右置；果穗升运器结构型式：刮板式；摘穗机型式：摘穗板式；摘穗辊/板数量：6个；剥皮机构型式：螺旋橡胶辊式；剥皮辊数量：12个；割台型式：卧式；风扇数量：1个；风扇型式：离心式；风扇直径：550mm；卸粮方式：液压左侧卸粮；秸秆粉碎还田机构型式：滚刀式；秸秆粉碎还田机构位置：割台后下方；秸秆粉碎还田机构工作幅宽：1500mm；驾驶室型式：普通式；变速机构型式：机械式；履带节数：56节；履带节距：90mm；履带宽度：350mm；履带轨距：1500mm。","37700","T201900220534","2024-12-30","136000.00","","通用类","吉林省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","玉米收获机械","自走式玉米收获机","4行摘穗剥皮型自走式玉米收获机","洛阳中收机械装备有限公司","自走式玉米收获机","4YZ-4D3","收获行数:4行;工作幅宽:2.32m;形式:自走式(摘穗剥皮型):是 ;","结构型式（自走式）:摘穗剥皮型；工作状态外形尺寸长×宽×高（mm）：6830×2745×3460；结构质量（kg）：7500；工作行数：4；适应行距范围（mm）：500、580；果穗升运器布置位置：中置；果穗升运器结构型式：刮板式；摘穗机构型式：摘穗辊式；剥皮机型式：旋转对辊式；剥皮辊数量（个）：20；秸秆粉碎还田机构型式：甩刀式；工作幅宽（mm）：2250；位置:中置；驱动方式：4x2；制动器型式：前钳盘式后鼓式；驱动桥型式：液压驱动；轮胎规格 ：导向轮轮胎规格10.0/75-15.3；驱动轮15.5/80-24。","56200","T202000410088","2025-03-31","215000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","玉米收获机械","自走式玉米收获机","4行摘穗剥皮型自走式玉米收获机","洛阳中收机械装备有限公司","自走式玉米收获机","4YZ-4C","收获行数:4行;工作幅宽:2.41m;形式:自走式(摘穗剥皮型):是 ;","结构型式（自走式）:摘穗剥皮型；工作状态外形尺寸长×宽×高（mm）：7400×2745×3580；结构质量（kg）：7500；工作行数：4；适应行距范围（mm）：565；果穗升运器布置位置：中置；果穗升运器结构型式：刮板式；摘穗机构型式：摘穗板式+拉茎辊；剥皮机型式：旋转对辊式；剥皮辊数量（个）：20；秸秆粉碎还田机构型式：甩刀式；工作幅宽（mm）：2160；位置:中置；驱动方式：4x2；制动器型式：前钳盘式后鼓式；驱动桥型式：机械驱动；轮胎规格 ：导向轮轮胎规格10.0/75-15.3；驱动轮15-24。","56200","T202000410090","2025-03-31","195000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","玉米收获机械","自走式玉米收获机","4行摘穗剥皮型自走式玉米收获机","洛阳福格森机械装备有限公司","自走式玉米收获机","4YZ-6A","收获行数:6行;工作幅宽:2.32m;形式:自走式(摘穗剥皮型):是 ;","工作行数（通道数）：6；工作幅宽：2.32m；形式：自走式（摘穗剥皮型）整机外形尺寸(长×宽×高)mm:7550×2500×3600;最大通过高度mm:3600;最小离地间隙mm:250;果穗升运器布置位置：右置；果穗升运器结构型式:刮板式;轴距mm:3170;导向轮轮胎规格:10.0/75-15.3;驱动轮轮胎规格:15-24;导向轮轮距:1650;驱动轮轮距:1800;结构质量Kg:7450；","56200","T202000410092","2025-03-31","214000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。投档技术参数中，幅宽不符合要求。","","","","",""]
["收获机械","玉米收获机械","自走式玉米收获机","4行摘穗剥皮型自走式玉米收获机","山东瑞泽重工有限公司","自走式玉米收获机","4YZP-4","收获行数:4行;工作幅宽:2.6m;形式:自走式(摘穗剥皮型):是 ;","收获行数：4行  工作幅宽：2.6m  行距：650mm  形式：自走式摘穗剥皮型","56200","部20171856","2021-12-31","210000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","玉米收获机械","自走式玉米收获机","4行摘穗剥皮型自走式玉米收获机","山东瑞泽重工有限公司","自走式玉米收获机","4YZB-4","收获行数:4行;工作幅宽:2.25m;形式:自走式(摘穗剥皮型):是 ;","收获行数：4行  工作幅宽：2.25m 工作行距：580mm 形式：自走式摘穗剥皮型","56200","部20171554","2021-12-31","180000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","玉米收获机械","自走式玉米收获机","4行摘穗剥皮型自走式玉米收获机","山东金大丰机械有限公司","自走式玉米收获机","4YZP-5FG","收获行数:5行;工作幅宽:2.455m;形式:自走式(摘穗剥皮型):是 ;","型号名称：4YZP-5FG型自走式玉米收获机；结构型式：轮式、摘穗、剥皮、秸秆还田；果穗升运器布置位置：中置；秸秆粉碎还田机构工作幅宽（mm）：2250；驱动桥型式（前/后）：机械变速箱＋封闭边减箱/无；制动器型式（前/后）：盘式/无；轴距（mm）：3100；导向轮轮距（mm）：1640；驱动轮轮距（mm）：1750；导向轮轮胎规格：10/75-15.3；驱动轮轮胎规格：15-24；","56200","鄂2019448","2024-11-15","202000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。铭牌背景颜色与机器照片颜色不符；割台应为4行割台。","","","","",""]
["收获机械","玉米收获机械","自走式玉米收获机","4行摘穗剥皮型自走式玉米收获机","新疆牧神机械有限责任公司","自走式玉米收获机","4YZB-4CS","收获行数:4行;工作幅宽:2.23m;形式:自走式(摘穗剥皮型):是 ;","结构型式：自走式；作业行数（行）：4；适用行距范围mm：550~575；工作幅宽mm：2230；配套发动机额定功率kW：140；剥皮辊型式：铸铁直辊加橡胶直辊；","56200","T202000650324","2025-07-05","221000.00","","通用类","新疆维吾尔自治区","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","玉米收获机械","自走式玉米收获机","4行摘穗剥皮型自走式玉米收获机","新疆牧神机械有限责任公司","自走式玉米收获机","4YZB-4C","收获行数:4行;工作幅宽:2.23m;形式:自走式(摘穗剥皮型):是 ;","结构型式：自走式；作业行数（行）：4；适用行距范围mm：550~575；工作幅宽mm：2230；配套发动机额定功率kW：140；剥皮辊型式：铸铁直辊加橡胶直辊；","56200","T202000650324","2025-07-05","209000.00","","通用类","新疆维吾尔自治区","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","玉米收获机械","自走式玉米收获机","4行摘穗剥皮型自走式玉米收获机","新疆牧神机械有限责任公司","自走式玉米收获机","4YZB-6AS","收获行数:6行;工作幅宽:2.22m;形式:自走式(摘穗剥皮型):是 ;","结构型式：自走式；作业行数（行）：6；适用行距范围mm：300；工作幅宽mm：2220；配套发动机额定功率kW：129；剥皮辊型式：铸铁直辊加橡胶直辊；","56200","T202000650325","2025-07-05","250000.00","","通用类","新疆维吾尔自治区","评阅不通过","初评员：不通过","专家：不通过。企业承诺书、投档技术参数不符合要求。","","","","",""]
["收获机械","玉米收获机械","自走式玉米收获机","4行摘穗剥皮型自走式玉米收获机","新疆牧神机械有限责任公司","自走式玉米收获机","4YZB-6A","收获行数:6行;工作幅宽:2.22m;形式:自走式(摘穗剥皮型):是 ;","结构型式：自走式；作业行数（行）：6；适用行距范围mm：300；工作幅宽mm：2220；配套发动机额定功率kW：129；剥皮辊型式：铸铁直辊加橡胶直辊；","56200","T202000650325","2025-07-05","238000.00","","通用类","新疆维吾尔自治区","评阅不通过","初评员：不通过","专家：不通过。企业承诺书、投档技术参数不符合要求。","","","","",""]
["收获机械","玉米收获机械","自走式玉米收获机","5行及以上摘穗剥皮型自走式玉米收获机","勇猛机械股份有限公司","自走式玉米收获机","4YZ-5G","收获行数:5行;工作幅宽:2.923/2.81m;形式:自走式(摘穗剥皮型):是 ;","5行割台；幅宽:2.923m/2.81m；形式:自走式(摘穗剥皮型)；","56200","T201900220518","2024-12-30","230000.00","","通用类","天津市","评阅不通过","初评员：不通过","专家：不通过。产品铭牌背景颜色与机器图片颜色不符。","","","","",""]
["收获机械","玉米收获机械","自走式玉米收获机","5行及以上摘穗剥皮型自走式玉米收获机","新疆牧神机械有限责任公司","自走式玉米收获机","4YZB-8B","收获行数:8行;工作幅宽:2.82m;形式:自走式(摘穗剥皮型):是 ;","结构型式：自走式；作业行数：8行；适用行距范围mm：300；工作幅宽mm：2820；配套发动机额定功率kW：140；剥皮辊型式：铸铁直辊加橡胶辊；","56200","T202000650322","2025-07-05","358000.00","","通用类","新疆维吾尔自治区","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","玉米收获机械","自走式玉米收获机","5行及以上摘穗剥皮型自走式玉米收获机","新疆牧神机械有限责任公司","自走式玉米收获机","4YZB-8BS","收获行数:8行;工作幅宽:2.62/2.82m;形式:自走式(摘穗剥皮型):是 ;","结构型式：自走式；作业行数：8行；适用行距范围mm：300；工作幅宽mm：2820；配套发动机额定功率kW：140；剥皮辊型式：铸铁直辊加橡胶辊；","56200","T202000650322","2025-07-05","385000.00","","通用类","新疆维吾尔自治区","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","玉米收获机械","自走式玉米收获机","5行及以上摘穗剥皮型自走式玉米收获机","新疆牧神机械有限责任公司","自走式玉米收获机","4YZB-5A","收获行数:5行;工作幅宽:3.04/3.2/3.28/3.4m;形式:自走式(摘穗剥皮型):是 ;","结构型式：自走式；作业行数：5行；适用行距范围mm：560-650；工作幅宽mm：3040/3200/3280/3400；配套发动机额定功率kW：140；剥皮辊型式：铸铁直辊加橡胶辊；","56200","T202000650323","2025-07-05","340000.00","","通用类","新疆维吾尔自治区","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","玉米收获机械","自走式玉米收获机","5行及以上摘穗剥皮型自走式玉米收获机","新疆牧神机械有限责任公司","自走式玉米收获机","4YZB-5AS","收获行数:5行;工作幅宽:3.04/3.2/3.28/3.4m;形式:自走式(摘穗剥皮型):是 ;","结构型式：自走式；作业行数：5行；适用行距范围mm：560-650；工作幅宽mm：3040/3200/3280/3400；配套发动机额定功率kW：140；剥皮辊型式：铸铁直辊加橡胶辊；","56200","T202000650323","2025-07-05","367000.00","","通用类","新疆维吾尔自治区","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","玉米收获机械","穗茎兼收玉米收获机","4行摘穗型穗茎兼收自走式玉米收获机","新疆牧神机械有限责任公司","自走式穗茎兼收玉米收获机","4YZB-4B","收获行数:4行;形式:自走式(摘穗型):是 ;工作幅宽:2.62/2.82m;","结构型式：自走式；作业行数（行）：4；适用行距范围mm：600~650；工作幅宽mm：2620-2820；配套发动机额定功率kW：199；剥皮辊型式：铸铁直辊加橡胶直辊；","38800","T202065650087","2025-06-21","428000.00","","通用类","新疆维吾尔自治区","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","玉米收获机械","穗茎兼收玉米收获机","4行摘穗型穗茎兼收自走式玉米收获机","新疆牧神机械有限责任公司","自走式穗茎兼收玉米收获机","4YZB-4BS","收获行数:4行;形式:自走式(摘穗型):是 ;工作幅宽:2.62/2.82m;","结构型式：自走式；作业行数（行）：4；适用行距范围mm：600~650；工作幅宽mm：2620-2820；配套发动机额定功率kW：199；剥皮辊型式：铸铁直辊加橡胶直辊；","38800","T202065650087","2025-06-21","455000.00","","通用类","新疆维吾尔自治区","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","玉米收获机械","穗茎兼收玉米收获机","4行摘穗型穗茎兼收自走式玉米收获机","山东省聊城会晟农业机械有限公司","自走式茎穗兼收玉米收获机","4YZQ-4","收获行数:4行割台行;形式:自走式(摘穗型):是 ;工作幅宽:2.4m≤幅宽＜2.8mm;","GB/T21962-2008     http://202.127.42.49:8080/nongji/front/main/findInfo.do?id=49311 \n配套发动机（kW ）：162 ；工作状态外形尺寸(长×宽×高mm)：7200×2800×3500；工作行数（行）：4；最大卸果穗高度(mm)  ：2360；果穗升运器 ：右侧偏置、封闭刮板式；作业速度（km/h）2-4；剥皮机结构：4组；作业小时生产率（hm2/h）0.4-0.7；摘穗辊/板尺寸(mm) ∅70×735；秸秆处理机构型式 转子切碎；变速方式：（无级变速）3+1；驱动桥型式：液压+机械驱动；制动器型式：前碟刹、后制动毂；轴距(mm)：2660；轮距：驱动轮(mm) 1870、导向轮(mm) 1640；轮胎规格；驱动轮15-24、导向轮10-15","38800","新2018021","2022-12-31","287000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","玉米收获机械","穗茎兼收玉米收获机","3行摘穗剥皮型穗茎兼收玉米收获机","河北君峰收获机械有限公司","自走式茎穂兼收玉米收获机","4YZQ-3","收获行数:3行;工作幅宽:1.98m;形式:自走式(摘穗剥皮型):是 ;","结构尺寸（长*宽*高mm）：\t6440×2160×4060； 配套动力（kw）：\t113； 工作行数：\t3行； 行距： 宽：570 窄：550 工作幅宽：\t1980mm； 最小离地间隙：\t270mm； 摘穗机构型式： 摘穗辊式 剥皮辊形式：\t胶辊； 变速箱类型：机械式；","37700","T201913130029","2024-08-29","168000.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","玉米收获机械","穗茎兼收玉米收获机","4行摘穗剥皮型穗茎兼收玉米收获机","河北元正农业机械有限公司","茎穂兼收玉米收获机","4YZQ-4","收获行数:4行;工作幅宽:2.5m;形式:自走式(摘穗剥皮型):是 ;","自走式；收获行数：4行；割幅：2.5m；结构质量：7400kg","56200","T201913130027","2024-08-29","300000.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","花卉（茶叶）采收机械","采茶机","单人采茶机","金华九奇机械有限公司","电动采茶机","4CD-260","单人操作:是 ;","结构形式:单人手提式;蓄电池类型:锂电池;蓄电池额定容量:12Ah;蓄电池额定电压:24V;切割器宽度:260mm","460","T201933330094","2024-12-25","1400.00","","非通用类","浙江省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","花卉（茶叶）采收机械","采茶机","单人采茶机","金华九奇机械有限公司","电动采茶机","4CD-300","单人操作:是 ;","结构形式:单人手提式;蓄电池类型:锂电池;蓄电池额定容量:12Ah;蓄电池额定电压:24V;切割器宽度:300mm","460","T201933330095","2024-12-25","1400.00","","非通用类","浙江省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","花卉（茶叶）采收机械","采茶机","双人采茶机","金华九奇机械有限公司","双人采茶机","4CJH-1100","双人操作:是 ;","结构形式:双人弧形式;配套动力类型:汽油发动机;汽油机标定功率:2.2kW;汽油机标定转速:6500r/min;切割器切割宽度:1100mm","2300","T201933330096","2024-12-25","7000.00","","非通用类","浙江省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","根茎作物收获机械","薯类收获机","0.7-1m分段式薯类收获机","河南远邦机械有限公司","马铃薯挖掘机","4U-900","作业幅宽:0.9m;形式:分段收获 ;","型号名称:4U-900型马铃薯挖掘机 工作状态1外形尺寸(长×宽×高):2335mm×1210mm×1100mm 配套(发动机额定)功率:22.0-36.7kW 结构型式:悬挂式工作幅宽:900mm 挖掘铲型式:平铲 除茎蔓装置型式:圆盘切刀 输送装置型式:格栅筛输送链式 清选分离装置型式:振动格栅筛输送链式","940","T202041410050","2025-03-30","8500.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","根茎作物收获机械","薯类收获机","1-1.5m分段式薯类收获机","河南远邦机械有限公司","马铃薯挖掘机","4U-1000","作业幅宽:1m;形式:分段收获 ;","型号名称:4U-1000型马铃薯挖掘机 工作状态1外形尺寸(长×宽×高):2335mm×1310mm×1100mm 配套(发动机额定)功率:22.0-36.7kW 结构型式:悬挂式工作幅宽:1000mm 挖掘铲型式:平铲 除茎蔓装置型式:圆盘切刀 输送装置型式:格栅筛输送链式 清选分离装置型式:振动格栅筛输送链式","1800","T202041410050","2025-03-30","10500.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","根茎作物收获机械","薯类收获机","1.5m及以上分段式薯类收获机","河南远邦机械有限公司","马铃薯挖掘机","4U-1700","作业幅宽:1.7m;形式:分段收获 ;","型号名称\t：\t4U-1700型马铃薯挖掘机 工作状态1外形尺寸 (长×宽×高)\t：\t3900mm×2160mm×1270mm 配套（发动机额定）功率\t88-118kW\t结构型式\t：\t悬挂式 工作幅宽\t：\t1700mm 挖掘铲型式：\t组合式铲刀 除茎蔓装置型式：\t圆盘切刀 输送装置型式\t：\t格栅筛输送链式 清选分离装置型式\t：振动格栅筛输送链式","3200","T202041410038","2025-03-30","49000.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","根茎作物收获机械","花生收获机","与四轮配套,幅宽0.8-1.5m花生收获机","宁津县奥华农业机械有限公司","花生收获机","4HW-810","配套四轮拖拉机:是 ;幅宽:0.81m;","形式配套四轮拖拉机，宽幅0.81m.","1800","T201937370102","2024-10-24","6800.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","根茎作物收获机械","花生收获机","与四轮配套,幅宽0.8-1.5m花生收获机","正阳县程功机械有限公司","花生挖掘机","4HW-2(800)","配套四轮拖拉机:是 ;幅宽:0.8m;","型号名称：4HW-2(800)下花生挖掘机    结构形式：悬挂式    配套动力型式及功率：四轮13.3~25.7kw      \n工作状态外形尺寸（长x宽x高）mm:2520x900x910","1800","T201941410069","2024-12-30","6500.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","根茎作物收获机械","花生收获机","与四轮配套,幅宽0.8-1.5m花生收获机","河北凯安农业机械制造有限公司","花生挖掘机","4HW-2(1260)","配套四轮拖拉机:是 ;幅宽:1.26m;","结构型式：悬挂式，配套动力型式及功率（kW）：四轮拖拉机、14.7～23.5\n工作状态外形尺寸 (长×宽×高)（mm）：3110×1310×1045，工作垄/行数（垄/行）：双垄双行\n挖掘机构型式：三角形铲，挖掘机构工作幅宽（mm）：1260，作物输送机构型式：皮带夹送\n秧土分离机构型式：振动","1800","T201913130062","2024-12-08","8500.00","","非通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","根茎作物收获机械","花生收获机","与四轮配套,幅宽1.5-2.1m花生收获机","正阳县程功机械有限公司","花生挖掘机","4HW-4(1500)","配套四轮拖拉机:是 ;幅宽:1.5m;","产品型号名称：4HW-4(1500)型花生挖掘机    结构形式：悬挂式      配套动力型式及功率：四轮36.8~55.2kw\n工作状态外形尺寸(mm)：2800x1700x1040","3200","T201941410070","2024-12-30","11000.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","饲料作物收获机械","割草机","2.1-2.8m旋转式割草机","天津库恩农业机械有限公司","割草机","GMD280","形式:旋转式 ;割幅:2.8m;","结构型式：旋转式\n与拖拉机配套连接方式：三点悬挂\n外形尺寸（长x宽x高）：1330x4650x1170mm\n结构质量：691kg\n割幅：2.8m\n作业速度：8~12km/h\n配套动力：51.5~73.5kw","7200","黑垦鉴2016132","2021-12-31","81000.00","","非通用类","天津市","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求；铭牌未使用铆钉铆接，无法确认为整机铭牌。","","","","",""]
["收获机械","饲料作物收获机械","割草机","2.8m及以上旋转式割草机","天津库恩农业机械有限公司","割草机","GMD310","形式:旋转式 ;割幅:3.1m;","结构型式：旋转式\n与拖拉机配套连接方式：三点悬挂\n外形尺寸（长x宽x高）：1330x4980x1170mm\n结构质量：734kg\n割幅：3.1m\n作业速度：8~12km/h\n配套动力：58.8-88.2kw","29900","黑垦鉴2016133","2021-12-31","87200.00","","非通用类","天津市","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","割草机","2.8m及以上旋转式割草机","上海世达尔现代农机有限公司","旋转式割草压扁机","9GYQ-3.0","形式:旋转式 ;割幅:3m;","割幅：3m,旋转式，带压扁辊","29900","T201931310007","2024-10-20","198000.00","","非通用类","上海市","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","割草机","2.8m及以上旋转式割草压扁机","天津库恩农业机械有限公司","割草压扁机","FC302RG","形式:旋转式 ;割幅:3m;带压扁装置:是 ;","结构型式：旋转式\n与拖拉机连接方式：牵引式\n外形尺寸（长x宽x高）：5180x4840x1240mm\n结构质量：1800kg\n割幅：3m\n作业速度：8-12km/h\n刀盘转速：2900r/min","46500","T20190606054","2024-12-31","240000.00","","非通用类","天津市","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求；铭牌未使用铆钉铆接，无法确认为整机铭牌。","","","","",""]
["收获机械","饲料作物收获机械","割草机","2.8m及以上旋转式割草压扁机","天津库恩农业机械有限公司","割草压扁机","FC352RG","形式:旋转式 ;割幅:3.5m;带压扁装置:是 ;","结构型式：旋转式\n外形尺寸（长x宽x高）：5180x5310x1240\n结构质量：2050kg\n割幅：3.5m\n作业速度：8-12km/h\n刀盘转速：2900r/min\n配套动力：66.2-88.2kw","46500","T20190606058","2024-12-31","249000.00","","非通用类","天津市","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求；铭牌未使用铆钉铆接，无法确认为整机铭牌。","","","","",""]
["收获机械","饲料作物收获机械","搂草机","5.4m及以上侧向指盘式搂草机","牙克石市兴农农机具制造有限公司","液压折叠侧置指盘式搂草机","9CPL-6.0","搂幅宽度:6m;侧向指盘式:是 ;","结构形式:指轮式挂接方式:牵引式规格型号:9CPL-6.0外形尺寸(长*宽*高)(运输状态):12300MM*2300MM*1700MM结构质量:1300KG搂幅:6M作业速度:10-15KM/H配套动力范围:≥26KW搂齿数量:780个","5500","内蒙古2017-005","2021-12-31","23000.00","","非通用类","内蒙古自治区","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","搂草机","5.4m及以上侧向指盘式搂草机","牙克石市兴农农机具制造有限公司","液压折叠指盘式搂草机","9PL-10.00","搂幅宽度:10m;侧向指盘式:是 ;","结构型式:指轮式挂接方式:牵引式规格型号:9PL-10.00外形尺寸(长*宽*高)(运输状态):10500MM*2400MM*1700MM结构质量:2100KG搂幅:10M作业速度:12-18KM/H配套动力范围:≥26KW搂齿数量:1080个","5500","内蒙古2017-006","2021-12-31","30000.00","","非通用类","内蒙古自治区","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","饲料作物收获机械","搂草机","5.4m及以上侧向指盘式搂草机","牙克石市兴农农机具制造有限公司","指轮式搂草机","9LP-5.4","搂幅宽度:5.4m;侧向指盘式:是 ;","结构型式:指轮式挂接方式:牵引式规格型号:9LP-5.4外形尺寸(长×宽×高)4500MM×2700MM×2700MM(运输状态)结构质量:720KG搂幅:5.4M作业速度:8-15KM/H配套动力范围:22-25KW搂齿数量:320个","5500","T201915150015","2024-12-30","18000.00","","非通用类","内蒙古自治区","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","饲料作物收获机械","搂草机","5.4m及以上侧向指盘式搂草机","吉林省远航农业机械有限公司","搂草机","9LQ-5.4","搂幅宽度:5.4m;侧向指盘式:是 ;","(结构型式：指轮式)(挂接方式：牵引式)(工作状态外形尺寸：6500×6700×1540mm)(结构质量：450kg)(指轮数量：8个)(弹齿数量：60齿/盘)(指轮直径：1540mm)(作业最大搂幅：5400mm)(配套动力范围：≥29.4kW（40马力）(作业速度范围：10-15km/h)","5500","T201922220066","2024-12-15","29000.00","","非通用类","吉林省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","搂草机","5.4m及以上侧向指盘式搂草机","吉林省远航农业机械有限公司","搂草机","9LQ-5.6","搂幅宽度:5.6m;侧向指盘式:是 ;","(结构型式：指轮式)(挂接方式：牵引式)(工作状态外形尺寸：6960×6850×1540mm)(结构质量：850kg)(指轮数量：10个)(弹齿数量：80齿/盘)(指轮直径：1540mm)(作业最大搂幅：5600mm)(配套动力范围：≥36.8kW（50马力）(作业速度范围：10-15km/h)","5500","T201922220065","2024-12-15","36000.00","","非通用类","吉林省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","搂草机","5.4m及以上侧向指盘式搂草机","吉林省远航农业机械有限公司","搂草机","9LQ-6.0","搂幅宽度:6.0m;侧向指盘式:是 ;","(结构型式：指轮式)(挂接方式：牵引式)(工作状态外形尺寸：8100×7200×1540mm)(结构质量：960kg)(指轮数量：12个)(弹齿数量：80齿/盘)(指轮直径：1540mm)(作业最大搂幅：6000mm)(配套动力范围：≥58.8kW（80马力）(作业速度范围：10-15km/h)","5500","T201922220064","2024-12-15","43500.00","","非通用类","吉林省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","搂草机","5.4m及以上侧向指盘式搂草机","吉林省隆博农业发展有限公司","指轮式搂草机","9LZ-5.5","搂幅宽度:5.5m;侧向指盘式:是 ;","型号名称:9LZ-5.5型指轮式搂草机;结构型式:指轮式;挂接方式:牵引式;折叠机构型式:液压式;搂齿数量:60（可选80）×8;指轮数量:8mm;指轮直径:1500mm;搂幅:5.5m;配套动力范围:22.1～29.4kW;作业速度范围:10～15km/h。","5500","T202022220102","2025-05-28","30000.00","","非通用类","吉林省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","饲料作物收获机械","搂草机","5.4m及以上侧向指盘式搂草机","吉林省隆博农业发展有限公司","指轮式搂草机","9LZ-6.5","搂幅宽度:6.5m;侧向指盘式:是 ;","型号名称:9LZ-6.5型指轮式搂草机;结构型式:指轮式;挂接方式:牵引式;折叠机构型式:液压式;搂齿数量:60（可选80）×10;指轮数量:10mm;指轮直径:1500mm;搂幅:6.5m;配套动力范围:29.4～44.1kW;作业速度范围:10～15km/h。","5500","T202022220100","2025-05-28","40000.00","","非通用类","吉林省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","饲料作物收获机械","搂草机","5.4m及以上侧向指盘式搂草机","河北凯安农业机械制造有限公司","指轮式搂草机","9LZ-7.4","搂幅宽度:7.4m;侧向指盘式:是 ;","搂幅（m）：7.4，配套动力范围（kW）：36.8～73.5，作业速度范围（km/h):8～12,结构型式: 侧向指轮式，挂接方式：牵引式\n折叠机构型式：液压折叠式，搂齿数量：960（80×12），指轮数量：12，指轮直径（mm）1540","5500","T201913130036","2024-08-29","20000.00","","非通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","搂草机","5.4m及以上侧向指盘式搂草机","河北凯安农业机械制造有限公司","指轮式搂草机","9LZ-6.5","搂幅宽度:6.5m;侧向指盘式:是 ;","搂幅（m）：6.5，配套动力范围（kW）：29.4～73.5，作业速度范围（km/h）：8～12，结构型式：侧向指轮式，挂接方式：牵引式，折叠机构型式：液压折叠式，搂齿数量：800（80×10），指轮数量：10,指轮直径(mm):1540","5500","T201913130035","2024-08-29","20000.00","","非通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","搂草机","5.4m及以上侧向指盘式搂草机","河北凯安农业机械制造有限公司","指轮式搂草机","9LZ-5.5","搂幅宽度:5.5m;侧向指盘式:是 ;","搂幅(m:)5.5,配套动力范围(kW):22.1～73.5,作业速度范围(km/h):8～12,结构型式：侧向指轮式，挂接方式：牵引式\n折叠机构型式：液压式，搂齿数量：640(80×8)，指轮数量：8，指轮直径（mm）：1540","5500","T201913130034","2024-08-29","20000.00","","非通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","搂草机","5.4m及以上侧向指盘式搂草机","河北耿军农业机械制造有限公司","指轮式搂草机","9LZ-7.5","搂幅宽度:7.5m;侧向指盘式:是 ;","搂幅：7.5m，牵引式，侧向指盘式，液压 折叠式","5500","T201913130014","2024-08-13","19800.00","","非通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","搂草机","5.4m及以上侧向指盘式搂草机","河北耿军农业机械制造有限公司","指轮式搂草机","9LZ-6.5","搂幅宽度:6.5m;侧向指盘式:是 ;","搂幅：6.5m，牵引式，侧向指盘式，液压 折叠式","5500","T201913130013","2024-08-13","18800.00","","非通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","搂草机","5.4m及以上侧向指盘式搂草机","河北耿军农业机械制造有限公司","指轮式搂草机","9LZ-5.5","搂幅宽度:5.5m;侧向指盘式:是 ;","搂幅：5.5m，牵引式，侧向指盘式，液压 折叠式","5500","T201913130015","2024-08-13","17800.00","","非通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","山东铁甲农牧机械制造有限公司","捡拾圆捆机","9YJ-1800","形式:圆捆机 ;捡拾宽度:1.8m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","捡拾器结构型式:甩刀式,卷压滚筒数量(个):15,工作状态外形尺寸（长×宽×高）:2400mm×2200mm×1400mm\n配套动力非固定式(kW):≥40.4,捡拾器宽度(mm):1800","7300","部20180775","2022-12-31","55000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","淮滨县祥盛再生资源有限公司","方形秸秆打捆机","9YFQ-1.9","形式:方捆机 ;捡拾宽度:1.98m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥200×2 ;打结器数量:2个;","捡拾宽度：1.98m；打结器类型：D型；工作状态外形尺寸（长*宽*高）mm：4975*2550*1710；打捆活塞速度行程/min：100；配套动力kW：≥25。","7300","豫2015279","2020-12-31","30000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合机具分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","菏泽市天艺农业机械制造有限公司","秸秆打捆机","9YJ-2250","形式:圆捆机 ;捡拾宽度:2.25m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","挂接方式：牵引式；捡拾宽度mm：2250；捡拾器结构型式：甩刀式；喂入器结构型式：螺旋连续喂入机构；压缩室成捆机构型式：滚筒式；压缩室宽度mm：1250；压缩室直径mm：700；卷压滚筒数量（个）：15；卷压滚筒直径mm：157；缠捆方式（绳或网）：绳；配套动力范围kw：≥75。","7300","GZNJ/TJ 2019-254","2024-08-22","28000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合机具分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","菏泽市天艺农业机械制造有限公司","秸秆捡拾打捆机","9YZD-700","形式:圆捆机 ;捡拾宽度:2.2m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","挂接方式：牵引式；捡拾宽度mm：2200；捡拾器结构型式：甩刀式；喂入器结构型式：链耙喂入机构；压缩室成捆机构型式：滚筒式；压缩室宽度mm：1250；压缩室直径mm：700；卷压滚筒数量（个）：13；卷压滚筒直径mm：157；缠捆方式（绳或网）：网；配套动力范围kw：≥75。","7300","GZNJ/TJ 2019-252","2024-08-22","28000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合机具分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","菏泽市天艺农业机械制造有限公司","秸秆捡拾打捆机","9Y-70125","形式:圆捆机 ;捡拾宽度:1.25m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","挂接方式：牵引式；捡拾宽度：1250mm；捡拾器结构型式：弹齿式；压缩室成捆机构型式：滚筒式；压缩室宽度：1250mm；压缩室直径：700mm；卷压辊筒数量：13个；卷压辊筒直径：157mm；缠捆方式：缠绳；配套动力：32-40kW","7300","黑垦鉴2017099","2021-12-31","27000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","菏泽市天艺农业机械制造有限公司","秸秆打捆机","9YJ-130","形式:圆捆机 ;捡拾宽度:1.3m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","挂接方式：牵引式；捡拾宽度：1300mm；捡拾器结构型式：甩刀式；压缩室成捆机构型式：滚筒式；压缩室宽度：1000mm；压缩室直径：700mm；卷压辊筒数量：13个；卷压辊筒直径：157mm；缠捆方式：缠绳；配套动力：45-55kW","7300","黑垦鉴2017101","2021-12-31","28000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","菏泽市天艺农业机械制造有限公司","秸秆打捆机","9YJ-180","形式:圆捆机 ;捡拾宽度:1.8m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","挂接方式：牵引式；捡拾宽度：1800mm；捡拾器结构型式：甩刀式；压缩室成捆机构型式：滚筒式；压缩室宽度：1000mm；压缩室直径：700mm；卷压辊筒数量：13个；卷压辊筒直径：157mm；缠捆方式：缠绳；配套动力：65-75kW","7300","黑垦鉴2017102","2021-12-31","30000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","河北春翔机械有限公司","圆草捆打捆机","9YQ-1.8A","形式:圆捆机 ;捡拾宽度:1.8m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","挂接方式：牵引式；捡拾宽度mm：1800；捡拾器结构型式：甩刀式；喂入器结构型式：螺旋连续喂入机构；压缩室成捆机构型式：滚筒式；压缩室宽度mm：850；压缩室直径mm：600；卷压滚筒数量（个）：12；卷压滚筒直径mm：156；缠捆方式（绳或网）：绳；配套动力范围kw：73.5~100。","7300","GZNJ/TJ 2019-325","2024-09-26","28000.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","尉氏县鑫盛源机械有限公司","圆草捆打捆机","9YQY-1260","形式:圆捆机 ;捡拾宽度:1.26m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:0个;","草捆形状：圆捆；捡拾宽度（m）：1.26；捡拾器结构型式：弹齿式；配套动力：35-80kW","7300","T201941410023","2024-11-13","25000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","山东奥翔农业机械设备股份有限公司","秸秆捡拾打捆机","9YDT6080","形式:圆捆机 ;捡拾宽度:1.9m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","捡拾器宽度：1900mm；卷压滚筒转速：260r/min；卷压滚筒数量：11个；工作状态外型尺寸：（长x宽x高）3560mmx2650mmx1680mm；配套动力：≥36.8kw","7300","部20160392","2020-12-31","76000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求，基本配置和参数承诺书中参数名称有误。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","山东奥翔农业机械设备股份有限公司","秸秆捡拾打捆机","9YD6080","形式:圆捆机 ;捡拾宽度:1.5m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","捡拾器宽度：1500mm；卷压滚筒转速：260r/min；卷压滚筒数量：11个；工作状态外型尺寸：（长x宽x高）3560mmx1820mmx1680mm；配套动力：≥36.8kw","7300","部20160391","2020-12-31","76000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。投档技术参数中，捡拾宽度不符合要求；基本配置和参数承诺书中参数名称有误。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","潍坊汉腾机械有限公司","圆草捆打捆机","9YQ-1200","形式:圆捆机 ;捡拾宽度:1.2m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","挂接方式：牵引式；捡拾宽度（mm）:1200；捡拾器结构型式：弹齿式；喂入器结构型式：弹齿直接喂入；压缩室成捆机构型式：滚筒式；压缩室宽度（mm）：1200；压缩室直径（mm）:710；卷压滚筒数量（个）：14；卷压滚筒直径（mm）157；配套动力范围（kw）：29.4～51.5","7300","鄂2019567","2024-12-29","35000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","潍坊轩沃农业机械有限公司","圆草捆打捆机","9YQ-2350","形式:圆捆机 ;捡拾宽度:2.35m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","捡拾器宽度：2350mm；捡拾器结构型式:甩刀式；压缩室截面尺寸（宽×高）mm：700mm×1000mm；卷压滚筒数量:15个；工作状态外形尺寸（长×宽×高）mm：2700×2740×1480；配套动力:≥66.2kw.","7300","GZNJ/TJ 2019-067","2023-12-31","30000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","华创机器人制造有限公司","圆草捆打捆机","9YQ-180","形式:圆捆机 ;捡拾宽度:1.8m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","型号：9YQ-180；捡拾器宽度mm:1800;捡拾器结构型式:甩刀式;卷压滚筒数量(个）:14；工作状态外形尺寸（长×宽×高）mm:2400×2200×1300;配套动力（非固定式）kW:40.4-58.5","7300","鄂2018009","2022-12-31","117000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求；捡拾宽度不符合分档基本配置与参数要求；产品配置参数证明文件不符合要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","临颍县颍机机械制造有限公司","圆草捆打捆机","9YQ-1.8A","形式:圆捆机 ;捡拾宽度:1.8m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","捡拾器宽度：1.8m，压缩室直径：0.6m，压缩室宽度：0.9m","7300","部20180252","2022-12-31","35800.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","临颍县颍机机械制造有限公司","圆草捆打捆机","9YQ-1.3A","形式:圆捆机 ;捡拾宽度:1.3m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","捡拾器宽度：1.3m，压缩室直径：0.6m，压缩室宽度：0.9m","7300","部20190454","2023-12-31","30800.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","山东新圣泰机械制造有限公司","圆草捆打捆机","9YY-0.7","形式:圆捆机 ;捡拾宽度:1.8m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","捡拾器宽度:1800mm；捡拾器结构形式:甩刀式；卷压滚筒转速:320r/min；卷压滚筒数量:13个；工作状态外形尺寸(长x宽x高):2260x2200x1360mm；配套动力:55.8-88.2kW.","7300","鄂2019037","2023-12-31","25000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合机具分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","平顶山市久久实业有限公司","圆捆捡拾压捆机","9YG-1.40","形式:圆捆机 ;捡拾宽度:1.4m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","捡拾器宽度mm：1400；捡拾器结构型式：甩刀捡拾器；卷压滚筒转速\tr/min：325；卷压滚筒数量\t个：12；工作状态外形尺寸(长×宽×高)\tmm：1995×1760×1740；配套动力\tkW：44.1～62.5。","7300","豫2018043","2022-12-31","28000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","平顶山市久久实业有限公司","圆捆捡拾压捆机","9YG-1.35","形式:圆捆机 ;捡拾宽度:1.35m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","捡拾器宽度\tmm：1350；捡拾器结构型式\t/\t弹齿卷压滚筒转速\tr/min：325；卷压滚筒数量\t个：12；工作状态外形尺寸（长×宽×高）mm：\t2200×1580×1740；配套动力非固定式\tkW\t：22.1～36.8。","7300","豫2017068","2021-12-31","28000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","平顶山市久久实业有限公司","圆捆捡拾压捆机","9YG-1.80","形式:圆捆机 ;捡拾宽度:1.8m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","挂接方式：牵引式；捡拾宽度\tmm：1800；捡拾器结构型式：甩刀式；喂入器结构型式：拨叉喂入机构；喂入器结构型式：拨叉喂入机构；压缩室成捆机构型式\t：滚筒式；压缩室宽度mm：1280；\n压缩室直径mm\t：610；卷压滚筒数量个：15；卷压滚筒直径\tmm：156。","7300","GZNJ/TJ 2019-182","2023-12-31","28000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","山东天华农业机械制造有限公司","秸秆捡拾打捆机","9YQ-1250","形式:圆捆机 ;捡拾宽度:1.25m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","挂接方式：牵引式；捡拾宽度mm：1250；捡拾器结构型式：弹齿式；压缩室成捆机构型式：滚筒式；压缩室宽度mm：1250；压缩室直径mm：700；卷压滚筒数量（个）：13；卷压滚筒直径mm：157；缠捆方式（绳或网）：绳；配套动力范围kw：32~40。","7300","GZNJ/TJ 2019-256","2024-08-22","28000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合机具分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","山东天华农业机械制造有限公司","秸秆捡拾打捆机","9YZD-700","形式:圆捆机 ;捡拾宽度:2.2m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","挂接方式：牵引式；捡拾宽度mm：2200；捡拾器结构型式：甩刀式；喂入器结构型式：链耙喂入机构；压缩室成捆机构型式：滚筒式；压缩室宽度mm：1250；压缩室直径mm：700；卷压滚筒数量（个）：13；卷压滚筒直径mm：157；缠捆方式（绳或网）：网；配套动力范围kw：≥75。","7300","GZNJ/TJ 2019-257","2024-08-22","28000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合机具分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","山东天华农业机械制造有限公司","秸秆打捆机","9YJ-130","形式:圆捆机 ;捡拾宽度:1.3m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","挂接方式：牵引式；捡拾宽度mm：1300；捡拾器结构型式：甩刀式；压缩室成捆机构型式：滚筒式；压缩室宽度mm：980；压缩室直径mm：700；卷压滚筒数量（个）：17；卷压滚筒直径mm：157；缠捆方式（绳或网）：绳；配套动力范围kw：≥45。","7300","GZNJ/TJ 2019-259","2024-08-22","28000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合机具分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","山东天华农业机械制造有限公司","秸秆捡拾打捆机","9YQ-180","形式:圆捆机 ;捡拾宽度:1.8m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","挂接方式：牵引式；捡拾宽度mm：1800；捡拾器结构型式：锤爪式；喂入器结构型式：螺旋连续喂入机构；压缩室成捆机构型式：滚筒式；压缩室宽度mm：980；压缩室直径mm：700；卷压滚筒数量（个）：15；卷压滚筒直径mm：157；缠捆方式（绳或网）：绳；配套动力范围kw：≥75。","7300","GZNJ/TJ 2019-255","2024-08-22","28000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合机具分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","郓城县鑫达机械有限公司","捡拾圆捆机","9YQ-2210","形式:圆捆机 ;捡拾宽度:2250m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:0个;","型号名称 / 9YQ-2210型捡拾圆捆机\n2 挂接方式 / 牵引式\n3 捡拾宽度 mm 2210\n4 喂入口宽度 mm /\n5 捡拾器结构型式 / 甩刀式\n6 喂入器结构型式 / 螺旋连续喂入机构\n7 压缩室成捆机构型式 / 滚筒式\n8 压缩室宽度 mm 980\n9 压缩室直径 mm 565\n10 卷压工作部件数量 个 滚筒 15\n11 卷压滚筒直径 mm 152\n12 捆扎方式 / 缠绳\n13 配套动力范围 kW 59～112","7300","T202000370249","2025-07-05","53000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合机具分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","潍坊智胜农业装备科技有限公司","圆草捆打捆机","9YQ-2350","形式:圆捆机 ;捡拾宽度:2.35m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","配套动力范围（kW）：≥73.5kW；工作状态外形尺寸（长×宽×高）2400mm×2700mm×1450mm；捡拾器结构型式：甩刀式；压缩室宽度：1000mm；压缩室直径：700mm；卷压滚筒转速：320r/min；卷压滚筒数量：15个；捡拾宽度：2350mm","7300","GZNJ/TJ 2019-058","2023-12-31","50000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","莱州华能机械有限公司","圆草捆打捆机","9YQ-1800","形式:圆捆机 ;捡拾宽度:1.8m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","捡拾器宽度（mm）：1800；捡拾器结构型式：甩刀式；卷压滚筒数量（个）：15；工作外形尺寸（mm）:2700×2200×1450;配套动力（kw）：≥38","7300","部20190123","2023-12-31","35000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","莱州华能机械有限公司","圆草捆打捆机","9YQ-2300","形式:圆捆机 ;捡拾宽度:2.3m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","捡拾器宽度（mm）：2300；捡拾器结构型式：甩刀式；卷压滚筒数量（个）：15；工作外形尺寸（mm）:2700×2700×1450;配套动力（kw）：≥58","7300","部20190124","2023-12-31","54000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","曲阜鑫联重工机械制造有限公司","圆草捆打捆机","9YQ-1300","形式:圆捆机 ;捡拾宽度:1.3m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","捡拾器宽度：1300mm；捡拾器结构型式：甩刀式；配套动力：≥28kw；卷压滚筒数量：15个；工作状态外形尺寸（长*宽*高）：2770mm*1700mm*1400mm","7300","部20180785","2022-12-31","29000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。未提供配置参数证明文件。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","曲阜鑫联重工机械制造有限公司","圆草捆打捆机","9YQ-1720","形式:圆捆机 ;捡拾宽度:1.72m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","捡拾器宽度：1720mm；捡拾器结构型式：甩刀式；配套动力：≥55kw；卷压滚筒数量：15个；工作状态外形尺寸（长*宽*高）：2770mm*2150mm*1400mm","7300","部20180784","2022-12-31","32000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。未提供配置参数证明文件。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","山东富垠农业科技有限公司","捡拾圆捆打捆机","9YQ-2200A","形式:圆捆机 ;捡拾宽度:2.2m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","捡拾宽度（mm）：2200；捡拾器结构型式：甩刀式；卷压滚筒数量（个）：15；工作状态外形尺寸（长×宽×高）（mm）：2650×2700×1500；配套动力（kW）：66.1~99.2；","7300","GZNJ/TJ 2019-110","2023-12-31","60000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。未提供产品配置参数证明文件，无法确认是否符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","潍坊飞奥农业机械有限公司","圆草捆打捆机","9YQ-180","形式:圆捆机 ;捡拾宽度:1.8m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","型号名称：9YQ-180型圆草捆打捆机；挂接方式：牵引式；捡拾宽度mm：1800；捡拾器结构型式：甩刀式；喂入器结构型式：螺旋连续喂入机构；压缩室成捆机构型式：滚筒式；压缩室宽度mm：930；压缩室直径mm：570；卷压滚筒数量：14个；卷压滚筒直径mm:150；缠捆方式（绳或网）：缠绳；配套动力范围KW：40.4-58.5；","7300","鄂2019333","2024-07-17","117000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求；捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","潍坊飞奥农业机械有限公司","圆草捆打捆机","9YQ-230","形式:圆捆机 ;捡拾宽度:2.3m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","型号名称:9YQ-230型圆草捆打捆机;挂接方式:牵引式;捡拾宽度mm:2300;捡拾器结构型式:甩刀式;喂入器结构型式:螺旋连续喂入机构;压缩室成捆机构型式:滚筒式;压缩室宽度mm:1050;压缩室直径mm:570;卷压滚筒数量:14个；卷压滚筒直径mm:150;缠捆方式（绳或网）:缠绳；配套动","7300","鄂2019334","2024-07-17","148000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求；捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","潍坊鑫牧机械有限公司","圆草捆打捆机","9YK-1270","形式:圆捆机 ;捡拾宽度:1.27m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","挂接方式：牵引式；捡拾宽度（mm）:1270;捡拾器结构型式：弹齿式；压缩室宽度（mm）：1270；压缩式直径（mm）：580；卷压滚筒数量（个）：12；卷压滚筒直径（mm）:150;配套动力范围：（kw）≥29.1","7300","鄂2019211","2024-07-17","30000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","潍坊鑫牧机械有限公司","圆草捆打捆机","9YK-1300","形式:圆捆机 ;捡拾宽度:1.3m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","挂接方式：牵引式；捡拾宽度（mm）:1300;捡拾器结构型式：甩刀式；压缩室宽度（mm）：930；压缩式直径（mm）：580；卷压滚筒数量（个）：14；卷压滚筒直径（mm）:150;配套动力范围：（kw）≥36.7","7300","鄂2019212","2024-07-17","35000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","宁津县鹏宇环保节能设备有限公司","捡拾圆捆机","9YQ-1800","形式:圆捆机 ;捡拾宽度:1.8m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","捡拾宽度=1800mm；圆捆机压缩室直径=700mm；圆捆机压缩室宽度=1000mm","7300","部20190130","2023-12-31","62000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合机具分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","宁津县鹏宇环保节能设备有限公司","捡拾圆捆机","9YQ-1300","形式:圆捆机 ;捡拾宽度:1.3m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","捡拾宽度=1300mm；圆捆机压缩室直径=700mm；圆捆机压缩室宽度=1000mm","7300","部20190131","2023-12-31","60000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合机具分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","开封市富农机械装备有限公司","圆草捆打捆机","9YQ-2300","形式:圆捆机 ;捡拾宽度:2.3m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","捡拾器宽度mm：2300；捡拾器结构型式：甩刀式；卷压滚筒转速r/min：560；卷压滚筒数量个：15；工作状态外形尺寸（长×宽×高）mm：3250×2700×1415；配套动力kW：70-80；","7300","鄂2018162","2022-12-31","98000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","开封市富农机械装备有限公司","圆草捆打捆机","9YDJ-1260","形式:圆捆机 ;捡拾宽度:1.26m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","捡拾器结构型式：弹齿式；卷压滚筒转速r/min：560；卷压滚筒数量个：13；工作状态外型尺寸（长×宽×高）mm：1510×1850×1440；配套动力kW：35-80；捡拾器宽度mm：1260；","7300","鄂2019105","2023-12-31","50000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","潍坊雷泰机械有限公司","圆草捆打捆机","9YQ-1250","形式:圆捆机 ;捡拾宽度:1.25m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","捡拾器宽度：1250mm；捡拾器结构型式:弹齿式；卷压滚筒转速:320r/min；卷压滚筒数量:15个；压缩室截面尺寸（宽×高）mm：700×1000；工作状态外形尺寸（长×宽×高）mm：1950×1750×1510；配套动力:≥29.5kw。","7300","GZNJ/TJ 2019-028","2023-12-31","30000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","潍坊雷泰机械有限公司","圆草捆打捆机","9YQ-1300","形式:圆捆机 ;捡拾宽度:1.3m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","捡拾器宽度：1300mm；捡拾器结构型式:甩刀式；卷压滚筒转速:320r/min；卷压滚筒数量:15个；压缩室截面尺寸（宽×高）mm：700×1000；工作状态外形尺寸（长×宽×高）mm:2740×1750×1480；配套动力:≥36.8kw。","7300","GZNJ/TJ 2019-026","2023-12-31","30000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","潍坊雷泰机械有限公司","圆草捆打捆机","9YQ-2350","形式:圆捆机 ;捡拾宽度:2.35m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","捡拾器宽度：2350mm；捡拾器结构型式:甩刀式；压缩室截面尺寸（宽×高）mm：700×1000；卷压滚筒转速:320r/min；卷压滚筒数量:15个；工作状态外形尺寸（长×宽×高）mm:2470×2740×1480；配套动力:≥73.5kw。","7300","GZNJ/TJ 2019-038","2023-12-31","31000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","潍坊丰益来收割机制件有限公司","圆草捆打捆机","9YQ-1800","形式:圆捆机 ;捡拾宽度:1.8m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:15个;","型号：9YQ-1800      捡拾器宽度：1800mm     捡拾器结构型式：甩刀式       卷压滚筒转速：320r/min        卷压滚筒数量：15个       工作状态外形尺寸（长×宽×高）：2440mm×2200mm×1530mm   配套动力非固定式：40.4~66.1kW    压缩室直径：700mm","7300","部20190161","2023-12-31","50000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合机具分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","潍坊丰益来收割机制件有限公司","圆草捆打捆机","9YQ-2350","形式:圆捆机 ;捡拾宽度:2350m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:15个;","型号：9YQ-2350         捡拾器宽度：2350mm         捡拾器结构型式：甩刀式      卷压滚筒转数：320r/min     卷压滚筒数量：15个         工作状态外形尺寸（长×宽×高）：2500mm×2750mm×1530mm       配套动力非固定式：66.1~99.2kW       压缩室直径：700mm","7300","部20190162","2023-12-31","50000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合机具分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","潍坊泰业机械有限公司","圆草捆打捆机","9TY1800","形式:圆捆机 ;捡拾宽度:1.8m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","捡拾器宽度：1800mm 捡拾器结构型式：甩刀式  卷压滚筒数量：14个","7300","鄂2019129","2023-12-31","61400.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","潍坊泰业机械有限公司","圆草捆打捆机","9TY2300","形式:圆捆机 ;捡拾宽度:2.3m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","捡拾器宽度：2300mm  捡拾器结构型式：甩刀式  卷压滚筒数量：14个","7300","鄂2019130","2023-12-31","115500.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数证明。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","舞钢市恒利达机械制造有限责任公司","圆捆捡拾压捆机","9YG-1.39A","形式:圆捆机 ;捡拾宽度:1.39m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","型号 / 9YG-1.39A  捡拾器宽度  mm  1390   捡拾器结构型式  /  弹齿捡拾器   卷压滚筒转速  r/min  325  卷压滚筒数量  个  12\n工作状态外形尺寸(长×宽×高)  mm  2012×1735×1685  配套动力  kW  22.1～36.8 圆捆压缩室直径  mm  600 \n圆捆压缩室宽度 mm 900","7300","豫2018024","2022-12-31","25000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合机具分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","舞钢市恒利达机械制造有限责任公司","圆捆捡拾压捆机","9YG-1.3","形式:圆捆机 ;捡拾宽度:1.3m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","型号 / 9YG-1.3  捡拾器宽度 mm 1300  捡拾器结构型式  /  甩刀式   卷压滚筒转速  r/min 457  卷压滚筒数量  个 12\n工作状态外形尺寸(长×宽×高)  mm   2445×1700×1750   配套动力 kW 36.8～73.5 圆捆压缩室直径 mm  600 \n圆捆压缩室宽度 mm 900","7300","豫2018047","2022-12-31","25000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合机具分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","舞钢市恒利达机械制造有限责任公司","圆捆捡拾压捆机","9YG-1.8","形式:圆捆机 ;捡拾宽度:1.8m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","型号 /  9YG-1.8  捡拾器宽度 mm  1800   捡拾器结构型式 /  甩刀式  卷压滚筒转速  r/min 457 卷压滚筒数量 个 12\n工作状态外形尺寸(长×宽×高)  mm 2430×2220×1730 配套动力 kW  66～103 圆捆压缩室直径 mm 600 圆捆压缩室宽度  mm 900","7300","豫2018048","2022-12-31","55000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合机具分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","新乡市正鑫农业机械制造有限公司","圆捆捡拾压捆机","9YJY-0.9","形式:圆捆机 ;捡拾宽度:0.9m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","型号名称：9YJY-0.9型圆捆捡拾压捆机，捡拾宽度：900mm，捡拾器结构型式：弹齿，工作状态外形尺寸：2350*1680*1600mm，配套动力：22.1～36.8kW.","7300","豫2017046","2021-12-31","25000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求；未提供产品配置参数证明文件。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","河南省躬耕农业机械制造有限公司","圆草捆打捆机","9YG-1.45","形式:圆捆机 ;捡拾宽度:1.45m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","型号:9YG-1.45 捡拾器宽度: 1450 mm 捡拾器结构型式: 弹齿滚筒式  卷压滚筒转速:  325r/min 卷压滚筒数量: 14个 工作状态外型尺寸（长×宽×高）: 2610×1700×1800 mm 配套动力 :36.8～58.8kW","7300","鄂2019193","2023-12-31","25000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。未提供产品配置参数证明文件，无法确认是否符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","山东格奥机械有限公司","捡拾圆捆机","9YQ-2250","形式:圆捆机 ;捡拾宽度:2.25m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","捡拾宽度：2.25m；捡拾器结构型式：甩刀式；卷压滚筒数量：15个；工作状态外形尺寸（长x宽x高）：2850mmx2650mmx1550mm。","7300","部20190441","2023-12-31","30000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","山东格奥机械有限公司","捡拾圆捆机","9YQ-1800","形式:圆捆机 ;捡拾宽度:1.8m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","捡拾宽度：1.8m；捡拾器结构型式：甩刀式；卷压滚筒数量：15个；工作状态外形尺寸（长x宽x高）：2850mmx2150mmx1550mm。","7300","部20190442","2023-12-31","30000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","山东格奥机械有限公司","捡拾圆捆机","9YQ-1300","形式:圆捆机 ;捡拾宽度:1.3m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","捡拾宽度：1.3m；捡拾器结构型式：甩刀式；卷压滚筒数量：15个；工作状态外形尺寸（长x宽x高）：2850mmx1650mmx1550mm。","7300","部20190443","2023-12-31","30000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","山东博豪农机技术服务有限公司","圆草捆打捆机","9YQ-1800","形式:圆捆机 ;捡拾宽度:1.8m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","1\t型号\t/\t9YQ-1800\n2\t捡拾器宽度\tmm\t1800\n3\t捡拾器结构型式\t/\t甩刀式\n4\t卷压滚筒转速\tr/min\t320\n5\t卷压滚筒数量\t个\t13\n6\t工作状态外型尺寸（长×宽×高）\tmm\t2470×2210×1480\n7\t配套动力\tkw\t40.4~66.1\n8      压缩室直径 mm  600","7300","鄂2019123","2023-12-31","50000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","山东博豪农机技术服务有限公司","圆草捆打捆机","9YQ-2350","形式:圆捆机 ;捡拾宽度:2.35m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","1\t型号\t/\t9YQ-2350\n2\t捡拾器宽度\tmm\t2350\n3\t捡拾器结构型式\t/\t甩刀式\n4\t卷压滚筒转速\tr/min\t320\n5\t卷压滚筒数量\t个\t15\n6\t工作状态外型尺寸（长×宽×高）\tmm\t2470×2740×1480\n7\t配套动力\tkw\t66.1~99.2\n8      压缩室直径  mm   600","7300","鄂2019124","2023-12-31","60000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","潍坊百牧机械有限公司","圆草捆打捆机","9YK-2250","形式:圆捆机 ;捡拾宽度:2.25m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","捡拾器宽度：2250mm；捡拾器结构型式：甩刀式；卷压滚筒数量：14个；工作状态外形尺寸（长×宽×高）：2700mm×2650mm×1350mm;配套动力（型式）：非固定式≥65KW","7300","部20180782","2022-12-31","35000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","宁津方盛农业机械有限公司","捡拾圆捆机","9YQ-180","形式:圆捆机 ;捡拾宽度:1.8m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","捡拾器宽度mm：1800；捡拾器结构型式：甩刀式；卷压滚筒数量\t个：15；工作状态外形尺寸（长×宽×高）：3100mm×2200mm×1600mm；非固定式配套动力\tkW：40.4～75.0。","7300","部20190415","2023-12-31","28000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","平顶山市久久实业有限公司","圆捆捡拾压捆机","9YG-2.30","形式:圆捆机 ;捡拾宽度:2.3m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","挂接方式：牵引式；捡拾宽度\tmm：2300；捡拾器结构型式：甩刀式；喂入器结构型式：拨叉喂入机构；压缩室成捆机构型式：滚筒式；压缩室宽度\tmm：1280；压缩室直径mm\t：610；卷压滚筒数量个：15；卷压滚筒直径\tmm：156；缠捆方式（绳或网）：绳。","7300","GZNJ/TJ 2019-184","2023-12-31","28000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","山东川国机械制造有限公司","圆草捆打捆机","9YQ-1300","形式:圆捆机 ;捡拾宽度:1.3m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","配套动力范围（kW）：40.4-66.1kW；工作状态外形尺寸（长×宽×高）2410mm×1780mm×1540mm；结构质量（kg）1275kg；捡拾器结构型式：甩刀式；压缩室直径：700mm；压缩室宽度：1000mm ；打结器类型：无；打结器数量：无；卷压滚筒转速：320r/min；卷压滚筒数量：13个；捡拾宽度：1300mm","7300","鄂2019150","2023-12-31","24800.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","山东川国机械制造有限公司","圆草捆打捆机","9YQ-1800","形式:圆捆机 ;捡拾宽度:1.8m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","配套动力范围（kW）：40.4-66.1kW；工作状态外形尺寸（长×宽×高）2470mm×2210mm×1480mm；结构质量（kg）：1410kg；捡拾器结构型式：甩刀式；压缩室截面尺寸（宽×高）mm：700mm×1000mm；打结器类型：无；打结器数量：无；卷压滚筒数量：15个；捡拾宽度：1800mm","7300","部20180778","2022-12-31","25400.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","山东川国机械制造有限公司","圆草捆打捆机","9YQ-2350","形式:圆捆机 ;捡拾宽度:2.35m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","配套动力范围（kW）：66.1-99.2kW；工作状态外形尺寸（长×宽×高）2470mm×2740mm×1480mm；结构质量（kg）：1700kg；捡拾器结构型式：甩刀式；压缩室直径：700mm；压缩室宽度：1000mm ；打结器类型：无；打结器数量：无；卷压滚筒数量：15个；捡拾宽度：2350mm","7300","部20180779","2022-12-31","25800.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","山东瑞科农业装备有限公司","圆草捆打捆机","9YQ-1250","形式:圆捆机 ;捡拾宽度:1.25m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","捡拾器宽度：1250mm；捡拾器结构型式:弹齿式；压缩室截面尺寸（宽×高）mm：700mm×1000mm；卷压滚筒转速:320r/min；卷压滚筒数量:15个；工作状态外形尺寸（长×宽×高）mm:1950×1750×1510；配套动力:≥29.5kw。","7300","GZNJ/TJ 2019-019","2023-12-31","30000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","0.7-1.2m捡拾压捆机","山东瑞科农业装备有限公司","圆草捆打捆机","9YQ-1300","形式:圆捆机 ;捡拾宽度:1.3m;压缩室大小:圆捆机压缩室直径≥550mm,压缩室宽度≥550mm ;打结器数量:/个;","捡拾器宽度：1300mm；捡拾器结构型式:甩刀式；压缩室截面尺寸（宽×高）mm：700mm×1000mm；卷压滚筒转速:320r/min；卷压滚筒数量:15个；工作状态外形尺寸（长×宽×高）mm: 2740×1750×1480 ；配套动力:≥36.8kw。","7300","GZNJ/TJ 2019-017","2023-12-31","30000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","克雷斯曼河北农业机械有限公司","圆草捆打捆机","9YGQ-1.0","形式:圆捆机 ;捡拾宽度:2.3m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","挂接方式：牵引式；捡拾宽度：2300mm；捡拾器结构型式：甩刀式；喂入器结构型式：螺旋连续喂入机构；压缩室成捆机构型式：滚筒式；压缩室宽度：1250mm；压缩室直径：1000mm。","16000","鄂2019547","2024-12-29","55000.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","河南省颍骏机械制造有限公司","圆草捆打捆机","9YQ-2.3","形式:圆捆机 ;捡拾宽度:2.3m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","捡拾器宽度：2.3m，压缩室直径：1m，压缩室宽度：1.25m","16000","GZNJ/TJ 2019-195","2023-12-31","65800.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","河北春翔机械有限公司","圆草捆打捆机","9YQ-2.3","形式:圆捆机 ;捡拾宽度:2.3m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","挂接方式：牵引式；捡拾宽度mm：2300；捡拾器结构型式：甩刀式；喂入器结构型式：螺旋连续喂入机构；压缩室成捆机构型式：滚筒式；压缩室宽度mm：1250；压缩室直径mm：1000；卷压滚筒数量（个）：18；卷压滚筒直径mm：194；缠捆方式（绳或网）：网；配套动力范围kw：73.5~100。","16000","GZNJ/TJ 2019-326","2024-09-26","70000.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","雷沃重工股份有限公司","圆草捆打捆机","9YRZ-1.1","形式:圆捆机 ;捡拾宽度:1.83m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","结构型式：牵引式；捡拾器宽度：1830mm；草捆体积（㎥）：0.94；压缩室直径1110，压缩室宽度1000","16000","黑垦鉴2017084","2021-12-31","258600.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","平顶山市久久实业有限公司","圆捆捡拾压捆机","9YG-1.80B","形式:圆捆机 ;捡拾宽度:1.8m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","挂接方式\t：牵引式；捡拾宽度\tmm：1800；捡拾器结构型式：甩刀式；喂入器结构型式：拨叉喂入机构；压缩室成捆机构型式：滚筒式；压缩室宽度\tmm：1280；压缩室直径mm：990；卷压滚筒数量\t个：18；卷压滚筒直径\tmm：194；缠捆方式（绳或网）：绳。","16000","GZNJ/TJ 2019-183","2023-12-31","70000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","呼伦贝尔市蒙力农牧业机械制造有限公司","圆草捆打捆机","9YG-1.1A","形式:圆捆机 ;捡拾宽度:1.844m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","捡拾器宽度：1844mm；卷压滚筒数量：16个；卷压滚筒转速：131.2r/min；工作状态外形尺寸（长*宽*高）：3760mm*2300mm*2120mm；配套动力：≥66kw；压缩室直径：1100mm；压缩室宽度：1250mm","16000","部20170100","2021-12-31","178000.00","","通用类","内蒙古自治区","评阅不通过","初评员：不通过","专家：不通过。产品配置参数不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","呼伦贝尔市蒙力农牧业机械制造有限公司","秸秆圆捆机","9YGJ-1.1A","形式:圆捆机 ;捡拾宽度:1.844m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","捡拾器宽度：1844mm；捡拾器结构形式：锤爪式；卷压滚筒数量：16个；工作状态外形尺寸（长*宽*高）：3760mm*2400mm*2120mm；配套动力：≥66kw；压缩室直径：1100mm；压缩室宽度：1250mm","16000","部20180248","2022-12-31","198000.00","","通用类","内蒙古自治区","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","潍坊国安工程机械有限公司","圆草捆打捆机","9YGT-1.2","形式:圆捆机 ;捡拾宽度:1.28m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:0个;","型号：9YGT-1.2;捡拾宽度：1280mm;捡拾器结构型式：弹齿式；卷压滚筒数量：16个；工作状态外形尺寸：1540mm×1690mm×1480mm；配套动力：非固定式≥30kw","16000","部20190681","2023-12-31","55000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求；产品配置参数证明文件不符合要求，无法确认是否符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","牙克石市兴农农机具制造有限公司","牧草秸秆圆捆机","92YG-1.2","形式:圆捆机 ;捡拾宽度:1.65m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:0个;","型号:92YG-1.2；捡拾器宽度:1650MM；卷压滚筒转速:127R/MIN；滚筒数量:14个；工作状态外型尺寸(长×宽×高):4580MM×2570MM×2240MM；配套动力:≥29.4KW；草捆直径1.2m；压缩室直径1200mm，压缩室宽度1500mm","16000","内蒙古2018-053","2022-12-31","63000.00","","通用类","内蒙古自治区","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","内蒙古瑞丰农牧业装备股份有限公司","圆草捆打捆机","9YG-1.0","形式:圆捆机 ;捡拾宽度:1.73m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","捡拾器宽度：1.73m；捡拾器结构型式：弹齿式；卷压滚筒数量：16个；工作状态外形尺寸mm：3250x2530x1920；配套动力：51.4kW","16000","黑垦鉴2019088","2023-12-31","115000.00","","通用类","内蒙古自治区","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求；产品配置参数证明文件不符合要求，无法确认是否符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","江苏沃得高新农业装备有限公司（原：江苏沃得植保机械有限公司、原：沃得重工（中国）有限公司）","圆草捆打捆机","9YGQ-1000B","形式:圆捆机 ;捡拾宽度:2.32m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","捡拾宽度（mm）:2320；配套动力（kW）：≥51.5；挂接方式：牵引式；捡拾器结构型式：弹齿式；喂入器结构型式：螺旋连续喂入机构；压缩室成捆机构型式：滚筒式；压缩室宽度（mm）：1200；压缩室直径（mm）：990；卷压滚筒数量（个）：14；卷压滚筒直径（mm）：1Φ264，13个Φ220。","16000","T2019320040","2024-10-30","180000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合机具分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","江苏沃得高新农业装备有限公司（原：江苏沃得植保机械有限公司、原：沃得重工（中国）有限公司）","捡拾打捆机","9YGQ-1000","形式:圆捆机 ;捡拾宽度:2.35m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","捡拾宽度:2.35m;卷压滚筒转速(r/min):160;卷压滚筒数量:14个;工作状态外形尺寸(长×宽×高)(mm):4300×3100×2150;配套动力:≥51.5.","16000","2016TJ292","2020-12-31","145800.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合机具分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","华创机器人制造有限公司","圆草捆打捆机","9YQ-230A","形式:圆捆机 ;捡拾宽度:2.3m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","型号：9YQ-230A；配套动力（非固定式）kw：≥95.6；工作状态外形尺寸（长×宽×高）mm:4020×3140×3100；捡拾器宽度mm:2300；捡拾器结构型式:甩刀式；卷压滚筒数量：21个；","16000","鄂2019107","2023-12-31","148000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求；捡拾宽度不符合分档基本配置与参数要求；产品配置参数证明文件不符合要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","高唐绿荫环保科技有限公司","圆捆打捆机","9YG-1.1","形式:圆捆机 ;捡拾宽度:1.52m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","1、型号：9YG-1.1型，\n2、捡拾宽度：1520mm，\n3、卷压滚筒转速：124r/min，\n4、卷压滚筒数量：16个，\n5、工作状态外形尺寸（长×宽×高）：4300mm×2150mm×2100mm，\n6、配套动力：≥66kW","16000","部20170087","2021-12-31","172000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。产品配置参数不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","郑州豫飞达机械制造有限公司","圆捆捡拾打捆机","9YGQ-1.8","形式:圆捆机 ;捡拾宽度:1.8m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","结构尺寸(长×宽×高)3085×2216×1825(㎜)配套动力51.5-73.5(KW)捡拾器宽度1800(MM)捡拾器结构型式(/)粉碎滚筒式滚筒转速300(R/MIN)卷压滚筒数量11(个)，压缩室直径810mm，压缩室宽度1000mm","16000","豫2017196","2021-12-31","55500.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","郑州豫飞达机械制造有限公司","圆捆捡拾打捆机","9YGQ-2.2","形式:圆捆机 ;捡拾宽度:2.2m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","结构尺寸(长×宽×高)3041×2470×1749(㎜)配套动力73.5-88.2(KW)捡拾器宽度2200(MM)捡拾器结构型式(/)粉碎滚筒式滚筒转速300(R/MIN)卷压滚筒数量11(个)，压缩室直径810mm，压缩室宽度1000mm","16000","豫2017197","2021-12-31","56000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求；产品配置参数证明文件不符合要求","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","潍坊恺欧机械有限公司","圆草捆打捆机","9YQ-2300","形式:圆捆机 ;捡拾宽度:2.3m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","挂接方式：牵引式；捡拾宽度（mm）：2300；捡拾器结构型式：甩刀式；喂入器结构型式：螺旋连续喂入机构；压缩室成捆机构型式：滚筒式；压缩室宽度（mm）：1250；压缩室直径（mm）：970；卷压滚筒数量（个）：16；卷压滚筒直径（mm）220；配套动力范围（KW）：58.8-88.2","16000","鄂2019279","2024-07-17","100000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","潍坊轩沃农业机械有限公司","圆草捆打捆机","9YQ-2300","形式:圆捆机 ;捡拾宽度:2.3m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","捡拾器宽度：2300mm；捡拾器结构型式:甩刀式；压缩室截面尺寸（宽×高）mm：1000mm×1250mm；卷压滚筒转速:350r/min；卷压滚筒数量:18个；工作状态外形尺寸（长×宽×高）mm:3200×2700×1900；配套动力:≥66.2kw。","16000","GZNJ/TJ 2019-066","2023-12-31","85000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","山东瑞科农业装备有限公司","圆草捆打捆机","9YQ-2300","形式:圆捆机 ;捡拾宽度:2.3m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","捡拾器宽度：2300mm；捡拾器结构型式:甩刀式；压缩室截面尺寸（宽×高）mm：1000mm×1250mm；卷压滚筒转速:235r/min；卷压滚筒数量:18个；工作状态外形尺寸（长×宽×高）mm:3650×2710×1900；配套动力:≥73.5kw。","16000","GZNJ/TJ 2019-018","2023-12-31","90000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","平顶山市久久实业有限公司","圆捆捡拾压捆机","9YG-2.30B","形式:圆捆机 ;捡拾宽度:2.3m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","挂接方式：牵引式；捡拾宽度\tmm：2300；捡拾器结构型式：甩刀式；喂入器结构型式：拨叉喂入机构；压缩室成捆机构型式：滚筒式；压缩室宽度mm：1280；压缩室直径\tmm：990；卷压滚筒数量个：18；卷压滚筒直径\tmm：194；缠捆方式（绳或网）：绳。","16000","GZNJ/TJ 2019-185","2023-12-31","80000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","宁津方盛农业机械有限公司","圆捆捡拾打捆机","9YQ-230","形式:圆捆机 ;捡拾宽度:2.3m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","挂接方式：牵引式；捡拾宽度mm：2300；捡拾器结构型式：甩刀式；喂入器结构型式：螺旋连续喂入机构；压缩室成捆机构型式：滚筒式；压缩室宽度mm：1250；压缩室直径mm：1100；卷压滚筒数量（个）：18；卷压滚筒直径mm：194；缠捆方式（绳或网）：网；配套动力范围kw：68-120。","16000","GZNJ/TJ 2019-208","2023-12-31","60000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合机具分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","山东瑞科农业装备有限公司","圆草捆打捆机","9YJQ-2200","形式:圆捆机 ;捡拾宽度:2.2m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","捡拾器宽度：2200mm；捡拾器结构型式:弹齿式；压缩室宽度：1250mm：压缩室直径：∅1000mm；压缩室容积：0.98m³；卷压滚筒转速:235r/min；卷压滚筒数量:15个；配套动力:≥73.5kw。","16000","GZNJ/TJ 2019-247","2024-08-05","85000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","山东瑞科农业装备有限公司","圆草捆打捆机","9YQC-2210","形式:圆捆机 ;捡拾宽度:2.21m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","捡拾器宽度：2210mm；捡拾器结构型式:甩刀式；压缩室截面尺寸（宽×高）mm：1100mm×1200mm；卷压滚筒转速:185r/min；卷压滚筒数量:18个；工作状态外形尺寸（长×宽×高）mm：4660×2960×3350；配套动力:≥110kw。","16000","GZNJ/TJ 2019-016","2023-12-31","100000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","山东瑞科农业装备有限公司","圆草捆打捆机","9YZ-2250A","形式:圆捆机 ;捡拾宽度:2.25m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","捡拾器宽度：2250mm；捡拾器结构型式:弹齿式；压缩室截面尺寸（宽×高）mm：1000mm×1250mm；卷压滚筒转速:235r/min；卷压滚筒数量:18个；工作状态外形尺寸（长×宽×高）mm：5180×2700×2770；配套动力:73.5（选装81、88）kw。","16000","GZNJ/TJ 2019-022","2023-12-31","100000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","山东冉沪环保科技有限公司","捡拾圆捆机","9YQ-225A","形式:圆捆机 ;捡拾宽度:2.25m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","圆捆型号名称 / 9YQ-225A型，捡拾圆捆机 挂接方式 / 牵引式， 捡拾宽度 mm 2250 ， 捡拾器结构型式 / 甩刀式， 喂入器结构型式 / 螺旋连续喂入机构， 压缩室成捆机构型式 / 滚筒式 ，压缩室宽度 mm 1450 ，压缩室直径 mm 900。","16000","T202000370269","2025-07-05","85000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","河南省躬耕农业机械制造有限公司","圆草捆打捆机","9YGF-2.3","形式:圆捆机 ;捡拾宽度:2.3m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","型号：9YGF-2.3  捡拾器宽度：2300mm    捡拾器结构型式：甩刀式  卷压滚筒转速：325r/min卷压滚筒数量：12个 工作状态外型尺寸（长×宽×高）：3020×2700×1650mm配套动力88.5-139.7kw","16000","鄂2019067","2023-12-31","54000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合机具分档基本配置与参数要求","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","新乡市正鑫农业机械制造有限公司","圆捆捡拾压捆机","9YJY-1.22","形式:圆捆机 ;捡拾宽度:1.22m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","型号名称：9YJY-1.22型圆捆捡拾压捆机，捡拾宽度：1220mm，捡拾器结构型式：弹齿，工作状态外形尺寸：2400*2000*1750mm，配套动力：22.1～36.8kW.","16000","豫2017047","2021-12-31","54000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求；未提供产品配置参数证明文件。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","舞钢市恒利达机械制造有限责任公司","圆捆捡拾压捆机","9YG-1.75A","形式:圆捆机 ;捡拾宽度:1.75m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","型号名称  /   9YG-1.75A型圆捆捡拾压捆机   挂接方式 / 悬挂式  捡拾宽度 mm  1750   喂入口宽度  mm /   捡拾器结构型式 / 弹齿式\n喂入器结构型式 /  螺旋连续喂入机构  压缩室成捆机构型式 个 滚筒式  压缩室宽度 mm 1250  压缩室直径 mm 800\n卷压滚筒数量  个  14  卷压滚筒直径 mm  177  缠捆方式（绳或网） / 绳   配套动力范围  kW  44.1～58.9","16000","T201941410025","2024-11-13","55000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合机具分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","潍坊泰业机械有限公司","圆草捆打捆机","9YGQ-1.0","形式:圆捆机 ;捡拾宽度:2.3m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","捡拾宽度：2300mm  捡拾器结构型式：甩刀式  压缩室宽度：1000mm  压缩室直径：980mm 卷压滚筒数量：21个","16000","鄂2019269","2024-07-17","115500.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","潍坊泰业机械有限公司","圆草捆打捆机","9YGQ-1.2","形式:圆捆机 ;捡拾宽度:2.3m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","捡拾器宽度：2300mm  捡拾器结构型式：甩刀式  压缩室宽度：1200mm  压缩室直径：1000mm  卷压滚筒数量：23个","16000","鄂2019268","2024-07-17","146700.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","潍坊雷泰机械有限公司","圆草捆打捆机","9YQ-2300","形式:圆捆机 ;捡拾宽度:2.3m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","捡拾器宽度：2300mm；捡拾器结构型式:甩刀式；卷压滚筒转速:235r/min；卷压滚筒数量:18个；压缩室截面尺寸（宽×高）mm：1000×1250；工作状态外形尺寸（长×宽×高）mm：3650×2710×1900；配套动力:≥73.5kw。","16000","GZNJ/TJ 2019-027","2023-12-31","90000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","潍坊雷泰机械有限公司","圆草捆打捆机","9YJQ-2200","形式:圆捆机 ;捡拾宽度:2.2m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","捡拾器宽度：2200mm；捡拾器结构型式:弹齿式；压缩室宽度：1250mm：压缩室直径：1000mm；卷压滚筒转速:235r/min；卷压滚筒数量:15个；配套动力:≥73.5kw。","16000","GZNJ/TJ 2019-248","2024-08-05","85000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","宁津县鹏宇环保节能设备有限公司","捡拾圆捆机","9YQ-235","形式:圆捆机 ;捡拾宽度:2.35m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","捡拾宽度=2350mm；圆捆机压缩室直径=1100mm；圆捆机压缩室宽度=1250mm","16000","部20190129","2023-12-31","120000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合机具分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","潍坊雷泰机械有限公司","圆草捆打捆机","9YQC-2210","形式:圆捆机 ;捡拾宽度:2.21m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","捡拾器宽度：2210mm；捡拾器结构型式:甩刀式；压缩室截面尺寸（宽×高）mm：1100×1200；卷压滚筒转速:185r/min；卷压滚筒数量:18个；工作状态外形尺寸（长×宽×高）mm:4660×2960×3350；配套动力:≥110kw。","16000","GZNJ/TJ 2019-025","2023-12-31","100000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","潍坊雷泰机械有限公司","圆草捆打捆机","9YZ-2250A","形式:圆捆机 ;捡拾宽度:2.25m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","捡拾器宽度：2250mm；捡拾器结构型式:弹齿式；压缩室截面尺寸（宽×高）mm：1000×1250；卷压滚筒转速:235r/min；卷压滚筒数量:18个；工作状态外形尺寸（长×宽×高）mm:5180×2700×2770；配套动力:73.5kw（选装81kW；88kW）。","16000","GZNJ/TJ 2019-031","2023-12-31","100000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","开封市富农机械装备有限公司","圆草捆打捆机","9YQ-2300B","形式:圆捆机 ;捡拾宽度:2.3m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","捡拾宽度mm：2300；捡拾器结构型式：甩刀式；喂入器结构型式：螺旋连续喂入机构；压缩室成捆机构型式：滚筒式；压缩室宽度mm：1250；压缩室直径mm：970；卷压滚筒数量个：16；卷压滚筒直径mm：220；缠捆方式（绳或网）：尼龙编织网；配套动力范围kW：58.8-88.2；","16000","鄂2019283","2024-07-17","140000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","宁津县鹏宇环保节能设备有限公司","捡拾圆捆机","9YQ-2250A","形式:圆捆机 ;捡拾宽度:2.25m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","捡拾宽度=2250mm；圆捆机压缩室直径=1050mm；圆捆机压缩室宽度=1000mm","16000","部20190504","2023-12-31","120000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合机具分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","潍坊鑫牧机械有限公司","圆草捆打捆机","9YK-2300","形式:圆捆机 ;捡拾宽度:2.3m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","挂接方式：牵引式；捡拾宽度（mm）:2300;捡拾器结构型式：弹齿式；压缩室宽度（mm）：1270；压缩式直径（mm）：1020；卷压滚筒数量（个）：23；卷压滚筒直径（mm）:152;配套动力范围：（kw）≥51.5","16000","鄂2019213","2024-07-17","105000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","宁津县永升机械制造有限公司","捡拾圆捆机","9YQ-180","形式:圆捆机 ;捡拾宽度:1.8m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","型号9YQ-180捡拾器宽度1800mm捡拾器结构型式甩刀式卷压滚筒数量15个工作状态外形尺寸(长×宽×高)2900mm×2220mm×1620mm非固定式配套动力40.4~75.0kw","16000","部20190430","2023-12-31","55000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求；捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","安陆市宏利机械有限公司","圆草捆打捆机","9YQ-1.0","形式:圆捆机 ;捡拾宽度:2.3m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","挂接方式:牵引式；捡拾宽度:2300mm；喂入口宽度:1260mm；捡拾器结构型式:甩刀式；喂入器结构型式:螺旋连续喂入机构；压缩室成捆机构型式:滚筒式；压缩室宽度:1250mm；压缩室直径:1000mm；卷压滚筒数量:18个；卷压滚筒直径:210mm；缠捆方式:缠网","16000","鄂2019566","2024-12-29","53450.00","","通用类","湖北省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","潍坊飞奥农业机械有限公司","圆草捆打捆机","9YQ-230D","形式:圆捆机 ;捡拾宽度:2.3m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","型号名称：9YQ-230D型圆草捆打捆机；挂接方式：牵引式；捡拾宽度mm：2300；捡拾器结构型式：甩刀式；喂入器结构型式：螺旋连续喂入机构；压缩室成捆机构型式  ：滚筒式；压缩室宽度mm:1200；压缩室直径mm:1050；卷压滚筒数量：22个；卷压滚筒直径mm:152；缠捆方式（绳或网）：尼龙编织网；配套动力范围KW:58.8-88.2；","16000","鄂2019335","2024-07-17","152000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求；捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","山东博通农机服务有限公司","圆草捆打捆机","9YK-2300","形式:圆捆机 ;捡拾宽度:2.3m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","1\t型号名称\t/\t9YK-2300型圆草捆打捆机\n2\t挂接方式\t/\t牵引式\n3\t捡拾宽度\tmm\t2300\n4\t喂入口宽度\tmm\t/\n5\t捡拾器结构型式\t/\t甩刀式\n6\t喂入器结构型式\t/\t螺旋连续喂入机构\n7\t压缩室成捆机构型式\t个\t滚筒式\n8\t压缩室宽度\tmm\t1270\n9\t压缩室直径\tmm\t1020\n10\t卷压滚筒数量\t个\t23\n11\t卷压滚筒直径\tmm\tφ152\n12\t缠捆方式（绳或网）\t/\t麻绳\n13\t配套动力范围\tkW\t≥51.5","16000","鄂2019214","2024-07-17","60000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","潍坊智胜农业装备科技有限公司","圆草捆打捆机","9YQ-2300","形式:圆捆机 ;捡拾宽度:2.3m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","配套动力范围（kW）：≥73.5kW；工作状态外形尺寸（长×宽×高）2890mm×2700mm×1920mm；捡拾器结构型式：甩刀式；压缩室宽度：1250mm；压缩室直径：1000mm；卷压滚筒转速：235r/min；卷压滚筒数量：18个；捡拾宽度：2300mm","16000","GZNJ/TJ 2019-059","2023-12-31","55000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","山东华拖农业装备有限公司","圆草捆打捆机","9YQ-2300","形式:圆捆机 ;捡拾宽度:2.3m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","捡拾器宽度：2300mm；捡拾器结构型式:甩刀式；压缩室宽度：1250mm：压缩室直径：∅1000mm；压缩室容积：0.98m³；卷压滚筒转速:235r/min；卷压滚筒数量:18个；工作状态外形尺寸（长×宽×高）mm:3650×2710×1900；配套动力:≥73.5kw。","16000","GZNJ/TJ 2019-332","2024-10-07","80000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。产品配置参数不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","山东华拖农业装备有限公司","圆草捆打捆机","9YJQ-2200","形式:圆捆机 ;捡拾宽度:2.2m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","捡拾器宽度：2200mm；捡拾器结构型式:弹齿式；压缩室宽度：1250mm：压缩室直径：∅1000mm；压缩室容积：0.98m³；卷压滚筒转速:235r/min；卷压滚筒数量:17个；配套动力:≥73.5kw。","16000","GZNJ/TJ 2019-331","2024-10-07","85000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。产品配置参数不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","山东天华农业机械制造有限公司","圆捆捡拾打捆机","9YQ-230","形式:圆捆机 ;捡拾宽度:2.3m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","挂接方式：牵引式；捡拾宽度mm：2300；捡拾器结构型式：甩刀式；喂入器结构型式：螺旋连续喂入机构；压缩室成捆机构型式：滚筒式；压缩室宽度mm：1250；压缩室直径mm：1000；卷压滚筒数量（个）：18；卷压滚筒直径mm：195；缠捆方式（绳或网）：网；配套动力范围kw：≥75。","16000","GZNJ/TJ 2019-260","2024-08-22","60000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合机具分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.2-1.7m捡拾压捆机","任丘市金威机械配件有限公司","圆捆捡拾打捆机","9YQ-225","形式:圆捆机 ;捡拾宽度:2.25m;压缩室大小:圆捆机压缩室直径≥800mm,压缩室宽度≥800mm ;打结器数量:/个;","挂接方式：牵引式；捡拾宽度mm：2250；捡拾器结构型式：甩刀式；压缩室宽度mm：1250；压缩室直径mm：1000；卷压滚筒数量：18个；卷压滚筒直径mm：195。","16000","GZNJ/TJ 2019-251","2024-08-22","70000.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。产品配置参数不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.7-2.2m捡拾压捆机","天津轩禾农业机械制造有限公司","圆草捆打捆机","9YG-1.2","形式:圆捆机 ;捡拾宽度:1.96m;压缩室大小:圆捆机压缩室直径≥1200mm,压缩室宽度≥1200mm ;打结器数量:/个;","捡拾器宽度1960mm，捡拾器结构形式弹齿辊筒式，卷压滚筒转速180r/min，卷压滚筒数量16个，工作状态外形尺寸（长×宽×高）3950*2710*2600mm，配套动力≥60kW，圆草捆打捆机的草捆尺寸为（直径×宽度）：1200mm×1200mm圆捆机压缩室容积（草捆体积）：1.36 m³","28400","TJ-2017T-2","2021-12-31","268000.00","","通用类","天津市","评阅不通过","初评员：不通过","专家：不通过。产品配置参数证明文件不符合要求，无法确认是否符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.7-2.2m捡拾压捆机","山东五征集团有限公司","青饲料收获圆捆打捆机","4QYZ-3","形式:圆捆机 ;捡拾宽度:２m;压缩室大小:圆捆机压缩室直径≥1200mm,压缩室宽度≥1200mm ;打结器数量:/个;","工作状态外形尺寸（长×宽×高）6900mm×2250×3000×结构质量（kg）：8660kg 压缩室截面尺寸（宽×高）：850mm×1000 配套动力范围（kW）:176kw ：卷压滚筒数量;８９个。","28400","T201937370115","2024-10-24","950000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。未提供产品配置参数证明文件，无法确认是否符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.7-2.2m捡拾压捆机","延津县祥宇机械有限公司","方捆打捆机","9YFQ-1.8","形式:方捆机 ;捡拾宽度:1.8m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:2个;","型号：9YFQ-1.8；捡拾宽度：1800mm；打捆活塞速度：100行程/min；打结器类型：D型；工作状态外形尺寸：4800*2160*1750；配套动力：≥22。","28400","豫2016057","2020-12-31","90000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。缺少产品配置参数证明文件，无法确定是否符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.7-2.2m捡拾压捆机","山东江华机械制造有限公司","方草捆打捆机","9YFQ-1.9","形式:方捆机 ;捡拾宽度:1.928m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:2个;","型号名称：9YFQ-1.9方草捆打捆机；挂接方式：牵引式；捡拾宽度（mm）：1928；捡拾器结构型式：弹齿式；喂入器结构型式：拨叉喂入机构；打结器型式：D型；打结器数量（个）：2；压缩室截面尺寸（宽×高）mm：442×356；配套动力范围（mm）：≥26","28400","GZNJ/TJ 2019-340","2024-11-20","97000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。产品配置参数不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.7-2.2m捡拾压捆机","东风井关农业机械有限公司","方捆打捆机","9YFQ-2.0(ENY2000)","形式:方捆机 ;捡拾宽度:2.0m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:2个;","捡拾器宽度：2000mm；打捆机活塞速度（行程/min)：100；打结器类型：D型；工作状态外形尺寸（mm)：4950×2630×1750；配套动力：35.3-58.8KW；纯工作小时工作率：≥1500kg/h.","28400","鄂2016109","2020-12-31","110000.00","","通用类","湖北省","评阅不通过","初评员：不通过","专家：不通过。未提供产品产品配置参数证明文件，无法确认是否符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.7-2.2m捡拾压捆机","上海世达尔现代农机有限公司","方草捆打捆机","9YFQ-2.1","形式:方捆机 ;捡拾宽度:1.96m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:2个;","捡拾宽度：1.96","28400","T201931310001","2024-10-20","110000.00","","通用类","上海市","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.7-2.2m捡拾压捆机","上海世达尔现代农机有限公司","方草捆打捆机(方草捆压捆机)","9YFQ-1.8(THB3060)","形式:方捆机 ;捡拾宽度:1.705m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:2个;","捡拾宽度：1.705m","28400","沪2017-016","2021-12-31","100000.00","","通用类","上海市","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.7-2.2m捡拾压捆机","内蒙古瑞丰农牧业装备股份有限公司","圆草捆打捆机","9YG-1.2","形式:圆捆机 ;捡拾宽度:2.03m;压缩室大小:圆捆机压缩室直径≥1200mm,压缩室宽度≥1200mm ;打结器数量:/个;","捡拾器宽度：2.03m；捡拾器结构型式：弹齿式；卷压滚筒数量：18个；工作状态外形尺寸mm：4200x2800x2280；配套动力：66.15kW","28400","部20171280","2021-12-31","198000.00","","通用类","内蒙古自治区","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求；产品配置参数证明文件不符合要求，无法确认是否符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.7-2.2m捡拾压捆机","灵璧县泰顺机械有限公司","捡拾式方捆压捆机","9YFQ-1950","形式:方捆机 ;捡拾宽度:1.8m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:2个;","产品型号:9YFQ-1950、捡拾器宽度:1800(MM)、打捆活塞速度:100(行程/MIN)、打结器类型:D型、工作状态外形尺寸:长4700X宽2780X高2090(MM)、配套动力:≥25.7(KW)","28400","2019TJ520","2024-12-23","108000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.7-2.2m捡拾压捆机","中国农业机械化科学研究院呼和浩特分院有限公司","三道捆绳方草捆捡拾压捆机","9YFS-2.2","形式:方捆机 ;捡拾宽度:2230m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:3个;","型号：9YFS-2.2\n捡拾器宽度：2230mm\n打捆活塞速度 90 行程/min\n打结器类型 D型\n配套动力 ≥44.1kW(牵引拖拉机) 50 （自带柴油机）\n工作状态外型尺寸（长×宽×高）7250mm×2998mm×2510mm","28400","部20170096","2021-12-31","245000.00","","通用类","内蒙古自治区","评阅不通过","初评员：不通过","专家：不通过。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.7-2.2m捡拾压捆机","天津威猛机械制造有限公司","圆草捆打捆机","404Pro","形式:圆捆机 ;捡拾宽度:1.97m;压缩室大小:圆捆机压缩室直径≥1200mm,压缩室宽度≥1200mm ;打结器数量:/个;","捡拾器宽度：1970mm，捡拾器结构型式：弹齿辊筒式，卷压滚筒转速：160r/min,卷压滚筒数量：18个，工作状态外型尺寸（长*宽*高）：4410mm*2810mm*2480mm。","28400","TJ-2017T-1","2021-12-31","408000.00","","通用类","天津市","评阅不通过","初评员：不通过","专家：不通过。产品配置参数证明文件不符合要求，无法确认是否符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.7-2.2m捡拾压捆机","四平双天机械装备有限公司","秸秆捡拾打捆机","9YJ-1.8","形式:方捆机 ;捡拾宽度:1.8m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:/个;","型号:9YJ-1.8捡拾器宽度:1800mm；捡拾器结构型式:锤爪式；压缩室截面尺寸(宽×高):450mm×350mm；工作状态外形尺寸(长×宽×高):4750mm×3180mm×3560mm；配套动力:≥74kw","28400","吉农机鉴2018-004","2022-12-31","150000.00","","通用类","吉林省","评阅不通过","初评员：不通过","专家：不通过。未提供产品配置参数证明文件，无法确认是否符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.7-2.2m捡拾压捆机","天津库恩农业机械有限公司","圆捆机","FB3130","形式:方捆机 ;捡拾宽度:2.13m;压缩室大小:圆捆机压缩室直径≥1200mm,压缩室宽度≥1200mm ;打结器数量:/个;","捡拾器宽度：2130mm\n卷压滚筒转速：540r/min\n卷压滚筒数量：18个\n工作状态外形尺寸（长x宽x高）：4100x2940x2390mm\n配套动力：＞65kw","28400","黑垦鉴2016144","2021-12-31","450000.00","","通用类","天津市","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求；铭牌未使用铆钉铆接，无法确认为整机铭牌。捡拾宽度不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.7-2.2m捡拾压捆机","河北江天农业机械有限公司","捡拾圆捆机","9YQ-1800","形式:圆捆机 ;捡拾宽度:1.8m;压缩室大小:圆捆机压缩室直径≥1200mm,压缩室宽度≥1200mm ;打结器数量:15个;","捡拾宽度:1800mm、监视器结构形式:甩刀式、卷压滚筒转速:388r/min、卷压滚筒数量:15个、工作状态外形尺寸:2975mm×2170mm×1485mm、配套动力:58.8-73.5kW","28400","冀2018T-110","2022-12-31","95000.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。产品配置参数证明文件不符合要求，无法确认是否符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.7-2.2m捡拾压捆机","吉林省凯迪能源科技有限公司","秸秆饲料捡拾打捆机","9YFQ-1.7","形式:方捆机 ;捡拾宽度:1.7m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:/个;","捡拾宽度:1.7m;捡拾器结构型式：锤爪式","28400","T202022220075","2025-05-28","114500.00","","通用类","吉林省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","1.7-2.2m捡拾压捆机","四平市硕丰机械制造有限公司","秸秆饲料捡拾打捆机","9YFQ-1.7","形式:方捆机 ;捡拾宽度:1.7m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:/个;","捡拾宽度:1700mm;捡拾器结构型式：锤爪式","28400","T202022220076","2025-05-28","114000.00","","通用类","吉林省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求；产品配置参数不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","黑龙江银锚建筑机械有限公司","玉米秸秆打捆机","9Y90-2.4","形式:方捆机 ;捡拾宽度:2.4m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:2个;","挂接方式:牵引式;捡拾宽度:2400mm;捡拾器结构型式:锤爪式;喂入器结构型式:拨叉喂入机构;打结器型式:D型打结器;数量:2个;压缩室截面尺寸:452×364;配套动力范围:≥66.2kW","28400","黑垦鉴2016038","2020-12-31","150000.00","","通用类","黑龙江","评阅不通过","初评员：不通过","专家：不通过。缺少产品配置参数证明文件，无法确认是否符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","黑龙江银锚建筑机械有限公司","方草捆打捆机","9YF-2.2","形式:方捆机 ;捡拾宽度:2.25m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:2个;","捡拾宽度:2250mm捡拾器结构型式:弹齿式喂入器结构型式:拨叉喂入机构打结器型式:D型打结器数量:2个配套动力范围:≥36.8kW","28400","T201923230060","2024-07-21","95000.00","","通用类","黑龙江","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","黑龙江银锚建筑机械有限公司","秸秆粉碎打捆机","9YF-2.2D","形式:方捆机 ;捡拾宽度:2.2m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:2个;","捡拾宽度:2200mm捡拾器结构型式:锤爪式喂入器结构型式:拨叉喂入机构打结器型式:D型打结器数量:2个配套动力范围:≥66.2kW","28400","T201923230061","2024-07-21","150000.00","","通用类","黑龙江","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","黑龙江银锚建筑机械有限公司","双刀轴秸秆粉碎打捆机","9YF-2.2S","形式:方捆机 ;捡拾宽度:2.2m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:2个;","捡拾宽度:2200mm捡拾器结构型式:锤爪式喂入器结构型式:拨叉喂入机构打结器型式:D型打结器数量:2个配套动力范围:≥88.2kW","28400","T201923230062","2024-07-21","160000.00","","通用类","黑龙江","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","黑龙江银锚建筑机械有限公司","秸秆粉碎打捆机","9YF-2.4D","形式:方捆机 ;捡拾宽度:2.4m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:2个;","捡拾宽度:2400mm捡拾器结构型式:锤爪式喂入器结构型式:拨叉喂入机构打结器型式:D型打结器数量:2个配套动力范围:≥66.2kW","28400","T201923230063","2024-07-21","150000.00","","通用类","黑龙江","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","黑龙江银锚建筑机械有限公司","双刀轴秸秆粉碎打捆机","9YF-2.4S","形式:方捆机 ;捡拾宽度:2.4m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:2个;","捡拾宽度:2400mm捡拾器结构型式:锤爪式喂入器结构型式:拨叉喂入机构打结器型式:D型打结器数量:2个配套动力范围:≥88.2kW","28400","T201923230064","2024-07-21","168000.00","","通用类","黑龙江","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","黑龙江银锚建筑机械有限公司","圆草捆打捆机","9YG-2.2","形式:圆捆机 ;捡拾宽度:2.24m;压缩室大小:圆捆机压缩室直径≥1200mm,压缩室宽度≥1200mm ;打结器数量:/个;","捡拾宽度:2240mm捡拾器结构型式:弹齿式喂入器结构型式:螺旋连续喂入机构压缩室成捆机构型式:滚筒式压缩室宽度:1230mm压缩室直径:1200mm卷压滚筒数量:18个卷压滚筒直径:222mm缠捆方式(绳或网):缠网配套动力范围:≥75kW","28400","T201923230065","2024-07-21","210000.00","","通用类","黑龙江","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","烟台泰通重工机械有限公司","捡拾压捆机","9YFQ-2.3A","形式:方捆机 ;捡拾宽度:2.3m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:/个;","型号:9YFQ-2.3A,捡拾器宽度:2300mm,捡拾器结构型式:锤爪式,打结器类型:D,打结器数量:2个,压缩室截面尺寸(宽×高):460mm×370mm,打捆活塞往复次数:102次/min,工作状态外型尺寸(长×宽×高):5400mm×2730mm×1750mm,配套动力:≥110KW.","28400","鄂2017235","2021-12-31","100000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","烟台泰通重工机械有限公司","捡拾压捆机","9YFQ-2.3B","形式:方捆机 ;捡拾宽度:2.3m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:/个;","型号:9YFQ-2.3B,捡拾器宽度:2300mm,捡拾器结构型式:弹齿式,打结器类型:D,打结器数量:2个,压缩室截面尺寸(宽×高):460mm×370mm,打捆活塞往复次数:102次/min,工作状态外型尺寸(长×宽×高):4590mm×2920mm×1750mm,配套动力:≥60KW.","28400","鄂2017236","2021-12-31","100000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","河南省颍骏机械制造有限公司","圆草捆打捆机","9YQ-2.3A","形式:圆捆机 ;捡拾宽度:2.3m;压缩室大小:圆捆机压缩室直径≥1200mm,压缩室宽度≥1200mm ;打结器数量:/个;","捡拾宽度：2.3m，压缩室直径：1.25m，压缩室宽度：1.25m","28400","部20190455","2023-12-31","158000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。产品配置参数证明文件不符合要求，无法确定是否符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","四平市隆发机械制造有限公司","圆草捆打捆机","9YJ-1.3","形式:圆捆机 ;捡拾宽度:2.2m;压缩室大小:圆捆机压缩室直径≥1200mm,压缩室宽度≥1200mm ;打结器数量:/个;","捡拾器宽度：2200mm\n捡拾器结构型式：弹齿式","28400","吉农机鉴2018-019","2022-12-31","298000.00","","通用类","吉林省","评阅不通过","初评员：不通过","专家：不通过。产品配置参数证明文件不符合要求，无法确定是否满足分档基本配置和参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","牙克石市兴农农机具制造有限公司","牧草秸秆圆捆机","9YG-1.2","形式:圆捆机 ;捡拾宽度:2.236m;压缩室大小:圆捆机压缩室直径≥1200mm,压缩室宽度≥1200mm ;打结器数量:0个;","型号:9YG-1.2捡拾宽度:2236MM捡拾器结构型式:弹齿式卷压滚筒数量:18个工作状态外形尺寸(长*宽*高):4670MM*3196MM*2340MM配套动力非固定式:≥73KW，压缩室直径1210mm，压缩室宽度1230mm","28400","部20171518","2021-12-31","188000.00","","通用类","内蒙古自治区","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","吉林省远航农业机械有限公司","圆草捆打捆机","9YY-1.4B3","形式:圆捆机 ;捡拾宽度:2.2m;压缩室大小:圆捆机压缩室直径≥1200mm,压缩室宽度≥1200mm ;打结器数量:/个;","（捡拾器类型：锤爪；数量：22）（捡拾器宽度：2200mm）（辊筒数量：17个）（外形尺寸：3980×2850×2250mm）（配套动力：≥110kW）（整机重量：3460kg）","28400","吉农机鉴2019-045","2023-12-31","358000.00","","通用类","吉林省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求；铭牌未用铆钉铆，无法确认为整机铭牌；产品配置参数证明文件不符合要求，无法确认是否满足分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","吉林省远航农业机械有限公司","捡拾方捆打捆机","9YJFS-2.2","形式:方捆机 ;捡拾宽度:2.2m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:2个;","（捡拾器类型：锤爪）（捡拾器宽度：2200mm）（外形尺寸： 6230×2588×1790mm ）（整机重量：2960kg）（配套动力 ≥80kW(110马力)（锤爪数量：14个）（压缩式尺寸：440×360mm）","28400","T201922220062","2024-12-15","281000.00","","通用类","吉林省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求；铭牌未用铆钉铆，无法确认为整机铭牌。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","吉林省远航农业机械有限公司","捡拾方捆打捆机","9YJ-2.2A2","形式:方捆机 ;捡拾宽度:2.23m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:2个;","（捡拾器类型：弹齿）(外形尺寸4600 mm ×2860 mm ×1750 mm )(总重 1680kg )(捡拾宽度 2230mm )(配套功率≥37 kW （50马力）)(压缩室截面尺寸 450mm ×360mm )(草捆长度  500mm -1350mm )(打结器类型 加强D型）（打结器数量：2个）","28400","T201922220063","2024-12-15","206000.00","","通用类","吉林省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求；铭牌未用铆钉铆，无法确认为整机铭牌。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","吉林省远航农业机械有限公司","捡拾方捆打捆机","9YJ-2.2B2","形式:方捆机 ;捡拾宽度:2.2m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:2个;","（捡拾器类型：锤爪）（外形尺寸 长×宽×高： 5500mm ×2660mm ×1850mm） (总重 2400 kg)(捡拾器宽度 2200 mm)(锤爪数量  22个)(刀座宽度  86mm)(压捆室 横截面尺寸  360mm ×440mm )(草捆长度 30cm ～130cm） (打结器类型  D型)(打捆机构主轴转速 100r/min )","28400","T201922220067","2024-12-15","219000.00","","通用类","吉林省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求；铭牌未用铆钉铆，无法确认为整机铭牌。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","吉林省远航农业机械有限公司","捡拾方捆打捆机","9YJF-2.2","形式:方捆机 ;捡拾宽度:2.2m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:/个;","(捡拾器结构型式 / 锤爪)(外形尺寸 5400mm×2900mm×3900mm)(配套动力≥95.6 kW ）(整机质量 5240 Kg)(草捆规格800 mm ×320 mm ×420 mm )(主油缸 行程  900mm)(最大压力20 Mpa )(压缩油缸 行程 400 mm)(最大压力 20 Mpa)(推料油缸 行程  820mm)( 最大压力 20 Mpa)( 捡拾工作幅宽  2200mm）(捡拾锤爪数量 22 个)(压缩室 横截面积 320mm ×420mm )( 秸秆捆密度 ≥150 Kg/m³)(草捆密度 ≥150 Kg/m³)","28400","T201922220068","2024-12-15","267000.00","","通用类","吉林省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求；铭牌未用铆钉铆，无法确认为整机铭牌。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","吉林省远航农业机械有限公司","圆草捆打捆机","9YJ-1.4B","形式:圆捆机 ;捡拾宽度:2.2m;压缩室大小:圆捆机压缩室直径≥1200mm,压缩室宽度≥1200mm ;打结器数量:/个;","（捡拾器类型：弹齿；数量：72）（捡拾器宽度：2200mm）（辊筒数量：14个）（外形尺寸：4200x2830x2470mm）（配套动力：≥110kW）（整机重量：3250kg）","28400","吉农机鉴2019-022","2023-12-31","254000.00","","通用类","吉林省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求；铭牌未用铆钉铆，无法确认为整机铭牌；产品配置参数证明文件不符合要求，无法确认是否满足分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","吉林省远航农业机械有限公司","圆草捆打捆机","9YJ-1.4A4","形式:圆捆机 ;捡拾宽度:2.2m;压缩室大小:圆捆机压缩室直径≥1200mm,压缩室宽度≥1200mm ;打结器数量:/个;","（捡拾器类型：锤爪；数量：14）（捡拾器宽度：2200mm）（辊筒数量：14个）（外形尺寸：4200x2830x2470mm）（配套动力：≥110kW）（整机重量：3430kg）","28400","吉农机鉴2019-023","2023-12-31","267000.00","","通用类","吉林省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求；铭牌未用铆钉铆，无法确认为整机铭牌；产品配置参数证明文件不符合要求，无法确认是否满足分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","吉林省远航农业机械有限公司","圆草捆打捆机","9YJ-1.4B4","形式:圆捆机 ;捡拾宽度:2.2m;压缩室大小:圆捆机压缩室直径≥1200mm,压缩室宽度≥1200mm ;打结器数量:/个;","（捡拾器类型：弹齿；数量：72）（捡拾器宽度：2200mm）（辊筒数量：14个）（外形尺寸：4200x2830x2470mm）（配套动力：≥110kW）（整机重量：3250kg）","28400","吉农机鉴2019-024","2023-12-31","251000.00","","通用类","吉林省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求；铭牌未用铆钉铆，无法确认为整机铭牌；产品配置参数证明文件不符合要求，无法确认是否满足分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","吉林省远航农业机械有限公司","圆草捆打捆机","9YY-1.4A2","形式:圆捆机 ;捡拾宽度:2.2m;压缩室大小:圆捆机压缩室直径≥1200mm,压缩室宽度≥1200mm ;打结器数量:/个;","（捡拾器类型：弹齿；数量：72）（捡拾器宽度：2200mm）（辊筒数量：14个）（外形尺寸：3980×2545×2250mm）（配套动力：≥110kW）（整机重量：3250kg）","28400","吉农机鉴2019-046","2023-12-31","324000.00","","通用类","吉林省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求；铭牌未用铆钉铆，无法确认为整机铭牌；产品配置参数证明文件不符合要求，无法确认是否满足分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","吉林省远航农业机械有限公司","圆草捆打捆机","9YY-1.4B2","形式:圆捆机 ;捡拾宽度:2.2m;压缩室大小:圆捆机压缩室直径≥1200mm,压缩室宽度≥1200mm ;打结器数量:/个;","（捡拾器类型：锤爪；数量：14）（捡拾器宽度：2200mm）（辊筒数量：14个）（外形尺寸：3980×2545×2250mm）（配套动力：≥110kW）（整机重量：3430kg）","28400","吉农机鉴2019-044","2023-12-31","331000.00","","通用类","吉林省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求；铭牌未用铆钉铆，无法确认为整机铭牌；产品配置参数证明文件不符合要求，无法确认是否满足分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","吉林省远航农业机械有限公司","圆草捆打捆机","9YY-1.4A3","形式:圆捆机 ;捡拾宽度:2.2m;压缩室大小:圆捆机压缩室直径≥1200mm,压缩室宽度≥1200mm ;打结器数量:/个;","（捡拾器类型：弹齿；数量：72）（捡拾器宽度：2200mm）（辊筒数量：17个）（外形尺寸：3980×2545×2250mm）（配套动力：≥110kW）（整机重量：3280kg）","28400","吉农机鉴2019-047","2023-12-31","351000.00","","通用类","吉林省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求；铭牌未用铆钉铆，无法确认为整机铭牌；产品配置参数证明文件不符合要求，无法确认是否满足分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","吉林省远航农业机械有限公司","捡拾方捆压捆机","9YJ-2.2A","形式:方捆机 ;捡拾宽度:2.2m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:2个;","（捡拾器类型：弹齿）（捡拾器宽度：2200mm）（外形尺寸：4975*2850*1710）（整机净重：1700kg）（配套动力：≥45kW）（打结器类型：D型）（打结器数量：2个）（压缩室截面尺寸：440*355）","28400","吉农机鉴2017-033","2021-12-31","186000.00","","通用类","吉林省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","吉林省远航农业机械有限公司","捡拾方捆压捆机","9YJ-2.2A-1","形式:方捆机 ;捡拾宽度:2.2m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:2个;","（捡拾器类型：锤爪）（捡拾器宽度：2200mm）（外形尺寸：4975*2850*1710）（整机净重：1700kg）（配套动力：≥52kW）（打结器类型：D型）（打结器数量：2个））压缩室截面尺寸：440*355）","28400","吉农机鉴2017-034","2021-12-31","199000.00","","通用类","吉林省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","吉林省远航农业机械有限公司","捡拾压捆机","9YJ-2.2","形式:方捆机 ;捡拾宽度:2.2m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:/个;","（外形尺寸（长×宽×高）：8800mm×4560mm×3570mm）（整机重量：5500kg）（工作幅宽：2200mm）（粉碎捡拾转速：1600r/min）（粉碎捡拾机构安装甩刀对数：30对）（生产效率：1～2公顷/h）（配套动力：≥81kw）（秸秆捆截面尺寸：835mm×1145mm）（捆长：1500～2300mm）（压密秸秆密度：150～180kg/m3）（机组作业速度：6-8km/h）","28400","吉农机鉴2016-06","2020-12-31","335000.00","","通用类","吉林省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","吉林省远航农业机械有限公司","圆草捆打捆机","9YJ-1.4A","形式:圆捆机 ;捡拾宽度:2.2m;压缩室大小:圆捆机压缩室直径≥1200mm,压缩室宽度≥1200mm ;打结器数量:/个;","（捡拾器类型：锤爪；数量：14）（捡拾器宽度：2200mm）（辊筒数量：14个）（外形尺寸：4200x2830x2470mm）（配套动力：≥110kW）（整机重量：3430kg）","28400","吉农机鉴2019-021","2023-12-31","240000.00","","通用类","吉林省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求；铭牌未用铆钉铆，无法确认为整机铭牌；产品配置参数证明文件不符合要求，无法确认是否满足分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","四平双天机械装备有限公司","秸秆捡拾打捆机","9YT-2.2","形式:方捆机 ;捡拾宽度:2.2m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:/个;","型号:9YT-2.2捡拾器宽度:2200MM；捡拾器结构型式:锤爪式；压缩室截面尺寸(宽×高):450MM×350MM；工作状态外形尺寸(长×宽×高):4750MM×3180MM×3560MM；配套动力:≥88KW","28400","吉农机鉴2018-003","2022-12-31","168000.00","","通用类","吉林省","评阅不通过","初评员：不通过","专家：不通过。未提供产品配置参数证明文件，无法确认是否符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","中国农业机械化科学研究院呼和浩特分院有限公司","切割揉碎圆草捆打捆机","9YGR-2.2A","形式:圆捆机 ;捡拾宽度:2220m;压缩室大小:圆捆机压缩室直径≥1200mm,压缩室宽度≥1200mm ;打结器数量:/个;","型号：9YGR-2.2\n捡拾器宽度：2220mm\n捡拾器结构形式：锤爪式\n卷压滚筒数量：18个\n工作状态外型尺寸（长×宽×高）：4727 mm×2691mm×2304mm\n配套动力：非固定式≥75kW","28400","部20190425","2023-12-31","168000.00","","通用类","内蒙古自治区","评阅不通过","初评员：不通过","专家：不通过。产品配置参数证明文件提供信息不全，无法确认是否符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","中国农业机械化科学研究院呼和浩特分院有限公司","切割揉碎圆草捆打捆机","9YGR-2.2","形式:圆捆机 ;捡拾宽度:2220m;压缩室大小:圆捆机压缩室直径≥1200mm,压缩室宽度≥1200mm ;打结器数量:/个;","型号：9YGR-2.2\n捡拾器宽度：2220mm\n捡拾器结构形式：锤爪式\n卷压滚筒数量：18个\n工作状态外型尺寸（长×宽×高）：4727 mm×2769mm×2353mm\n配套动力：非固定式≥75kW","28400","部20190424","2023-12-31","168000.00","","通用类","内蒙古自治区","评阅不通过","初评员：不通过","专家：不通过。产品配置参数证明文件提供信息不全，无法确认是否符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","中国农业机械化科学研究院呼和浩特分院有限公司","圆草捆打捆机","9YGJ-2.2B","形式:圆捆机 ;捡拾宽度:2.235m;压缩室大小:圆捆机压缩室直径≥1200mm,压缩室宽度≥1200mm ;打结器数量:0个;","型号\t/\t9YGJ-2.2B\n捡拾器宽度\tmm\t2235\n捡拾器结构型式\t/\t弹齿式\n卷压滚筒数量\t个\t18\n工作状态外形尺寸（长×宽×高）\t/\t4190mm×2994mm×2397mm\n配套动力固定式\tkW\t/\n配套动力非固定式\tkW\t≥75","28400","部20190192","2023-12-31","198000.00","","通用类","内蒙古自治区","评阅不通过","初评员：不通过","专家：不通过。未提供产品配置参数证明文件，无法确认是否符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","中国农业机械化科学研究院呼和浩特分院有限公司","直连方草捆捡拾压捆机","9YFSZ-2.2","形式:方捆机 ;捡拾宽度:2233m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:3个;","型号：9YFSZ-2.2\n捡拾器宽度：2233mm\n打捆活塞速度 90 行程/min\n打结器类型 D型\n配套动力 ≥75kW\n工作状态外型尺寸（长×宽×高）7250mm×2998mm×1867mm","28400","部20170095","2021-12-31","240000.00","","通用类","内蒙古自治区","评阅不通过","初评员：不通过","专家：不通过。产品配置参数证明文件信息不全，无法确认是否符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","灵璧县泰顺机械有限公司","秸秆粉碎压捆机","9YFQ-2200","形式:方捆机 ;捡拾宽度:2.24m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:2个;","产品型号:9YFQ-2200、捡拾器宽度:2240MM、捡拾器结构型式:甩刀式、打结器类型:D型、打结器数量:2个、压缩室截机尺寸:440MMX370MM、打捆活塞往复次数:100次/MIN、工作状态外形尺寸:(长X宽X高)6300MMX2730MMX1900/2000MM(高度可调)、配套动力:≥80KW(轮式拖拉机)、捡拾宽度:2240MM","28400","2017TJ387","2021-12-31","168000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","内蒙古瑞丰农牧业装备股份有限公司","圆草捆打捆机","9YG-1.4D","形式:圆捆机 ;捡拾宽度:2.26m;压缩室大小:圆捆机压缩室直径≥1200mm,压缩室宽度≥1200mm ;打结器数量:/个;","捡拾器宽度：2260mm；捡拾器结构形式：弹齿式；卷压滚筒数量：18个；工作状态外形尺寸（长X宽X高）：4100X3040X2290mm；配套动力：80.85kW","28400","部20171281","2021-12-31","218000.00","","通用类","内蒙古自治区","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求；产品配置参数证明文件不符合要求，无法确认是否符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","内蒙古瑞丰农牧业装备股份有限公司","圆草捆打捆机","9YG-1.4E","形式:圆捆机 ;捡拾宽度:2.26m;压缩室大小:圆捆机压缩室直径≥1200mm,压缩室宽度≥1200mm ;打结器数量:/个;","捡拾器宽度：2260mm；捡拾器结构形式：弹齿式；卷压滚筒数量：18个；工作状态外形尺寸（长X宽X高）：4100X2960X2320mm；配套动力：95.6kW","28400","黑垦鉴2019086","2023-12-31","168000.00","","通用类","内蒙古自治区","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求；产品配置参数证明文件不符合要求，无法确认是否符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","内蒙古瑞丰农牧业装备股份有限公司","秸秆圆捆机","9YGJ-1.2","形式:圆捆机 ;捡拾宽度:2.26m;压缩室大小:圆捆机压缩室直径≥1200mm,压缩室宽度≥1200mm ;打结器数量:/个;","捡拾器宽度：2270mm；捡拾器结构形式：锤爪式；卷压滚筒数量：18个；工作状态外形尺寸（长X宽X高）：5100X2600X2300mm；配套动力：99.2kW","28400","部20171282","2021-12-31","268000.00","","通用类","内蒙古自治区","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","华创机器人制造有限公司","圆草捆打捆机","9YQ-230S","形式:圆捆机 ;捡拾宽度:2.3m;压缩室大小:圆捆机压缩室直径≥1200mm,压缩室宽度≥1200mm ;打结器数量:/个;","型号：9YQ-230S；配套动力（非固定式）kw:≥110.3；工作状态外形尺寸（长×宽×高）mm:4320×3140×3100；捡拾器宽度mm:2300；捡拾器结构型式:甩刀式；卷压滚筒数量:19个；","28400","鄂2019108","2023-12-31","150000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求；产品配置参数证明文件不符合要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","华创机器人制造有限公司","圆草捆打捆机","9YQ-230T","形式:圆捆机 ;捡拾宽度:2.3m;压缩室大小:圆捆机压缩室直径≥1200mm,压缩室宽度≥1200mm ;打结器数量:/个;","型号：9YQ-230T；配套动力（非固定式）kw：≥58.8；工作状态外形尺寸（长×宽×高）mm:4500×2750×2780；捡拾器宽度mm:2300；捡拾器结构型式:弹齿式；卷压滚筒数量:19个；","28400","鄂2019106","2023-12-31","152000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求；产品配置参数证明文件不符合要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","山东骏玛道机械有限公司","秸秆饲料捡拾打捆机","9YJF-2250","形式:方捆机 ;捡拾宽度:2.25m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:/个;","捡拾宽度：2250mm；压缩室截面尺寸：320×420mm；配套动力范围：≥132.3；捡拾器结构型式：锤爪式；","28400","T202000340218","2025-07-05","150000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。缺少产品配置参数证明文件，无法确定是否符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","安阳市豫工农业机械有限公司","履带自走式方草捆打捆机","9YFZ-2.36","形式:方捆机 ;捡拾宽度:2.36m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:2个;","型号名称 / 9YFZ-2.36型履带自走式方草捆打捆机 \n挂接方式 / 自走式 \n捡拾宽度 mm 2360 \n喂入口宽度 mm / \n捡拾器结构型式 / 弹齿式 \n喂入器结构型式 / 螺旋连续喂入机构 \n打结器型式 / D型 \n打结器数量 个 2 \n压缩室截面尺寸（宽×高） mm 450×300 \n配套动力范围 kW / \n配套发动机（电动机）额定功率 kW 73.6 \n配套发动机（电动机）额定转速 r/min 2400 \n驾驶室型式 / 无驾驶室 \n变速方式 / 手动变速 \n驱动方式 / 机械驱动(最终) \n制动器型式 / 湿式摩擦片式 \n轴距 mm / \n导向轮轮距 mm / \n驱动轮轮距 mm / \n导向轮轮胎规格 / / \n驱动轮轮胎规格 / / \n履带型式 / 橡胶履带 \n履带宽度 / 450mm \n履带接地长 mm 1460 \n轨距 mm 1200","28400","T201941410024","2024-11-13","185000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","喀什旺达机械制造有限责任公司","青贮压捆机","9YT-220","形式:方捆机 ;捡拾宽度:2.2m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:/个;","捡拾器宽度：2200mm;捡拾器结构型式：摔倒时；压缩室截面尺寸（宽×高）：680×1061mm;配套动力：≥90","28400","新2018050","2022-12-31","130000.00","","通用类","新疆维吾尔自治区","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","四平市硕丰机械制造有限公司","圆捆打捆机","9YGT-2200","形式:圆捆机 ;捡拾宽度:2.22m;压缩室大小:圆捆机压缩室直径≥1200mm,压缩室宽度≥1200mm ;打结器数量:/个;","捡拾宽度：2.22m；结构形式：弹齿式；卷压滚筒数量14个","28400","吉农机鉴2018-082","2022-12-31","145000.00","","通用类","吉林省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","四平市硕丰机械制造有限公司","秸秆饲料捡拾打捆机","9YFQ-2220C","形式:方捆机 ;捡拾宽度:2.22m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:/个;","捡拾宽度:2.22m;捡拾器结构形式:锤爪式;工作状态外形尺寸（长*宽*高）:5300*3300*3360mm","28400","吉农机鉴2019-053","2023-12-31","147000.00","","通用类","吉林省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","四平市硕丰机械制造有限公司","秸秆饲料捡拾打捆机","9YFQ-2.22","形式:方捆机 ;捡拾宽度:2.22m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:/个;","捡拾宽度：2.22m;捡拾器结构型式：锤爪式","28400","GZNJ/TJ 2019-288","2024-09-16","162000.00","","通用类","吉林省","评阅不通过","初评员：不通过","专家：不通过。未提供产品配置参数证明文件。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","四平市硕丰机械制造有限公司","秸秆饲料捡拾打捆机","9YFQ-2.2A","形式:方捆机 ;捡拾宽度:2.2m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:/个;","捡拾宽度:2200mm;捡拾器结构型式：锤爪式","28400","T202022220080","2025-05-28","167000.00","","通用类","吉林省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求；未提供产品配置参数证明文件。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","四平市硕丰机械制造有限公司","秸秆饲料捡拾打捆机","9YFQ-2.2B","形式:方捆机 ;捡拾宽度:2.2m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:/个;","捡拾宽度:2200mm;捡拾器结构型式：锤爪式","28400","T202022220078","2025-05-28","182000.00","","通用类","吉林省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求；未提供产品配置参数证明文件。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","天津沃农农业机械有限公司","方草捆打捆机","9YF-2200D","形式:方捆机 ;捡拾宽度:2.2m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:2个;","外形尺寸（长×宽×高）mm：5920×2550×1780；捡拾器宽度mm：2200；捡拾器结构型式：甩刀式；打结器类型：D型；打结器数量个：2；压缩室截面尺寸（宽×高）mm：457×356；打捆活塞往复次数次/min：100；配套动力非固定式kW：≥73.5","28400","GZNJ/TJ 2019-084","2023-12-31","132000.00","","通用类","天津市","评阅不通过","初评员：不通过","专家：不通过。产品配置参数证明文件不符合要求，无法确认是否符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","内蒙古华禹农牧机械有限公司","圆草捆卷捆机","9YGQ-2.2","形式:圆捆机 ;捡拾宽度:2280m;压缩室大小:圆捆机压缩室直径≥1200mm,压缩室宽度≥1200mm ;打结器数量:/个;","型号：9YGQ-2.2\n捡拾器宽度：2280mm\n捡拾器结构形式：弹齿式\n卷压滚筒数量：15个\n工作状态外型尺寸（长×宽×高）：3750mm×2940mm×2250mm\n配套动力：固定式\n          非固定式＞51kW","28400","部20190418","2023-12-31","168000.00","","通用类","内蒙古自治区","评阅不通过","初评员：不通过","专家：不通过。未提供产品配置参数证明文件，无法确认是否符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","吉林省德沃农机装备有限公司","秸秆饲料打捆机","9YFZ-2.2","形式:方捆机 ;捡拾宽度:2.2m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:/个;","捡拾器宽度2200mm；捡拾器结构型式：锤爪式；压缩室截面尺寸（宽×高）：340mm×440mm；工作状态外形尺寸（长×宽×高）：5100mm×2950mm×3930mm；配套动力：≥88kW；","28400","吉农机鉴2019-007","2023-12-31","172000.00","","通用类","吉林省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书、配置参数证明文件不符合要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","吉林省凯迪能源科技有限公司","秸秆饲料捡拾打捆机","9YFQ-2.22","形式:方捆机 ;捡拾宽度:2.22m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:/个;","捡拾宽度：2220mm；捡拾器结构型式：锤爪式","28400","GZNJ/TJ 2019-287","2024-09-16","225000.00","","通用类","吉林省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","吉林省凯迪能源科技有限公司","秸秆饲料捡拾打捆机","9YFQ-2220F","形式:方捆机 ;捡拾宽度:2.22m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:/个;","捡拾宽度:2220mm;捡拾器结构型式：锤爪式","28400","T202022220046","2025-03-19","182500.00","","通用类","吉林省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","吉林省凯迪能源科技有限公司","秸秆饲料捡拾打捆机","9YGT-2.22","形式:圆捆机 ;捡拾宽度:2.22m;压缩室大小:圆捆机压缩室直径≥1200mm,压缩室宽度≥1200mm ;打结器数量:/个;","捡拾宽度:2220mm;捡拾器结构型式：弹齿式","28400","T202022220074","2025-05-28","145500.00","","通用类","吉林省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","吉林省凯迪能源科技有限公司","秸秆饲料捡拾打捆机","9YFQ-2.2A","形式:方捆机 ;捡拾宽度:2.2m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:/个;","捡拾宽度：2200mm；捡拾器结构型式：锤爪式","28400","T202022220077","2025-05-28","167500.00","","通用类","吉林省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","山东天鹅棉业机械股份有限公司","圆草捆打捆机","9YT-2.2C","形式:圆捆机 ;捡拾宽度:2.2m;压缩室大小:圆捆机压缩室直径≥1200mm,压缩室宽度≥1200mm ;打结器数量:/个;","圆草捆；捡拾宽度：2.2m；压缩室容积：1.2m3；捡拾器结构型式：弹齿式","28400","鄂2019182","2023-12-31","340000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求；未提供产品配置参数证明文件，无法确认是否符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","沧州佰林机械制造有限公司","粉碎捡拾压捆机","9FJY-220","形式:方捆机 ;捡拾宽度:2.2m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:/个;","捡拾器宽度：2200mm;捡拾器结构型式：垂爪式；压缩室截面尺寸（宽×高）：1470×1720mm;配套动力：≥110.2KW","28400","新2019117","2024-04-10","100000.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","潍坊同顺机械有限公司","方草捆打捆机","9YF-2200A","形式:方捆机 ;捡拾宽度:2.2m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:2个;","型号名称\n/\n9YF-2200A型方草捆打捆机\n挂接方式\n/\n牵引式\n捡拾宽度\nmm\n2200\n喂入口宽度\nmm\n/\n捡拾器结构型式\n/\n弹齿式\n喂入器结构型式\n/\n拨叉喂入机构\n打结器型式\n/\nD型\n打结器数量\n个\n2\n压缩室截面尺寸（宽×高）\nmm\n458×362\n配套动力范围\nkW\n≥36.8","28400","GZNJ/TJ 2019-201","2023-12-31","95000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","山东富垠农业科技有限公司","捡拾圆捆打捆机","9YQ-2200","形式:圆捆机 ;捡拾宽度:2.2m;压缩室大小:圆捆机压缩室直径≥1200mm,压缩室宽度≥1200mm ;打结器数量:/个;","捡拾宽度（mm）：2200；捡拾器结构型式：弹齿式；卷压滚筒数量（个）：14；工作状态外形尺寸（长×宽×高）（mm）：4380×2970×2250；配套动力（kW）：≥73.5；","28400","GZNJ/TJ 2019-111","2023-12-31","160000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。未提供产品配置参数证明文件，无法确认是否符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","吉林纳海农业装备有限公司","秸秆饲料打捆机","9YZ-2250","形式:方捆机 ;捡拾宽度:2.25m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:/个;","1.型号名称：9YZ-2250型秸秆饲料打捆机 。2.挂接方式：牵引式。3.捡拾宽度：2250mm。4.捡拾器结构型式：锤爪式。5.压缩室截面尺寸（宽×高）：320×420mm。6.捆扎方式：自动网打捆。7.配套动力范围：≥88kW。","28400","T202022220083","2025-05-28","193000.00","","通用类","吉林省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","2.2m及以上捡拾压捆机","吉林纳海农业装备有限公司","秸秆饲料打捆机","9YZ-2300","形式:方捆机 ;捡拾宽度:2.3m;压缩室大小:方捆机压缩室截面尺寸(宽度×高度)≥400×300mm ;打结器数量:/个;","1.型号名称：9YZ-2300型秸秆饲料打捆机 。2.挂接方式：牵引式。3.捡拾宽度：2300mm。4.捡拾器结构型式：锤爪式。5.压缩室截面尺寸（宽×高）：320×420mm。6.捆扎方式：自动网打捆。7.配套动力范围：≥88kW。","28400","T202022220104","2025-05-28","193000.00","","通用类","吉林省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","4kW及以上圆捆压捆机","山东陵盛机械制造有限公司","青贮圆捆机","DK5252","形式:圆捆 ;功率:5.5kW;","配套动力：5.5kW；卷压滚筒数量：30个；喂入口宽度：520mm","7200","部20171266","2021-12-31","24000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","4kW及以上圆捆压捆机","喀什旺达机械制造有限责任公司","圆草捆压捆机","9YG-55","形式:圆捆 ;功率:5.5kW;","喂入口宽度：525mm;作业方式：固定式；草捆形状：圆捆","7200","新2017079","2021-12-31","35000.00","","通用类","新疆维吾尔自治区","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","4kW及以上圆捆压捆机","乐陵市原野机械设备有限公司","圆草捆打捆机","9QYG-0.5","形式:圆捆 ;功率:5.5kW;","圆捆；功率5.5kw","7200","部20190447","2023-12-31","24500.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","7.5-15kW方捆压捆机","西安新天地草业股份有限公司","方草捆压捆机","9YF-110","形式:方捆 ;功率:7.5kW;","1喂入口宽度：485mm； \n2 打捆活塞速度：3.57行程/min；            \n3 打结器类型：手工打结；                  \n4 工作状态外形尺寸（长×宽×高）2800×1100×1150；              \n5 配套动力7.5KW","2800","陕2017005","2021-12-31","11500.00","","通用类","陕西省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","打（压）捆机","15kW及以上方捆压捆机","西安新天地草业股份有限公司","方草捆压捆机","9YFZ-5","形式:方捆 ;功率:15kW;","1喂入口宽度：685mm； \n2 打捆活塞速度：0.97行程/min；            \n3 打结器类型：手工打结；                  \n4 工作状态外形尺寸（长×宽×高）2900×3000×2300；              \n5 配套动力15KW","11100","陕2017004","2021-12-31","43000.00","","通用类","陕西省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","圆草捆包膜机","1.1kW及以上圆草捆包膜机","安徽四方精工机械制造股份有限公司","圆捆包膜机","BMJ5552A","电机功率:1.1kW;电机:是 ;","1、外形尺寸：1500×1000×1060mm；2、配套动力：1.1 kW；3、包装工作速度80-140托/h。","2300","2018TJ626","2022-12-31","10000.00","","非通用类","安徽省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","青饲料收获机","110cm及以上悬挂单圆盘式青饲料收获机","山东犇牛畜牧机械设备有限公司","悬挂式青饲料收获机","4QX-1400","割幅:130cm;割台型式:悬挂双圆盘 ;","型号名称：4QX-1400型悬挂式青饲料收获机、结构型式（挂接方式）：悬挂式、\n工作状态外形尺寸（长*宽*高）3700mm*1500mm*3200mm  \n割台的有效收获宽度：1300mm\n割台切割器型式：双圆盘式、秸秆切碎机构型式：圆盘式、抛送筒高度：3200mm","7100","部20190175","2023-12-31","20000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。产品为悬挂双圆盘式，不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","青饲料收获机","110cm及以上悬挂单圆盘式青饲料收获机","山东犇牛畜牧机械设备有限公司","背负式青饲料收获机","4QX-1800","割幅:165cm;割台型式:悬挂双圆盘 ;","型号名称：4QX-1800型悬挂式青饲料收获机、结构型式:圆盘割刀式、挂接方式：悬挂式、\n工作状态外形尺寸（长*宽*高）4900mm*1830mm*4070mm  、结构质量：1200kg、工作幅宽：1650mm\n最低割茬高度：50mm、生产率：0.3~0.6（≧21t/h）、秸秆切碎机构型式：圆盘式、秸秆切碎机构转子直径：Φ900mm、秸秆切碎机构主轴转速：1000r/min、\n抛送高度：4000mm、抛送距离：≧8、抛送筒回转角度：360度","7100","部20170105","2021-12-31","20500.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。产品为悬挂双圆盘式，不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","青饲料收获机","110cm及以上悬挂单圆盘式青饲料收获机","石家庄驰田机械制造有限公司","青饲料收获机","9QX-1200","割幅:121cm;割台型式:悬挂双圆盘 ;","型号名称 / 9QX-1200青饲料收获机 \n形式 / 悬挂式 \n工作状态外形尺寸（长×宽×高） mm 3500×1380×3430 \n配套动力范围 kW 29～45 \n配套发动机额定功率 kW / \n配套发动机额定转速 r/min / \n割幅 mm 1210 \n作物收集割台型式 / 直切割台 \n割台切割器型式 / 圆盘式割刀 \n喂入机构型式 / 喂入辊 \n喂入机构数量 个 2 \n秸秆切碎机构型式 / 盘式 \n籽粒破碎机构型式 / / \n驾驶室型式(自走式） / / \n变速方式(自走式） / / \n驱动方式(自走式） / / \n制动器型式(自走式） / / \n导向轮轮距（自走式） mm / \n导向轮轮胎规格（自走式） / / \n驱动轮轮距（自走式） mm / \n驱动轮轮胎规格（自走式） / / \n履带宽度(自走式） mm / \n履带接地长(自走式） mm / \n轨距(自走式） mm / \n轴距(自走式） mm / \n作业速度范围 km/h 2～5 \n设计切段长度 mm 10、15、20、25","7100","T201913130261","2024-12-30","30000.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","青饲料收获机","110-210cm悬挂双圆盘式青饲料收获机","喀什旺达机械制造有限责任公司","青饲料收获机","4QS-1400","割幅:140cm;割台型式:悬挂双圆盘 ;","结构型式：悬挂式；割台切割器型式：双圆盘式；割台有效收获宽度：140cm,秸秆切碎机构型式：轮盘式；抛送筒高度，mm:3400,","7100","新2018260","2022-12-31","70000.00","","通用类","新疆维吾尔自治区","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","饲料作物收获机械","青饲料收获机","110-210cm悬挂双圆盘式青饲料收获机(籽粒破碎)","山东慧百机械设备有限公司","悬挂式青饲料收获机","4QX-1400","割幅:130cm;割台型式:悬挂双圆盘 ;含籽粒破碎功能:是 ;","型号名称：4QX-1400型悬挂式青饲料收获机、结构型式（挂接方式）：悬挂式；                   外形尺寸：4150mm×1500mm×3400mm；        割台的有效收获宽度：1300mm； 割台切割器型式：双圆盘式；秸秆切碎机构型式：盘式；抛送筒高度：3400mm","14300","部20190413","2023-12-31","37800.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","饲料作物收获机械","青饲料收获机","110-210cm悬挂双圆盘式青饲料收获机(籽粒破碎)","山东慧百机械设备有限公司","悬挂式青饲料收获机","4QX-1800","割幅:165cm;割台型式:悬挂双圆盘 ;含籽粒破碎功能:是 ;","型号名称：4QX-1800型悬挂式青饲料收获机、   结构型式（挂接方式）：悬挂式；             外形尺寸：5100mm×1840mm×4200mm；割台的有效收获宽度：1650mm； 割台切割器型式：双圆盘式；秸秆切碎机构型式：盘式；抛送筒高度：4200mm","14300","部20190412","2023-12-31","38000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","饲料作物收获机械","青饲料收获机","220cm及以上悬挂双圆盘式青饲料收获机","石家庄鑫茂机械有限公司","青饲料收获机","4QS-2400","割幅:240cm;割台型式:悬挂双圆盘 ;","型号名称：4QS-2400青饲料收获机；工作状态外形尺寸（长×宽×高）（mm）：5150×2410×3800（抛送筒向后方）；割幅（mm）：2300；作物收集割台形式：直切割台；割台切割器形式：圆盘式割刀；喂入机构形式：喂入辊；喂入机构数量：秸秆切碎机构形式：盘式；作业速度范围（km/h）：2-15；设计切段长度（mm）：20.","23400","T201913130096","2024-12-08","100000.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。铭牌未用铆钉铆，无法确定为整机铭牌。","","","","",""]
["收获机械","饲料作物收获机械","青饲料收获机","220cm及以上悬挂双圆盘式青饲料收获机","喀什旺达机械制造有限责任公司","青饲料收获机","4QS-2630","割幅:263cm;割台型式:悬挂双圆盘 ;","结构型式：悬挂式；割台切割器型式：双圆盘式；割台有效收获宽度：263cm；秸秆切碎机构型式：轮盘式；抛送筒高度，mm:4350","23400","新2018261","2022-12-31","125000.00","","通用类","新疆维吾尔自治区","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","青饲料收获机","220cm及以上悬挂双圆盘式青饲料收获机","沧州佰林机械制造有限公司","青饲料收获机","4QS-2400","割幅:240cm;割台型式:悬挂双圆盘 ;","结构型式：悬挂式；割台切割器型式：双圆盘式；割台有效收获宽度：240cm；秸秆切碎机构型式：盘刀式；抛送筒高度，mm:4600","23400","新2019112","2024-04-10","130000.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","饲料作物收获机械","青饲料收获机","220cm及以上悬挂双圆盘式青饲料收获机","沧州佰林机械制造有限公司","青饲料收获机","4QS-2700","割幅:265cm;割台型式:悬挂双圆盘 ;","结构型式：悬挂式；割台切割器型式：双圆盘式；割台有效收获宽度：265cm；秸秆切碎机构型式：盘刀式；抛送筒高度，mm:4580","23400","新2019113","2024-04-10","130000.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","饲料作物收获机械","青饲料收获机","220cm及以上悬挂双圆盘式青饲料收获机(籽粒破碎)","山东慧百机械设备有限公司","悬挂式青饲料收获机","4QX-2300","割幅:225cm;割台型式:悬挂双圆盘 ;含籽粒破碎功能:是 ;","型号名称：4QX-2300型悬挂式青饲料收获机     结构型式（挂接方式）：悬挂式； 外形尺寸：5600mm×2380mm×3900mm；割台的有效收获宽度：2250mm； 割台切割器型式：双圆盘式；秸秆切碎机构型式：盘式；抛送筒高度：3900mm","46800","部20190414","2023-12-31","121900.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","饲料作物收获机械","青饲料收获机","220cm及以上悬挂其他式青饲料收获机","河北牧泽农牧机械有限公司","青饲料收获机","4QB-10","割幅:220cm;割台型式:自走其他式 ;","形式：悬挂式 ;工作状态外形尺寸（长*宽*高）：4800*2590*3650mm ；配套动力范围：66-95KW；工作幅宽：220cm ；作物收集割台型式：直切割台；割台切割器型式：往复式割刀；喂入机构型式：喂入辊；喂入机构数量：4；秸秆切碎机构型式：盘式；作业速度范围：1-3.5km/h；设计切段长度：35mm","7900","T201913130055","2024-12-08","61000.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","饲料作物收获机械","青饲料收获机","200-260cm自走圆盘式青饲料收获机","喀什旺达机械制造有限责任公司","自走式青（黄）贮饲料收获机","4QSZ-2400","割幅:235cm;割台型式:自走圆盘式 ;","结构型式：自走式；割台有效收获宽度，mm:2350;割台切割器型式：圆盘式；配套发动机额定功率，kw：154；秸秆切碎机构型式：盘刀式；抛送筒高度，mm:4450;轴距，mm：2650；轮胎规格：导向轮：10.0-75-15.3；驱动轮：13.6-24；导向轮轮距，mm:1650;驱动轮轮距，mm:1730；","31900","新2019063","2024-04-10","295000.00","","通用类","新疆维吾尔自治区","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","青饲料收获机","200-260cm自走圆盘式青饲料收获机","河北元正农业机械有限公司","青饲料收获机","9QZ-2100","割幅:212cm;割台型式:自走圆盘式 ;","自走圆盘式；割幅：212cm；结构质量：5940kg","31900","T201913130026","2024-08-29","250000.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","青饲料收获机","200-260cm自走圆盘式青饲料收获机(籽粒破碎)","新乡市凯航机械制造有限公司","自走式青饲料收获机","4QZ-8A","割幅:240cm;割台型式:自走圆盘式 ;含籽粒破碎功能:是 ;","型号名称：4QZ-8A型自走式青饲料收获机 、 工作状态外形尺寸：长X宽X高6700mmX2500mmX4550mm 、 结构质量：5450kg、 配套发动机 型号规格：WP6G180E330 、 额定功率：132.5KW 、 额定转速：2200r/min 、 割副：2400mm 、 割台切割器型式：圆盘式、 轮距：导向轮1630mm .驱动轮1710mm 、 轮胎规格：导向轮10.0/75-15.3 驱动轮15-24、 轴距：2730mm 、 最小离地间隙：310mm 、 驾驶室型式：普通式。","63700","T202000410086","2025-03-31","225000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","青饲料收获机","200-260cm自走圆盘式青饲料收获机(籽粒破碎)","新乡市凯航机械制造有限公司","自走式青饲料收获机","4QZ-8","割幅:240cm;割台型式:自走圆盘式 ;含籽粒破碎功能:是 ;","型号名称：4QZ-8型自走式青饲料收获机 、 工作状态外形尺寸：长X宽X高6700mmX2500mmX4550mm 、 结构质量：5450kg、 配套发动机 型号规格：YCD4P33T6-155 、 额定功率：113KW 、 额定转速：2300r/min 、 割副：2400mm 、 割台切割器型式：圆盘式、 轮距：导向轮1630mm .驱动轮1710mm 、 轮胎规格：导向轮10.0/75-15.3 驱动轮15-24、 轴距：2660mm 、 最小离地间隙：310mm 、 驾驶室型式 ：普通式。","63700","豫2018049","2022-12-31","225000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","饲料作物收获机械","青饲料收获机","200-260cm自走圆盘式青饲料收获机(籽粒破碎)","沧州佰林机械制造有限公司","自走式青（黄）贮饲料收获机","4QSZ-2200","割幅:220cm;割台型式:自走圆盘式 ;含籽粒破碎功能:是 ;","结构型式：自走式；;配套发动机额定功率，kw：154；作物收集割台型式：直切割台；割台切割器型式：旋转圆盘刀；割幅，mm:2200；喂入机构型式：喂入辊；喂入机构数量，个：4；秸秆切碎机构型式：盘式；籽粒破碎机构型式：揉搓板式；驾驶室型式：普通驾驶室；;轴距，mm：2600；轮胎规格：导向轮：10/.0-75-15.3；驱动轮：13.6-24；导向轮轮距，mm:1680;驱动轮轮距，mm:1680;","63700","新2019285","2024-12-24","335000.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","青饲料收获机","260cm及以上自走圆盘式青饲料收获机(籽粒破碎)","山东运德机械制造有限公司","青饲料收获机","4QZ-830A","割幅:290cm;割台型式:自走圆盘式 ;含籽粒破碎功能:是 ;","序号\t项目\t单位\t设计值\n1\t型号名称\t/\t4QZ-830A型青饲料收获机\n2\t形式\t/\t自走式\n3\t工作状态外形尺寸（长*宽*高）\tmm\t7600X3070X5150\n4\t配套动力范围（牵引式、悬挂式）\tKw\t/\n5\t配套发动机额定功率（自走式、配有发动机的牵引式）\tKw\t266\n6\t配套发动机额定转速（自走式、配有发动机的牵引式）\tr/min\t2200\n7\t割幅\tmm\t2900\n8\t作物收集割台型式\t/\t直切割台\n9\t割台切割器型式\t/\t圆盘式割刀（2个圆盘）\n10\t喂入机构型式\t/\t喂入辊\n11\t喂入机构数量\t/\t6\n12\t秸秆切碎机构型式\t/\t滚筒式\n13\t籽粒破碎机构型式\t/\t对辊式\n14\t驾驶室型式（自走式）\t/\t普通驾驶室\n15\t变速方式（自走式）\t/\t手动变速\n16\t驱动方式（自走式）\t/\t液压驱动\n17\t制动器型式（自走式）\t/\t盘式\n18\t导向轮轮距（自走式）\tmm\t2050\n19\t导向轮轮胎规格（自走式）\t/\t12.00-18\n20\t驱动轮轮距（自走式）\tmm\t2350\n21\t驱动轮轮胎规格（自走式）\t/\t23.1-26\n22\t履带宽度（自走式）\tmm\t/\n23\t履带接地长（自走式）\tmm\t/\n24\t轨距（自走式）\tmm\t/\n25\t轴距（自走式）\tmm\t2700\n26\t作业速度范围\tkm/h\t2-6\n27\t设计切段长度\tmm\t10~30","129600","T202000150027","2025-03-31","550000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。承诺书不规范。","","","","",""]
["收获机械","饲料作物收获机械","青饲料收获机","260cm及以上自走圆盘式青饲料收获机(籽粒破碎)","新疆牧神机械有限责任公司","自走式青（黄）贮饲料收获机","4QZ-3000BS","割幅:300cm;割台型式:自走圆盘式 ;含籽粒破碎功能:是 ;","结构型式:自走圆盘式；配套动力kW：247；割台结构型式：不对行立式滚筒式；工作幅宽mm：3000；具有籽粒破碎装置","129600","T202000650320","2025-07-05","610000.00","","通用类","新疆维吾尔自治区","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","青饲料收获机","260cm及以上自走圆盘式青饲料收获机(籽粒破碎)","河北牧泽农牧机械有限公司","青饲料收获机","4QZ-18A","割幅:290cm;割台型式:自走圆盘式 ;含籽粒破碎功能:是 ;","结构形式：自走式；外形尺寸：7700*3080*5200mm；额定功率：247W，额定转速：2200r/min； 工作幅宽：2900mm；作物收集割台型式：直切割台；割台切割器型式：圆盘式割刀；喂入机构型式：喂入辊；喂入机构数量：7；秸秆切碎机构形式：滚筒式；籽粒破碎机构型式：对辊式；驾驶室型式：普通；变速型式：手动变速；驱动方式：液压驱动；制动器型式：盘式；导向轮轮距1920mm，导向轮轮胎规格10.0/75-15.3；驱动轮轮距：2280mm；驱动轮轮胎规格：19.5L-24；轴距：2480mm；作业速度范围2-9km/h；设计切段长度21.6、15mm","129600","T201900130004","2024-10-22","568000.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","饲料作物收获机械","青饲料收获机","260cm及以上自走圆盘式青饲料收获机(籽粒破碎)","河北利裕丰机械有限公司","自走式青饲料收获机","9QZ-2600","割幅:260cm;割台型式:自走圆盘式 ;含籽粒破碎功能:是 ;","结构型式（挂接方式）：悬挂式；结构质量（kg）：6500；；工作状态外形尺寸（长×宽×高）mm：7200*2870*4900；割台的有效收获宽度（mm）：2600；割台切割器型式：圆盘式割刀；导向轮轮距：1570mm；驱动轮轮距：2000；轮胎规格：460/70R24*10.0/75-15.3；驾驶室型式：普通式；秸秆切碎机构型式：滚筒式；抛送筒高度：4900mm","129600","T201900130396","2024-12-30","360000.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。机型属于自走圆盘式，不符合分档基本配置与参数要求。","","","","",""]
["收获机械","饲料作物收获机械","青饲料收获机","260cm及以上自走圆盘式青饲料收获机(籽粒破碎)","山东省聊城会晟农业机械有限公司","自走式青贮饲料收获机","4QZP-3000","割幅:≥260cmcm;割台型式:自走圆盘式 ;含籽粒破碎功能:是 ;","结构型式：自走式；割台切割器型式：转盘式；配套动力（kW）：247；割台的有效收获宽度(mm)：3000；工作状态外形尺寸（长×宽×高mm）7700*3100*3350；最小离地间隙(mm)：350；轮距(mm)：导向轮1580、驱动轮1930；轮胎规格：导向轮10.0-7.5-15.3、驱动轮17.5-25；轴距(mm)：2660；秸秆切碎机构型式：一字刀斜切式、转子直径(mm)800；抛送筒高度(mm)：4000；作业速度范围（km/h）：1-4；","129600","新2018020","2022-12-31","432000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","饲料作物收获机械","青饲料收获机","260cm及以上自走圆盘式青饲料收获机(籽粒破碎)","沧州佰林机械制造有限公司","自走式青（黄）贮饲料收获机","4QSZ-2600","割幅:260cm;割台型式:自走圆盘式 ;含籽粒破碎功能:是 ;","结构型式：自走式；;配套发动机额定功率，kw：154；作物收集割台型式：直切割台；割台切割器型式：旋转圆盘刀；割幅，mm:2600；喂入机构型式：喂入辊；喂入机构数量，个：4；秸秆切碎机构型式：滚筒式；籽粒破碎机构型式：揉搓板式；驾驶室型式：普通驾驶室；;轴距，mm：3150；轮胎规格：导向轮：10/.0-75-15.3；驱动轮：13.6-24；导向轮轮距，mm:1680;驱动轮轮距，mm:1680;","129600","T202065650006","2025-04-16","436000.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","青饲料收获机","260cm及以上自走圆盘式青饲料收获机(籽粒破碎)","新乡市凯航机械制造有限公司","自走式青饲料收获机","4QZ-12","割幅:265cm;割台型式:自走圆盘式 ;含籽粒破碎功能:是 ;","型号名称：4QZ-12型自走式青饲料收获机、工作状态外形尺寸：长X宽X高6700mmX2700mmX4500mm 、 结构质量：5800kg、 配套发动机 型号规格：WP6G210E330 、 额定功率：154KW 、 额定转速：2200r/min 、 割副：2650mm 、 割台切割器型式：圆盘式、 轮距：导向轮1720mm .驱动轮1850mm 、 轮胎规格：导向轮10.0/75-15.3 驱动轮15-24、 轴距：2730mm 、 最小离地间隙：300mm 、 驾驶室型式：普通式","129600","豫2018050","2022-12-31","438000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","饲料作物收获机械","青饲料收获机","220-260cm自走其他式青饲料收获机","山东省聊城会晟农业机械有限公司","青贮饲料收获机","4QZ-2200","割幅:220cm≤割幅＜260cmcm;割台型式:自走其他式 ;","结构尺寸（长x宽x高cm）:8400x2660x3180 整机质量（kg）:5700 配套动力（kw）:132   工作宽幅(mm):2200 结构形式:自走式导向轮轮距(mm):1470 驱动轮轮距(mm):1765 作业速度(km/h):3~6 生产率(kg/h):≥0.6 抛送高度(mm):4570 抛送距离(mm):10000 抛物筒回转角度（º）:210","31000","新2016114","2020-12-31","251000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","饲料作物收获机械","青饲料收获机","260-290cm自走其他式青饲料收获机","山东省聊城会晟农业机械有限公司","自走式青贮饲料收获机","4QZ-2600A","割幅:260cmcm;割台型式:自走其他式 ;","工作状态外形尺寸（长×宽×高mm）7100*2800*3500；最小离地间隙(mm)：260；轮距(mm)：导向轮1640、驱动轮1870；轮胎规格：导向轮  10-15、驱动轮15-24；结构型式：自走式；配套动力（kW）：162；割台的有效收获宽度(mm)：2600；轴距(mm)：2930；秸秆切碎机构型式：一字刀斜切式、转子直径(mm)550；抛送筒高度(mm)：4000；作业速度范围（km/h）：2-4；","39800","新2018247","2022-12-31","295000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","饲料作物收获机械","青饲料收获机","260-290cm自走其他式青饲料收获机","山东省聊城会晟农业机械有限公司","青贮饲料收获机","4QZ-2600","割幅:260cm≤割幅＜290cmcm;割台型式:自走其他式 ;","配套动力（kw）:162 ；；结构形式:自走式 ；结构尺寸（长x宽x高cm）:8800x2970x3380； 整机质量（kg）:5900  ；割台结构形式：拨禾轮式；工作宽幅(mm):2600 ；割台升降范围0-800mm；切碎机构型式：组合刀片式；切碎抛送器型式：组合刀片式。导向轮轮距(mm):1450 驱动轮轮距(mm):1850 作业速度(km/h):3~6 生产率(kg/h):80000（玉米秸秆含水率折算到78%）抛送高度(mm):4570 抛送距离(mm):10000 抛物筒回转角度（º）:210","39800","新2016115","2020-12-31","293000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","饲料作物收获机械","青饲料收获机","290cm及以上自走其他式青饲料收获机","山东省聊城会晟农业机械有限公司","青贮饲料收获机","4QZ-2900A","割幅:≥290cmcm;割台型式:自走其他式 ;","结构尺寸（长x宽x高cm）:8300x3350x3480 整机质量（kg）:6300 配套动力（kw）:206   工作宽幅(mm):2950  结构形式:自走式导向轮轮距(mm):1670 驱动轮轮距(mm):2070  作业速度(km/h):3~6  生产率(kg/h):71000 抛送高度(mm):4570 抛送距离(mm):10000 抛物筒回转角度（º）:210","64800","新2016117","2020-12-31","312000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","饲料作物收获机械","青饲料收获机","290cm及以上自走其他式青饲料收获机","山东省聊城会晟农业机械有限公司","青贮饲料收获机","4QZ-2900","割幅:≥290cmcm;割台型式:自走其他式 ;","结构尺寸（长x宽x高cm）:8700x3330x3180 整机质量（kg）:6100 配套动力（kw）:162   工作宽幅(mm):2950 结构形式:自走式导向轮轮距(mm):1450  驱动轮轮距(mm):1850 作业速度(km/h):3~6 生产率(kg/h):71000 抛送高度(mm):4570 抛送距离(mm):10000 抛物筒回转角度（º）:210","64800","新2016116","2020-12-31","313000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","茎秆收集处理机械","秸秆粉碎还田机","1-1.5m秸秆粉碎还田机","河北利宏农业机械制造有限公司","秸秆粉碎还田机","1JHY-100","作业幅宽:1m;","工作状态外形尺寸(长×宽×高)：1280×1220×900mm；配套动力输出轴转速：540/720r/min；作业速度：3.0-5.0km/h；工作幅宽：100cm；刀轴最大回转半径：250mm；刀片总安装数量：42把。","800","鄂2019496","2024-12-29","3000.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。名牌背景颜色与机具照片颜色不符。","","","","",""]
["收获机械","茎秆收集处理机械","秸秆粉碎还田机","1.5-2m秸秆粉碎还田机","河北圣和农业机械有限公司","秸秆切碎还田机","1JQ-150L","作业幅宽:1.5m;","作业幅宽：1.50m；结构形式：侧边皮带传动；配套动力：37～55kW；结构质量：500kg；外形尺寸（长×宽×高）：1380×1770×1100mm。","1600","T202014140012","2025-03-03","7600.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","茎秆收集处理机械","秸秆粉碎还田机","1.5-2m秸秆粉碎还田机","普劳恩德河北农业机械有限公司","秸秆粉碎还田机","1JH-165","作业幅宽:1.65m;","作业幅宽：1.65m；结构形式：侧边皮带传动；配套动力：44.1～88.2kW；结构质量：613kg；外形尺寸（长×宽×高）：1530×1980×1050mm。","1600","T202014140013","2025-03-03","8650.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","茎秆收集处理机械","秸秆粉碎还田机","1.5-2m秸秆粉碎还田机","普劳恩德河北农业机械有限公司","秸秆粉碎还田机","1JH-150","作业幅宽:1.5m;","作业幅宽：1.5m；结构形式：侧边皮带传动；配套动力：44.1～58.8kW；结构质量：560kg；外形尺寸（长×宽×高）：1530×1830×1050mm。","1600","T202014140014","2025-03-03","8450.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","茎秆收集处理机械","秸秆粉碎还田机","1.5-2m秸秆粉碎还田机","江苏神农农业装备有限公司","秸秆粉碎还田机","1JH-180","作业幅宽:1.8m;","幅宽：1.8m,传动方式：皮带传动","1600","部20160250","2020-12-31","8200.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","茎秆收集处理机械","秸秆粉碎还田机","1.5-2m秸秆粉碎还田机","山东华运农机设备有限公司","秸秆粉碎还田机","1JH-165","作业幅宽:1.65m;","结构型式：后悬挂式；配套拖拉机标定功率：45~66KW；外形尺寸（长x宽x高）：1390X2074X1074mm；结构质量：750kg；理论作业速度：3.3~5.5km/h；幅宽：165cm；与拖拉机联接方式：三点悬挂；刀片型式：两片弯刀+一片直刀。","1600","t201900030309","2024-12-30","9000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。产品铭牌未铆接，无法确认为整机铭牌。","","","","",""]
["收获机械","茎秆收集处理机械","秸秆粉碎还田机","1.5-2m秸秆粉碎还田机","石家庄茂丰农业机械制造有限公司","秸秆切碎还田机","4JQ-180","作业幅宽:1.8m;","外形尺寸（mm)：1250*2070*1020 结构质量：436kg  工作宽幅：1.8m  配套动力（kw）：58.8-73.5","1600","冀2016T—248","2020-12-31","5000.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","茎秆收集处理机械","秸秆粉碎还田机","2-2.5m秸秆粉碎还田机","汝南县源信机械制造有限公司","秸秆粉碎还田机","4JH-230A","作业幅宽:230m;","作业幅宽:2.3M;结构型式:悬挂式;配套动力:80.9~118KW","1800","T202000410085","2025-03-31","11000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。产品铭牌未用铆钉铆，无法确认为整机铭牌。","","","","",""]
["收获机械","茎秆收集处理机械","秸秆粉碎还田机","2-2.5m秸秆粉碎还田机","江苏神农农业装备有限公司","秸秆粉碎还田机","1JH-200","作业幅宽:2m;","幅宽，传动方式：皮带传动","1800","部20160251","2020-12-31","8500.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","茎秆收集处理机械","秸秆粉碎还田机","2-2.5m秸秆粉碎还田机","河北圣和农业机械有限公司","秸秆切碎还田机","1JQ-230","作业幅宽:2.3m;","作业幅宽：2.30m；结构形式：侧边皮带传动；配套动力：88.2～110.2kW；结构质量：793kg；外形尺寸（长×宽×高）：1300×2550×1140mm。","1800","T202014140010","2025-03-03","8900.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","茎秆收集处理机械","秸秆粉碎还田机","2-2.5m秸秆粉碎还田机","河北圣和农业机械有限公司","秸秆切碎还田机","1JQ-215","作业幅宽:2.15m;","作业幅宽：2.15m；结构形式：侧边皮带传动；配套动力：73.5～95.5kW；结构质量：765kg；外形尺寸（长×宽×高）：1300×2400×1140mm。","1800","T202014140010","2025-03-03","8600.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","茎秆收集处理机械","秸秆粉碎还田机","2-2.5m秸秆粉碎还田机","河北圣和农业机械有限公司","秸秆切碎还田机","1JQ-215L","作业幅宽:2.15m;","作业幅宽：2.15m；结构形式：侧边皮带传动；配套动力：73.5～95.5kW；结构质量：650kg；外形尺寸（长×宽×高）：1380×2420×1100mm。","1800","T202014140011","2025-03-03","9100.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","茎秆收集处理机械","秸秆粉碎还田机","2-2.5m秸秆粉碎还田机","石家庄茂丰农业机械制造有限公司","秸秆切碎还田机","4JQ-200","作业幅宽:2m;","外形尺寸（mm)：1250*2450*1020 结构质量：480kg 工作宽幅：2.0m  配套动力（kw）：73.5-88.2","1800","冀2016T—247","2020-12-31","5400.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","茎秆收集处理机械","秸秆粉碎还田机","2-2.5m秸秆粉碎还田机","郓城县工力有限公司","双轴式秸秆粉碎还田机","4JGH-220（A）","作业幅宽:2.2m;","配套动力≧90kW、外形尺寸：2250×2430×980、作业幅宽220cm、粉碎机构总安装刀数：粉碎138把、灭茬54把、刀片型式：L型、","1800","鄂2018066","2022-12-31","18000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求","","","","",""]
["收获机械","茎秆收集处理机械","秸秆粉碎还田机","2.5m及以上秸秆粉碎还田机","河北圣和农业机械有限公司","秸秆切碎还田机","1JQ-280S","作业幅宽:2.8m;","作业幅宽：2.80m；结构形式：侧边皮带传动；配套动力：154.4～176.47kW；刀轴数量：2根；外形尺寸（长×宽×高）：2182×3273×1282mm。","2200","T202014140009","2025-03-03","30000.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","茎秆收集处理机械","秸秆粉碎还田机","2.5m及以上秸秆粉碎还田机","河北圣和农业机械有限公司","秸秆切碎还田机","1JQ-250","作业幅宽:2.5m;","作业幅宽：2.50m；结构形式：侧边皮带传动；配套动力：108.2～130.2kW；结构质量：821kg；外形尺寸（长×宽×高）：1300×2750×1140mm。","2200","T202014140010","2025-03-03","10200.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","茎秆收集处理机械","秸秆粉碎还田机","2.5m及以上秸秆粉碎还田机","德州市华北农机装备有限公司","秸秆粉碎还田机","1JH-265","作业幅宽:2.65m;","工作幅宽（cm）：265.配套动力范围（kW）：≥95.配套动力输出轴转速（r/min）:760、1000.与配套拖拉机联接方式：三点悬挂式.工作状态外形尺寸（长×宽×高）（mm）：1500×3110×1280.作业小时生产率（h㎡/h）：0.9～1.2.作业速度（km/h）：≥3.3.刀轴总成传动方式：双侧边皮带传动.刀轴数量（根）：1..刀轴设计转速（r/min）：≥2160.刀轴最大回转半径（mm）：300.刀片型式：甩刀式（弯刀+直刀+弯刀）.刀片总安装数量（把）：120（40组）.","2200","T201900370870","2024-12-30","16300.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获机械","茎秆收集处理机械","秸秆粉碎还田机","2.5m及以上秸秆粉碎还田机","德州市华北农机装备有限公司","秸秆粉碎还田机","1JH-400","作业幅宽:4m;","工作幅宽（cm）：400.配套动力范围（kW）：≥147. 配套动力输出轴转速（r/min）:540、760、830、1000.与配套拖拉机联接方式：三点悬挂式.工作状态外形尺寸（长×宽×高）（mm）：1500×4470×1290.作业小时生产率（h㎡/h）：≥0.8.作业速度（km/h）：≥2.0.刀轴总成传动方式：双侧边皮带传动.刀轴数量（根）：1. 刀轴设计转速（r/min）：≥2000.刀轴最大回转半径（mm）：300.刀片型式：甩刀式（弯刀+直刀+弯刀）.刀片总安装数量（把）：204（68组）.","2200","T201900370871","2024-12-30","34800.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。企业承诺书不符合要求。","","","","",""]
["收获后处理机械","脱粒机械","玉米脱粒机","生产率10t/h及以上玉米脱粒机","昆明佳亿农业机械有限公司","玉米脱粒机","5TY-620-125","生产率:10t/h;","结构型式\t/\t双滚筒\n外形尺寸（长X宽X高）\tmm\t1220X530X820\n配套动力型式\t/\t单项电机\n配套动力功率\tkW\t3\n配套动力转速\tr/min\t2800\n喂入方式\t/\t人工喂入\n滚筒数量\t个\t2\n主滚筒结构型式\t/\t螺旋杆式\n主滚筒工作直径\tmm\t125\n主滚筒工作长度\tmm\t620\n主滚筒工作转速\tr/min\t1540","2400","T20205353078","2025-06-04","8200.00","","非通用类","云南省","评阅不通过","初评员：不通过","专家：产品铭牌机体颜色与机具图片颜色不符。","","","","",""]
["收获后处理机械","脱粒机械","玉米脱粒机","生产率10t/h及以上玉米脱粒机","龙江景西机械制造有限公司","玉米脱粒机","5TY-95X2A","生产率:10-t/h;","尺寸:5060X2700X6100(作业)6950X2700X3390(行走)配套动力:≥35KW生产率:≥20T-28T/H,配套动力:≥35KW生产率:≥12T-25T/H","2400","黑2017011","2021-12-31","36000.00","","非通用类","黑龙江","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["收获后处理机械","脱粒机械","玉米脱粒机","生产率10t/h及以上玉米脱粒机","云南长威机械制造有限公司","玉米脱粒机","5TY-625-120","生产率:10t/h;","全喂入简易式，有分离清选，尺寸1230*540*800，配套动力3.0，喂入方式人工，滚筒类纹杆式，直径120mm,长度625mm，转速2800mm\t每小时≥10吨","2400","T20205353118","2025-06-16","8000.00","","非通用类","云南省","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["收获后处理机械","脱粒机械","玉米脱粒机","生产率10t/h及以上玉米脱粒机","云南长威机械制造有限公司","玉米脱粒机","5TY-560-95D","生产率:10t/h;","全喂入简易式，有分离清选，尺寸1050*770*700，配套动力4.0，喂入方式人工，滚筒类纹杆式，直径95mm,长度560mm，转速1710mm\t每小时≥10吨","2400","T20205353116","2025-06-16","8000.00","","非通用类","云南省","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["收获后处理机械","脱粒机械","花生摘果机","花生摘果机,配套动力7-11kW","正阳县豫丰机械有限公司","花生摘果机","5HZ-690","配套动力:11kW;","整机质量170kg，整机外形尺寸：1470*1200*1570mm,配套动力11kW，喂入方式：人工喂入，摘果滚筒形式：刀齿式，摘果滚筒尺寸440*690mm,凹版型式：栅格式，凹板尺寸：720*720mm,风扇型式：叶片式","1300","T202041410073","2025-06-29","4400.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：营业执照、承诺书过期；产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["收获后处理机械","脱粒机械","花生摘果机","花生摘果机,配套动力7-11kW","正阳县富田农机设备有限公司","花生摘果机","5HZ-690","配套动力:11kW;","整机质量170kg，整机外形尺寸：1470*1200*1570mm,配套动力11kW，喂入方式：人工喂入，摘果滚筒形式：刀齿式，摘果滚筒尺寸440*690mm,凹版型式：栅格式，凹板尺寸：720*720mm,风扇型式：叶片式","1300","T202041410074","2025-06-29","4400.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["收获后处理机械","脱粒机械","花生摘果机","花生摘果机,配套动力11-15kW","宁津县奥华农业机械有限公司","花生摘果机","5HZ-2070","配套动力:11kW;","结构型式：全喂入式，外型尺寸（mm）：5800×2300×2400，整机质量(kg)：810kg，配套动力：11kw，喂入方式：人工喂入+输送带式，滚筒主滚筒型式：螺旋杆式，滚筒尺寸（mm）：720*2070，凹版型式：栅格式，分离、清选型式：风吸+筛选式。","1400","T201937370072","2024-10-24","12800.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量4-10t循环式谷物烘干机","合肥麦稻之星机械有限公司","批式循环谷物干燥机","5HGM-4","处理型式:循环式 ;批处理量:4t;","结构形式：循环式；批处理量：4T；干燥机机体外形尺寸（长×宽×高）：2086*1886*4540mm（不含提升机、扶梯、围栏等）；电机总功率：7.55kW；整机质量：1490kg；加热方式：间接加热；装机容量：10.34m³；安全装置:温控装置、故障报警装置、满粮报警装置、电气过载保护装置、漏电保护装置","14700","2018TJ340","2022-12-31","75000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量4-10t循环式谷物烘干机","浙江如雷实业有限公司","批式循环谷物干燥机","5HRL-6.0","处理型式:循环式 ;批处理量:6.0t;","1.结构形式/批次循环；2.处理量t/批6；3.外形尺寸mm3920X1970X5510；4.整机质量kg1620；5.装机总容量KW6.963；6.燃料种类/0#柴油","14700","部20170033","2021-12-31","80000.00","","通用类","浙江省","评阅不通过","初评员：不通过","专家：无铆钉，无法确认为整机铭牌。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量10-20t循环式谷物烘干机","浙江如雷实业有限公司","批式循环谷物干燥机","5HRL-12.5","处理型式:循环式 ;批处理量:12.5t;","1.结构形式/批式循环式；2.处理量t/批12.5；3.外形尺寸mm3920X1970X8510；4.整机质量kg2150；5.装机总容量KW7.363；6.燃料种类/0#柴油","29500","部20170034","2021-12-31","120000.00","","通用类","浙江省","评阅不通过","初评员：不通过","专家：无铆钉，无法确认为整机铭牌。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量10-20t循环式谷物烘干机","合肥麦稻之星机械有限公司","批式循环谷物干燥机","5HGM-10","处理型式:循环式 ;批处理量:10t;","10T循环式 （下本体 干燥部 储留部 提升机  风机  水分仪 控制柜）结构形式：固定式；处理方式：批式循环；批处理量：10T；外形尺寸（长×宽×高）：4750*2472*8460mm；；电机总功率：7.55kW；整机质量：2150kg；加热方式：间接加热；安全装置:温控装置、故障报警装置、满粮报警装置、电气过载保护装置、漏电保护装置;箱体内尺寸（长×宽×高）：2086*1886*6030MM","29500","2017TJ393","2021-12-31","100000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量10-20t循环式谷物烘干机","合肥麦稻之星机械有限公司","批式循环谷物干燥机","5HGM-12","处理型式:循环式 ;批处理量:12t;","12T 循环式 （下本体 干燥部 储留部 提升机  风机  水分仪 控制柜 ）结构形式：固定式；批式循环；批处理量：12T；外形尺寸（长×宽×高）：4750×2472×9460mm；热源方式：燃烧机；燃料：柴油；电机总功率：7.55 KW；整机质量：2370kg；加热方式：间接加热；安全装置:温控装置、故障报警装置、满粮报警装置、电气过载保护装置、漏电保护装置;箱体内尺寸（长×宽×高）：2086*1886*7030MM","29500","2017TJ394","2021-12-31","105000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量10-20t循环式谷物烘干机","合肥麦稻之星机械有限公司","批式循环谷物干燥机","5HGM-15","处理型式:循环式 ;批处理量:15t;","15T 循环式 （下本体 干燥部 储留部 提升机  风机  水分仪 控制柜）结构形式：批式循环；批处理量：15T；外形尺寸（长×宽×高）：4750×2672×10662mm；热源方式：燃烧机/热风炉；燃料：柴油/无烟煤、柴、秸秆、稻壳；电机总功率：7.55KW；整机质量：2570kg；加热方式：间接加热；安全装置:温控装置、故障报警装置、满粮报警装置、电气过载保护装置、漏电保护装置;箱体内尺寸（长×宽×高）：2086*2086*8232MM","29500","2017TJ395","2021-12-31","115000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量10-20t循环式谷物烘干机","安徽森米诺农业科技有限公司","批式循环谷物干燥机","5HXH-15B","处理型式:循环式 ;批处理量:15t;","型号名称：5HXH-15B型批式循环谷物干燥机；结构形式：循环式；干燥方式：间接加热;干燥机机体外形尺寸（长*宽*高）mm：2082*1855*9746；干燥段数量/每段高度（个/mm）：1/1220；缓苏段数量/每段高度（个/mm）：1/7320；热风机数量：1个，型号：4-72，电机功率kw：5.5；排粮电机功率kw：0.2","29500","2019TJ370","2023-12-31","108000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量10-20t循环式谷物烘干机","山东瑞良烘干机械科技有限公司","批式循环谷物干燥机","5HRS-16","处理型式:循环式 ;批处理量:16t;","结构型式：循环式；外形尺寸（mm）：3270X3380X11460；处理方式：批次式循环式；循环批处理量：≥16t（稻谷）；电机总功率：9.75kw","29500","GZNJ/TJ 2018-224","2023-12-31","135000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量10-20t循环式谷物烘干机","全椒金竹机械制造有限公司","热风吸入式谷物干燥机","5HX-15","处理型式:循环式 ;批处理量:15t;","结构型式:循环式；批处理量(t):15；干燥方式：间接加热；电机总功率(KW):7.9","29500","2019TJ564","2024-12-23","105000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：营业执照过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量10-20t循环式谷物烘干机","全椒金竹机械制造有限公司","热风压入式谷物干燥机","5HY-15","处理型式:循环式 ;批处理量:15t;","结构型式:循环式；批处理量(t):15；干燥方式：间接加热；电机总功率(KW):7.9","29500","2019TJ565","2024-12-23","120000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：营业执照过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量20-30t循环式谷物烘干机","安徽森米诺农业科技有限公司","批式循环谷物干燥机","5HXH-20B","处理型式:循环式 ;批处理量:20t;","型号名称：5HXH-20B型批式循环谷物干燥机；结构形式：循环式；干燥方式：间接加热;干燥机机体外形尺寸（长*宽*高）mm：2275*2275*9955；干燥段数量/每段高度（个/mm）：1/1240；缓苏段数量/每段高度（个/mm）：1/7320；热风机数量：1个，型号：4-72，电机功率kw：7.5；排粮电机功率kw：0.4","34600","2019TJ371","2023-12-31","148000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量20-30t循环式谷物烘干机","安徽森米诺农业科技有限公司","批式循环谷物干燥机","5HXH-20C","处理型式:循环式 ;批处理量:20t;","型号名称：5HXH-20C型批式循环谷物干燥机；结构形式：循环式；干燥方式：间接加热;干燥机机体外形尺寸（长*宽*高）mm：2279*2279*11704；干燥段数量/每段高度（个/mm）：1/1240；缓苏段数量/每段高度（个/mm）：1/7320；热风机数量：1个，型号：4-72，电机功率kw：5.5；排粮电机功率kw：0.4","34600","2019TJ246","2023-12-31","148000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量20-30t循环式谷物烘干机","安徽森米诺农业科技有限公司","批式循环谷物干燥机","5HXH-22C","处理型式:循环式 ;批处理量:22t;","型号名称：5HXH-22C型批式循环谷物干燥机；结构形式：循环式；干燥方式：间接加热;干燥机机体外形尺寸（长*宽*高）mm：2779*2279*11297；干燥段数量/每段高度（个/mm）：1/1240；缓苏段数量/每段高度（个/mm）：1/6710；热风机数量：2个，型号：CRF/L7S-4，电机功率kw：3.0；排粮电机功率kw：0.4","34600","2019TJ247","2023-12-31","158000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量20-30t循环式谷物烘干机","合肥麦稻之星机械有限公司","批式循环谷物干燥机","5HGM-20D","处理型式:循环式 ;批处理量:20t;","20D 结构形式：循环式；批处理量：20T；干燥机机体外形尺寸（长×宽×高）：2086*2586*10250mm（不含提升机、扶梯、围栏等）；电机总功率：11.1kW；整机质量：4050kg；加热方式：间接加热；装机容量：40.38m³；安全装置:温控装置、故障报警装置、满粮报警装置、电气过载保护装置、漏电保护装置","34600","2018TJ341","2022-12-31","145000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量20-30t循环式谷物烘干机","合肥麦稻之星机械有限公司","批式循环谷物干燥机","5HGM-20","处理型式:循环式 ;批处理量:20t;","20T 循环式 （下本体 干燥部 储留部 提升机  风机  水分仪 控制柜）结构形式：批式循环；批处理量：20T；外形尺寸（长×宽×高）：5650*3199*10994mm；整机质量：5550kg；电机总功率：11.62KW；加热方式：间接加热；安全装置:温控装置、故障报警装置、满粮报警装置、电气过载保护装置、漏电保护装置;箱体内尺寸（长×宽×高）：2384*2584*7232MM","34600","2017TJ396","2021-12-31","165000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量20-30t循环式谷物烘干机","合肥麦稻之星机械有限公司","批式循环谷物干燥机","5HGM-25","处理型式:循环式 ;批处理量:25t;","25T:循环式 （下本体 干燥部 储留部 提升机  风机  水分仪 控制柜）结构形式：固定式；处理方式：批式循环；批处理量：25T；外形尺寸（长×宽×高）：5650×3199×12694mm；；电机总功率：11.62kW；整机质量：5850kg；加热方式：间接加热；安全装置:自动水分仪、自动点火、自动停机、温控装置、故障报警装置、满粮报警装置、电气过载保护装置、漏电保护装置;箱体内尺寸：2300*2500*10330mm","34600","2016TJ571","2020-12-31","180000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量20-30t循环式谷物烘干机","浙江如雷实业有限公司","批式循环谷物干燥机","5HRL-20.0","处理型式:循环式 ;批处理量:20.0t;","1.结构形式/批式循环式；2.处理量t/批20；3.外形尺寸mm3920X2370X11190；4.整机质量kg2850；5.燃料种类/0#柴油；6.燃料消耗量L/h12；7.点火方式/自动点火；8.电机总功率KW10.36","34600","2016TJ203","2020-12-31","200000.00","","通用类","浙江省","评阅不通过","初评员：不通过","专家：无铆钉，无法确认为整机铭牌。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量20-30t循环式谷物烘干机","滁州奥岚格机械有限公司","批式循环谷物干燥机","5H-20H","处理型式:循环式 ;批处理量:20t;","干燥机机体外形尺寸(长×宽×高):2480×2250×9625mm,批次处理量:20t,电机总功率:10.25kw,干燥速率：≥0.5%/h，装机容量：36.19m³，干燥方式：间接加热,结构形式：循环式","34600","2017TJ591","2021-12-31","130000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量20-30t循环式谷物烘干机","滁州奥岚格机械有限公司","批式循环谷物干燥机","5H-25","处理型式:循环式 ;批处理量:25t;","干燥机机体外形尺寸(长×宽×高):2480×2250×11140mm,批次处理量:25t，电机总功率:10.25kw,干燥速率：≥0.5%/h，装机容量：44.87m³,干燥方式：间接加热,结构形式：循环式","34600","2017TJ592","2021-12-31","130000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量20-30t循环式谷物烘干机","滁州奥岚格机械有限公司","批式循环谷物干燥机","5H-25H","处理型式:循环式 ;批处理量:25t;","干燥机机体外形尺寸(长×宽×高):2480×2250×11260mm,批次处理量:25t，电机总功率:10.25kw,干燥速率：≥0.5%/h，装机容量：44.86m³,干燥方式：间接加热,结构形式：循环式","34600","2017TJ593","2021-12-31","140000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量20-30t循环式谷物烘干机","全椒金竹机械制造有限公司","热风压入式谷物干燥机","5HY-20","处理型式:循环式 ;批处理量:20t;","结构型式:循环式；批处理量(t):20；干燥方式：间接加热；电机总功率(KW):14","34600","2019TJ567","2024-12-23","160000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：营业执照过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量20-30t循环式谷物烘干机","全椒金竹机械制造有限公司","热风吸入式谷物干燥机","5HX-20","处理型式:循环式 ;批处理量:20t;","结构型式:循环式；批处理量(t):20；干燥方式：间接加热；电机总功率(KW):8.7","34600","2019TJ566","2024-12-23","135000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：营业执照过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量20-30t循环式谷物烘干机","合肥易祥农业机械智能装备有限公司","批式循环谷物干燥机","5HYX-22A","处理型式:循环式 ;批处理量:22t;","干燥机机体外形尺寸（mm)：2700X2350X9640、批次处理量(t)：22、结构型式:循环式、装机容量（m3)：41.17、热风机电机功率(KW）：5.5、排粮电机功率（KW）：0.4、提升机电机功率（KW）：3、提升机生产率（t/h)：30、干燥能力( t.%/h ) : ≥16","34600","2017TJ665","2021-12-31","132000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：不通过","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量20-30t循环式谷物烘干机","合肥易祥农业机械智能装备有限公司","批式循环谷物干燥机","5HYX-22B","处理型式:循环式 ;批处理量:22t;","干燥机机体外形尺寸（mm)：2700X2350X10140、批次处理量(t)：22、结构型式:循环式、装机容量（m3)：42.23、热风机电机功率(KW）：5.5、排粮电机功率（KW）：0.4、提升机电机功率（KW）：3、提升机生产率（t/h)：30、干燥能力( t.%/h ) : ≥16","34600","2017TJ666","2021-12-31","135000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量30t及以上循环式谷物烘干机","滁州奥岚格机械有限公司","批式循环谷物干燥机","5H-35","处理型式:循环式 ;批处理量:35t;","干燥机机体外形尺寸(长×宽×高):3260×2540×10880mm,批次处理量:35t，电机总功率:15.25kw,干燥速率：≥0.5%/h，装机容量：62.85m³,干燥方式：间接加热,结构形式：循环式","62800","2017TJ627","2021-12-31","255000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量30t及以上循环式谷物烘干机","滁州奥岚格机械有限公司","批式循环谷物干燥机","5H-35H","处理型式:循环式 ;批处理量:35t;","干燥机机体外形尺寸(长×宽×高):3260×2540×10960mm,批次处理量:35t，电机总功率:15.25kw,干燥速率：≥0.5%/h，装机容量：62.85m³,干燥方式：间接加热,结构形式：循环式","62800","2017TJ594","2021-12-31","270000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量30t及以上循环式谷物烘干机","江苏天禹农业机械有限公司","通用型谷物干燥机","5HXG-320","处理型式:循环式 ;批处理量:32t;","1.结构型式：循环式； 2.干燥方式；直接加热；3.烘干机机体外形尺寸（长×宽×高）：2272×2902×12136mm ；4.干燥段高度：1221（数量一段）mm；5.缓苏段高度：9150 （数量1段）mm；6.热风机型号名称：CRF/7.5S-4A斜流风机；7.热风机数量:2；8.热风机电机功率:5.5x2kW；9.燃烧器型号名称：TBL45P/RL34MZ燃烧器；10.燃烧器燃料种类：轻柴油；11.燃烧器喷火头数量：2个；12.排粮电机功率:0.2kw；13.烘干机电机总功率：16.65kW。","62800","T202032320030","2025-03-30","370000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量30t及以上循环式谷物烘干机","合肥麦稻之星机械有限公司","批式循环谷物干燥机","5HGM-30D","处理型式:循环式 ;批处理量:30t;","30d:循环式 （下本体 干燥部 储留部 提升机  风机  水分仪 控制柜）结构形式：固定式；处理方式：批式循环；批处理量：30T；外形尺寸（长×宽×高）：5650×3199×14194mm；；电机总功率：15.12kW；整机质量：6150kg；加热方式：间接加热；安全装置:自动水分仪、自动点火、自动停机、温控装置、故障报警装置、满粮报警装置、电气过载保护装置、漏电保护装置; 箱体内尺寸：2300*2500*11830mm","62800","2016TJ573","2020-12-31","240000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量30t及以上循环式谷物烘干机","合肥麦稻之星机械有限公司","批式循环谷物干燥机","5HGM-30H","处理型式:循环式 ;批处理量:30t;","30h:循环式 （下本体 干燥部 储留部 提升机  风机  水分仪 控制柜）结构形式：固定式；处理方式：批式循环；批处理量：30T；外形尺寸（长×宽×高）7350×3436×14844mm；；电机总功率：15.12kW；整机质量：6450kg；加热方式：间接加热；安全装置:自动水分仪、自动点火、自动停机、温控装置、故障报警装置、满粮报警装置、电气过载保护装置、漏电保护装置; 箱体内尺寸：2300*2500*12480mm","62800","2016TJ572","2020-12-31","260000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量30t及以上循环式谷物烘干机","合肥麦稻之星机械有限公司","批式循环谷物干燥机","5HGM-50","处理型式:循环式 ;批处理量:50t;","50T  循环式 （下本体 干燥部 储留部 提升机  风机  水分仪 控制柜 满量报警器）结构形式：批式循环；批处理量：50T；外形尺寸（长×宽×高）：7653×4724×18918mm；加热方式：间接加热；热源方式：燃烧机/热风炉；燃料：柴油/无烟煤、柴、秸秆、稻壳；电机总功率：28.25KW；整机质量：13890kg;箱体内尺寸：3064*3128*12734mm","62800","2017TJ397","2021-12-31","450000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量30t及以上循环式谷物烘干机","合肥麦稻之星机械有限公司","批式循环谷物干燥机","5HGM-60","处理型式:循环式 ;批处理量:60t;","60t: 循环式 （下本体 干燥部 储留部 提升机  风机  水分仪 控制柜 满量报警器）结构形式：固定式；处理方式：批式循环；批处理量：60T；外形尺寸（长×宽×高）：7653×4724×20958mm；；电机总功率：28.25kW；整机质量：14190kg；加热方式：间接加热；安全装置:自动水分仪、自动点火、自动停机、温控装置、故障报警装置、满粮报警装置、电气过载保护装置、漏电保护装置: 箱体内尺寸：2984*3048*15412mm","62800","2016TJ574","2020-12-31","550000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量30t及以上循环式谷物烘干机","合肥麦稻之星机械有限公司","批式循环谷物干燥机","5HGM-30","处理型式:循环式 ;批处理量:30t;","30 结构形式：循环式；批处理量：30T；干燥机机体外形尺寸（长×宽×高）：2386*3426*9530mm（不含提升机、扶梯、围栏等）；电机总功率：20.15kW；整机质量：6350kg；加热方式：间接加热；装机容量：56.67m³；安全装置:温控装置、故障报警装置、满粮报警装置、电气过载保护装置、漏电保护装置","62800","2018TJ342","2022-12-31","280000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量30t及以上循环式谷物烘干机","合肥麦稻之星机械有限公司","批式循环谷物干燥机","5HGM-35","处理型式:循环式 ;批处理量:35t;","结构形式：循环式；批处理量：35T；干燥机机体外形尺寸（长×宽×高）：3064*3128*9540mm（不含提升机、扶梯、围栏等）；电机总功率：17.8kW；整机质量：11500kg；加热方式：间接加热；装机容量：63.87m³；安全装置:温控装置、故障报警装置、满粮报警装置、电气过载保护装置、漏电保护装置","62800","2018TJ343","2022-12-31","280000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量30t及以上循环式谷物烘干机","滁州奥岚格机械有限公司","批式循环谷物干燥机","5H-30HA","处理型式:循环式 ;批处理量:30t;","干燥机机体外形尺寸(长×宽×高):3270×2550×11708mm,批次处理量:30t，电机总功率:16.3kw,干燥速率：≥15t.%/h，装机容量：57.2m³,干燥方式：间接加热,结构形式：循环式","62800","2019TJ477","2023-12-31","240000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量30t及以上循环式谷物烘干机","安徽森米诺农业科技有限公司","批式循环谷物干燥机","5HXH-30D","处理型式:循环式 ;批处理量:30t;","型号名称：5HXH-30D型批式循环谷物干燥机；结构形式：循环式；干燥方式：间接加热;干燥机机体外形尺寸（长*宽*高）mm：(2280*2974*11149)+(1697*1390*600)；干燥段数量/每段高度（个/mm）：1/1220；缓苏段数量/每段高度（个/mm）：1/8530；热风机数量：2个，型号：4-72，电机功率kw：5.5*2；排粮电机功率kw：0.75","62800","2019TJ248","2023-12-31","268000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量30t及以上循环式谷物烘干机","安徽森米诺农业科技有限公司","批式循环谷物干燥机","5HXH-30E","处理型式:循环式 ;批处理量:30t;","型号名称：5HXH-30E型批式循环谷物干燥机；结构形式：循环式；干燥方式：间接加热;干燥机机体外形尺寸（长*宽*高）mm：(2280*2974*12556)+(1697*1390*600)；干燥段数量/每段高度（个/mm）：1/1220；缓苏段数量/每段高度（个/mm）：1/8530；热风机数量：2个，型号：4-72，电机功率kw：5.5*2；排粮电机功率kw：0.75","62800","2019TJ249","2023-12-31","288000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量30t及以上循环式谷物烘干机","安徽森米诺农业科技有限公司","批式循环谷物干燥机","5HXH-30C","处理型式:循环式 ;批处理量:30t;","型号名称：5HXH-30C型批式循环谷物干燥机；结构形式：循环式；干燥方式：间接加热;干燥机机体外形尺寸（长*宽*高）mm：2282*3581*11926；干燥段数量/每段高度（个/mm）：1/1500；缓苏段数量/每段高度（个/mm）：1/7320；热风机数量：2个，型号：4-72，电机功率kw：5.5*2；排粮电机功率kw：0.75","62800","2019tj372","2023-12-31","298000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量30t及以上循环式谷物烘干机","上海三久机械有限公司","粗糠炉干燥机","SB-130-PRO-300HB","处理型式:循环式 ;批处理量:30t;","外形尺寸固定尺寸(长×宽×高)\tmm\t4999×3786×11629；干燥机功率：16.75kw，批次处理量30吨，热风炉型号名称：SB-130生质能热风炉，热风炉尺寸：4256×6645×9612，热风炉配套动力：16.75kw；","62800","部20170211","2021-12-31","1380000.00","","通用类","上海市","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量30t及以上循环式谷物烘干机","安徽正阳机械科技有限公司","谷物干燥机","5H-30B","处理型式:循环式 ;批处理量:30t;","批次处理量：30t;循环式;干燥方式：间接加热；干燥机机体外形尺寸：2700*3490*11360mm；干燥段数量1个；干燥段高度：2010mm；缓苏段数量：1个，缓苏段高度6000mm。电机总功率：16.2kw/H.","62800","2019TJ353","2023-12-31","230000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量30t及以上循环式谷物烘干机","合肥易祥农业机械智能装备有限公司","批式循环谷物干燥机","5HYX-32A","处理型式:循环式 ;批处理量:32t;","干燥机机体外形尺寸（mm)：3670X2570X11812、批次处理量(t)：32、结构型式:循环式、装机容量（m3)：58.14、热风机电机功率(KW）：5.5X2、排粮电机功率（KW）：0.4、提升机电机功率（KW）：4、提升机生产率（t/h)：40、干燥能力( t.%/h ) : ≥ 20","62800","2018TJ500","2022-12-31","320000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量30t及以上循环式谷物烘干机","全椒金竹机械制造有限公司","热风压入式谷物干燥机","5HY-30B","处理型式:循环式 ;批处理量:30t;","结构型式:循环式；批处理量(t):30；干燥方式：间接加热；电机总功率(KW):18.5","62800","2019TJ373","2023-12-31","240000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：营业执照过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量30t及以上循环式谷物烘干机","全椒金竹机械制造有限公司","热风压入式谷物干燥机","5HY-30A","处理型式:循环式 ;批处理量:30t;","结构型式:循环式；批处理量(t):30；干燥方式：间接加热；电机总功率(KW):21.4","62800","2019TJ568","2024-12-23","240000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：营业执照过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量30t及以上循环式谷物烘干机","全椒金竹机械制造有限公司","热风压入式谷物干燥机","5HY-50","处理型式:循环式 ;批处理量:50t;","结构型式:循环式；批处理量(t):50；干燥方式：间接加热；电机总功率(KW):30.7","62800","T201900320621","2024-12-30","450000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：营业执照过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量30t及以上循环式谷物烘干机","全椒金竹机械制造有限公司","热风压入式谷物干燥机","5HY-75","处理型式:循环式 ;批处理量:75t;","结构型式:循环式；批处理量(t):75；干燥方式：间接加热；电机总功率(KW):33.5","62800","T201900320622","2024-12-30","600000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：营业执照过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量30t及以上循环式谷物烘干机","山东瑞良烘干机械科技有限公司","批式循环谷物干燥机","5HRX-40","处理型式:循环式 ;批处理量:50t;","结构型式：循环式；外形尺寸（mm）：3600×4100×10800；处理方式：批次式循环式；循环批处理量：≥50t（玉米）；电机总功率：19.1kw","62800","GZNJ/TJ 2019-373","2024-12-29","260000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","批处理量30t及以上循环式谷物烘干机","山东瑞良烘干机械科技有限公司","批式循环谷物干燥机","5HRX-33","处理型式:循环式 ;批处理量:41t;","结构型式：循环式；外形尺寸（mm）：3600×4100×9700；处理方式：批次式循环式；循环批处理量：≥41t（玉米）；电机总功率：19.1kw","62800","GZNJ/TJ 2019-373","2024-12-29","250000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","处理量100t/d及以上连续式谷物烘干机","铁岭精达机械制造有限公司","粮食干燥机","5HT-25(TZH-500)","处理型式:连续式 ;处理量:500t/d;","型号规格:5HT-25(TZH-500)；干燥方式:间接加热；干燥机机体外形尺寸(长×宽×高)mm:7500×6900×25560；处理量t/d:50010%≤降水幅度≤15%6005%≤降水幅度<10%；t/h:20.810%≤降水幅度≤15%25.05%≤降水幅度<10%；降水幅度%:5~15；加热方式:间接换热式；燃料种类:煤；结构型式:连续式；整机质量kg:55000；燃烧机点火方式:人工；燃料消耗量:kg/h:1025；电机总功率kw:381.45.","106900","辽2017041","2021-12-31","1260000.00","","通用类","辽宁省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","处理量100t/d及以上连续式谷物烘干机","铁岭精达机械制造有限公司","粮食干燥机","5HT-10","处理型式:连续式 ;处理量:200t/d;","型号名称\t/\t5HT-10粮食干燥机\n结构型式\t/\t连续式\n干燥方式\t/\t间接加热\n干燥机机体外形尺寸（长×宽×高）\tmm\t3300×3500×17500\n处理量\tt/d\t   200    10%≤降水幅度≤15%\n300    5%≤降水幅度＜10%\n降水幅度，%\t\t5%~15%\n干燥段数量\t个\t2\n缓苏段数量\t个\t1\n冷却段高度\tmm\t2000\n烘干机净容积\tm³\t90\n热风温度范围\t℃\t110℃~140℃\n1号热风机型号名称\t/\t4-72-12C离心通风机\n1号热风机风压\tPa\t1859\n1号热风机流量\tm³/h\t63953\n1号热风机电机功率\tkW\t55\n冷却风机型号名称\t/\t4-72-8C离心通风机\n冷却风机电机功率\tkW\t11\n排粮电机功率\tkW\t1.5\n烘干机电机总功率\tkW\t123.3\n热风炉型号名称/燃料种类\t/\tWRF-Ⅲ4燃煤热风炉/煤\n热风炉热功率（输出热量）\tkJ/h（Kcal/h）\t10032000kJ/h\n2400000Kcal/h\n热风炉引烟风机型号名称\t/\tY5-48-6.3C锅炉引风机\n热风炉引烟风机电机功率\tkW\t22","106900","T201900210147","2024-11-28","550000.00","","通用类","辽宁省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","处理量100t/d及以上连续式谷物烘干机","铁岭精达机械制造有限公司","粮食干燥机","5HT-15","处理型式:连续式 ;处理量:300t/d;","型号名称\t/\t5HT-15粮食干燥机\n结构型式\t/\t连续式\n干燥方式\t/\t间接加热\n干燥机机体外形尺寸（长×宽×高）\tmm\t6400×3500×19870\n处理量\tt/d\t300    10%≤降水幅度≤15%\n560     5%≤降水幅度＜10%\n降水幅度，%\t\t5%~15%\n干燥段数量\t个\t2\n缓苏段数量\t个\t1\n冷却段高度\tmm\t1896\n烘干机净容积\tm³\t167\n热风温度范围\t℃\t110℃~140℃\n1号热风机型号名称\t/\tY4-73No11D通风机\n1号热风机风压\tPa\t2463\n1号热风机流量\tm³/h\t47427\n1号热风机电机功率\tkW\t55\n2号热风机型号名称\t/\tY4-73No10D通风机\n2号热风机风压\tPa\t2011\n2号热风机流量\tm³/h\t39926\n2号热风机电机功率\tkW\t37\n冷却风机型号名称\t/\t4-72No10C通风机\n冷却风机电机功率\tkW\t15\n排粮电机功率\tkW\t1.5\n烘干机电机总功率\tkW\t184.3\n热风炉型号名称/燃料种类\t/\tWRF-Ⅲ6燃煤热风炉/煤\n热风炉热功率（输出热量）\tkJ/h（Kcal/h）\t15048000kJ/h\n3600000Kcal/h\n热风炉引烟风机型号名称\t/\tY5-48No8C通风机\n热风炉引烟风机电机功率\tkW\t30","106900","T201900210148","2024-11-28","720000.00","","通用类","辽宁省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","处理量100t/d及以上连续式谷物烘干机","铁岭精达机械制造有限公司","粮食干燥机","5HT-5","处理型式:连续式 ;处理量:100t/d;","型号名称\t/\t5HT-5粮食干燥机\n结构型式\t/\t连续式\n干燥方式\t/\t间接加热\n干燥机机体外形尺寸（长×宽×高）\tmm\t3300×2500×12265\n处理量\tt/d\t   100    10%≤降水幅度≤15%\n170     5%≤降水幅度＜10%\n降水幅度，%\t\t5%~15%\n干燥段数量\t个\t1\n缓苏段数量\t个\t无\n冷却段高度\tmm\t1800\n烘干机净容积\tm³\t37\n热风温度范围\t℃\t110℃~140℃\n1号热风机型号名称\t/\tY4-73-9C通风机\n1号热风机风压\tPa\t2000\n1号热风机流量\tm³/h\t35000\n1号热风机电机功率\tkW\t30\n冷却风机型号名称\t/\t4-72-6A通风机\n冷却风机电机功率\tkW\t4\n排粮电机功率\tkW\t1.5\n烘干机电机总功率\tkW\t59.8\n热风炉型号名称/燃料种类\t/\tWRF-Ⅲ2燃煤热风炉/煤\n热风炉热功率（输出热量）\tkJ/h（Kcal/h）\t5016000kJ/h\n1200000Kcal/h\n热风炉引烟风机型号名称\t/\tY5-48-5C通风机\n热风炉引烟风机电机功率\tkW\t11","106900","T201900210146","2024-11-28","438000.00","","通用类","辽宁省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","处理量100t/d及以上连续式谷物烘干机","开原金鑫烘干设备有限公司","粮食烘干机","5HS200","处理型式:连续式 ;处理量:200t/d;","结构尺寸:3000×2500×24000(长×宽×高)、结构型式:连续式、日处理量：≥240（5%≤降水幅度＜10%） ≥200（10%≤降水幅度≤15%）、烘干机净容积:105m³、电机总功率:127.45kW、热风机型号:Y4-73№9D、热风炉:RFL-4链带式链条炉排、热风温度：120-140℃、燃料：煤。","106900","T202000210134","2025-07-05","480000.00","","通用类","辽宁省","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","处理量100t/d及以上连续式谷物烘干机","开原金鑫烘干设备有限公司","粮食烘干机","5HS300","处理型式:连续式 ;处理量:300t/d;","结构尺寸:3000×3500×24000(长×宽×高)、结构型式:连续式、日处理量：≥360（5%≤降水幅度＜10%） ≥300（10%≤降水幅度≤15%）、烘干机净容积:147m³、电机总功率:172.95kW、热风机型号:Y4-73№10D、热风炉:RFL-6链带式链条炉排、热风温度：120-140℃、燃料：煤。","106900","T202000210135","2025-07-05","580000.00","","通用类","辽宁省","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","处理量100t/d及以上连续式谷物烘干机","开原金鑫烘干设备有限公司","粮食烘干机","5HGJ150","处理型式:连续式 ;处理量:150t/d;","结构尺寸:2600×2600×18000(长×宽×高)、结构型式:连续式、日处理量：≥180（5%≤降水幅度＜10%） ≥150（10%≤降水幅度≤15%）、烘干机净容积:56m³、电机总功率:87.95kW、热风机型号:Y4-73№9D、热风炉:RFL-3链带式链条炉排、热风温度：120-140℃、燃料：煤。","106900","T202000210132","2025-07-05","380000.00","","通用类","辽宁省","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","处理量100t/d及以上连续式谷物烘干机","开原金鑫烘干设备有限公司","粮食烘干机","5HGJ200","处理型式:连续式 ;处理量:200t/d;","结构尺寸:3000×3000×23500(长×宽×高)、结构型式:连续式、日处理量：≥240（5%≤降水幅1度＜10%） ≥200（10%≤降水幅度≤15%）、烘干机净容积:89m³、电机总功率:131.45kW、热风机型号:Y4-73№9D、热风炉:RFL-4链带式链条炉排、热风温度：120-140℃、燃料：煤。","106900","T202000210133","2025-07-05","480000.00","","通用类","辽宁省","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","处理量100t/d及以上连续式谷物烘干机","铁岭市清河区金锋干燥设备有限公司","粮食干燥机","SNH-5","处理型式:连续式 ;处理量:120t/d;","结构尺寸（㎜）：2000×2500×13200；整机质量（㎏）：12000；结构型式：固定式；处理量（t/h）：5；装机溶积（㎥）：60；电机总功率（kW）：56.2；热风机型号：Y4-68-9C；热风炉型号：RFL2.1-180；燃烧机型式：机烧热风炉；燃烧机点火方式：采用人工方式，点燃秸秆类农作物进而使煤炭燃烧，使机具运行；燃料：秸秆类农作物、煤炭 处理方式：连续式；结构形式：固定式；连续式处理量（t/d)：120","106900","辽2017075","2021-12-31","360000.00","","通用类","辽宁省","评阅不通过","初评员：不通过","专家：产品铭牌铆钉未按要求铆接，铆接不完整，容易脱落。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","处理量100t/d及以上连续式谷物烘干机","铁岭市清河区金锋干燥设备有限公司","粮食干燥机","SNH-7.5","处理型式:连续式 ;处理量:180t/d;","结构尺寸（㎜）：3000×3000×11570；整机质量（㎏）：16000；结构型式：固定式；处理量（t/h）：7.5；装机溶积（㎥）：80；电机总功率（kW）：81.25；热风机型号：G4-73№9D；热风炉型号：RFL2.1-180；燃烧机型式：机烧热风炉；燃烧机点火方式：采用人工方式，点燃秸秆类农作物进而使煤炭燃烧，使机具运行；燃料：秸秆类农作物、煤炭 处理方式：连续式；结构形式：固定式；连续式处理量（t/d)：180","106900","T201900060318","2024-12-30","380000.00","","通用类","辽宁省","评阅不通过","初评员：不通过","专家：产品铭牌铆钉未按要求铆接，铆接不完整，容易脱落。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","处理量100t/d及以上连续式谷物烘干机","铁岭市清河区金锋干燥设备有限公司","粮食干燥机","SNH-10","处理型式:连续式 ;处理量:240t/d;","结构尺寸（mm）：3000×3000×18800；整机质量（kg）：26000；结构型式：固定式；处理量（t/h）：10；装机溶积（㎥）：110；电机总功率（kW）：106.25；热风机型号：G4-73№9D×2台；热风炉型号：RFL2.8-240；燃烧机型式：机烧热风炉；燃烧机点火方式：采用人工方式，点燃秸秆类农作物进而使煤炭燃烧，使机具运行；燃料：秸秆类农作物、煤炭 处理方式：连续式；结构形式：固定式；连续式处理量（t/d)：240","106900","T201900060319","2024-12-30","430000.00","","通用类","辽宁省","评阅不通过","初评员：不通过","专家：产品铭牌铆钉未按要求铆接，铆接不完整，容易脱落。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","处理量100t/d及以上连续式谷物烘干机","铁岭市清河区金锋干燥设备有限公司","粮食干燥机","SNH-15","处理型式:连续式 ;处理量:360t/d;","结构尺寸（mm）：3000×3500×20600；整机质量（kg）：32000；结构型式：固定式；处理量（t/h）：15；装机溶积（㎥）：150；电机总功率（kW）：143.25；热风机型号：Y4-73№10D、Y4-73№09D；热风炉型号：RFL4.2-360；燃烧机型式：机烧热风炉；燃烧机点火方式：采用人工方式，点燃秸秆类农作物进而使煤炭燃烧，使机具运行；燃料：秸秆类农作物、煤炭 处理方式：连续式；结构形式：固定式；连续式处理量（t/d)：360","106900","T201900060320","2024-12-30","630000.00","","通用类","辽宁省","评阅不通过","初评员：不通过","专家：产品铭牌铆钉未按要求铆接，铆接不完整，容易脱落。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","处理量100t/d及以上连续式谷物烘干机","铁岭市清河区金锋干燥设备有限公司","粮食干燥机","SNH-25","处理型式:连续式 ;处理量:600t/d;","结构尺寸（mm）：4000×3500×19580；整机质量（kg）：52000；结构型式：固定式；处理量（t/h）：25；装机溶积（㎥）：260；电机总功率（kW）：237.5；热风机型号：Y4-73№11D、Y4-73№10D、Y4-73№09D；热风炉型号：RFL7-600；燃烧机型式：机烧热风炉；燃烧机点火方式：采用人工方式，点燃秸秆类农作物进而使煤炭燃烧，使机具运行；燃料：秸秆类农作物、煤炭 处理方式：连续式；结构形式：固定式；连续式处理量（t/d)：600","106900","T201900060317","2024-12-30","900000.00","","通用类","辽宁省","评阅不通过","初评员：不通过","专家：产品铭牌铆钉未按要求铆接，铆接不完整，容易脱落。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","处理量100t/d及以上连续式谷物烘干机","开原凯尔烘干设备有限公司","粮食干燥机","5HSH-150","处理型式:连续式 ;处理量:150t/d;","外型尺寸（长×宽×高）mm ：  2600×2000×17800   \n结构型式:连续式（间接加热）\n处理量：150t/d;\n电机总功率：73.8KW\n1号热风机型号：Y4-73№9D  \n2号热风机型号：Y4-73№9D  \n冷却风机型号：4-72-№6C\n燃烧机型式：热风炉\n燃烧机点火方式：人工\n燃料：煤","106900","T20202121010","2025-06-22","350000.00","","通用类","辽宁省","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","处理量100t/d及以上连续式谷物烘干机","开原市鑫昊源粮食烘干设备有限公司","粮食干燥机","5HSHN-200","处理型式:连续式 ;处理量:200t/d;","结构形式：连续式；处理量：200t/d;裝粮容积93立方米。","106900","黑垦鉴2017020","2021-12-31","400000.00","","通用类","辽宁省","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","处理量100t/d及以上连续式谷物烘干机","开原市鑫昊源粮食烘干设备有限公司","粮食干燥机","5HSHN-300","处理型式:连续式 ;处理量:300t/d;","结构形式：连续式；处理量：300t/d;裝粮容积143立方米。","106900","黑垦鉴2017021","2021-12-31","620000.00","","通用类","辽宁省","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["收获后处理机械","干燥机械","谷物烘干机","处理量100t/d及以上连续式谷物烘干机","开原市鑫昊源粮食烘干设备有限公司","粮食干燥机","5HSHN-500","处理型式:连续式 ;处理量:500t/d;","结构形式：连续式；处理量：500t/d;裝粮容积：213立方米。","106900","黑垦鉴2017022","2021-12-31","890000.00","","通用类","辽宁省","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["收获后处理机械","干燥机械","果蔬烘干机","容积5m³以下果蔬烘干机(整体脱水)","厦门春田科技有限公司","热泵果蔬烘干机","5HGKB-0.3CTB","处理型式:整体脱水 ;容积:0.3m³;","烘干方式:整体脱水;\n 加热方式:空气能热泵;\n 温湿控制方式:自动控制; \n结构形式:槽式; \n外形尺寸(长x宽x高)mm:1000×1150×1020 \n热风风机功率(kw):0.22kw; \n排湿风机功率(kw):0.1kw \n有效干燥体积:0.3m³; \n有效干燥面积:无;\n 安全装置:漏电保护开关","1100","T202062620052","2025-06-08","4500.00","","非通用类","福建厦门","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["收获后处理机械","干燥机械","果蔬烘干机","容积5m³以下果蔬烘干机(整体脱水)","厦门春田科技有限公司","热泵果蔬烘干机","5HGKB-0.3CTA","处理型式:整体脱水 ;容积:0.3m³;","烘干方式:整体脱水; \n加热方式:空气能热泵; \n温湿控制方式:自动控制; \n结构形式:槽式;\n 外形尺寸(长x宽x高)mm:910×910×1140 \n热风风机功率(kw):0.22kw; \n电辅热功率(kw):1.2kw; \n有效干燥体积:0.3m³; \n有效干燥面积：无 \n安全装置:漏电保护开关","1100","T202062620053","2025-06-08","3650.00","","非通用类","福建厦门","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["收获后处理机械","干燥机械","果蔬烘干机","容积5m³以下果蔬烘干机(整体脱水)","厦门春田科技有限公司","热泵果蔬烘干机","5HGKB-0.5CTA","处理型式:整体脱水 ;容积:0.5m³;","烘干方式:整体脱水;\n 加热方式:空气能热泵;\n 温湿控制方式:自动控制; \n结构形式:槽式; \n外形尺寸(长x宽x高)mm:1000×1150×1020 \n热风风机功率(kw):0.22kw; \n排湿风机功率(kw):0.1kw \n有效干燥体积:0.5m³; \n有效干燥面积:无;\n 安全装置:漏电保护开关","1100","T202062620051","2025-06-08","4500.00","","非通用类","福建厦门","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["收获后处理机械","干燥机械","果蔬烘干机","容积5m³以下果蔬烘干机(整体脱水)","三明市同硕机械制造有限公司","果蔬烘干机","5HGS-3-RL","处理型式:整体脱水 ;容积:3m³;","1、烘干室容积：3m³，整体脱水；2、外型尺寸(mm):2580×1220×2600；3、干燥室尺寸(mm):830×1060×2150×2个；4、处理量(kg/h):8(萝卜)；5、装机总容量(kw):2.4；6、加热方式:间接；7、燃烧室尺寸(mm):1060×810×2050；8、燃料种类:生物质颗粒；9、排潮口型式:百叶窗。","1100","黑垦鉴2016089","2020-12-31","9800.00","","非通用类","福建省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","果蔬烘干机","容积5m³以下果蔬烘干机(整体脱水)","三明市鸿达智能农业设备有限公司","电能果蔬烘干机","5HGD-1-X","处理型式:整体脱水 ;容积:1m³;","1.烘干室容积:1M3,整体脱水；2.结构形式:箱体式；3.外形尺寸(长×宽×高):1545×900×1915(MM)；4.冷/热循环风机(数量):1个；5.冷/热循环风机(电机功率):0.35KW；6.供热方式(类型):电加热.","1100","GZNJ/TJ 2018-199","2023-12-31","4800.00","","非通用类","福建省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","果蔬烘干机","容积5-15m³果蔬烘干机(整体脱水)","云南万合农机有限公司","果蔬烘干机","5HG-10C","处理型式:整体脱水 ;容积:10m³;","外形尺寸（长*宽*高）：5150*2070*1800mm（不含烟囱、雨棚）；烘干方式（连续式/循环式）：循环式；结构型式（烤槽敞开式/密封箱体式）：烤槽敞开式；烘干室材质（砖混/板房及板房材质）：板房，50mm双面彩钢聚苯乙烯夹芯板；烘干室容积：10m³。","4800","滇2018094","2022-12-31","16800.00","","非通用类","云南省","评阅不通过","初评员：不通过","专家：营业执照过期。","","","","",""]
["收获后处理机械","干燥机械","果蔬烘干机","容积5-15m³果蔬烘干机(整体脱水)","三明市同硕机械制造有限公司","果蔬烘干机","5HGS-6.2-RL","处理型式:整体脱水 ;容积:6.2m³;","1、烘干室容积:6.2m³,整体脱水；2、外型尺寸(长×宽×高mm):3060×1830×2590；3、整机质量(kg):720；4、处理量(kg/批):650(笋)；5、装机总容量(kw):3.2；6、风机数量(台):2；7、供热方式:间接加热；8、燃料种类:煤、生物质；9、控制方式:自动控制。","4800","黑垦鉴2016021","2020-12-31","18000.00","","非通用类","福建省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","果蔬烘干机","容积15m³及以上果蔬烘干机(整体脱水)","安徽欧瑞达电器科技有限公司","果蔬烘干机","ORD5HGS-40RB","处理型式:整体脱水 ;容积:40m³;","此果蔬烘干机的加热主机为空气源热泵 1.加热方式:空气源热泵加热和电加热器辅助加热相结合；2.加热主机的制热量：42kW; 3.烘干方式：热风烘干，整体脱水；4.结构形式：批式（分置式烘干）；5.外形尺寸（长×宽×高）：7300×3500×2800mm; 6.内部尺寸（长×宽×高）：6000×3350×2200mm； 7.风机功率：7kW; 8.配套总功率：22.0kW（不包括辅助电加热）；9.辅助电加热功率：24kW; 10.容积：40m3；11.有限干燥体积：40m3；12.有效干燥面积：190㎡；13.温湿度控制方式：1）根据物料的特性，分阶段设置烘干温度；2）温湿度自动控制；14.热风温度范围≤75℃；15.安全装置：1）热风温度、物料温度、超温报警装置；2）相序保护，过欠电压保护；3）加热主机氟系统高低压保护、排气温度过高保护；4）避雷装置；5）电器系统过载和漏电保护；6）配备灭火器；16.控制系统：1)PLC控制系统，操作界面友好；2）7英寸液晶触摸屏；3）根据物料的特性分阶段设置温湿度；4）可实现多台联机，5）根据客户要求可实现远程监控；17.根据客户所处的环境温度和物料的特性，可配置热回收装置，热回收效率62%；18.节能环保，无任何三废排放; 19.烘干架：1）尺寸（长×宽×高）：1500×950×1900mm; 2)层数：3层；3）层高：138mm。","9300","2019TJ171","2023-12-31","108000.00","","非通用类","安徽省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","果蔬烘干机","容积15m³及以上果蔬烘干机(整体脱水)","滁州奥岚格机械有限公司","果蔬烘干机","5HGS-18","处理型式:整体脱水 ;容积:18m³;","外形尺寸（长×宽×高）：3600×2800×2400mm，风机功率1.1kw，配套功率：9.0kw，有效干燥体积：18m3，有效干燥面积：68m2，烘干方式：热风烘干式，加热装置：电加热，结构型式：整体，厢体批式","9300","2016TJ535","2020-12-31","42000.00","","非通用类","安徽省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","果蔬烘干机","容积15m³及以上果蔬烘干机(整体脱水)","滁州奥岚格机械有限公司","果蔬烘干机","5HGS-18E","处理型式:整体脱水 ;容积:18m³;","外形尺寸（长×宽×高）：4300×2800×2400mm，风机功率1.1kw，配套功率：7.5kw，有效干燥体积：18m3，有效干燥面积：68m2，烘干方式：热风烘干式，加热装置：空气能热泵+电辅热，结构型式：整体，厢体批式","9300","2016TJ577","2020-12-31","43000.00","","非通用类","安徽省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","果蔬烘干机","容积15m³及以上果蔬烘干机(整体脱水)","云南万合农机有限公司","果蔬烘干机","5HG-40B","处理型式:整体脱水 ;容积:40m³;","外形尺寸（长*宽*高）：5630*2815*3560mm（不含烟囱、雨棚）；烘干方式（连续式/循环式）：循环式；结构型式（烤槽敞开式/密封箱体式）：密封箱体式；烘干室材质（砖混/板房及板房材质）：板房结构。加热室：50mm双面彩钢岩棉夹芯板；烘干室：50mm双面彩钢聚氨酯夹芯板；烘干容积：40m³。","9300","滇2019039","2023-12-31","34500.00","","非通用类","云南省","评阅不通过","初评员：不通过","专家：营业执照过期。","","","","",""]
["收获后处理机械","干燥机械","果蔬烘干机","容积15m³及以上果蔬烘干机(整体脱水)","云南万合农机有限公司","果蔬烘干机","5HG-40A","处理型式:整体脱水 ;容积:40m³;","外形尺寸（长*宽*高）：5740*2810*3520mm（不含烟囱、雨棚）；烘干方式（连续式/循环式）：循环式；结构型式（烤槽敞开式/密封箱体式）：密封箱体式；烘干室材质（砖混/板房及板房材质）：板房结构。加热室：50mm双面彩钢岩棉夹芯板；烘干室：50mm双面彩钢聚苯乙烯夹芯板；烘干室容积：40m³。","9300","滇2019038","2023-12-31","32200.00","","非通用类","云南省","评阅不通过","初评员：不通过","专家：营业执照过期。","","","","",""]
["收获后处理机械","干燥机械","果蔬烘干机","容积15m³及以上果蔬烘干机(整体脱水)","云南万合农机有限公司","果蔬烘干机","5HG-30","处理型式:整体脱水 ;容积:30m³;","外形尺寸（长*宽*高）：≥6010*2820*2420mm；结构质量：≤1000kg；烘干容量：≤1500kg；烘干容积：30m³。","9300","滇2016161","2020-12-31","31800.00","","非通用类","云南省","评阅不通过","初评员：不通过","专家：营业执照过期。","","","","",""]
["收获后处理机械","干燥机械","果蔬烘干机","容积15m³及以上果蔬烘干机(整体脱水)","云南万合农机有限公司","果蔬烘干机","5HG-75","处理型式:整体脱水 ;容积:75m³;","外形尺寸（长*宽*高）：≥9680*3280*3690mm；结构质量：≤1800kg；烘干容量：≤4500kg；烘干容积：75m³。","9300","滇2016162","2020-12-31","37500.00","","非通用类","云南省","评阅不通过","初评员：不通过","专家：营业执照过期。","","","","",""]
["收获后处理机械","干燥机械","果蔬烘干机","容积15m³及以上果蔬烘干机(整体脱水)","云南万合农机有限公司","果蔬烘干机","5HG-51","处理型式:整体脱水 ;容积:51m³;","外形尺寸（长*宽*高）：6600*3150*3650mm（不含烟囱、雨棚）；烘干方式（连续式/循环式）：循环式；结构用型式（烤槽敞开式/密封箱体式）：密封箱体式；烘干室材质（砖混/板房及板房材质）：板房，50mm聚苯乙烯双面彩钢夹芯板；烘干容积：51m³。","9300","滇2018097","2022-12-31","33000.00","","非通用类","云南省","评阅不通过","初评员：不通过","专家：营业执照过期。","","","","",""]
["收获后处理机械","干燥机械","果蔬烘干机","容积15m³及以上果蔬烘干机(整体脱水)","三明市同硕机械制造有限公司","果蔬烘干机","5HGS-16-RL","处理型式:整体脱水 ;容积:16m³;","1、烘干室容积:6.2m³,整体脱水；2、外型尺寸(长×宽×高mm):3060×1830×2590；3、整机质量(kg):720；4、处理量(kg/批):650(笋)；5、装机总容量(kw):3.2；6、风机数量(台):2；7、供热方式:间接加热；8、燃料种类:煤、生物质；9、控制方式:自动控制。","9300","黑垦鉴2016090","2020-12-31","34000.00","","非通用类","福建省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["收获后处理机械","干燥机械","果蔬烘干机","容积15m³及以上果蔬烘干机(整体脱水)","广东奥伯特节能设备有限公司","果蔬烘干机","5HG-52","处理型式:整体脱水 ;容积:30m³;","烘干室容积，30m3，整体脱水，空气能热泵","9300","GZNJ/TJ 2018-079","2022-12-31","95000.00","","非通用类","广东省","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["收获后处理机械","干燥机械","果蔬烘干机","容积15m³及以上果蔬烘干机(整体脱水)","广东奥伯特节能设备有限公司","果蔬烘干机","5HG-30R","处理型式:整体脱水 ;容积:52m³;","烘干室容积，52m3，整体脱水，空气能热泵","9300","GZNJ/TJ 2018-078","2022-12-31","180000.00","","非通用类","广东省","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["收获后处理机械","干燥机械","果蔬烘干机","容积15m³及以上果蔬烘干机(整体脱水)","杭州真心热能电器有限公司","空气源热泵果蔬烘干机","5HG-30K","处理型式:整体脱水 ;容积:29m³;","项目                                     设计值                                核测值\n        规格型号                               5HG-30K                           5HG-30K\n       结构型式                              密封箱体式                         密封箱体式\n      外形尺寸（mm）     （7800×2800×3000）±5%        7912×2812×3011\n冷热循环风机数量（个）                   5                                        5\n冷热循环风机电机功率（kW）      0.75                                    0.75\n      排湿风机数量（个）                  1                                         1\n排湿风机电机功率（kW）             0.25                                   0.25\n       供热方式型号                 DKWHG-36II-G             DKWHG-36II-G    \n       供热方式类型                   空气源热泵                       空气源热泵\n       供热方式数量 (个)                   1                                       1\n          烘干方式                          整体脱水                          整体脱水\n      烘干室容积（m³）                 30±5%                               29","9300","GZNJ/TJ 2019-220","2023-12-31","93000.00","","非通用类","浙江省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["农产品初加工机械","茶叶加工机械","茶叶杀青机","滚筒直径40-60cm杀青机","信阳市华阳工贸有限公司","茶叶滚筒杀青机","6CST-52","滚筒直径:52cm;","外形尺寸（长*宽*高）mm：3500*820*1410；滚筒（内径*长度）mm：520*2700；电动机功率/电压（KW/V）：0.75/220；加热源形式：煤或柴；整机质量（kg）：780.","1600","豫2017127","2021-12-31","6400.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["农产品初加工机械","茶叶加工机械","茶叶杀青机","滚筒直径40-60cm杀青机","信阳市华阳工贸有限公司","茶叶滚筒杀青机","6CST-55","滚筒直径:55cm;","外形尺寸（长*宽*高）mm：3800*880*1490；滚筒（内径*长度）mm：550*3000；电动机功率/电压（KW/V）：0.75/220；加热源形式：煤或柴；整机质量（kg）：1200.","1600","豫2017128","2021-12-31","9000.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["农产品初加工机械","茶叶加工机械","茶叶杀青机","滚筒直径60cm及以上杀青机","浙江武义增荣食品机械有限公司","茶叶滚筒杀青机","6CST-110S","滚筒直径:110cm;","外形尺寸（长×宽×高）：6250×1550×2060（mm）；结构形式：滚筒式；滚筒外径:1100mm；滚筒内部直段长度：6000mm；滚筒转速：25r/min；运转电机功率：2.2kW；热源形式：生物质燃烧颗粒。","2400","T201933330155","2025-03-30","52000.00","","非通用类","浙江省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["农产品初加工机械","茶叶加工机械","茶叶杀青机","滚筒直径60cm及以上杀青机","浙江武义增荣食品机械有限公司","茶叶滚筒杀青机","6CST-90S","滚筒直径:90cm;","外形尺寸（长×宽×高）：4750×1200×1740（mm）；结构形式：滚筒式；滚筒外径:900mm；滚筒内部直段长度：4050mm；滚筒转速：21r/min；运转电机功率：1.1kW；热源形式：生物质燃烧颗粒。","2400","T201933330154","2025-03-30","29800.00","","非通用类","浙江省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["农产品初加工机械","茶叶加工机械","茶叶杀青机","滚筒直径60cm及以上杀青机","信阳市华阳工贸有限公司","茶叶滚筒杀青机","6CST-60","滚筒直径:60cm;","外形尺寸（长*宽*高）mm：3800*960*1600；滚筒（内径*长度）mm：600*3500；电动机功率/电压（KW/V）：0.75/220；加热源形式：煤或柴；整机质量（kg）：1600.","2400","豫2017129","2021-12-31","10500.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["农产品初加工机械","茶叶加工机械","茶叶杀青机","其它杀青机","浙江武义增荣食品机械有限公司","茶叶滚筒杀青机","6CST-100D","杀青方式:电磁 ;","外形尺寸(长×宽×高)：5750×1680×1980(mm)； 结构形式：滚筒式；滚筒外径:1000mm；滚筒内部直段长度：5500mm；滚筒转速：28r/min；运转电机功率：2.2kW；电加热功率：200kW；热源形式：电磁加热。","2100","T201933330156","2025-03-30","34000.00","","非通用类","浙江省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["农产品初加工机械","茶叶加工机械","茶叶揉捻机","揉筒直径35-50cm揉捻机","信阳市华阳工贸有限公司","茶叶揉捻机","6CR-35","揉筒直径:35cm;","外形尺寸（长*宽*高）mm：980*850*1040；结构形式：盘式。传动方式：皮带+齿轮减速箱传动。加压型式：单柱丝杆式（手动）加压；控制方式：人工（手动）；揉筒（内径*外径*高度）340*350*280；电动机功率（KW）：0.55；整机质量（kg）：180。","1100","豫2017125","2021-12-31","4500.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["农产品初加工机械","茶叶加工机械","茶叶揉捻机","揉筒直径35-50cm揉捻机","信阳市华阳工贸有限公司","茶叶揉捻机","6CR-45","揉筒直径:45cm;","外形尺寸（长*宽*高）mm：1185*1125*1300；结构形式：盘式。传动方式：皮带+齿轮减速箱传动。加压型式：单柱丝杆式（手动）加压；控制方式：人工（手动）；揉筒（内径*外径*高度）440*450*280；电动机功率（KW）：1.1；整机质量（kg）：260。","1100","豫2017126","2021-12-31","5900.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["农产品初加工机械","茶叶加工机械","茶叶炒（烘）干机","烘干面积10m²及以上连续自动式茶叶烘干机","浙江武义增荣食品机械有限公司","茶叶烘干机","6CHB-30Z","烘干面积:30㎡;连续自动式茶叶烘干机:是 ;","结构型式：自动连续链条烘板式；外形尺寸(长×宽×高)：7000×2010×2600(mm)；\n风机转速：2920（r/min）；有效干燥面积：30M2；匀叶轮工作宽度：114cm；烘板层数：8层；每层烘板有效烘干长度：310/314/314/314/314/314/314/314；电机功率：1.5KW；加热源形式：生物质燃烧颗粒；生产率≥180kg/h。","9000","T201933330153","2025-03-30","70000.00","","非通用类","浙江省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["农产品初加工机械","茶叶加工机械","茶叶炒（烘）干机","烘干面积10m²及以上连续自动式茶叶烘干机","浙江品峰机械有限公司","茶叶烘干机","6CH-10","烘干面积:10㎡;连续自动式茶叶烘干机:是 ;","连续自动链板式茶叶烘干机，烘干面积10平方米，外形尺寸长5250mm，宽2100mm，高2100mm，功率0.75kw,6层。","9000","T201933330088","2024-10-22","38000.00","","非通用类","浙江省","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["排灌机械","水泵","潜水电泵","4-7.5kW潜水电泵","上海义民电机有限公司","潜水电泵","QY65-13-4","电机功率:4kW;","配套功率 : 4kW，动力类型 : 三相，电压：380V，频率：50Hz，电流：9.3A，流量：65m3/h，扬程：13m，电泵\n效率：51.2%，质量：65kg，外形尺寸：250x240x650（mm）","170","T201900500968","2024-12-30","1625.00","","非通用类","上海市","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["排灌机械","水泵","潜水电泵","4-7.5kW潜水电泵","上海义民电机有限公司","潜水电泵","QY100-9-4","电机功率:4kW;","配套功率 : 4kW，动力类型 : 三相，电压：380V，频率：50Hz，电流：9.3A，流量：100m3/h，扬程：9m，电泵\n效率：50.5%，质量：65kg，外形尺寸：250x240x660（mm）。","170","T201900500968","2024-12-30","1625.00","","非通用类","上海市","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["排灌机械","水泵","潜水电泵","4-7.5kW潜水电泵","上海义民电机有限公司","潜水电泵","QY160-6-4","电机功率:4kW;","配套功率 : 4kW，动力类型 : 三相，电压：380V，频率：50Hz，电流：9.3A，流量：160m3/h，扬程：6m，电泵\n效率：51.7%，质量：65kg，外形尺寸：230x250x680（mm）。","170","T201900500968","2024-12-30","1585.00","","非通用类","上海市","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["排灌机械","水泵","潜水电泵","4-7.5kW潜水电泵","上海义民电机有限公司","潜水电泵","QY65-18-5.5","电机功率:5.5kW;","配套功率 : 5.5kW，动力类型 : 三相，电压：380V，频率：50Hz，电流：12.6A，流量：65m3/h，扬程：18m，电泵\n效率：53.9%，质量：85kg，外形尺寸：230x275x715（mm）。","170","T201900500968","2024-12-30","2205.00","","非通用类","上海市","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["排灌机械","水泵","潜水电泵","4-7.5kW潜水电泵","上海义民电机有限公司","潜水电泵","QY100-13-5.5","电机功率:5.5kW;","配套功率 : 5.5kW，动力类型 : 三相，电压：380V，频率：50Hz，电流：12.6A，流量：100m3/h，扬程：13m，电泵\n效率：53.9%，质量：85kg，外形尺寸：230x275x715（mm）。","170","T201900500968","2024-12-30","2205.00","","非通用类","上海市","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["排灌机械","水泵","潜水电泵","4-7.5kW潜水电泵","上海义民电机有限公司","潜水电泵","QY200-8-5.5","电机功率:5.5kW;","配套功率 : 5.5kW，动力类型 : 三相，电压：380V，频率：50Hz，电流：12.6A，流量：200m3/h，扬程：6m，电泵\n效率：52.4%，质量：85kg，外形尺寸：230x275x720（mm）。","170","T201900500968","2024-12-30","2205.00","","非通用类","上海市","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["排灌机械","水泵","潜水电泵","4-7.5kW潜水电泵","上海义民电机有限公司","潜水电泵","QY250-5-5.5","电机功率:5.5kW;","配套功率 : 5.5kW，动力类型 : 三相，电压：380V，频率：50Hz，电流：12.6A，流量：250m3/h，扬程：5m，电泵\n效率：52.5%，质量：85kg，外形尺寸：230x275x720（mm）。","170","T201900500968","2024-12-30","2340.00","","非通用类","上海市","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["排灌机械","水泵","潜水电泵","4-7.5kW潜水电泵","上海义民电机有限公司","潜水电泵","QY200-4-4","电机功率:4kW;","配套功率 : 4kW，动力类型 : 三相，电压：380V，频率：50Hz，电流：9.3A，流量：200m3/h，扬程：4m，电泵\n效率：51.7%，质量：65kg，外形尺寸：230x250x680（mm）。","170","T201900500968","2024-12-30","1585.00","","非通用类","上海市","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["排灌机械","水泵","潜水电泵","7.5-9.2kW潜水电泵","上海义民电机有限公司","潜水电泵","QY100-17-7.5","电机功率:7.5kW;","配套功率 : 7.5kW，动力类型 : 三相，电压：380V，频率：50Hz，电流：16.8A，流量：100m3/h，扬程：17m，电\n泵效率：55.6%，质量：97kg，外形尺寸：230x275x780（mm）。","570","T201900500968","2024-12-30","3205.00","","非通用类","上海市","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["排灌机械","水泵","潜水电泵","7.5-9.2kW潜水电泵","上海义民电机有限公司","潜水电泵","QY40-40-7.5","电机功率:7.5kW;","配套功率 : 7.5kW，动力类型 : 三相，电压：380V，频率：50Hz，电流：16.8A，流量：40m3/h，扬程：40m，电泵\n效率：53.0%，质量：97kg，外形尺寸：230x275x895（mm）。","570","T201900500968","2024-12-30","3205.00","","非通用类","上海市","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["排灌机械","水泵","潜水电泵","7.5-9.2kW潜水电泵","上海义民电机有限公司","潜水电泵","QY65-25-7.5","电机功率:7.5kW;","配套功率 : 7.5kW，动力类型 : 三相，电压：380V，频率：50Hz，电流：16.8A，流量：65m3/h，扬程：25m，电泵\n效率：55.6%，质量：97kg，外形尺寸：230x275x780（mm）。","570","T201900500968","2024-12-30","3165.00","","非通用类","上海市","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["排灌机械","水泵","潜水电泵","7.5-9.2kW潜水电泵","上海义民电机有限公司","潜水电泵","QY200-9-7.5","电机功率:7.5kW;","配套功率 : 7.5kW，动力类型 : 三相，电压：380V，频率：50Hz，电流：16.8A，流量：200m3/h，扬程：9m，电泵\n效率：53.1%，质量：97kg，外形尺寸：230x275x855（mm）。","570","T201900500968","2024-12-30","3205.00","","非通用类","上海市","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["排灌机械","水泵","潜水电泵","9.2-18.5kW潜水电泵","上海义民电机有限公司","潜水电泵","QY65-37-11","电机功率:11kW;","配套功率 : 11kW，动力类型 : 三相，电压：380V，频率：50Hz，电流：24.3A，流量：65m3/h，扬程：37m，电泵\n效率：54.4%，质量：125kg，外形尺寸：328x328x888（mm）。","720","T201900500968","2024-12-30","4320.00","","非通用类","上海市","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["排灌机械","水泵","潜水电泵","9.2-18.5kW潜水电泵","上海义民电机有限公司","潜水电泵","QY100-25-11","电机功率:11kW;","配套功率 : 11kW，动力类型 : 三相，电压：380V，频率：50Hz，电流：24.3A，流量：100m3/h，扬程：25m，电泵\n效率：56.5%，质量：125kg，外形尺寸：328x328x888（mm）。","720","T201900500968","2024-12-30","4320.00","","非通用类","上海市","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["排灌机械","水泵","潜水电泵","9.2-18.5kW潜水电泵","上海义民电机有限公司","潜水电泵","QY160-15-11","电机功率:11kW;","配套功率 : 11kW，动力类型 : 三相，电压：380V，频率：50Hz，电流：24.3A，流量：160m3/h，扬程：15m，电泵\n效率：55.1%，质量：125kg，外形尺寸：328x328x888（mm）。","720","T201900500968","2024-12-30","4360.00","","非通用类","上海市","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["排灌机械","喷灌机械设备","喷灌机","管径65mm以下卷盘式喷灌机","江苏科翔制泵有限公司","绞盘式喷灌机","JP50/180","喷灌机型式:卷盘式喷灌机 ;管径:50mm;","整机尺寸(长*宽*高mm):3100×1580×1500,PE管规格(mm*m):50*160,有效喷洒长度(m):≥180,入机压力(MPa):0.43-0.75,入机流量(m3/h)5.5-19.7喷嘴直径:Φ10-14水涡轮:TX10","3500","苏农机（2016）第（0520）号","2020-12-31","15000.00","","非通用类","江苏省","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["排灌机械","喷灌机械设备","喷灌机","管径65mm以下卷盘式喷灌机","徐州大有灌排设备有限公司","卷盘式喷灌机","JP50-150","喷灌机型式:卷盘式喷灌机 ;管径:50mm;","整机尺寸(长*宽*高mm):3100×1600×1500,PE管规格(mm*m):50*135,有效喷洒长度(m):≥150,入机压力(MPa):0.45-0.76,入机流量(M3/h):8.5-19.8喷嘴直径:Φ9-16,水涡轮:TX10","3500","苏农机（2016）第（0518）号","2020-12-31","15000.00","","非通用类","江苏省","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["排灌机械","喷灌机械设备","喷灌机","管径75-85mm卷盘式喷灌机","江苏科翔制泵有限公司","绞盘式喷灌机","JP75/300","喷灌机型式:卷盘式喷灌机 ;管径:75mm;","整机尺寸(长*宽*高mm):5190×2010×2620,整机质量(kg):2400,PE管规格(mm*m):75*280,有效喷洒长度(m):≥300,入机压力(MPa):0.55-1.00,入机流量(m3/h):15.0-45.喷嘴直径:Φ14-20水涡轮:TX20","9200","苏农机（2016）第（0521）号","2020-12-31","33000.00","","非通用类","江苏省","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["排灌机械","喷灌机械设备","喷灌机","管径75-85mm卷盘式喷灌机","泰安市霖丰机械科技有限公司","绞盘式喷灌机","JP75","喷灌机型式:卷盘式喷灌机 ;管径:75mm;","1.型号名称：JP75型绞盘式喷灌机；2.外形尺寸：5300×1900×2660mm；3.绞盘回卷驱动方式：水涡轮；4.绞盘回卷变速方式：变速箱；5.绞盘水平转向角度：20~320°；6.绞盘卷绕层数：5层；7.卷管材质：PE管；8.卷管外径：75mm；9.卷管壁厚：6.0mm；10.卷管长度：300000mm；11.喷头车型式：龙门架式；12.喷头车驱动方式：牵引式；13.喷头车轮距：1450~2800mm；14.喷头车通过间隙：1150mm；15.喷射装置型式：摇臂式喷枪；16.喷射装置数量：1；17.喷射装置型号：KOMET-TWIN101；18.配套水泵额定流量：15~40m³/h；19.配套水泵扬程：54~100m；20.配套水泵额定功率：5.5~22KW；21.运输间隙：280mm。","9200","T202037370062","2025-07-06","42800.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","铡草机","1-3t/h铡草机","郑州市松海机械制造有限公司","铡草机","9Z-1.5","生产率:1.5t/h;","规格型号:9Z-1.5,配套动力:3KW,结构形式:盘式;外形尺寸:920mm×1100mm×1860mm;生产效率:1.5T/H.喂入口宽度:170MM;主轴转速:1300R/MIN,喂入辊转:285R/MIN,动刀片数量:6片;圆盘或滚筒直径:530mm","390","部20190713","2023-12-31","1900.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","铡草机","1-3t/h铡草机","云南长威机械制造有限公司","铡草机","9ZP-1.6","生产率:1.6t/h;","尺寸1030*760*1800，配套动力3.0，喂入方式人工，结构形式盘式，设计切草长度10、20、30.喂入口宽度130mm，主轴额定转速1040r/min，动刀6片，滚筒直径500mm\t每小时1.6吨","390","T20205353112","2025-06-16","1300.00","","非通用类","云南省","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","铡草机","1-3t/h铡草机","云南长威机械制造有限公司","铡草机","9ZT-1.0","生产率:1.0t/h;","尺寸1030*475*830，配套动力3.0，喂入方式人工，结构形式筒式，设计切草长度10、20.喂入口宽度240mm，主轴额定转速1180r/min，动刀4片，滚筒直径210mm\t每小时1.0吨","390","T20205353111","2025-06-16","1300.00","","非通用类","云南省","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","铡草机","3-6t/h铡草机","云南精旭农机制造有限公司","铡草机","9ZP-4.0","生产率:4t/h;","外形尺寸长宽高：930mmX980mmX1460、配套动力：4kw、设计切草长度：10、15、20mm、结构形式：盘式、喂入口宽度：200mm、喂入方式：自动喂入、生产率：4000kg/h。","630","T20205353041","2025-04-15","2050.00","","非通用类","云南省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","铡草机","3-6t/h铡草机","云南精驰农机有限公司","铡草机","9ZT-4.0","生产率:4t/h;","外形尺寸长宽高：930mmX980mmX1460、配套动力：4kw、设计切草长度：10、15、20mm、结构形式：盘式、喂入口宽度：200mm、喂入方式：自动喂入、生产率：4000kg/h。","630","T20205353043","2025-04-15","2150.00","","非通用类","云南省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","铡草机","3-6t/h铡草机","云南长威机械制造有限公司","铡草机","9ZT-4.0","生产率:4.0t/h;","尺寸1060*480*860，配套动力4.0，喂入方式自动，结构形式筒式，设计切草长度10、20.喂入口宽度235mm，主轴额定转速1450r/min，动刀4片，滚筒直径205mm\t每小时4吨","630","T20205353113","2025-06-16","2100.00","","非通用类","云南省","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","铡草机","6-9t/h铡草机","云南精驰农机有限公司","铡草机","9ZP-6.3","生产率:6t/h;","外形尺寸长宽高：1250mmX1100mmX1800、配套动力：7.5kw、设计切草长度：5、10、15mm、结构形式：盘式、喂入口宽度：155mm、喂入方式：自动喂入、生产率：6300kg/h。","1200","T20205353044","2025-04-15","4680.00","","非通用类","云南省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","铡草机","6-9t/h铡草机","云南长威机械制造有限公司","铡草机","9ZP-6.3","生产率:6.3t/h;","尺寸1700*1120*2050，配套动力4.0，喂入方式自动，结构形式盘式，设计切草长度15、25、35.喂入口宽度240mm，主轴额定转速910r/min，动刀6片，滚筒直径710mm\t每小时6.3吨","1200","T20205353114","2025-06-16","4000.00","","非通用类","云南省","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","铡草机","6-9t/h铡草机","肥城市畜丰农牧机械有限公司","铡草机","9ZP-7","生产率:7t/h;","型号名称\n/\n9ZP-7\n配套动力\nkW\n7.5\n结构型式\n/\n盘式\n外形尺寸(长×宽×高)\nmm\n2210x1600x2425\n生产效率\nkg/h\n7000(鲜秸秆)\n设计切草长度\nmm\n9-35\n喂入口宽度\nmm\n270\n喂入方式\n/\n链条自动喂入\n主轴额定转速\nr/min\n700\n动刀片数量\n个\n3\n动刀片刀形\n/\n/\n圆盘或滚筒直径（工作部件）\nmm\n1028","1200","T20190606086","2024-12-31","7500.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","铡草机","9-15t/h铡草机","肥城市畜丰农牧机械有限公司","铡草机","9ZP-9A","生产率:9t/h;","结构型式\n/\n盘刀式\n外形尺寸（长×宽×高）\nmm\n3840×2250×3950\n喂入口宽度\nmm\n640\n喂入方式\n/\n对辊式\n主轴额定转速\nr/min\n580\n喂入辊额定转速\nr/min\n100\n动刀片数\n/\n3\n定刀片数\n/\n1\n圆盘或滚筒直径\nmm\n1300","2500","鲁T2017065","2021-12-31","9800.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","铡草机","15-20t/h铡草机","肥城市畜丰农牧机械有限公司","铡草机","9ZP-15.0","生产率:15t/h;","型号名称\n/\n9ZP-15.0铡草机\n配套动力\nkW\n18.5\n结构型式\n/\n盘刀式\n外形尺寸（长×宽×高）\nmm\n2600×2200×4200\n生产率\nkg/h\n≥15000（鲜秸秆）\n设计切草长度\nmm\n12、18、25、35\n喂入口宽度\nmm\n390\n喂入方式\n/\n对辊式+链条自动喂入\n主轴额定转速\nr/min\n500\n喂入辊额定转速\nr/min\n118、126、150、237\n动刀片数量\n/\n3\n定刀片刀形\n/\n/\n圆盘或滚筒直径（含刀片）\nmm\n1317","2900","鲁T2019009","2023-12-31","12800.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","铡草机","20t/h及以上铡草机","肥城市畜丰农牧机械有限公司","铡草机","9ZP-30","生产率:30t/h;","型号名称\n/\n9ZP-30型铡草机\n配套动力 主电机\nkW\n30\n配套动力 给进电机\nkW\n5.5\n结构型式\n/\n盘刀式\n外形尺寸（长×宽×高）\nmm\n4870×2900×4650\n生产率\nkg/h\n≥30000（鲜秸秆）\n设计切草长度\nmm\n15、25、30、40\n喂入口宽度\nmm\n900\n喂入方式\n/\n对辊式+自动喂入\n主轴额定转速\nr/min\n450\n喂入辊额定转速\nr/min\n65\n动刀片数量\n/\n3\n定刀片刀形\n/\n长方形\n圆盘或滚筒直径（含刀片）\nmm\n1670","8000","鲁T2018014","2022-12-31","36800.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","青贮切碎机","9-15t/h青贮切碎机","云南精旭农机制造有限公司","青贮切碎机","93QS-9","生产率:9t/h;","外形尺寸长宽高：1210mmX570mmX880、配套动力：4kw、设计切草长度：15、25mm、结构形式：筒式、喂入口宽度：280mm、喂入方式：手动喂入、生产率：9000kg/h。","1300","T20205353042","2025-04-15","4450.00","","非通用类","云南省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","青贮切碎机","9-15t/h青贮切碎机","云南长威机械制造有限公司","青贮切碎机","93QS-9","生产率:9t/h;","尺寸1040*470*810，配套动力3.0，喂入方式人工，结构形式筒式，设计切草长度15、20.喂入口宽度245mm，主轴额定转速1180r/min，动刀4片，滚筒直径200mm\t每小时9吨","1300","T20205353115","2025-06-16","4340.00","","非通用类","云南省","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","青贮切碎机","15t/h及以上青贮切碎机","云南精旭农机制造有限公司","青贮切碎机","93QS-15","生产率:15t/h;","外形尺寸长宽高：1880mm*570mm*1000、配套动力：7.5kw、设计切草长度10、15mm、结构形式：筒式、喂入口宽度：240mm、喂入方式：自动喂入、生产率：15000kg/h。","2400","T20205353089","2025-06-04","9520.00","","非通用类","云南省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","青贮切碎机","15t/h及以上青贮切碎机","云南精驰农机有限公司","青贮切碎机","93QS-20","生产率:20t/h;","外形尺寸长宽高：1180mm*700mm*820、配套动力：7.5kw、设计切草长度：15-30mm、结构形式：筒式、喂入口宽度：455mm、喂入方式：人工喂入、生产率：20000kg/h。","2400","T20205353088","2025-06-04","12500.00","","非通用类","云南省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","揉丝机","2-4t/h揉丝机","西安新天地草业股份有限公司","秸秆揉丝机","9RSZ-10","生产率:2t/h;","1 结构形式：锤片式；\n2 配套动力：22+3kW；\n3 外形尺寸（长×宽×高）3200×950×1200mm；\n4 结构质量585kg（不含电机）；\n5 生产率≥10000kg/h（秸秆含水率80%），\n≥5000kg/h（秸秆含水率60%），≥2000kg/h（秸秆含水率20%）；\n6主轴转速2100r/min；\n7 转子直径350mm；\n8 锤片数量40片；\n9 锤片尺寸:（长×宽×高）：175×50×4mm；\n10 喂入方式：自动喂入","800","陕2017002","2021-12-31","18700.00","","非通用类","陕西省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","揉丝机","2-4t/h揉丝机","西安新天地草业股份有限公司","秸秆揉丝机","9RSZ-15","生产率:3t/h;","1 结构形式：锤片式；\n2 配套动力30+5.5kW；\n3 外形尺寸（长×宽×高）：3600×1150×1150mm；\n4 结构质量：683kg（不含电机）；\n5 生产率≥15000kg/h（秸秆含水率80%），\n≥7500 kg/h（秸秆含水率60%），            ≥3000kg/h（秸秆含水率20%）；\n6 主轴转速2100r/min \n7 转子直径：350mm；\n8 锤片数量：54片；\n9 锤片尺寸（长×宽×高）：175×50×4mm； \n10 喂入方式：自动喂入","800","陕2017003","2021-12-31","23800.00","","非通用类","陕西省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","揉丝机","2-4t/h揉丝机","西安新天地草业股份有限公司","秸秆揉丝机","9RSZ-6","生产率:3t/h;","结构形式：锤片式\n配套动力：11kW\n外形尺寸（长×宽×高）：2950×810×1110mm\n结构质量：320kg（不含电机）\n生产率：3000kg/h（秸秆含水率64%）\n主轴转速：2280r/min\n转子直径：350mm\n锤片数量：40个\n锤片尺寸（长×宽×高）：148×36×4mm\n喂入方式：自动喂入","800","陕2019004","2023-12-31","12600.00","","非通用类","陕西省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","揉丝机","4-6t/h揉丝机","西安新天地草业股份有限公司","秸秆揉丝机","9RS-10Z","生产率:5t/h;","结构形式：带刀锤片式\n配套动力：22kW\n外形尺寸（长×宽×高）：2500×1850×3050mm\n结构质量：670kg（不含电机）\n生产率：5000kg/h\t:（秸秆含水率64%）\n动刀转速：660r/min\n锤片风叶转速：1200r/min\n动刀固定架直径（不含刀片）：940mm\n锤片风叶固定座直径：1050mm\n锤片数量：24个\n锤片尺寸（长×宽×高）：148×36×4mm\n喂入方式：自动喂入","880","陕2019003","2023-12-31","17500.00","","非通用类","陕西省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","饲料（草）粉碎机","400mm以下饲料粉碎机","云南长威机械制造有限公司","饲料粉碎机","9FQ-26-20","转子直径:260mm;","锤片式（无粉碎秸蔓类功能），尺寸780*660*1050配套动力2.2KW，锤片24片，主轴转速4600r/min,转子盘直径205mm,转子工作直径260mm，粉碎室宽度200mm","190","T20205353110","2025-06-16","640.00","","非通用类","云南省","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","饲料（草）粉碎机","400-550mm饲料粉碎机","郑州金宏兴机械有限公司","饲料粉碎机","9F50-13","转子直径:500mm;","结构形式：锤片式；外形尺寸：1210×1080×1710mm；配套动力：7.5-15kw；转子盘工作直径：500mm；主轴转速：2950r/min；锤片数量：16-20片","530","部20190693","2023-12-31","1800.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","饲料（草）粉碎机","400-550mm饲料粉碎机","云南长威机械制造有限公司","饲料粉碎机","9FQ-40-20","转子直径:400mm;","锤片式（无粉碎秸蔓类功能），尺寸1250*430*1160配套动力3.0KW，锤片24片，主轴转速3480r/min,转子盘直径300mm,转子工作直径400mm，粉碎室宽度200mm","530","T20205353109","2025-06-16","1770.00","","非通用类","云南省","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","饲料（草）粉碎机","550mm及以上饲料粉碎机","云南长威机械制造有限公司","饲料粉碎机","9FQ-55-20","转子直径:550mm;","锤片式（无粉碎秸蔓类功能），尺寸1220*420*1130配套动力7.8KW，锤片16片，主轴转速2960r/min,转子盘直径320mm,转子工作直径550mm，粉碎室宽度205mm","1000","T20205353108","2025-06-16","3340.00","","非通用类","云南省","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","饲料（草）粉碎机","550mm及以上饲料粉碎机","郑州嵩威机械制造有限公司","饲料粉碎机","9FZ-55-15A","转子直径:555mm;","结构型式：锤片式，配套动力：11kw，转子直径：555mm","1000","T201941410002","2024-11-13","3800.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","饲料（草）粉碎机","550mm及以上饲料粉碎机","郑州嵩威机械制造有限公司","饲料粉碎机","9FZ-55-15B","转子直径:555mm;","结构型式：锤片式，配套动力：11kw，转子直径：555mm","1000","T201941410001","2024-11-13","3600.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","饲料混合机","2m³及以上卧式(单轴)混合机","郑州金宏兴机械有限公司","卧式饲料混合机","9HWD-1000","混合机类型:卧式混合机单轴 ;混合机容积:2.07m³;","有效容积：2.07m³；结构形式：卧式，双环带；配套动力：11kw；混合轴数量：1根；额定批次混入量：1000kg；外形尺寸：3350传1150×2220mm；主轴转速：25r/min","5600","部20190684","2023-12-31","17000.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","饲料混合机","2m³及以上卧式(单轴)混合机","郑州嵩威机械制造有限公司","饲料混合机","9HW-1000","混合机类型:卧式混合机单轴 ;混合机容积:2.05m³;","结构型式：卧式单轴螺带，配套动力：7.5kw，混合室容积：2.05m³。","5600","T202014140019","2025-04-23","25000.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","颗粒饲料压制机","平模颗粒饲料压制机","郑州金宏兴机械有限公司","颗粒饲料压制机","9KLP-300","平模直径:300mm;","结构形式：立式平模；外形尺寸：1380×560×1240mm；配套动力：22kw；模盘直径：300mm；压辊数量：3个；压模有效宽度：85mm；生产率：700-1200kg/h","700","GZNJ/TJ 2019-452","2025-01-13","7300.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","颗粒饲料压制机","平模颗粒饲料压制机","郑州金宏兴机械有限公司","颗粒饲料压制机","9KLP-250","平模直径:250mm;","结构形式：立式平模；外形尺寸：1240×530×1190mm；配套动力：15kw；压模直径：250mm；压辊数量：3个；生产率：500-800kg/h","700","GZNJ/TJ 2019-452","2025-01-13","4800.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","颗粒饲料压制机","平模颗粒饲料压制机","郑州金宏兴机械有限公司","颗粒饲料压制机","9KLP-200","平模直径:200mm;","结构形式：立式平模；外形尺寸：1100×450×930mm；配套动力：7.5kw；压模直径：200mm；压辊数量：2个；生产率：200-300kg/h","700","GZNJ/TJ 2019-452","2025-01-13","2900.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","饲料制备（搅拌）机","4-9m³饲料全混合日粮制备机","司达特（北京）畜牧设备有限公司","卧式牵引式动物饲料制备机","9JQW-7","搅拌室容积:7m³;","外形尺寸：3130*1750*1934mm结构质量：6700kg，搅拌室容积：7m3，刀片形式：椭圆锯齿刀片、大月牙刀片，刀片数量：动刀56片，定刀2片，配套动力形式：拖拉机；配套动力的范围：≥35Kw；","15400","部20180465","2022-12-31","190300.00","","非通用类","北京市","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","饲料制备（搅拌）机","4-9m³饲料全混合日粮制备机","北京国科诚泰农牧设备有限公司","立式牵引式全混合日粮饲料制备机","9JQL-8","搅拌室容积:8m³;","外形尺寸：3175*2215*1700mm结构质量：3690kg，搅拌室容积：8m3，刀片形式：大型锯齿花刀，刀片数量：动刀9片，定刀2片，配套动力形式：拖拉机；配套动力的范围：≥56Kw","15400","部20171258","2021-12-31","150000.00","","非通用类","北京市","评阅不通过","初评员：不通过","专家：承诺书过期；产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","饲料制备（搅拌）机","4-9m³饲料全混合日粮制备机","郑州嵩威机械制造有限公司","饲料制备机","9JGW-5","搅拌室容积:5m³;","结构型式：固定式、卧式，配套动力：16.5kw，搅拌仓容积：5m³","15400","T202014140002","2025-03-03","120000.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","饲料制备（搅拌）机","4-9m³饲料全混合日粮制备机","石家庄诺达机械设备有限公司","全日粮饲料制备机","9TMRW-4","搅拌室容积:4m³;","序号\t项目\t计量单位\t设计值\t核测结果\n1\t规格型号\t/\t9TMRW-4\t9TMRW-4\n2\t外形尺寸（长*宽*高）\tmm\t3050*1400*2600\t3050*1400*2600\n3\t结构质量\tkg\t1100\t1100\n4\t搅龙转速\tr/min\t18\t18\n5\t搅拌仓容积\t立方\t4\t4\n6\t结构形式\t/\t卧式\t卧式\n7\t配套动力范围\tkW\t11\t11\n8\t刀片型式\t/\t梅花刀\t梅花刀\n9\t刀片数量（片）\t/\t21\t21\n10\t配套动力形式\t/\t电机\t电机","15400","冀2016T—037","2020-12-31","55000.00","","非通用类","河北省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","饲料制备（搅拌）机","4-9m³饲料全混合日粮制备机","石家庄诺达机械设备有限公司","全日粮饲料制备机","9TMRW-5","搅拌室容积:5m³;","序号\t项目名称\t计量单位\t设计值\n1\t规格型号\t/\t9TMRW-5\n2\t外形尺寸（长*宽*高）\tMm\t5200*1720*2230\n3\t结构质量\tkg\t2000\n4\t搅龙转速\tr/min\t18\n5\t搅拌仓容积\t立方\t5\n6\t结构形式\t/\t卧式\n7\t配套动力范围\tKW\t15\n8\t刀片型式\t/\t梅花刀\n9\t刀片数量（片）\t/\t45\n10\t配套动力形式\t/\t电机","15400","冀2016T—002","2020-12-31","59000.00","","非通用类","河北省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","饲料制备（搅拌）机","4-9m³饲料全混合日粮制备机","肥城市畜丰农牧机械有限公司","全混合日粮制备机","9JGW-8","搅拌室容积:8m³;","型号名称\n/\n9JGW-8全混合日粮制备机\n型式\n/\n卧式\n称重系统最大称量\nkg\n20000\n配套动力型式\n/\n电动机\n配套动力功率范围\nkW\n30(15+15)\n配套动力转速\n转/分\n1460\n搅拌仓容积\nm3\n8\n搅拌仓仓体外形尺寸 （长×宽×高）\nmm\n3190×1700×1650\n主搅龙数量\n个\n2\n副搅龙数量\n个\n0","15400","T201937370196","2024-12-23","78000.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","饲料制备（搅拌）机","4-9m³饲料全混合日粮制备机","肥城市畜丰农牧机械有限公司","全混合日粮制备机","9JGL-8","搅拌室容积:8m³;","型号名称\n/\n9JGL-8全混合日粮制备机\n型式\n/\n立式\n称重系统最大称量\nkg\n15000\n配套动力型式\n/\n电动机\n配套动力功率范围\nkW\n30\n配套动力转速\n转/分\n1475\n搅拌仓容积\nm3\n8\n搅拌仓仓体外形尺寸 （长×宽×高）\nmm\n3072×2075×1873\n主搅龙数量\n个\n1\n副搅龙数量\n个\n0","15400","T201937370197","2024-12-23","78000.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","饲料制备（搅拌）机","9-12m³饲料全混合日粮制备机","郑州嵩威机械制造有限公司","饲料制备机","9JGW-9","搅拌室容积:9.05m³;","结构型式：固定式、卧式，配套动力：31.5kw，搅拌仓容积：9.05m³","17200","T202014140001","2025-03-03","140000.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","饲料制备（搅拌）机","12m³及以上饲料全混合日粮制备机","司达特（北京）畜牧设备有限公司","立式牵引式动物饲料制备机","9JQL-21","搅拌室容积:21m³;","外形尺寸：5575*2448*2049mm结构质量：16500kg，搅拌室容积：21m3，刀片形式：大型锯齿花刀，刀片数量：动刀18片，定刀2片，配套动力形式：拖拉机；配套动力的范围：≥82Kw","20000","部20180698","2022-12-31","422000.00","","非通用类","北京市","评阅不通过","初评员：不通过","专家：承诺书过期；产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","饲料制备（搅拌）机","12m³及以上饲料全混合日粮制备机","司达特（北京）畜牧设备有限公司","立式牵引式动物饲料制备机","9JQL-25","搅拌室容积:25m³;","外形尺寸：5770*2490*2387mm结构质量：16500kg，搅拌室容积：25m3，刀片形式：大型锯齿花刀，刀片数量：动刀18片，定刀2片，配套动力形式：拖拉机；配套动力的范围：≥89Kw","20000","部20180697","2022-12-31","470000.00","","非通用类","北京市","评阅不通过","初评员：不通过","专家：承诺书过期；产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","饲料制备（搅拌）机","12m³及以上饲料全混合日粮制备机","司达特（北京）畜牧设备有限公司","卧式牵引式动物饲料制备机","9JQW-12","搅拌室容积:12m³;","外形尺寸：4018*2012*2252mm结构质量：9900kg，搅拌室容积：12m3，刀片形式：椭圆锯齿刀片、大月牙刀片，刀片数量：动刀81片，定刀2片，配套动力形式：拖拉机；配套动力的范围：≥46Kw","20000","部20180464","2022-12-31","258500.00","","非通用类","北京市","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","饲料制备（搅拌）机","12m³及以上饲料全混合日粮制备机","司达特（北京）畜牧设备有限公司","卧式牵引式动物饲料制备机","9JQW-16","搅拌室容积:16m³;","外形尺寸：4768*2140*2358mm结构质量：11900kg，搅拌室容积：16m3，刀片形式：椭圆锯齿刀片、大月牙刀片，刀片数量：动刀96片，定刀2片，配套动力形式：拖拉机；配套动力的范围：≥53Kw","20000","部20180463","2022-12-31","350000.00","","非通用类","北京市","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","饲料制备（搅拌）机","12m³及以上饲料全混合日粮制备机","新乡市新东轻工机械有限公司","全混合日粮制备机","9JGW-12","搅拌室容积:12m³;","固定式卧式，电机，动力功率范围kw≧30，动力转速 1480转/分，主搅龙1个，副搅龙2个","20000","T201900010192","2024-12-30","126000.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确定为整机铭牌。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","饲料制备（搅拌）机","12m³及以上饲料全混合日粮制备机","北京国科诚泰农牧设备有限公司","立式牵引式动物饲料制备机","9JQL-21","搅拌室容积:21m³;","外形尺寸：5575*2448*2049mm结构质量：6850kg，搅拌室容积：21m3，刀片形式：大型锯齿花刀，刀片数量：动刀18片，定刀2片，配套动力形式：拖拉机；配套动力的范围：≥82Kw","20000","部20180698","2022-12-31","320000.00","","非通用类","北京市","评阅不通过","初评员：不通过","专家：承诺书过期；产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","饲料制备（搅拌）机","12m³及以上饲料全混合日粮制备机","天津库恩农业机械有限公司","全混日粮饲料搅拌机","Profile 20.2.DS","搅拌室容积:20m³;","型式：牵引，立式\n搅拌仓仓体外形尺寸（长x宽x高）：4800x2300x2300mm\n配套动力：88~111kw\n搅龙数量：2个","20000","黑垦鉴2019096","2023-12-31","367400.00","","非通用类","天津市","评阅不通过","初评员：不通过","专家：承诺书过期；产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","饲料制备（搅拌）机","12m³及以上饲料全混合日粮制备机","郑州嵩威机械制造有限公司","饲料制备（搅拌）机","9JGW-12","搅拌室容积:12m³;","结构型式：固定式、卧式，配套动力：38.5kw，搅拌仓容积：12m³","20000","T201900140446","2024-12-30","160000.00","","非通用类","河南省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","饲料制备（搅拌）机","12m³及以上饲料全混合日粮制备机","石家庄诺达机械设备有限公司","全日粮饲料制备机","9TMRW-12","搅拌室容积:12m³;","序号 \t项目\t计量单位\t设计值\n1\t规格型号\t/\t9TMRW-12\n2\t外形尺寸（长×宽×高）\tmm\t4400×2000×2700\n3\t结构质量\tkg\t2800\n4\t搅龙转速\tr/min\t18\n5\t搅拌仓容积\tm³\t12\n6\t结构形式\t/\t卧式\n7\t配套动力范围\tKW\t22\n8\t刀片型式\t/\t梅花刀\n9\t刀片数量（片）\t/\t55\n10\t配套动力形式\t/\t电动机","20000","冀2016T—003","2020-12-31","68000.00","","非通用类","河北省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","饲料制备（搅拌）机","12m³及以上饲料全混合日粮制备机","石家庄诺达机械设备有限公司","全日粮饲料制备机","9TMRW-14","搅拌室容积:14m³;","序号\t项目\t计量单位\t设计值\n1\t规格型号\t/\t9TMRW-14全日粮饲料制备机\n2\t型式\t/\t卧式\n3\t称重系统最大称量\tkg\t8000\n4\t配套动力型式\t/\t电机\n5\t配套动力功率\tkW\t22\n6\t配套动力转速\t转/分\t1450\n7\t搅拌仓容积\tM³\t14\n8\t搅拌仓仓体外形尺寸（长×宽×高）\tmm\t4300×2000×2400\n9\t主搅龙数量\t个\t1\n10\t副搅龙数量\t个\t2\n11\t取料滚筒宽度\tmm\t/\n12\t最大取料高度\tmm\t/\n13\t轮胎规格\t/\t/\n14\t轮距\tmm\t/\n15\t轴距\tmm\t/\n16\t驾驶室\t/\t/","20000","T201913130305","2024-12-30","75000.00","","非通用类","河北省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","饲料制备（搅拌）机","12m³及以上饲料全混合日粮制备机","肥城市畜丰农牧机械有限公司","全混合日粮制备机","9JGW-12","搅拌室容积:12m³;","项目\n单位\n设计值\n型号名称\n/\n9JGW-12全混合日粮制备机\n型式\n/\n固定式、卧式\n称重系统最大称量\nkg\n20000\n配套动力型式\n/\n电动机\n配套动力功率范围\nkW\n38.5\n配套动力转速\n转/min\n1470\n搅拌仓容积\nm3\n12\n搅拌仓仓体外形尺寸（长×宽×高）\nmm\n4310×1700×1940\n主搅龙数量\n个\n2\n副搅龙数量\n个\n0","20000","T201900230573","2024-12-30","118000.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["畜牧机械","饲料（草）加工机械设备","饲料制备（搅拌）机","12m³及以上饲料全混合日粮制备机","肥城市畜丰农牧机械有限公司","全混合日粮制备机","9JQL-12","搅拌室容积:12m³;","型号名称\n/\n9JQL-12全混合日粮制备机\n型式\n/\n牵引式、立式\n称重系统最大称量\nkg\n15000\n配套动力型式\n/\n拖拉机\n配套动力功率范围\nkW\n≥58.8\n搅拌仓容积\nm3\n12\n搅拌仓仓体外形尺寸（长×宽×高）\nmm\n3565×2460×2270\n主搅龙数量\n个\n1\n副搅龙数量\n个\n0\n轮胎规格\n/\n28×9-15\n轮距\nmm\n1750","20000","T201900230574","2024-12-30","118000.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["畜牧机械","畜产品采集加工机械设备","挤奶机","18-20杯组手动脱杯中置(鱼骨)式挤奶机","石家庄诺达机械设备有限公司","挤奶机","9JGJ-20","形式:中置(鱼骨)式 ;杯组数:20组;脱杯方式:手动 ;","序号\t项目\t单位\t设计值（涵盖机型）\n1\t产品型号名称\t/\t9JGJ-20挤奶机\n2\t形式\t/\t管道式\n3\t真空泵品牌\t/\t利拉伐\n4\t真空泵规格型号\t/\t2100L\n5\t真空泵台数\t台\t1\n6\t挤奶杯组数\t组\t20\n7\t脉动器品牌\t/\t意大利LE20\n8\t脉动器规格型号\t/\tLE20\n9\t脉动器形式\t/\t电子\n10\t脉动器频率\t次/min\t60\n11\t脉动器比率\t％\t60\n12\t计量方式\t/\t计量瓶\n13\t脱杯方式\t/\t手动","31900","冀2016T—143","2020-12-31","160000.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：承诺书过期；产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["畜牧机械","畜产品采集加工机械设备","挤奶机","24杯组手动脱杯中置(鱼骨)式挤奶机","石家庄诺达机械设备有限公司","挤奶机","9JGJ-24","形式:中置(鱼骨)式 ;杯组数:24组;脱杯方式:手动 ;","序号\t项目\t单位\t设计值\n1\t产品型号名称\t/\t9JGJ-24挤奶机\n2\t形式\t/\t管道式\n3\t真空泵品牌\t/\t利拉伐\n4\t真空泵规格型号\t/\t2100L\n5\t真空泵台数\t台\t1\n6\t挤奶杯组数\t组\t24\n7\t脉动器品牌\t/\t意大利LE20\n8\t脉动器规格型号\t/\tLE20\n9\t脉动器形式\t/\t电子\n10\t脉动器频率\t次/min\t60\n11\t脉动器比率\t％\t60\n12\t计量方式\t/\t计量瓶\n13\t脱杯方式\t/\t手动","42300","冀2016T—143","2020-12-31","220000.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：承诺书过期；产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["畜牧机械","畜产品采集加工机械设备","挤奶机","14杯组及以上自动脱杯中置(鱼骨)式挤奶机","石家庄诺达机械设备有限公司","挤奶机","9JGD-16","形式:中置(鱼骨)式 ;杯组数:16组;脱杯方式:自动 ;","序号\t项目\t单位\t设计值\n1\t产品型号名称\t/\t9JGD-16挤奶机\n2\t形式\t/\t管道式\n3\t真空泵品牌\t/\t利拉伐\n4\t真空泵规格型号\t/\t2100L\n5\t真空泵台数\t台\t1\n6\t挤奶杯组数\t组\t16\n7\t脉动器品牌\t/\t意大利LE20\n8\t脉动器规格型号\t/\tLE20\n9\t脉动器形式\t/\t电子\n10\t脉动器频率\t次/min\t60\n11\t脉动器比率\t％\t60\n12\t计量方式\t/\t电子\n13\t脱杯方式\t/\t自动","84200","冀2016T—142","2020-12-31","320000.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：承诺书过期；产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["畜牧机械","畜产品采集加工机械设备","挤奶机","14杯组及以上自动脱杯中置(鱼骨)式挤奶机","石家庄诺达机械设备有限公司","挤奶机","9JGD-14","形式:中置(鱼骨)式 ;杯组数:14组;脱杯方式:自动 ;","序号\t项目\t单位\t设计值（涵盖机型）\n1\t产品型号名称\t/\t9JGD-14挤奶机\n2\t形式\t/\t管道式\n3\t真空泵品牌\t/\t利拉伐\n4\t真空泵规格型号\t/\t2100L\n5\t真空泵台数\t台\t1\n6\t挤奶杯组数\t组\t14\n7\t脉动器品牌\t/\t意大利LE20\n8\t脉动器规格型号\t/\tLE20\n9\t脉动器形式\t/\t电子\n10\t脉动器频率\t次/min\t60\n11\t脉动器比率\t％\t60\n12\t计量方式\t/\t电子\n13\t脱杯方式\t/\t自动","84200","冀2016T—142","2020-12-31","300000.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：承诺书过期；产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["畜牧机械","畜产品采集加工机械设备","挤奶机","16杯组及以上自动脱杯并列(转盘)式挤奶机","北京国科诚泰农牧设备有限公司","智能挤奶机","9JZD-60","形式:并列(转盘)式 ;杯组数:60组;脱杯方式:自动 ;","转盘式；配套电机功率23Kw；真空泵型号SAC UNIPUMP2750数量2；脉动器型式SAC数量60；计量方式：电子计量。稳压罐不锈钢32升  2套、集乳器UNIFLOW容积430CC  60套、集乳罐不锈钢100升2套、奶泵8吨/小时 2套、清洗水槽不锈钢500升 1套。","120000","部20171265","2021-12-31","2000000.00","","通用类","北京市","评阅不通过","初评员：不通过","专家：承诺书过期；产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["畜牧机械","畜产品采集加工机械设备","挤奶机","16杯组及以上自动脱杯并列(转盘)式挤奶机","北京国科诚泰农牧设备有限公司","智能挤奶机","9JBD-48","形式:并列(转盘)式 ;杯组数:48组;脱杯方式:自动 ;","并列式；配套电机功率18Kw；真空泵型号SAC UNIPUMP4200数量2；脉动器型式SAC数量48；计量方式：电子计量。稳压罐不锈钢32升  1套、集乳器UNIFLOW容积430CC   48套、集乳罐不锈钢100升1套、奶泵8吨/小时 1套、清洗水槽不锈钢250升 1套。","120000","部20171264","2021-12-31","1500000.00","","通用类","北京市","评阅不通过","初评员：不通过","专家：承诺书过期；产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["水产机械","水产养殖机械","增氧机","普通型增氧机","上海义民电机有限公司","叶轮式增氧机","YL-1.5","普通型增氧机:是 ;","外形尺寸（直径×高）：Ф2050×715(mm)，整机质量：42kg，配套动力功率：1.5kW","310","GZNJ/TJ 2019-458","2025-03-19","1250.00","","非通用类","上海市","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["水产机械","水产养殖机械","增氧机","普通型增氧机","上海义民电机有限公司","叶轮式增氧机","YL-3.0","普通型增氧机:是 ;","外形尺寸（直径×高）：2500×600(mm)，整机质量：62kg，配套动力功率：3.0kW，额定转速：1450r/min","310","GZNJ/TJ 2019-387","2025-03-19","1550.00","","非通用类","上海市","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["水产机械","水产养殖机械","增氧机","普通型增氧机","上海义民电机有限公司","水车式增氧机","YC3-0.75","普通型增氧机:是 ;","电压:380V,频率:50HZ,额定功率:0.75KW增氧能力:2.4KG/H,动力效率:1.55KG/KW.H,净浮率:125%,质量:42KG,外形尺寸:1320X1300X440(MM)。","310","部20180847","2022-12-31","1750.00","","非通用类","上海市","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["水产机械","水产养殖机械","增氧机","普通型增氧机","上海义民电机有限公司","水车式增氧机","YC5-1.5","普通型增氧机:是 ;","电压:380V,频率:50HZ,额定功率:1.5KW增氧能力:2.4KG/H,动力效率:1.55KG/KW.H,净浮率:125%,质量:62KG,外形尺寸:1650X1520X440(MM)。","310","部20180848","2022-12-31","2100.00","","非通用类","上海市","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["水产机械","水产养殖机械","增氧机","普通型增氧机","金湖金龙祥渔业设备有限公司","叶轮式增氧机","ZY-3G","普通型增氧机:是 ;","型号ZY-3G,电机功率3.0KW,整机重量85KG,负荷水面7-12亩,动力效率≥1.5KG(KW·H),增氧能力≥4.5KG/H,噪声≤100DB(A),绝缘电阻>1MΩ,外形尺寸(直径*高)2700*900MM,浮体材料:塑料,浮体体积0.0461?,叶轮转速128R/MIN,叶轮直径650MM,叶片数12片,叶轮锥角118°","310","苏农机（2016）第（0496)号","2020-12-31","1280.00","","非通用类","江苏省","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["水产机械","水产养殖机械","增氧机","普通型增氧机","金湖金龙祥渔业设备有限公司","水车式增氧机","YC-1.5","普通型增氧机:是 ;","1、配套电机功率1.5kw，2、整机重量80kg，3、外形尺寸（长*宽*高）（2030*1770*889）mm，4、叶轮转速（水车转速）101r/min，5、叶轮（材料：塑料，直径φ638，叶轮数4只，叶片数4*8片），6、浮体（材料：塑料，体积0.058㎥，数量3只）","310","苏农机（2016）第（0164）号","2020-12-31","1280.00","","非通用类","江苏省","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["动力机械","拖拉机","轮式拖拉机","20-30马力两轮驱动拖拉机","邢台市同德机械有限公司","轮式拖拉机","XT200-B","功率:20马力;驱动方式:两轮驱动 ;","发动机功率：14.5KW  驱动方式:两轮驱动","5400","T201900430934","2024-12-30","19000.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019DFH015","河南省拖拉机柴油机产品质量监督检验中心","LT15GK0191","国家拖拉机质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","30-40马力两轮驱动拖拉机","雷沃重工股份有限公司","轮式拖拉机","M350-E","功率:35马力;驱动方式:两轮驱动 ;","驱动方式：两轮驱动；功率（kw）：25.8KW","7700","T201900510983","2024-12-30","33500.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","JW201701009","机械工业农业机械产品质量检测中心（济南）","W201109018-Ⅱ","山东省农业机械产品质量监督检验站"]
["动力机械","拖拉机","轮式拖拉机","30-40马力两轮驱动拖拉机","山东联诚农业装备有限公司","轮式拖拉机","LC350-A","功率:35马力;驱动方式:两轮驱动 ;","外廓尺寸：3180×1490×2360；轴距1900mm；常用轮距（前轮/后轮）：1135/1200；轮距（前轮/后轮）调整方式：伸缩套管/辐板或轮辋；最小使用质量：1490kg；标准配重（前/后）：30/160；档位数（前进/倒退/爬行）：8/2/0；主变速档位数*副变速档位数/其他档位数：4+1*2；发动机与离合器联接方式：直联；起动方式：电启动；翻倾防护装置（驾驶室或安全框架）：安全框架；前照灯型号：方形35W×12；转向系型式：全液压；行车制动系型式：机械、蹄式；驻车制动系型式：机械式；前驱动桥型式：旱地型；离合器型式：干式、单片、单作用；传动系动力输出轴离合器型式：干式、单片、单作用；传动系变速箱型式：机械平面组成式；主变速箱换挡型式：机械有级档；副变速箱换挡型式：机械有级档；轮胎型号（前轮/后轮）：6.00-16/11.2-28，选配5.00-15/11.2-24、6.50-16/11.2-28","7700","T202043430025","2025-04-09","27000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW201912021","山东省农业机械科学研究院产品质量检测中心","W201606118","机械工业农业机械产品质量检测中心（济南）"]
["动力机械","拖拉机","轮式拖拉机","40-50马力两轮驱动拖拉机","山东时风（集团）有限责任公司","轮式拖拉机","SF400-D","功率:40马力;驱动方式:两轮驱动 ;","大棚王扬动YD4R40V1国Ⅲ、风云机罩、前轮450-12后轮950-16、液压转向、 前防撞器、单层后配重。","10100","T201900220489","2024-12-30","33734.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。未提供翻倾防护装置强度检验与可靠性试验报告。","","","","",""]
["动力机械","拖拉机","轮式拖拉机","40-50马力两轮驱动拖拉机","山东时风（集团）有限责任公司","轮式拖拉机","SF400E","功率:40马力;驱动方式:两轮驱动 ;","江动\tJD4B4M2、国Ⅲ、风云Ⅱ机罩、前轮500-15后轮9.5-24、0.96m轮距、侧置变速、液压转向、双速输出（540/720）、便携前配、单层后配。","10100","部20170760","2021-12-31","33734.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW201909030-X01","山东省农业机械科学研究院产品质量检测中心","WJ201610106","机械工业农业机械产品质量检测中心（济南）"]
["动力机械","拖拉机","轮式拖拉机","40-50马力两轮驱动拖拉机","潍坊百利拖拉机有限公司","轮式拖拉机","400-B","功率:40马力;驱动方式:两轮驱动 ;","整机外廓尺寸（长×宽×高）：3350×1510×2200mm（安全架顶）；轴距：1750mm；整机型式：4×2两轮驱动；标准配重：前100kg/后400kg；发动机标定功率：29.5kW；轮胎型号：前轮6.50-16/后轮11.2-24；最小使用质量：1300kg。","10100","T201900320725","2024-12-30","36000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2020GFH022","河南省拖拉机柴油机产品质量监督检验中心","W201303050-Ⅱ","山东省农业机械产品质量监督检验站"]
["动力机械","拖拉机","轮式拖拉机","40-50马力两轮驱动拖拉机","潍坊百利拖拉机有限公司","轮式拖拉机","400-D","功率:40马力;驱动方式:两轮驱动 ;","整机外廓尺寸（长×宽×高）：3020×1450×2100mm（安全架顶）；轴距：1600mm；整机型式：4×2两轮驱动；标准配重：前100kg/后400kg；发动机标定功率：29.5kW；轮胎型号：前轮18.0/7.50-12/后轮13.8-20（后轮选装13.6-16）；最小使用质量：1300kg。","10100","T201900320723","2024-12-30","35000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2020GFH022","河南省拖拉机柴油机产品质量监督检验中心","W201303050-Ⅱ","山东省农业机械产品质量监督检验站"]
["动力机械","拖拉机","轮式拖拉机","40-50马力两轮驱动拖拉机","第一拖拉机股份有限公司","轮式拖拉机","SG400Y","功率:40马力;驱动方式:两轮驱动 ;","功率：29.4kw/40马力；驱动形式：两轮驱动","10100","T201900020205","2024-12-30","36000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH19GW1001","国家拖拉机质量监督检验中心","采信LT11GK0081","国家拖拉机质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","40-50马力两轮驱动拖拉机","江苏悦达智能农业装备有限公司","轮式拖拉机","黄海金马—400-C","功率:40马力;驱动方式:两轮驱动 ;","原：（黄海金马-400C）；发动机功率29.4千瓦；国三排放；两轮驱动；前进8个挡倒退2个挡；直联式干式单作用；液压转向；动力输出轴后置非独立式。","10100","T201900320748","2024-12-30","33800.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH19GW1062","国家拖拉机质量监督检验中心","(2013)委字01类第086号","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","40-50马力两轮驱动拖拉机","山东联诚农业装备有限公司","轮式拖拉机","LC400-A","功率:40马力;驱动方式:两轮驱动 ;","外廓尺寸：3180×1490×2360；轴距1900mm；常用轮距（前轮/后轮）：1135/1200；轮距（前轮/后轮）调整方式：伸缩套管/辐板或轮辋；最小使用质量：1490kg；标准配重（前/后）：30/160；档位数（前进/倒退/爬行）：8/2/0；主变速档位数*副变速档位数/其他档位数：4+1*2；发动机与离合器联接方式：直联；起动方式：电启动；翻倾防护装置（驾驶室或安全框架）：安全框架；前照灯型号：方形35W×12；转向系型式：全液压；行车制动系型式：机械、蹄式；驻车制动系型式：机械式；前驱动桥型式：旱地型；离合器型式：干式、单片、单作用；传动系动力输出轴离合器型式：干式、单片、单作用；传动系变速箱型式：机械平面组成式；主变速箱换挡型式：机械有级档；副变速箱换挡型式：机械有级档；轮胎型号（前轮/后轮）：6.00-16/11.2-28，选配5.00-15/11.2-24、6.50-16/11.2-28","10100","T202043430025","2025-04-09","35000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW201912021","山东省农业机械科学研究院产品质量检测中心","W201606118","机械工业农业机械产品质量检测中心（济南）"]
["动力机械","拖拉机","轮式拖拉机","40-50马力两轮驱动拖拉机","常力工贸有限公司","轮式拖拉机","CL400-D","功率:40马力;驱动方式:两轮驱动 ;","整机外廓尺寸（长×宽×高mm）:3120×1380×1850（安全框架顶部）；最小使用质量:1265 kg；配套动力（kW）:30；型式:两轮驱动；轴距（mm）:1560 ； 轮距（前轮/后轮）（mm）:960/910-1050 ； 最小离地间隙（mm）:240；变速箱前端面至后驱动轴轴心线的水平距离：891； 标准配重（kg）:0/240 ； 档位数（前进/倒退/爬行）: 8/2；变速箱型式:（4+1）×2组成式；轮胎型号（前轮/后轮）:5.00-12/9.50-16。","10100","T202043430012","2025-03-24","34000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2020CFH030","河南省拖拉机柴油机产品质量监督检验中心","(2019)2040110","潍坊市产品质量检验所"]
["动力机械","拖拉机","轮式拖拉机","40-50马力两轮驱动拖拉机","常力工贸有限公司","轮式拖拉机","CL450-D","功率:45马力;驱动方式:两轮驱动 ;","整机外廓尺寸（长×宽×高mm）:3120×1380×1850（安全框架顶部） ；最小使用质量:1275 ；配套动力（kW）:33.1；型式:两轮驱动；轴距（mm）:1560 ； 轮距（前轮/后轮）（mm）:960/910-1050； 最小离地间隙（mm）:230；变速箱前端面至后驱动轴轴心线的水平距离：891 ； 标准配重（kg）:0/240 ； 档位数（前进/倒退/爬行）: 8/2；变速箱型式:（4+1）×2组成式；轮胎型号（前轮/后轮）:5.00-12/9.50-16。","10100","T202043430012","2025-03-24","34500.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2020CFH030","河南省拖拉机柴油机产品质量监督检验中心","(2019)2040110","潍坊市产品质量检验所"]
["动力机械","拖拉机","轮式拖拉机","40-50马力两轮驱动拖拉机","山东山拖凯泰农业装备有限公司","轮式拖拉机","400-B","功率:40马力;驱动方式:两轮驱动 ;","型式：轮式；机架型式：无架；用途：一般用途；外廓尺寸(长×宽×高):3560×1600×2510（安全架顶部) MM；驱动型式:两驱；功率:40马力；轴距: 1955MM；最小离地间隙及部位：405 mm（牵引板底部）；轮距（前轮/后轮）：1235、1335/1210、1300；最小使用质量: 1460KG；标准配重质量(前/后)：80/120 KG；最小使用比质量（kg/kw）：49.5；档位数(前进/倒退):10/2；变速箱型式: 机械平面组成式；主变速档位数：5+1；副变速档位数：2 ；翻倾防护装置（驾驶室或安全框架）:型号KT1204A.46B.010,安全框架；轮胎型号（前轮/后轮）：6.00-16/11.2-24， 选装件轮胎型号（前轮/后轮）5.50-16、5.00-15/9.5-24、11.2-20","10100","T202037370120","2025-07-06","42000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW202003026","山东省农业机械科学研究院产品质量检测中心","W201502025-Ⅱ","山东省农业机械产品质量监督检验站"]
["动力机械","拖拉机","轮式拖拉机","40-50马力两轮驱动拖拉机","邢台市同德机械有限公司","轮式拖拉机","XT450-B","功率:45马力;驱动方式:两轮驱动 ;","发动机功率：33.1KW  驱动方式;两轮驱动","10100","T201900430044","2024-10-22","35350.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019HFH005","河南省拖拉机柴油机产品质量监督检验中心","(2019)  2040138","潍坊市产品质量检验所"]
["动力机械","拖拉机","轮式拖拉机","50-60马力两轮驱动拖拉机","江苏悦达智能农业装备有限公司","轮式拖拉机","黄海金马—500-C","功率:50马力;驱动方式:两轮驱动 ;","原：（黄海金马-500C);发动机功率36.8千瓦;国三排放；两轮驱动；前进8个挡倒退2个挡；直联式干式单作用；液压转向；动力输出轴后置非独立式.。","12000","T201900320746","2024-12-30","42000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH19GW1571","国家拖拉机质量监督检验中心","(2012)委字01类第120号","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","50-60马力两轮驱动拖拉机","潍坊红柳机械开发有限公司","轮式拖拉机","500A","功率:50马力;驱动方式:两轮驱动 ;","发动机标定功率：50马力；驱动方式:两轮驱动","12000","部20180578","2022-12-31","48500.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","W201101009","山东省农业机械产品质量监督检验站","W201401030-II","山东省农业机械产品质量检验站"]
["动力机械","拖拉机","轮式拖拉机","50-60马力两轮驱动拖拉机","潍坊红柳机械开发有限公司","轮式拖拉机","500D","功率:50马力;驱动方式:两轮驱动 ;","发动机标定功率：50马力；驱动方式：两轮驱动","12000","部20170214","2021-12-31","49000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","W201101009","山东省农业机械产品质量监督检验站","W201401030-II","山东省农业机械产品质量检验站"]
["动力机械","拖拉机","轮式拖拉机","50-60马力两轮驱动拖拉机","潍坊百利拖拉机有限公司","轮式拖拉机","500-E","功率:50马力;驱动方式:两轮驱动 ;","整机外廓尺寸（长×宽×高）：2850×1230×2100mm（安全架顶部）；轴距：1400mm；整机型式：4×2两轮驱动；标准配重：前0kg/后30kg；发动机标定功率：36.8kW；轮胎型号：前轮4.50-14/后轮9.5-20；最小使用质量：1400kg。","12000","T202032320015","2025-02-27","41000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW201910018","山东省农业机械科学研究院产品质量检测中心","2016KKX061","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","50-60马力两轮驱动拖拉机","江苏常发农业装备股份有限公司","轮式拖拉机","CFC500-A","功率:50马力;驱动方式:两轮驱动 ;","整机型式：轮式；整机机架型式：无架；整机驱动型式：两驱；外廓尺寸（长×宽×高）mm：3564×1495×2490；轴距mm：1808；轮距（前轮/后轮）mm：前轮1250、1350、1450、1550，后轮1210、1310、1426，选装后轮1210-1660；最小使用质量kg：1680；最大配重（前/后）kg：120/360；最小使用比质量kg/kw：45.7；档位数(前进/倒退)：16/16；主变速箱档位数：4；副变速档位数：2×（1+1）×2；发动机与主离合器联结方式：直联式；翻倾防护装置：安全框架；转向系型式：全液压转向；转向系转向操纵机构：方向盘；转向系转向机构型式：前轮转向；变速箱型式：机械平面组成式；主变速箱换挡方式：机械有级挡；副变速箱换挡方式：机械有级挡；轮胎型号：前轮6.00-16、5.50-16、5.00-15后轮11.2-28、12.4-24、11.2-24；轮胎数量：前轮2个/后轮2个","12000","T201900320604","2024-12-30","47000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","2011QT2068","农业部农业机械试验鉴定总站","（2005）委字01类第093号","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","50-60马力两轮驱动拖拉机","江苏常发农业装备股份有限公司","轮式拖拉机","CFC500B","功率:50马力;驱动方式:两轮驱动 ;","整机型式：轮式；整机机架型式：无架；整机驱动型式：两驱；外廓尺寸（长×宽×高）mm：3723×1515×2640或3723×1365×2640，选装宽1515-1770或1365-1515；轴距mm：1808；轮距（前轮/后轮）mm：前轮1210、1310、1410、1510或1000、1100、1200，后轮1200或1050，选装后轮1200-1456（无极调节）或1050-1200（无极调节）；最小使用质量kg：1915；标准配重kg：后配重180；最小使用比质量kg/kw：52；档位数（前进/倒退）：8/8；主变速档位数：4；副变速档位数：2×（1+1）；发动机与离合器联结方式：直联式；翻倾防护装置：安全框架；转向系型式：全液压转向；转向系转向操纵机构：方向盘；转向系转向机构型式：前轮转向；变速箱型式：机械平面组成式；主变速换挡方式：机械有级档；副变速换挡方式：机械有级档；轮胎型号：前轮5.50-16或6.00-16，后轮12.4-28或11.2-28；轮胎数量：前轮2个/后轮2个","12000","T201932320109","2024-12-30","45000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH20GW0401/FH20GW0411","国家拖拉机质量监督检验中心（洛阳西苑车辆与动力检验所有限公司）","（2017）委检字整机类第2050号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","50-60马力两轮驱动拖拉机","山东双力现代农业装备有限公司","轮式拖拉机","SL500-C","功率:50马力;驱动方式:两轮驱动 ;","驱动型式：两轮驱动；配套功率：50马力；","12000","T202000430291","2025-07-05","40200.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW202001001-X01","山东省农业机械科学研究院产品质量检测中心","2016KKX072","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","50-60马力两轮驱动拖拉机","山东双力现代农业装备有限公司","轮式拖拉机","SL500-B","功率:50马力;驱动方式:两轮驱动 ;","驱动型式：两轮驱动；配套功率：50马力；","12000","部20170207","2021-12-31","41000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","W201307009","山东省农业机械产品质量监督检验站","2016KKX072","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","50-60马力两轮驱动拖拉机","山东瑞泽重工有限公司","轮式拖拉机","RC500","功率:50马力;驱动方式:两轮驱动 ;","驱动方式：两轮驱动  功率:50马力","12000","鄂2020066","2025-05-13","50000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。承诺书版本过期；可靠性试验报告与所投产品型号不符。",""," HB2020FHZ108\t\t\t","湖北三智农业机械检测有限公司","NW2019015","山东省农业机械科学研究院产品质量检测中心"]
["动力机械","拖拉机","轮式拖拉机","50-60马力两轮驱动拖拉机","山东山拖凯泰农业装备有限公司","轮式拖拉机","500D","功率:50马力;驱动方式:两轮驱动 ;","型式：轮式；机架型式：无架；用途：园艺；外廓尺寸(长×宽×高): 3340×1420×2200（安全架顶部）MM；驱动型式:两驱；功率:50马力；轴距: 1840 MM；最小离地间隙及部位：250 mm（后桥底部）；轮距（前轮/后轮）：1030、1130、1230/1050～1150mm；最小使用质量: 1400 KG；标准配重质量(前/后)：48/24 KG；最小使用比质量（kg/kw）：38.0；档位数(前进/倒退): 8/2；变速箱型式:机械平面组成式；主变速档位数：4+1；副变速档位数：2；翻倾防护装置（驾驶室或安全框架）:型号KT904.46N.010 安全框架；轮胎型号（前轮/后轮）：4.50-12/9.50-20，","12000","T202000370251","2025-07-05","50000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW201909059-X01","山东省农业机械科学研究院产品质量检测中心","W201502029-Ⅱ","山东省农业机械产品质量监督检验站"]
["动力机械","拖拉机","轮式拖拉机","50-60马力两轮驱动拖拉机","山东山拖凯泰农业装备有限公司","轮式拖拉机","500-E","功率:50马力;驱动方式:两轮驱动 ;","型式：轮式；机架型式：无架；用途：一般用途；外廓尺寸(长×宽×高): 3640×1635×2430（安全架顶部）MM；驱动型式:两驱；功率:50马力；轴距:1930MM；最小离地间隙及部位：420 mm（后桥底部）；轮距（前轮/后轮）：1240、1340/1200～1430mm；最小使用质量: 1768KG；标准配重质量(前/后) ：64/92KG；最小使用比质量（kg/kw）：48；档位数(前进/倒退): 8/2；变速箱型式:机械平面组成式；主变速档位数：4+1；副变速档位数：2；翻倾防护装置（驾驶室或安全框架）: KT1204A.46B.010  安全框架；轮胎型号（前轮/后轮）：6.00-16/12.4-28， 选装件轮胎型号（前轮/后轮）：5.50-16、5.00-15/12.4-24、11.2-24、11.2-20；","12000","T202000370237","2025-07-05","51800.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW201909060-X01","山东省农业机械科学研究院产品质量检测中心","W201502027-Ⅱ","山东省农业机械产品质量监督检验站"]
["动力机械","拖拉机","轮式拖拉机","50-60马力两轮驱动拖拉机","山东山拖凯泰农业装备有限公司","轮式拖拉机","550-E","功率:55马力;驱动方式:两轮驱动 ;","型式：轮式；机架型式：无架；用途：一般用途；外廓尺寸(长×宽×高及部位):3575×1620×2420（安全架顶部）MM；驱动型式:两驱；功率: 55马力；轴距:1870 MM；最小离地间隙及部位：420 mm（后桥底部）；轮距（前轮/后轮）：1240、1340/1200～1430mm；最小使用质量: 1768KG；标准配重质量(前/后)：64/92 KG；最小使用比质量（kg/kw）：43.7；档位数(前进/倒退): 8/2；变速箱型式:机械平面组成式；主变速档位数：4+1；副变速档位数：2；翻倾防护装置（驾驶室或安全框架）: KT1204A.46B.010  安全框架；轮胎型号（前轮/后轮）：6.00-16/12.4-28 ，选装件轮胎型号（前轮/后轮）：5.50-16、5.00-15/12.4-24、11.2-24、11.2-20","12000","T202000370237","2025-07-05","57800.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW201909060-X01","山东省农业机械科学研究院产品质量检测中心","W201502027-Ⅱ","山东省农业机械产品质量监督检验站"]
["动力机械","拖拉机","轮式拖拉机","50-60马力两轮驱动拖拉机","常力工贸有限公司","轮式拖拉机","CL500-D","功率:50马力;驱动方式:两轮驱动 ;","整机外廓尺寸（长×宽×高mm）:3240×1380×1880（安全框架顶部）；最小使用质量:1400 kg；配套动力（kW）:36.8；型式:两轮驱动；轴距（mm）:1560 ； 轮距（前轮/后轮）（mm）:960/910-1050； 最小离地间隙（mm）:230；变速箱前端面至后驱动轴轴心线的水平距离：891 ； 标准配重（kg）:0/240 ； 档位数（前进/倒退/爬行）:8/2；变速箱型式:（4+1）×2组成式；轮胎型号（前轮/后轮）:5.00-12/9.50-16","12000","T202043430012","2025-03-24","40500.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2020CFH030","河南省拖拉机柴油机产品质量监督检验中心","(2019)2040110","潍坊市产品质量检验所"]
["动力机械","拖拉机","轮式拖拉机","50-60马力两轮驱动拖拉机","邢台市同德机械有限公司","轮式拖拉机","XT-550","功率:55马力;驱动方式:两轮驱动 ;","发动机功率：40.5KW  驱动方式：两轮驱动","12000","T201900430045","2024-10-22","42000.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019HFH005","河南省拖拉机柴油机产品质量监督检验中心","（2019）委检字整机类第2029号","盐城市农业机械实验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","50-60马力两轮驱动拖拉机","邢台市同德机械有限公司","轮式拖拉机","XT-500","功率:50马力;驱动方式:两轮驱动 ;","发动机功率：36.75KW  驱动方式;两轮驱动","12000","T201900430045","2024-10-22","41900.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019HFH005","河南省拖拉机柴油机产品质量监督检验中心","（2018）委检字整机类第2029号","盐城市农业机械实验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","60-70马力两轮驱动拖拉机","山东瑞泽重工有限公司","轮式拖拉机","RC600","功率:60马力;驱动方式:两轮驱动 ;","驱动方式：两轮驱动  功率：60马力","13200","鄂2020066","2025-05-13","55000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。承诺书版本过期。","","   HB2020FHZ108\t\t\t","湖北三智农业机械检测有限公司","NW2019015","山东省农业机械科学研究院产品质量检测中心"]
["动力机械","拖拉机","轮式拖拉机","60-70马力两轮驱动拖拉机","雷沃重工股份有限公司","轮式拖拉机","M600-B","功率:60马力;驱动方式:两轮驱动 ;","驱动方式：两轮驱动；功率（kw）：44.2KW","13200","T201900510987","2024-12-30","75000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","e13 79/622 2006/96 0149 00","莱茵集团","W201401163-Ⅱ","山东省农业机械产品质量监督检验站"]
["动力机械","拖拉机","轮式拖拉机","60-70马力两轮驱动拖拉机","江苏常发农业装备股份有限公司","轮式拖拉机","CFC600B","功率:60马力;驱动方式:两轮驱动 ;","整机型式：轮式；整机机架型式：无架；整机驱动型式：两驱；外廓尺寸（长×宽×高）mm：3723×1515×2640或3723×1365×2640，选装宽1515-1770或1365-1515；轴距mm：1808；轮距（前轮/后轮）mm：前轮1210、1310、1410、1510或1000、1100、1200，后轮1200或1050，选装后轮1200-1456（无极调节）或1050-1200（无极调节）；最小使用质量kg：1990；标准配重kg：后配重180；最小使用比质量kg/kw：45.1；档位数（前进/倒退）：8/8；主变速档位数：4；副变速档位数：2×（1+1）；发动机与离合器联结方式：直联式；翻倾防护装置：安全架；转向系型式：全液压转向；转向系转向操纵机构：方向盘；转向系转向机构型式：前轮转向；变速箱型式：机械平面组成式；主变速换挡方式：机械有级档；副变速换挡方式：机械有级档；轮胎型号：前轮5.50-16或6.00-16，后轮12.4-28或11.2-28；轮胎数量：前轮2个/后轮2个","13200","T201932320109","2024-12-30","47000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH20GW0401/FH20GW0411","国家拖拉机质量监督检验中心（洛阳西苑车辆与动力检验所有限公司）","（2017）委检字整机类第2050号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","60-70马力两轮驱动拖拉机","潍坊红柳机械开发有限公司","轮式拖拉机","600D","功率:60马力;驱动方式:两轮驱动 ;","发动机标定功率：60马力；驱动方式：两轮驱动","13200","部20170215","2021-12-31","54000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","W201101009","山东省农业机械产品质量监督检验站","W201401034-II","山东省农业机械产品质量检验站"]
["动力机械","拖拉机","轮式拖拉机","60-70马力两轮驱动拖拉机","潍坊红柳机械开发有限公司","轮式拖拉机","600A","功率:60马力;驱动方式:两轮驱动 ;","发动机标定功率：60马力；驱动方式：两轮驱动","13200","部20180575","2022-12-31","54000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","W201101009","山东省农业机械产品质量监督检验站","W201401034-II","山东省农业机械产品质量检验站"]
["动力机械","拖拉机","轮式拖拉机","60-70马力两轮驱动拖拉机","江苏沃得高新农业装备有限公司（原：江苏沃得植保机械有限公司、原：沃得重工（中国）有限公司）","轮式拖拉机","WE600","功率:60马力;驱动方式:两轮驱动 ;","标定功率：60马力（44.1kW）；驱动方式：两轮驱动；配套发动机型号：常柴4G33T-60G31E（国Ⅲ排放标准）；标定转速(r/min)：2400；外廓尺寸（长×宽×高）（mm）：3650×1572×2400（至安全架顶）/2460（至驾驶室顶）；轴距或履带接地长（mm）：1835；最小使用质量(kg)：1700（带安全架）/1890（带驾驶室）；发动机与主离合器联接方式：直联；变速箱（器）型式：机械平面组成式；轮胎型号（前轮/后轮）：6.5-16/13.6-28。","13200","T202032320097","2025-06-30","52000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","SAM2020019、SAM2020020","南京赛姆认证科技发展有限公司、南京赛姆认证科技发展有限公司","(2018)委字整机类第01801206557号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","60-70马力两轮驱动拖拉机","邢台市同德机械有限公司","轮式拖拉机","XT-600","功率:60马力;驱动方式:两轮驱动 ;","发动机功率：44.1KW 驱动方式：两轮驱动","13200","T201900430045","2024-10-22","46200.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019HFH005","河南省拖拉机柴油机产品质量监督检验中心","（2018）委检字整机类第2029号","盐城市农业机械实验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","70-80马力两轮驱动拖拉机","潍坊红柳机械开发有限公司","轮式拖拉机","700A","功率:70马力;驱动方式:两轮驱动 ;","发动机标定功率：70马力；驱动方式：两轮驱动","17300","部20180574","2022-12-31","67000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","W201101009","山东省农业机械产品质量监督检验站","W201401036-II","山东省农业机械产品质量检验站"]
["动力机械","拖拉机","轮式拖拉机","70-80马力两轮驱动拖拉机","潍坊红柳机械开发有限公司","轮式拖拉机","700C","功率:70马力;驱动方式:两轮驱动 ;","发动机标定功率：70马力；驱动方式：两轮驱动","17300","部20180576","2022-12-31","73500.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","W201101009","山东省农业机械产品质量监督检验站","W201401036-11","山东省农业机械产品质量检验站"]
["动力机械","拖拉机","轮式拖拉机","70-80马力两轮驱动拖拉机","第一拖拉机股份有限公司","轮式拖拉机","MF700G","功率:70马力;驱动方式:两轮驱动 ;","功率：51.5kw/70马力；驱动形式：两轮驱动","17300","部20171099","2021-12-31","58000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH19GW0991","国家拖拉机质量监督检验中心","WJ2017CKKX011","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","70-80马力两轮驱动拖拉机","第一拖拉机股份有限公司","轮式拖拉机","MK750","功率:75马力;驱动方式:两轮驱动 ;","功率：55.2kw/75马力；驱动形式：两轮驱动","17300","部20160173","2020-12-31","59000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。鉴定报告、可靠性试验报告与所投产品型号不符。","","FH13GW0111","国家拖拉机质量监督检验中心","LT13GK0231","国家拖拉机质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","70-80马力两轮驱动拖拉机","第一拖拉机股份有限公司","轮式拖拉机","MK750-1","功率:75马力;驱动方式:两轮驱动 ;","功率：55.2kw/75马力；驱动形式：两轮驱动","17300","部20160173","2020-12-31","61000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。鉴定报告及可靠性试验报告与所投产品型号不符。","","201520","国家拖拉机质量监督检验中心","LT13GK0231","国家拖拉机质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","70-80马力两轮驱动拖拉机","江苏常发农业装备股份有限公司","轮式拖拉机","CFC700B","功率:70马力;驱动方式:两轮驱动 ;","整机型式：轮式；整机机架型式：无架；整机驱动型式：两驱；外廓尺寸（长×宽×高）mm：3723×1515×2640或3723×1365×2640，选装宽1515-1770或1365-1515；轴距mm：1808；轮距（前轮/后轮）mm：前轮1210、1310、1410、1510或1000、1100、1200，后轮1200或1050，选装后轮1200-1456（无极调节）或1050-1200（无极调节）；最小使用质量kg：1990；标准配重kg：后配重180；最小使用比质量kg/kw：38.6；档位数（前进/倒退）：8/8；主变速档位数：4；副变速档位数：2×（1+1）；发动机与离合器联结方式：直联式；翻倾防护装置：安全架；转向系型式：全液压转向；转向系转向操纵机构：方向盘；转向系转向机构型式：前轮转向；变速箱型式：机械平面组成式；主变速换挡方式：机械有级档；副变速换挡方式：机械有级档；轮胎型号：前轮5.50-16或6.00-16，后轮12.4-28或11.2-28；轮胎数量：前轮2个/后轮2个","17300","T201932320109","2024-12-30","50500.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH20GW0401/FH20GW0411","国家拖拉机质量监督检验中心（洛阳西苑车辆与动力检验所有限公司）","（2017）委检字整机类第2050号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","70-80马力两轮驱动拖拉机","江苏常发农业装备股份有限公司","轮式拖拉机","CFC700-X","功率:70马力;驱动方式:两轮驱动 ;","整机型式：轮式；整机机架型式：无架；整机驱动型式：两驱；外廓尺寸（长×宽×高）mm：3530×1525×2570或3530×（1295-1771）×2570（至安全架顶），选装宽1525-1975；轴距mm：1808；轮距（前轮/后轮）mm：前轮1250、1350、1450、1550或1000、1100、1200，后轮1210、1310、1426或980-1456（无极调节），选装后轮1210-1660（无极调节）；最小使用质量kg：2080；标准配重kg：前配重120；最小使用比质量kg/kw：40.4；档位数（前进/倒退）：8/8，选装档位数（前进/倒退/爬行或运输）：8/8/16；主变速档位数：4；副变速档位数：2×（1+1），选装2×（1+1）×2；发动机与离合器联结方式：直联式；翻倾防护装置：安全框架；转向系型式：全液压转向；转向系转向操纵机构：方向盘；转向系转向机构型式：前轮转向；变速箱型式：机械平面组成式；主变速换挡方式：机械有级档；副变速换挡方式：机械有级档；轮胎型号（前轮/后轮）：5.50-16、5.00-15、6.00-16/12.4-28、11.2-24、12.4-24、11.2-28；轮胎数量（前轮/后轮）：2/2","17300","T202032320067","2025-05-28","51500.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH20GW0401/FH20GW0411","国家拖拉机质量监督检验中心（洛阳西苑车辆与动力检验所有限公司）","（2017）委检字整机类第2050号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","70-80马力两轮驱动拖拉机","江苏沃得高新农业装备有限公司（原：江苏沃得植保机械有限公司、原：沃得重工（中国）有限公司）","轮式拖拉机","WE700","功率:70马力;驱动方式:两轮驱动 ;","标定功率：70马力（51.5kW）；驱动方式：两轮驱动；配套发动机型号：常柴4L88-70G31E（国Ⅲ排放标准）；标定转速(r/min)：2400；外廓尺寸（长×宽×高）（mm）：3650×1572×2400（至安全架顶）/2460（至驾驶室顶）；轴距或履带接地长（mm）：1835；最小使用质量(kg)：1980（带安全架）/2170（带驾驶室）；发动机与主离合器联接方式：直联；变速箱（器）型式：机械平面组成式；轮胎型号（前轮/后轮）：6.5-16/13.6-28。","17300","T202032320097","2025-06-30","65000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","SAM2020019、SAM2020020","南京赛姆认证科技发展有限公司、南京赛姆认证科技发展有限公司","(2018)委字整机类第01801206557号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","80-90马力两轮驱动拖拉机","雷沃重工股份有限公司","轮式拖拉机","M800-A","功率:80马力;驱动方式:两轮驱动 ;","驱动方式：两轮驱动；功率（kw）：59KW","19400","T201900510985","2024-12-30","95000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW201908028","山东省农业机械科学研究院产品质量检测中心","W201109024-I","山东省农业机械产品质量监督检验站"]
["动力机械","拖拉机","轮式拖拉机","80-90马力两轮驱动拖拉机","江苏沃得高新农业装备有限公司（原：江苏沃得植保机械有限公司、原：沃得重工（中国）有限公司）","轮式拖拉机","WE800","功率:80马力;驱动方式:两轮驱动 ;","标定功率：80马力（58.8kW）；驱动方式：两轮驱动；配套发动机型号：常柴4L88-80G31C（国Ⅲ排放标准）；标定转速(r/min)：2400；外廓尺寸（长×宽×高）（mm）：3650×1572×2400（至安全架顶）/2460（至驾驶室顶）；轴距或履带接地长（mm）：1835；最小使用质量(kg)：2260（带安全架）/2350（带驾驶室）；发动机与主离合器联接方式：直联；变速箱（器）型式：机械平面组成式；轮胎型号（前轮/后轮）：6.5-16/13.6-28。","19400","T202032320097","2025-06-30","78000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","SAM2020019、SAM2020020","南京赛姆认证科技发展有限公司、南京赛姆认证科技发展有限公司","(2018)委字整机类第01801206557号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","90-100马力两轮驱动拖拉机","雷沃重工股份有限公司","轮式拖拉机","M900-D","功率:90马力;驱动方式:两轮驱动 ;","驱动方式：两轮驱动；功率（kw）：66.2KW","22300","T201900510986","2024-12-30","111200.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","W201606067","山东省农业机械产品质量监督检验站","W201210047-Ⅱ","山东省农业机械产品质量监督检验站"]
["动力机械","拖拉机","轮式拖拉机","90-100马力两轮驱动拖拉机","雷沃重工股份有限公司","轮式拖拉机","M900-DA","功率:90马力;驱动方式:两轮驱动 ;","驱动方式：两轮驱动；功率（kw）：66.2KW","22300","T201900510986","2024-12-30","84400.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","JW201701007","机械工业农业机械产品质量检测中心（济南）","W201210047-Ⅱ","山东省农业机械产品质量监督检验站"]
["动力机械","拖拉机","轮式拖拉机","90-100马力两轮驱动拖拉机","中联重机股份有限公司","轮式拖拉机","RC900-A","功率:90马力;驱动方式:两轮驱动 ;","功率：90马力；型式：4×2两轮驱动；","22300","T201900511010","2024-12-30","93200.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH13GW0091","国家拖拉机质量监督检验中心","W201401032-Ⅱ","山东省农业机械产品质量监督检验站"]
["动力机械","拖拉机","轮式拖拉机","100马力及以上两轮驱动拖拉机","中联重机股份有限公司","轮式拖拉机","RC1200-A","功率:120马力;驱动方式:两轮驱动 ;","功率：120马力；型式：4×2两轮驱动；","26900","T201900511010","2024-12-30","116800.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH12GW0301","国家拖拉机质量监督检验中心","W201401032-Ⅱ","山东省农业机械产品质量监督检验站"]
["动力机械","拖拉机","轮式拖拉机","100马力及以上两轮驱动拖拉机","山东双力现代农业装备有限公司","轮式拖拉机","SL1300-S","功率:130马力;驱动方式:两轮驱动 ;","驱动型式：两轮驱动；配套功率：130马力；","26900","T202000510315","2025-07-05","91500.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW201905012","山东省农业机械科学研究院产品质量检测中心","2016KKX075","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","100马力及以上两轮驱动拖拉机","山东双力现代农业装备有限公司","轮式拖拉机","SL1200-S","功率:120马力;驱动方式:两轮驱动 ;","驱动型式：两轮驱动；配套功率：120马力；","26900","T202000510315","2025-07-05","89700.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW201905012","山东省农业机械科学研究院产品质量检测中心","2016KKX075","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","100马力及以上两轮驱动拖拉机","江苏常发农业装备股份有限公司","轮式拖拉机","CFG1000-B","功率:100马力;驱动方式:两轮驱动 ;","整机型式：轮式；整机机架型式：无架；整机驱动型式：两驱；外廓尺寸（长×宽×高）mm：4705×2120×2856；轴距mm：2240；轮距（前轮/后轮）mm：前轮1550、1650、1750、1850，后轮1656、1688、1884、2088、；最小使用质量kg：3590；标准配重（前/后）kg：480/540；最小使用比质量kg/kw：48.8；档位数（前进/倒退）：12/12；主变速档位数：4；副变速档位数：3×（1+1）；发动机与离合器联结方式：直联式；翻倾防护装置：安全框架；转向系型式：全液压转向；转向系转向操纵机构：方向盘；转向系转向机构型式：前轮转向；变速箱型式：机械平面组成式；主变速换挡方式：机械有级档；副变速换挡方式：机械有级档；轮胎型号：前轮7.50-20，后轮16.9-34；轮胎数量：前轮2个/后轮2个","26900","T201900320605","2024-12-30","106000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","20110S2012","农业农村部农业机械试验鉴定总站","（2011）委字01类第119号","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","100马力及以上两轮驱动拖拉机","江苏常发农业装备股份有限公司","轮式拖拉机","CFG1100-B","功率:110马力;驱动方式:两轮驱动 ;","整机型式：轮式；整机机架型式：无架；整机驱动型式：两驱；外廓尺寸（长×宽×高）mm：4705×2120×2856；轴距mm：2240；轮距（前轮/后轮）mm：前轮1550、1650、1750、1850，后轮1656、1688、1884、2088、；最小使用质量kg：3600；标准配重（前/后）kg：480/540；最小使用比质量kg/kw：44.4；档位数（前进/倒退）：12/12；主变速档位数：4；副变速档位数：3×（1+1）；发动机与离合器联结方式：直联式；翻倾防护装置：安全框架；转向系型式：全液压转向；转向系转向操纵机构：方向盘；转向系转向机构型式：前轮转向；变速箱型式：机械平面组成式；主变速换挡方式：机械有级档；副变速换挡方式：机械有级档；轮胎型号：前轮7.50-20，后轮16.9-34；轮胎数量：前轮2个/后轮2个","26900","T201900320605","2024-12-30","109000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","20110S2012","农业农村部农业机械试验鉴定总站","（2013）委字01类第235号","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","100马力及以上两轮驱动拖拉机","江苏常发农业装备股份有限公司","轮式拖拉机","CFG1100-BJ","功率:110马力;驱动方式:两轮驱动 ;","整机型式：轮式；整机机架型式：无架；整机驱动型式：两驱；外廓尺寸（长×宽×高）mm：4705×2120×2924；轴距mm：2240；轮距（前轮/后轮）mm：前轮1550、1650、1750、1850，后轮1656、1688、1884、2088、；最小使用质量kg：3860；标准配重（前/后）kg：480/540；最小使用比质量kg/kw：47.7；档位数（前进/倒退）：12/12；主变速档位数：4；副变速档位数：3×（1+1）；发动机与离合器联结方式：直联式；翻倾防护装置：简易驾驶室；转向系型式：全液压转向；转向系转向操纵机构：方向盘；转向系转向机构型式：前轮转向；变速箱型式：机械平面组成式；主变速换挡方式：机械有级档；副变速换挡方式：机械有级档；轮胎型号：前轮7.50-20，后轮16.9-34；轮胎数量：前轮2个/后轮2个","26900","T201900320605","2024-12-30","116000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH20GW0351","国家拖拉机质量监督检验中心（洛阳西苑车辆与动力检验所有限公司）","（2013）委字01类第235号","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","100马力及以上两轮驱动拖拉机","江苏常发农业装备股份有限公司","轮式拖拉机","CFG1000-BJ","功率:100马力;驱动方式:两轮驱动 ;","整机型式：轮式；整机机架型式：无架；整机驱动型式：两驱；外廓尺寸（长×宽×高）mm：4705×2120×2924；轴距mm：2240；轮距（前轮/后轮）mm：前轮1550、1650、1750、1850，后轮1656、1688、1884、2088、；最小使用质量kg：3850；标准配重（前/后）kg：480/540；最小使用比质量kg/kw：52.4；档位数（前进/倒退）：12/12；主变速档位数：4；副变速档位数：3×（1+1）；发动机与离合器联结方式：直联式；翻倾防护装置：简易驾驶室；转向系型式：全液压转向；转向系转向操纵机构：方向盘；转向系转向机构型式：前轮转向；变速箱型式：机械平面组成式；主变速换挡方式：机械有级档；副变速换挡方式：机械有级档；轮胎型号：前轮7.50-20，后轮16.9-34；轮胎数量：前轮2个/后轮2个","26900","T201900320605","2024-12-30","113000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH20GW0351","国家拖拉机质量监督检验中心（洛阳西苑车辆与动力检验所有限公司）","（2011）委字01类第119号","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","100马力及以上两轮驱动拖拉机","雷沃重工股份有限公司","轮式拖拉机","M1200-DSA2","功率:120马力;驱动方式:两轮驱动 ;","驱动方式：两轮驱动；功率（kw）：88.2KW","26900","部20160045","2020-12-31","114000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","W201208013","山东省农业机械产品质量监督检验站","(2016)委检字整机类第0127号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","100马力及以上两轮驱动拖拉机","乐星农业装备（青岛）有限公司","轮式拖拉机","LS1000-1","功率:100马力;驱动方式:四轮驱动 ;","型式：4×2两轮驱动；用途：一般农用型；外廓尺寸（长×宽×高）4430×1980×2590mm；轴距：2345mm；轮距（前轮/后轮）：1572-1808/1532-1830mm；最小离地间隙：420mm（前桥）；最小使用质量：2992KG；档位数（前进/后退）：12/12；最大配重质量(前/后)：400/180KG；功率：73.5kw。","26900","T201900320614","2024-12-30","112000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH20GW0821","国家拖拉机质量监督检验中心（洛阳西苑车辆与动力检验所有限公司）","W090119","江西省农业机械产品质量监督检测中心，江西省农业机械产品质量监督检验一站"]
["动力机械","拖拉机","轮式拖拉机","100马力及以上两轮驱动拖拉机","山拖农机装备有限公司","轮式拖拉机","ME1200A","功率:120马力;驱动方式:两轮驱动 ;","外型尺寸（mm）：4360×2050×2850；\n驱动方式：两轮驱动\n功率（KW）:88.2（国三）\n轴距（mm）:2240\n最小使用质量（kg）:3915;\n轮距(前轮/后轮)（mm）;1540、1640、1740、1840/1490、1605、1700、1815、1890、2005;","26900","部20160136","2020-12-31","100900.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","W201508044、W201608032","山东省农业机械产品质量监督检验站、机械工业农业机械产品质量检测中心（济南）","W201210018-Ⅱ","山东省农业机械产品质量监督检验站"]
["动力机械","拖拉机","轮式拖拉机","100马力及以上两轮驱动拖拉机","江苏沃得高新农业装备有限公司（原：江苏沃得植保机械有限公司、原：沃得重工（中国）有限公司）","轮式拖拉机","WD1400-B1","功率:140马力;驱动方式:两轮驱动 ;","标定功率：140马力（103kW）；驱动方式：两轮驱动；配套发动机型号：一拖LR4M3LR23/1030（国Ⅲ排放标准）；标定转速(r/min)：2300；外廓尺寸（长×宽×高）（mm）：4440×2060×2760（至安全架顶）/2820（至驾驶室顶）；轴距或履带接地长（mm）：2207；最小使用质量(kg)：3940（带安全架）/4120（带驾驶室）；发动机与主离合器联接方式：直联；变速箱（器）型式：机械平面组成式；轮胎型号（前轮/后轮）：7.5-20/16.9-34。","26900","T202032320098","2025-06-30","115000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","SAM2020022、SAM2020023","南京赛姆认证科技发展有限公司、南京赛姆认证科技发展有限公司","(2018)委字整机类第01801206552号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","100马力及以上两轮驱动拖拉机","江苏沃得高新农业装备有限公司（原：江苏沃得植保机械有限公司、原：沃得重工（中国）有限公司）","轮式拖拉机","WD1300-B1","功率:130马力;驱动方式:两轮驱动 ;","标定功率：130马力（95.6kW）；驱动方式：两轮驱动；配套发动机型号：一拖LR4M3LR23/0956（国Ⅲ排放标准）；标定转速(r/min)：2300；外廓尺寸（长×宽×高）（mm）：4440×2060×2760（至安全架顶）/2820（至驾驶室顶）；轴距或履带接地长（mm）：2207；最小使用质量(kg)：3780（带安全架）/3960（带驾驶室）；发动机与主离合器联接方式：直联；变速箱（器）型式：机械平面组成式；轮胎型号（前轮/后轮）：7.5-20/16.9-34。","26900","T202032320098","2025-06-30","110000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","SAM2020022、SAM2020023","南京赛姆认证科技发展有限公司、南京赛姆认证科技发展有限公司","(2018)委字整机类第01801206552号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","100马力及以上两轮驱动拖拉机","江苏沃得高新农业装备有限公司（原：江苏沃得植保机械有限公司、原：沃得重工（中国）有限公司）","轮式拖拉机","WD1200-B1","功率:120马力;驱动方式:两轮驱动 ;","标定功率：120马力（88.2kW）；驱动方式：两轮驱动；配套发动机型号：一拖LR4A3LR23/0882（国Ⅲ排放标准）；标定转速(r/min)：2300；外廓尺寸（长×宽×高）（mm）：4440×2060×2760（至安全架顶）/2820（至驾驶室顶）；轴距或履带接地长（mm）：2207；最小使用质量(kg)：3780（带安全架）/3960（带驾驶室）；发动机与主离合器联接方式：直联；变速箱（器）型式：机械平面组成式；轮胎型号（前轮/后轮）：7.5-20/16.9-34。","26900","T202032320098","2025-06-30","105000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","SAM2020022、SAM2020023","南京赛姆认证科技发展有限公司、南京赛姆认证科技发展有限公司","(2018)委字整机类第01801206552号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","100马力及以上两轮驱动拖拉机","道依茨法尔机械有限公司","轮式拖拉机","CD1200-1","功率:120马力;驱动方式:四轮驱动 ;","整机驱动型式：两驱；发动机标定功率（kW）：88.2；最小使用质量（kg）：4000（安全架）、4100（驾驶室）；排放标准：第三阶段。","26900","T202000230176","2025-07-05","120000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH20GW0601/FH20GW0611","国家拖拉机质量监督检验中心","WJ2017CKKX006","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","30-40马力四轮驱动拖拉机","雷沃重工股份有限公司","轮式拖拉机","M354-E","功率:35马力;驱动方式:四轮驱动 ;","驱动方式：四轮驱动；功率（kw）：25.8KW","9700","T201900510988","2024-12-30","40200.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","W201603018","山东省农业机械产品质量监督检验站","W201109019-Ⅱ","山东省农业机械产品质量监督检验站"]
["动力机械","拖拉机","轮式拖拉机","30-40马力四轮驱动拖拉机","安徽天平机械股份有限公司","轮式拖拉机","354","功率:35马力;驱动方式:四轮驱动 ;","外廓尺寸(长×宽×高)：3090×1400×2050mm；轴距或履带接地长：1810mm；常用轮距(前轮/后轮)或轨距：1300/1300；轮距(前轮/后轮)调整方式：固定轮距式/翻转辐板可调轮距式；最小使用质量：1500kg；标准配重(前/后)：0/240kg；档位数(前进/倒退/爬行)：8/2/0；主变速档位数*副变速档位数/其他档位数：（4+1）*2/0；发动机与离合器联接方式：直联；起动方式：电起动；翻倾防护装置（驾驶室或安全框架）：安全框架；前照灯型号：ND140×90T-1；转向系型式：液压转向；行车制动系型式：干式、蹄式制动器，机械操纵；驻车制动系型式：锁定踏板式；前驱动桥型式；旱地型；离合器型式：单作用，单片、干式、常接合式；传动系动力输出轴离合器型式：双锥齿轮式/内置式，单级外啮合直齿圆柱齿轮式；传动系变速箱型式：二轴式、直齿（4+1）×2组成式；主变速箱换档方式：滑动齿轮换挡；副变速箱换档方式：啮合套换档；轮胎型号(前轮/后轮)：6.00-16/11.2-24","9700","2016TJ583","2020-12-31","38000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：不通过，可靠性试验报告与所投产品型号不符。","","FH16GW0261","国家拖拉机质量监督检验中心","LT16GK0131","国家拖拉机质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","30-40马力四轮驱动拖拉机","江苏常发农业装备股份有限公司","轮式拖拉机","CFC354-A","功率:35马力;驱动方式:四轮驱动 ;","整机型式：轮式；整机机架型式：无架；整机驱动型式：四驱；外廓尺寸（长×宽×高）mm：3564×1485×2440；轴距mm：1798；轮距（前轮/后轮）mm：前轮1210，后轮1100、1200、1300、1400，选装后轮1100-1640；最小使用质量kg：1730；最大配重（前/后）kg：80/180；最小使用比质量kg/kw：67.1；档位数(前进/倒退)：16/16；主变速箱档位数：4；副变速档位数：2×（2+1）×2；发动机与主离合器联结方式：直联式；翻倾防护装置：安全框架；转向系型式：全液压转向；转向系转向操纵机构：方向盘；转向系转向机构型式：前轮转向；变速箱型式：机械平面组成式；主变速箱换挡方式：机械有级挡；副变速箱换挡方式：机械有级挡；轮胎型号：前轮7.50-16、6.50-16、6.00-16/后轮13.6-24、11.2-28、12.4-24、11.2-24；轮胎数量：前轮2个/后轮2个","9700","T201900320603","2024-12-30","49500.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","2011QT2068","农业部农业机械试验鉴定总站","（2008）委字01类第046号","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","30-40马力四轮驱动拖拉机","山东联诚农业装备有限公司","轮式拖拉机","LC354-A","功率:35马力;驱动方式:四轮驱动 ;","外廓尺寸：3230×1490×2360；轴距1880mm；常用轮距（前轮/后轮）：1230/1200；轮距（前轮/后轮）调整方式：不可调/可调节；最小使用质量：1680kg；标准配重（前/后）：30/160；档位数（前进/倒退/爬行）：8/2/0；主变速档位数*副变速档位数/其他档位数：4+1*2；发动机与离合器联接方式：直联；起动方式：电启动；翻倾防护装置（驾驶室或安全框架）：安全框架；前照灯型号：方形35W×12；转向系型式：全液压；行车制动系型式：机械、蹄式；驻车制动系型式：机械式；前驱动桥型式：旱地型；离合器型式：干式、单片、单作用；传动系动力输出轴离合器型式：干式、单片、单作用；传动系变速箱型式：机械平面组成式；主变速箱换挡型式：机械有级档；副变速箱换挡型式：机械有级档；轮胎型号（前轮/后轮）：7.50-16/11.2-28，选配6.00-16/11.2-24、6.50-16/11.2-24","9700","T202043430024","2025-04-09","34000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW201912021","山东省农业机械科学研究院产品质量检测中心","W201606119","机械工业农业机械产品质量检测中心（济南）"]
["动力机械","拖拉机","轮式拖拉机","40-50马力四轮驱动拖拉机","江苏常发农业装备股份有限公司","轮式拖拉机","CFC404-A","功率:40马力;驱动方式:四轮驱动 ;","整机型式：轮式；整机机架型式：无架；整机驱动型式：四驱；外廓尺寸（长×宽×高）mm：3564×1515×2465；轴距mm：1798；轮距（前轮/后轮）mm：前轮1210，后轮1200、1300、1400，选装后轮1200-1640；最小使用质量kg：1740；最大配重（前/后）kg：80/180；最小使用比质量kg/kw：59；档位数(前进/倒退)：16/8；主变速箱档位数：4；副变速档位数：（2+1）×2；发动机与主离合器联结方式：直联式；翻倾防护装置：安全框架；转向系型式：全液压转向；转向系转向操纵机构：方向盘；转向系转向机构型式：前轮转向；变速箱型式：机械平面组成式；主变速箱换挡方式：机械有级挡；副变速箱换挡方式：机械有级挡；轮胎型号：前轮7.50-16、6.50-16、6.00-16/后轮13.6-24、11.2-28、12.4-24、11.2-24；轮胎数量：前轮2个/后轮2个","12300","T201900320603","2024-12-30","52500.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","2011QT2068","农业部农业机械试验鉴定总站","（2008）委字01类第047号","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","40-50马力四轮驱动拖拉机","江苏常发农业装备股份有限公司","轮式拖拉机","CFC454-A","功率:45马力;驱动方式:四轮驱动 ;","整机型式：轮式；整机机架型式：无架；整机驱动型式：四驱；外廓尺寸（长×宽×高）mm：3564×1526×2490；轴距mm：1798；轮距（前轮/后轮）mm：前轮1270，后轮1210、1310、1426，选装后轮1210-1660；最小使用质量kg：1820；最大配重（前/后）kg：120/360；最小使用比质量kg/kw：55；档位数(前进/倒退)：16/8；主变速箱档位数：4；副变速档位数：（2+1）×2；发动机与主离合器联结方式：直联式；翻倾防护装置：安全框架；转向系型式：全液压转向；转向系转向操纵机构：方向盘；转向系转向机构型式：前轮转向；变速箱型式：机械平面组成式；主变速箱换挡方式：机械有级挡；副变速箱换挡方式：机械有级挡；轮胎型号：前轮7.50-16/后轮11.2-28；轮胎数量：前轮2个/后轮2个","12300","T201900320603","2024-12-30","54000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","2011QT2068","农业部农业机械试验鉴定总站","（2006）委字01类第126号","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","40-50马力四轮驱动拖拉机","潍坊百利拖拉机有限公司","轮式拖拉机","404-B","功率:40马力;驱动方式:四轮驱动 ;","整机外廓尺寸（长×宽×高）：3350×1510×2200mm（安全架顶）；轴距：1800mm；整机型式：4×4四轮驱动；标准配重：：前100kg/后400kg；发动机标定功率：29.5kW；轮胎型号：前轮6.50-16/后轮11.2-24；最小使用质量：1400kg。","12300","T201900320726","2024-12-30","43200.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2020GFH022","河南省拖拉机柴油机产品质量监督检验中心","W201303051-Ⅱ","山东省农业机械产品质量监督检验站"]
["动力机械","拖拉机","轮式拖拉机","40-50马力四轮驱动拖拉机","潍坊百利拖拉机有限公司","轮式拖拉机","404-D","功率:40马力;驱动方式:四轮驱动 ;","整机外廓尺寸（长×宽×高）：3020×1450×2100mm（安全架顶）；轴距：1730mm；整机型式：4×4四轮驱动；标准配重：前100kg/后400kg；发动机标定功率：29.5kW；轮胎型号：前轮7.50-16/后轮13.8-20（后轮选装13.6-16）；最小使用质量：1400kg。","12300","T201900320724","2024-12-30","42200.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2020GFH022","河南省拖拉机柴油机产品质量监督检验中心","W201303051-Ⅱ","山东省农业机械产品质量监督检验站"]
["动力机械","拖拉机","轮式拖拉机","40-50马力四轮驱动拖拉机","安徽天平机械股份有限公司","轮式拖拉机","404","功率:40马力;驱动方式:四轮驱动 ;","外廓尺寸(长×宽×高)：3300×1600×2040mm；轴距或履带接地长：1810mm；常用轮距(前轮/后轮)或轨距：1300/1350；轮距(前轮/后轮)调整方式：固定轮距式/翻转辐板可调轮距式；最小使用质量：1635kg；标准配重(前/后)：90/230kg；档位数(前进/倒退/爬行)：8/2/0；主变速档位数*副变速档位数/其他档位数：（4+1）*2/0；发动机与离合器联接方式：直联；起动方式：电起动；翻倾防护装置（驾驶室或安全框架）：安全框架；前照灯型号：ND140×90T-1；转向系型式：液压转向；行车制动系型式：干式、蹄式制动器，机械操纵；驻车制动系型式：锁定踏板式；前驱动桥型式：旱地型；离合器型式：单作用，单片、干式、常接合式；传动系动力输出轴离合器型式：双锥齿轮式/内置式，单级外啮合直齿圆柱齿轮式；传动系变速箱型式：二轴式、直齿（4+1）×2组成式；主变速箱换档方式：滑动齿轮换挡；副变速箱换档方式：啮合套换档；轮胎型号(前轮/后轮)：7.50-16/11.2-28","12300","2016TJ584","2020-12-31","45000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：不通过，可靠性试验报告与所投产品型号不符。","","FH16GW0261","国家拖拉机质量监督检验中心","LT16GK0131","国家拖拉机质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","40-50马力四轮驱动拖拉机","安徽天平机械股份有限公司","轮式拖拉机","484","功率:48马力;驱动方式:四轮驱动 ;","外廓尺寸(长×宽×高)：3500×1600×2040mm；轴距或履带接地长：1955mm；常用轮距(前轮/后轮)或轨距：1300/1350；轮距(前轮/后轮)调整方式：固定轮距式/翻转辐板可调轮距式；最小使用质量：1820kg；标准配重(前/后)：91/240kg；档位数(前进/倒退/爬行)：8/2/0；主变速档位数*副变速档位数/其他档位数：（4+1）*2/0；发动机与离合器联接方式：直联；起动方式：电起动；翻倾防护装置（驾驶室或安全框架）：安全框架；前照灯型号：ND140×90T-1；转向系型式：液压转向；行车制动系型式：干式、双片盘式制动器；驻车制动系型式：锁定踏板式；前驱动桥型式：旱地型；离合器型式：单片、干式、常接合式；传动系动力输出轴离合器型式：双锥齿轮式/内置式，单级外啮合直齿圆柱齿轮式；传动系变速箱型式：二轴式、直齿（4+1）×2组成式；主变速箱换档方式：滑动齿轮换挡；副变速箱换档方式：啮合套换档；轮胎型号(前轮/后轮)：7.50-16/11.2-28","12300","2016TJ586","2020-12-31","52000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：不通过，可靠性试验报告与所投产品型号不符。","","FH16GW0261","国家拖拉机质量监督检验中心","LT16GK0141","国家拖拉机质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","40-50马力四轮驱动拖拉机","山东时风（集团）有限责任公司","轮式拖拉机","SF404-D","功率:40马力;驱动方式:四轮驱动 ;","大棚王扬动YD4R40V1,29.4KW，国Ⅲ、风云机罩、前轮600-12后轮950-16、液压转向、 前防撞器、单层后配重、安全架","12300","T201900220490","2024-12-30","41082.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。未提供翻倾防护装置强度检验与可靠性试验报告。","","","","",""]
["动力机械","拖拉机","轮式拖拉机","40-50马力四轮驱动拖拉机","山东五征集团有限公司","轮式拖拉机","NA404","功率:40马力;驱动方式:四轮驱动 ;","功率：40马力；驱动型式：四驱；外廓尺寸（长×宽×高及部位）：3095×1440×2050mm（安全架顶）；离合器壳体前端面至后驱动轴轴心线的水平距离：1027mm；最小使用质量：1410kg；翻倾防护装置型式：安全框架；转向系型式：全液压；变速箱（器）型式：机械平面组成式；主变速换挡方式：机械有级档；副变速换挡方式：机械有级档；悬挂装置型式：后置三点悬挂","12300","T201937370188","2024-12-23","45300.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW201907004","山东省农业机械科学研究院产品质量检测中心","NW201708035","山东省农业机械科学研究院产品质量检测中心"]
["动力机械","拖拉机","轮式拖拉机","40-50马力四轮驱动拖拉机","江苏悦达智能农业装备有限公司","轮式拖拉机","黄海金马—404-C","功率:40马力;驱动方式:四轮驱动 ;","原：（黄海金马-404C)；发动机功率29.4千瓦;国三排放；四轮驱动；前进8个挡倒退2个挡；直联式干式单作用/双作用；液压转向；动力输出轴后置非独立式。","12300","T201900320749","2024-12-30","41500.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH19GW1062","国家拖拉机质量监督检验中心","(2013)委字01类第079号","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","40-50马力四轮驱动拖拉机","英轩重工有限公司","轮式拖拉机","YX404-B1","功率:40马力;驱动方式:四轮驱动 ;","驱动方式：四轮驱动；功率(KW)：29.5KW","12300","T201932320056","2024-12-01","45300.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019IFH021","河南省拖拉机柴油机产品质量监督检验中心","(2016)委字整机类第012010223号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","40-50马力四轮驱动拖拉机","山东联诚农业装备有限公司","轮式拖拉机","LC404-A","功率:40马力;驱动方式:四轮驱动 ;","外廓尺寸：3230×1490×2360；轴距1940mm；常用轮距（前轮/后轮）：1230/1200；轮距（前轮/后轮）调整方式：不可调/可调节；最小使用质量：1680kg；标准配重（前/后）：30/160；档位数（前进/倒退/爬行）：8/2/0；主变速档位数*副变速档位数/其他档位数：4+1*2；发动机与离合器联接方式：直联；起动方式：电启动；翻倾防护装置（驾驶室或安全框架）：安全框架；前照灯型号：方形35W×12；转向系型式：全液压；行车制动系型式：机械、蹄式；驻车制动系型式：机械式；前驱动桥型式：旱地型；离合器型式：干式、单片、单作用；传动系动力输出轴离合器型式：干式、单片、单作用；传动系变速箱型式：机械平面组成式；主变速箱换挡型式：机械有级档；副变速箱换挡型式：机械有级档；轮胎型号（前轮/后轮）：7.50-16/11.2-28，选配6.00-16/11.2-24、6.50-16/11.2-24","12300","T202043430024","2025-04-09","43000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW201912021","山东省农业机械科学研究院产品质量检测中心","W201606119","机械工业农业机械产品质量检测中心（济南）"]
["动力机械","拖拉机","轮式拖拉机","40-50马力四轮驱动拖拉机","常力工贸有限公司","轮式拖拉机","CL454-A","功率:45马力;驱动方式:四轮驱动 ;","外廓尺寸（长×宽×高mm）:3300×1300×1900(安全框架)；最小使用质量:1400(安全框架)kg；配套动力（kW）:33.1；型式:四轮驱动；轴距（mm）:1750； 轮距（前轮/后轮）（mm）:1060、1280/910-1050； 最小离地间隙（mm）:230； 标准配重（kg）:42/60； 档位数（前进/倒退/爬行）: 8/2；变速箱型式:（4+1）×2组成式；轮胎型号（前轮/后轮）:6.00-12/9.50-16","12300","T201943430032","2024-09-29","42000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019IFH018","河南省拖拉机柴油机产品质量监督检验中心","（2019）2040109","潍坊市产品质量检验所"]
["动力机械","拖拉机","轮式拖拉机","40-50马力四轮驱动拖拉机","常力工贸有限公司","轮式拖拉机","CL454","功率:45马力;驱动方式:四轮驱动 ;","外廓尺寸（长×宽×高mm）:3600×1500×2100安全框架顶部、3600×1500×2300(驾驶室吊装环)；最小使用质量:1525（安全框架)、1675(驾驶室)kg；配套动力（kW）:33.1；型式:四轮驱动；轴距（mm）:1835； 轮距（前轮/后轮）（mm）:1100、1200、1300/1060-1200； 最小离地间隙（mm）:320； 标准配重（kg）:42/70； 档位数（前进/倒退/爬行）: 8/2；变速箱型式:（4+1）×2组成式；轮胎型号（前轮/后轮）:7.50-16/11.2-24。","12300","T201943430031","2024-09-29","43000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019IFH018/WJ2019IFH019","河南省拖拉机柴油机产品质量监督检验中心","（2019）2040107","潍坊市产品质量检验所"]
["动力机械","拖拉机","轮式拖拉机","40-50马力四轮驱动拖拉机","常力工贸有限公司","轮式拖拉机","CL404-A","功率:40马力;驱动方式:四轮驱动 ;","外廓尺寸（长×宽×高mm）:3300×1300×1900(安全框架)；最小使用质量:1400kg；配套动力（kW）:30；型式:四轮驱动；轴距（mm）:1750； 轮距（前轮/后轮）（mm）:1060、1280/910-1050； 最小离地间隙（mm）:230； 标准配重（kg）:42/60； 档位数（前进/倒退/爬行）:8/2；变速箱型式:（4+1）×2组成式；轮胎型号（前轮/后轮）:6.00-12/9.50-16","12300","T201943430032","2024-09-29","41500.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019IFH018","河南省拖拉机柴油机产品质量监督检验中心","（2019）2040109","潍坊市产品质量检验所"]
["动力机械","拖拉机","轮式拖拉机","40-50马力四轮驱动拖拉机","常力工贸有限公司","轮式拖拉机","CL404","功率:40马力;驱动方式:四轮驱动 ;","外廓尺寸（长×宽×高mm）:3600×1500×2100(安全框架)、3600×1500×2300(驾驶室吊装环)；最小使用质量:1550(安全框架)、1680(驾驶室)kg；配套动力（kW）:30；型式:四轮驱动；轴距（mm）:1800； 轮距（前轮/后轮）（mm）:1100、1200、1300/1060-1200； 最小离地间隙（mm）:320； 标准配重（kg）:42/70； 档位数（前进/倒退/爬行）:8/2；变速箱型式:（4+1）×2组成式；轮胎型号（前轮/后轮）:7.50-16/11.2-24。","12300","T201943430031","2024-09-29","42000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019IFH018/WJ2019IFH019","河南省拖拉机柴油机产品质量监督检验中心","（2019）2040107","潍坊市产品质量检验所"]
["动力机械","拖拉机","轮式拖拉机","40-50马力四轮驱动拖拉机","山东山拖凯泰农业装备有限公司","轮式拖拉机","404-B","功率:40马力;驱动方式:四轮驱动 ;","型式：轮式；机架型式：无架；用途：一般用途；外廓尺寸(长×宽×高):3438×1640×2430（安全架顶部）MM；驱动型式:四驱；功率: 40马力；轴距:1935 MM；最小离地间隙及部位：340 mm（前驱动桥下部）；轮距（前轮/后轮）：1200/1210、1300mm；最小使用质量: 1670KG；标准配重质量(前/后) KG；最小使用比质量（kg/kw）：56.6；档位数(前进/倒退): 10/2；变速箱型式: 机械平面组成式；主变速档位数：5+1；副变速档位数：2；翻倾防护装置（驾驶室或安全框架）:型号KT1204A.46B.010,安全框架；轮胎型号（前轮/后轮）：6.50-16/11.2-24，选装件轮胎型号（前轮/后轮）6.00-16/11.2-20、9.5-24","12300","T202037370121","2025-07-06","47800.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW202003026","山东省农业机械科学研究院产品质量检测中心","W201502026-Ⅱ","山东省农业机械产品质量监督检验站"]
["动力机械","拖拉机","轮式拖拉机","40-50马力四轮驱动拖拉机","潍坊米基林农业机械有限公司","轮式拖拉机","404-H","功率:40马力;驱动方式:四轮驱动 ;","结构尺寸（长×宽×高mm）:2950×1220×1960；最小使用质量（kg）:1350；轴距（mm）:1510； 轮距（前轮/后轮）（mm）:960/1100；；选装轮距（前轮/后轮）（mm）:960、1000/960、1100 ； 最小离地间隙（mm）: 245（ 前桥放油螺栓）;最大配重（kg）:100/180； 档位数（前进/倒退/爬行）:8/2 ；变速箱型式:（4+1）×2组成式；轮胎型号（前轮/后轮）:6.00-12/9.5-16；","12300","T202043430026","2025-04-09","41300.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，未提供翻倾防护装置强度检验及可靠性试验报告。","","","","",""]
["动力机械","拖拉机","轮式拖拉机","50-60马力四轮驱动拖拉机","英轩重工有限公司","轮式拖拉机","YX504-B1","功率:50马力;驱动方式:四轮驱动 ;","驱动方式：四轮驱动；功率(KW)：36.8KW","15200","T201932320056","2024-12-01","58600.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019IFH021","河南省拖拉机柴油机产品质量监督检验中心","(2016)委字整机类第012010223号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","50-60马力四轮驱动拖拉机","江苏悦达智能农业装备有限公司","轮式拖拉机","黄海金马—504-C","功率:50马力;驱动方式:四轮驱动 ;","原：（黄海金马-504C）；发动机功率36.8千瓦;国三排放；四轮驱动；前进8个挡倒退2个挡;直联式干式单作用/双作用，液压转向；动力输出轴后置非独立式","15200","T201900320747","2024-12-30","51800.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH19GW1571","国家拖拉机质量监督检验中心","(2012)委字01类第121号","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","50-60马力四轮驱动拖拉机","江苏悦达智能农业装备有限公司","轮式拖拉机","YCX504D","功率:50马力;驱动方式:四轮驱动 ;","发动机功率36.8千瓦；国三排放；外廓尺寸(长×宽×高)mm：2880×1250×2120；园艺用途四轮驱动拖拉机；前进8个挡倒退2个挡；直联式干式单作用,液压转向；动力输出轴后置非独立式,","15200","T201932320095","2024-12-30","50800.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH19GW1551","国家拖拉机质量监督检验中心","YH2019WJ01175","江苏沿海农业机械检测有限公司"]
["动力机械","拖拉机","轮式拖拉机","50-60马力四轮驱动拖拉机","山东巨明机械有限公司","轮式拖拉机","JM554","功率:55马力;驱动方式:四轮驱动 ;","发动机标定功率：40.5kW；型式：四轮驱动；外廓尺寸（长×宽×高）：3950×1800×2600mm；轴距：2000mm；最小离地间隙：370mm；最小使用质量：2630kg；最大配重（前/后）：120/360kg；档位数（前进/倒退/爬行）：12/12/0；最大牵引力：≥13.6kN；变速箱型式：4×3×（1+1）组成式；翻倾防护装置：驾驶室；悬挂装置型式：后置三点悬挂。","15200","部20190461","2023-12-31","62000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2018FFH017","河南省拖拉机柴油机产品质量监督检验中心","WJ2017FKKX036","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","50-60马力四轮驱动拖拉机","山东五征集团有限公司","轮式拖拉机","NS504","功率:50马力;驱动方式:四轮驱动 ;","功率：50马力；整机驱动型式：四驱；外廓尺寸（长×宽×高及部位）：3470×1500×2499mm（安全架顶）；离合器壳体前端面至后驱动轴轴心线的水平距离：1130mm；最小使用质量：1680kg；翻倾防护装置：安全框架；转向系型式：全液压；变速箱（器）型式：机械平面组成式；主变速换挡方式：机械有级档；副变速换挡方式：机械有级档；悬挂装置型式：后置三点悬挂","15200","T201900370884","2024-12-30","59300.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW201907048；NW201907004","山东省农业机械科学研究院产品质量检测中心","NO201701063","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","50-60马力四轮驱动拖拉机","第一拖拉机股份有限公司","轮式拖拉机","SG504Y","功率:50马力;驱动方式:四轮驱动 ;","功率：36.8kw/50马力；驱动形式：四轮驱动","15200","T202000410277","2025-07-05","52000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH19GW1001","国家拖拉机质量监督检验中心","LT12GK0181","国家拖拉机质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","50-60马力四轮驱动拖拉机","山东悍沃农业装备有限公司","轮式拖拉机","504-C","功率:50马力;驱动方式:四轮驱动 ;","整机外廓尺寸（长×宽×高）：3500×1500×2700mm（驾驶室顶部）/3500×1500×2200mm（安全架顶部）；轴距：1850mm；整机型式：4×4四轮驱动；标准配重：前72kg/后56kg；发动机标定功率：36.8kW；轮胎型号：前轮7.50-16/后轮12.4-28；最小使用质量：1800kg（驾驶室）/1600kg（安全架）。","15200","T202032320019","2025-02-27","54000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019KFH006/WJ2019KFH005","河南省拖拉机柴油机产品质量监督检验中心","YH2019WJ01025","江苏沿海农业机械检测有限公司"]
["动力机械","拖拉机","轮式拖拉机","50-60马力四轮驱动拖拉机","潍坊红柳机械开发有限公司","轮式拖拉机","504D","功率:50马力;驱动方式:四轮驱动 ;","发动机标定功率：50马力；驱动方式：四轮驱动","15200","部20170214","2021-12-31","51000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","W201101009","山东省农业机械产品质量监督检验站","W201401031-II","山东省农业机械产品质量检验站"]
["动力机械","拖拉机","轮式拖拉机","50-60马力四轮驱动拖拉机","潍坊红柳机械开发有限公司","轮式拖拉机","504A","功率:50马力;驱动方式:四轮驱动 ;","发动机标定功率：50马力；驱动方式：四轮驱动","15200","部20180578","2022-12-31","51000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","W201101009","山东省农业机械产品质量监督检验站","W201401031-II","山东省农业机械产品质量检验站"]
["动力机械","拖拉机","轮式拖拉机","50-60马力四轮驱动拖拉机","雷沃重工股份有限公司","轮式拖拉机","M554-B","功率:55马力;驱动方式:四轮驱动 ;","驱动方式：四轮驱动；功率（kw）：40.5KW","15200","T201900510989","2024-12-30","72000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","W201606070","山东省农业机械产品质量监督检验站","W2010-293-Ⅱ","山东省农业机械产品质量监督检验站"]
["动力机械","拖拉机","轮式拖拉机","50-60马力四轮驱动拖拉机","雷沃重工股份有限公司","轮式拖拉机","M554-BA","功率:55马力;驱动方式:四轮驱动 ;","驱动方式：四轮驱动；功率（kw）：40.5KW","15200","T201900510989","2024-12-30","65000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","W201606069","山东省农业机械产品质量监督检验站","W2010-293-Ⅱ","山东省农业机械产品质量监督检验站"]
["动力机械","拖拉机","轮式拖拉机","50-60马力四轮驱动拖拉机","安徽天平机械股份有限公司","轮式拖拉机","554","功率:55马力;驱动方式:四轮驱动 ;","外廓尺寸(长×宽×高)：3500×1635×2380mm；轴距或履带接地长：1955mm；常用轮距(前轮/后轮)或轨距：1300/1300；轮距(前轮/后轮)调整方式：固定轮距式/翻转辐板可调轮距式；最小使用质量：1960kg；标准配重(前/后)：91/80kg；档位数(前进/倒退/爬行)：8/2/0；主变速档位数*副变速档位数/其他档位数：（4+1）*2/0；发动机与离合器联接方式：直联；起动方式：电起动；翻倾防护装置（驾驶室或安全框架）：安全框架；前照灯型号：ND140×90T-1；转向系型式：液压转向；行车制动系型式：干式、双片盘式制动器；驻车制动系型式：锁定踏板式；前驱动桥型式：旱地型；离合器型式：单片、干式、常接合式；传动系动力输出轴离合器型式：双锥齿轮式/内置式，单级外啮合直齿圆柱齿轮式；传动系变速箱型式：二轴式、直齿（4+1）×2组成式；主变速箱换档方式：滑动齿轮换挡；副变速箱换档方式：啮合套换档；轮胎型号(前轮/后轮)：8.3-20/12.4-28","15200","2017TJ738","2021-12-31","60000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：不通过，未提供翻倾防护装置强度检验报告与可靠性试验报告。","","","","",""]
["动力机械","拖拉机","轮式拖拉机","50-60马力四轮驱动拖拉机","安徽天平机械股份有限公司","轮式拖拉机","JH504","功率:50马力;驱动方式:四轮驱动 ;","外廓尺寸(长×宽×高)：3490×1660×2580mm；轴距或履带接地长：1860mm；常用轮距(前轮/后轮)或轨距：1300/1300；轮距(前轮/后轮)调整方式：有级可调/有级可调；最小使用质量：1850kg；标准配重(前/后)：70/160kg；档位数(前进/倒退/爬行)：8/2/0；主变速档位数*副变速档位数/其他档位数：（4+1）*2/0；发动机与离合器联接方式：直联；起动方式：电起动；翻倾防护装置（驾驶室或安全框架）：安全框架；前照灯型号：ND140×90T-1；转向系型式：前轮液压转向；行车制动系型式：机械操纵、盘式制动器；驻车制动系型式：机械操纵、盘式制动器；前驱动桥型式：旱地型 水田型；离合器型式：单片、干式、单作用、常接合；传动系动力输出轴离合器型式：圆锥齿轮/内置式、单级直齿圆柱齿轮；传动系变速箱型式：（4+1）×2机械组成式；主变速箱换档方式：滑动齿轮换挡；副变速箱换档方式：啮合套换档；轮胎型号(前轮/后轮)：8.3-20/12.4-28","15200","2019TJ161","2023-12-31","58000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：不通过，可靠性试验报告与所投产品型号不符。","","FH16GW0261","国家拖拉机质量监督检验中心","NJJC20180712","山东宝鼎农业机械检查有限公司"]
["动力机械","拖拉机","轮式拖拉机","50-60马力四轮驱动拖拉机","山东瑞泽重工有限公司","轮式拖拉机","RC554","功率:55马力;驱动方式:四轮驱动 ;","驱动方式：四轮驱动  功率：55马力","15200","T202000430099","2025-03-31","60000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。承诺书版本过期；可靠性试验报告与所投产品型号不符。",""," NW201909017\t\t\t","山东省农业机械科学研究院产品质量检测中心","WJ2018DKKX002","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","50-60马力四轮驱动拖拉机","山东瑞泽重工有限公司","轮式拖拉机","RD504-A","功率:50马力;驱动方式:四轮驱动 ;","驱动方式：四轮驱动 功率：50马力","15200","鄂2020065","2025-05-13","50000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。承诺书版本过期；可靠性试验报告与所投产品型号不符。",""," HB2020FHZ108\t\t\t","湖北三智农业机械检测有限公司","W201301077-II","山东省农业机械产品质量监督检验站"]
["动力机械","拖拉机","轮式拖拉机","50-60马力四轮驱动拖拉机","潍坊百利拖拉机有限公司","轮式拖拉机","504-E","功率:50马力;驱动方式:四轮驱动 ;","整机外廓尺寸（长×宽×高）：2850×1230×2100mm（安全架顶部）；轴距：1500mm；整机型式：4×4四轮驱动；标准配重：前0kg/后50kg；发动机标定功率：36.8kW；轮胎型号：前轮6.00-14/后轮9.5-20；最小使用质量：1430kg。","15200","T202032320016","2025-02-27","55000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW201910018","山东省农业机械科学研究院产品质量检测中心","2016KKX062","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","50-60马力四轮驱动拖拉机","江苏常发农业装备股份有限公司","轮式拖拉机","CFC504-A","功率:50马力;驱动方式:四轮驱动 ;","整机型式：轮式；整机机架型式：无架；整机驱动型式：四驱；外廓尺寸（长×宽×高）mm：3564×1526×2490；轴距mm：1798；轮距（前轮/后轮）mm：前轮1270，后轮1210、1310、1426，选装后轮1210-1660；最小使用质量kg：1820；最大配重（前/后）kg：120/360；最小使用比质量kg/kw：49.5；档位数(前进/倒退)：16/8；主变速箱档位数：4；副变速档位数：（2+1）×2；发动机与主离合器联结方式：直联式；翻倾防护装置：安全框架；转向系型式：全液压转向；转向系转向操纵机构：方向盘；转向系转向机构型式：前轮转向；变速箱型式：机械平面组成式；主变速箱换挡方式：机械有级挡；副变速箱换挡方式：机械有级挡；轮胎型号：7.50-16、6.50-16、6.00-16/后轮13.6-24、11.2-28、12.4-24、11.2-24；轮胎数量：前轮2个/后轮2个","15200","T201900320603","2024-12-30","55500.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","2011QT2068","农业部农业机械试验鉴定总站","（2005）委字01类第093号","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","50-60马力四轮驱动拖拉机","江苏常发农业装备股份有限公司","轮式拖拉机","CFC504B","功率:50马力;驱动方式:四轮驱动 ;","整机型式：轮式；整机机架型式：无架；整机驱动型式：四驱；外廓尺寸（长×宽×高）mm：3713×1615×2640或3713×1365×2640，选装宽1515-1975或1365-1515；轴距mm：1798；轮距（前轮/后轮）mm：前轮1300或1050、1100、1200，后轮1300或1050，选装后轮1200-1660（无极调节）或1050-1200（无极调节）；最小使用质量kg：2065；标准配重kg：后配重180；最小使用比质量kg/kw：56.1；档位数（前进/倒退）：8/8；主变速档位数：4；副变速档位数：2×（1+1）；发动机与离合器联结方式：直联式；翻倾防护装置：安全架；转向系型式：全液压转向；转向系转向操纵机构：方向盘；转向系转向机构型式：前轮转向；变速箱型式：机械平面组成式；主变速换挡方式：机械有级档；副变速换挡方式：机械有级档；轮胎型号：前轮8.3-20或7.50-16，后轮12.4-28或11.2-28或12.4/11-28；轮胎数量：前轮2个/后轮2个","15200","T201932320110","2024-12-30","53000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH20GW0401/FH20GW0411","国家拖拉机质量监督检验中心（洛阳西苑车辆与动力检验所有限公司）","（2017）委检字整机类第2051号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","50-60马力四轮驱动拖拉机","江苏常发农业装备股份有限公司","轮式拖拉机","CFD554-A","功率:55马力;驱动方式:四轮驱动 ;","整机型式：轮式；整机机架型式：无架；整机驱动型式：四驱；外廓尺寸（长×宽×高）mm：3642×1820×2610或3642×1820×2520；轴距mm：2100；轮距（前轮/后轮）mm：前轮1410、1510、1610、1710，后轮1300、1400、1500、1600、1700；最小使用质量kg：2420（安全架）/2640（驾驶室）；标准配重（前/后）kg：160/360；最小使用比质量kg/kw：59.8（安全架）/65.2（驾驶室）；档位数（前进/倒退）：12/12；主变速档位数：4；副变速档位数：3×（1+1）；发动机与离合器联结方式：直联式；翻倾防护装置：安全架，选装简易驾驶室；转向系型式：全液压转向；转向系转向操纵机构：方向盘；转向系转向机构型式：前轮转向；变速箱型式：机械平面组成式；主变速换挡方式：机械有级档；副变速换挡方式：机械有级档；轮胎型号：前轮8.3-24，后轮14.9-28；轮胎数量：前轮2个/后轮2个","15200","T201900320599","2024-12-30","79000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","20190S2004/FH14GW0451","农业农村部农业机械试验鉴定总站/国家拖拉机质量监督检验中心","（2007）委字01类第016号","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","50-60马力四轮驱动拖拉机","山东双力现代农业装备有限公司","轮式拖拉机","SL504-C","功率:50马力;驱动方式:四轮驱动 ;","驱动型式：四轮驱动；配套功率：50马力；","15200","T202000430290","2025-07-05","51000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW202001001-X01","山东省农业机械科学研究院产品质量检测中心","2016KKX073","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","50-60马力四轮驱动拖拉机","山东山拖凯泰农业装备有限公司","轮式拖拉机","504D-1","功率:50马力;驱动方式:四轮驱动 ;","型式：轮式；机架型式：无架；用途：园艺；外廓尺寸(长×宽×高):3370×1550×2300  （安全架顶部）MM；驱动型式:四驱；功率: 50马力；轴距:1860MM；最小离地间隙及部位：250 mm（前桥底部）；轮距（前轮/后轮）：1070/1030～1110mm；最小使用质量:1570 KG；标准配重质量(前/后)：48/24KG；最小使用比质量（kg/kw）：42.7；档位数(前进/倒退):8/2；变速箱型式:机械平面组成式；主变速档位数：4+1；副变速档位数：2；翻倾防护装置（驾驶室或安全框架）:型号KT904.46N.010 安全框架；轮胎型号（前轮/后轮）：6.00-16/13.8-20   选装件轮胎型号（前轮/后轮）6.00-12/9.5-24；","15200","T202000370239","2025-07-05","56000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW201909059-X01","山东省农业机械科学研究院产品质量检测中心","W201502030-Ⅱ","山东省农业机械产品质量监督检验站"]
["动力机械","拖拉机","轮式拖拉机","50-60马力四轮驱动拖拉机","山东山拖凯泰农业装备有限公司","轮式拖拉机","504-E","功率:50马力;驱动方式:四轮驱动 ;","型式：轮式；机架型式：无架；用途：一般用途；外廓尺寸(长×宽×高): 3565×1595×2395（安全架）MM；驱动型式:四驱；功率:50马力；轴距:1860MM；最小离地间隙及部位：300 mm（前桥底部）；轮距（前轮/后轮）：1200、1285/1200～1430mm；最小使用质量:1790 KG；标准配重质量(前/后)：64/92 KG；最小使用比质量（kg/kw）：48.6；档位数(前进/倒退):8/2；变速箱型式:机械平面组成式；主变速档位数：4+1；副变速档位数：2；翻倾防护装置（驾驶室或安全框架）:KT1204A.46B.010，安全框架；轮胎型号（前轮/后轮）：7.50-16/12.4-28， 选装件轮胎型号（前轮/后轮）6.50-16、6.00-16/12.4-24、11.2-24、11.2-20","15200","T202000370238","2025-07-05","54800.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW201909060-X01","山东省农业机械科学研究院产品质量检测中心","W201502028-Ⅱ","山东省农业机械产品质量监督检验站"]
["动力机械","拖拉机","轮式拖拉机","50-60马力四轮驱动拖拉机","山东山拖凯泰农业装备有限公司","轮式拖拉机","554-E","功率:55马力;驱动方式:四轮驱动 ;","型式：轮式；机架型式：无架；用途：一般用途；外廓尺寸(长×宽×高及部位):3625×1630×2400（安全架顶部）MM；驱动型式: 四驱；功率: 55马力；轴距:1935 MM；最小离地间隙及部位：300 mm（前桥底部）；轮距（前轮/后轮）：1295、1375/1150～1430mm；最小使用质量:1898 KG；标准配重质量(前/后)：64/92 KG；最小使用比质量（kg/kw）：46.9；档位数(前进/倒退): 8/2；变速箱型式:机械平面组成式；主变速档位数：4+1；副变速档位数：2；翻倾防护装置（驾驶室或安全框架）: KT1204A.46B.010，安全框架；轮胎型号（前轮/后轮）：7.50-16/12.4-28，选装件轮胎型号（前轮/后轮）6.50-16、6.00-16/12.4-24、11.2-24、11.2-20","15200","T202000370238","2025-07-05","59800.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW201909060-X01","山东省农业机械科学研究院产品质量检测中心","W201502028-Ⅱ","山东省农业机械产品质量监督检验站"]
["动力机械","拖拉机","轮式拖拉机","50-60马力四轮驱动拖拉机","道依茨法尔机械有限公司","轮式拖拉机","SH554-C","功率:55马力;驱动方式:四轮驱动 ;","驱动轮数：四轮驱动；发动机标定功率（kW）：40.5；最小使用质量（kg）:2540；排放标准：第三阶段。","15200","T201900220502","2024-12-30","76000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。未提供翻倾防护装置强度检验及可靠性试验报告。","","","","",""]
["动力机械","拖拉机","轮式拖拉机","50-60马力四轮驱动拖拉机","道依茨法尔机械有限公司","轮式拖拉机","SH504-C","功率:50马力;驱动方式:四轮驱动 ;","驱动轮数：四轮驱动；发动机标定功率（kW）：36.8；最小使用质量（kg）:2315；排放标准：第三阶段。","15200","T201900220501","2024-12-30","66000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。未提供翻倾防护装置强度检验及可靠性试验报告。","","","","",""]
["动力机械","拖拉机","轮式拖拉机","50-60马力四轮驱动拖拉机","常力工贸有限公司","轮式拖拉机","CL504-A","功率:50马力;驱动方式:四轮驱动 ;","整机外廓尺寸（长×宽×高mm）:3290×1295×1955(安全框架)；最小使用质量:1435(安全框架)kg；配套动力（kW）:36.8；型式:四轮驱动；轴距（mm）:1750； 轮距（前轮/后轮）（mm）:1060、1280/910-1050； 最小离地间隙（mm）:230；变速箱前端面至后驱动轴轴心线的水平距离：900； 标准配重（kg）:42/60； 档位数（前进/倒退/爬行）: 8/2；变速箱型式:（4+1）×2组成式；轮胎型号（前轮/后轮）:6.00-12/9.50-16","15200","T201900430035","2024-10-22","51000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019IFH018","河南省拖拉机柴油机产品质量监督检验中心","（2019）2040109","潍坊市产品质量检验所"]
["动力机械","拖拉机","轮式拖拉机","50-60马力四轮驱动拖拉机","常力工贸有限公司","轮式拖拉机","CL554-1","功率:55马力;驱动方式:四轮驱动 ;","整机外廓尺寸3330×1410×2000(安全框架顶部)；最小使用质量:1560kg；配套动力（kW）:40.5；型式:四轮驱动；轴距（mm）:1750； 轮距（前轮/后轮）（mm）:980、1060/910-1060； 最小离地间隙（mm）:265；变速箱前端面至后驱动轴轴心线的水平距离：965； 标准配重（kg）:0/120； 档位数（前进/倒退/爬行）: 8/2；变速箱型式:（4+1）×2组成式；轮胎型号（前轮/后轮）:6.00-14/9.50-20。液压油泵型号：CBN-F316；液压悬挂系统型式：分置式","15200","T202000430098","2025-03-31","51500.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2020CFH030","河南省拖拉机柴油机产品质量监督检验中心","(2019)2040109","潍坊市产品质量检验所"]
["动力机械","拖拉机","轮式拖拉机","50-60马力四轮驱动拖拉机","常力工贸有限公司","轮式拖拉机","CL504-5","功率:50马力;驱动方式:四轮驱动 ;","整机外廓尺寸（长×宽×高mm）:3860×1500×2540防翻架 ；最小使用质量:1839 kg；配套动力（kW）:36.8；型式:四轮驱动；轴距（mm）:1840 ； 轮距（前轮/后轮）（mm）:1200、1400/1200、1270、1340； 最小离地间隙（mm）:380；变速箱前端面至后驱动轴轴心线的水平距离：1057 ； 标准配重（kg）:96/160 ； 档位数（前进/倒退/爬行）: 8/2；变速箱型式:（4+1）×2组成式；轮胎型（前轮/后轮）:7.50-16/11.2-28。","15200","T202043430010","2025-03-24","52000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019KFH014","河南省拖拉机柴油机产品质量监督检验中心","(2019)2240075","潍坊市产品质量检验所"]
["动力机械","拖拉机","轮式拖拉机","50-60马力四轮驱动拖拉机","常力工贸有限公司","轮式拖拉机","CL554-5","功率:55马力;驱动方式:四轮驱动 ;","整机外廓尺寸（长×宽×高mm）:3850×1474×2540防翻架；最小使用质量:1899 kg；配套动力（kW）:41；型式:四轮驱动；轴距（mm）:1840； 轮距（前轮/后轮）（mm）:1210、1410/1200、1270、1340； 最小离地间隙（mm）:380；变速箱前端面至后驱动轴轴心线的水平距离：1057； 标准配重（kg）:96/160 ； 档位数（前进/倒退/爬行）: 8/2；变速箱型式:（4+1）×2组成式；轮胎型号（前轮/后轮）:7.50-16/11.2-28。","15200","T202043430010","2025-03-24","53000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019KFH014","河南省拖拉机柴油机产品质量监督检验中心","(2019)2240075","潍坊市产品质量检验所"]
["动力机械","拖拉机","轮式拖拉机","50-60马力四轮驱动拖拉机","潍坊东科重工农业装备有限公司","轮式拖拉机","DK504A","功率:50马力;驱动方式:四轮驱动 ;","外廓尺寸：3650×1650×2300；驱动型式：四轮驱动；配套功率：36.8kW; 发动机型号及制造商：4DW91-50GAG3U,一汽解放汽车有限公司无锡柴油机厂；轴距：1880; 最小使用质量：1700; 配重：144/360; 档位数：8+2; 变速箱型式：(4+1)×2组成式；是否有驾驶室或安全架：有安全架。","15200","鄂2019385","2024-09-27","54500.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019HFH031","河南省拖拉机柴油机产品质量监督检验中心","(2017)委字整机类第0170100428号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","50-60马力四轮驱动拖拉机","山东联发野迪农业装备有限公司","轮式拖拉机","504-X","功率:50马力;驱动方式:四轮驱动 ;","标定功率：36.8kw;驱动方式：四轮驱动；外廓尺寸：3300x1620x2350mm（安全架）；轴距：1850mm；轮距（前轮/后轮）：1200、1300/1200、1300mm；常用轮距（前轮/后轮）1300/1300mm；轮距（前轮/后轮）调整方式：有级可调/有级可调；最小离地间隙：330mm；最小使用质量：1700kg；标准配重（前/后）：45/55kg；档位数（前进/倒退/爬行）：8/2/0；主变速挡位数：（4+1）副变速档位数：2；发动机与离合器联接方式：直联；起动方式：电启动。","15200","T201900220528","2024-12-30","50700.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019IFH032","河南省拖拉机柴油机产品质量监督检验中心   ","WJ2018DKKX029","河南省拖拉机柴油机产品质量监督检验中心   "]
["动力机械","拖拉机","轮式拖拉机","50-60马力四轮驱动拖拉机","潍坊米基林农业机械有限公司","轮式拖拉机","504-H","功率:50马力;驱动方式:四轮驱动 ;","结构尺寸（长×宽×高mm）:2950×1220×1960 安全架顶；最小使用质量（kg）:1400；轴距（mm）:1510； 轮距（前轮/后轮）（mm）:960/1100；；选装轮距（前轮/后轮）（mm）:960、1000/960、1100 ； 最小离地间隙（mm）:245（前桥放油螺栓） ;最大配重（kg）:100/180； 档位数（前进/倒退/爬行）:8/2 ；变速箱型式:（4+1）×2组成式；轮胎型号（前轮/后轮）:6.00-12/9.5-16","15200","T202043430026","2025-04-09","53000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，未提供翻倾防护装置强度检验及可靠性试验报告。","","","","",""]
["动力机械","拖拉机","轮式拖拉机","50-60马力四轮驱动拖拉机","潍坊米基林农业机械有限公司","轮式拖拉机","504-N","功率:50马力;驱动方式:四轮驱动 ;","结构尺寸（长×宽×高mm）:3350×1480×2580驾驶室顶部3350×1480×2360安全架顶部；最小使用质量（kg）:1600（驾驶室）1600安全架；轴距（mm）:1880； 轮距（前轮/后轮）（mm）:1200/1230；；选装轮距（前轮/后轮）（mm）:1200、1300/1230、1330 ； 最小离地间隙（mm）:325前桥底部 ;最大配重（kg）:60/56； 档位数（前进/倒退/爬行）:8/2 ；变速箱型式:（4+1）×2 组成式；轮胎型号（前轮/后轮）:7.50-16/11.2-24","15200","T202000430095","2025-03-31","54400.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，未提供翻倾防护装置强度检验及可靠性试验报告。","","","","",""]
["动力机械","拖拉机","轮式拖拉机","50-60马力四轮驱动拖拉机","邢台市同德机械有限公司","轮式拖拉机","XT-504","功率:50马力;驱动方式:四轮驱动 ;","发动机功率：36.75KW  驱动方式：四轮驱动","15200","T201900430046","2024-10-22","53300.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019DFH016","河南省拖拉机柴油机产品质量监督检验中心","（2018）委检字整机类第2027号","盐城市农业机械实验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","50-60马力四轮驱动拖拉机","山东乐地农业装备有限公司","轮式拖拉机","LD504D","功率:50马力;驱动方式:四轮驱动 ;","外廓尺寸(长×宽×高)mm:2980×1315×2065（安全架顶）；轴距或履带接地长:1515mm；\n常用轮距(前轮/后轮)或轨距:1110/1150mm；最小使用质量:1456kg；标准配重（前/后）：28/64kg； 档位数：前进/倒退/爬行：8/2/0；主变速器档位数：4+1；副变速器档位数/其他档位数：2","15200","T201900430952","2024-12-30","51000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW202006049","山东省农业机械科学研究院产品质量检测中心","NJJC20181008-BK","山东宝鼎农业机械检测有限公司"]
["动力机械","拖拉机","轮式拖拉机","60-70马力四轮驱动拖拉机","江苏常发农业装备股份有限公司","轮式拖拉机","CFD604-A","功率:60马力;驱动方式:四轮驱动 ;","整机型式：轮式；整机机架型式：无架；整机驱动型式：四驱；外廓尺寸（长×宽×高）mm：3642×1820×2610或3642×1820×2520；轴距mm：2100；轮距（前轮/后轮）mm：前轮1250、1350、1450、1550，后轮1300、1400、1500、1600；最小使用质量kg：2420（安全架）/2640（驾驶室）；标准配重（前/后）kg：160/360；最小使用比质量kg/kw：54.9（安全架）/59.9（驾驶室）；档位数（前进/倒退）：12/12；主变速档位数：4；副变速档位数：3×（1+1）；发动机与离合器联结方式：直联式；翻倾防护装置：安全架，选装简易驾驶室；转向系型式：全液压转向；转向系转向操纵机构：方向盘；转向系转向机构型式：前轮转向；变速箱型式：机械平面组成式；主变速换挡方式：机械有级档；副变速换挡方式：机械有级档；轮胎型号：前轮8.3-24，后轮14.9-28；轮胎数量：前轮2个/后轮2个","17000","T201900320599","2024-12-30","81000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","20190S2004/FH14GW0451","农业农村部农业机械试验鉴定总站/国家拖拉机质量监督检验中心","（2011）委字01类第116号","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","60-70马力四轮驱动拖拉机","江苏常发农业装备股份有限公司","轮式拖拉机","CFC604B","功率:60马力;驱动方式:四轮驱动 ;","整机型式：轮式；整机机架型式：无架；整机驱动型式：四驱；外廓尺寸（长×宽×高）mm：3713×1615×2640或3713×1365×2640，选装宽1515-1975或1365-1515；轴距mm：1798；轮距（前轮/后轮）mm：前轮1300或1050、1100、1200，后轮1300或1050，选装后轮1200-1660（无极调节）或1050-1200（无极调节）；最小使用质量kg：2140；标准配重kg：后配重180；最小使用比质量kg/kw：48.5；档位数（前进/倒退）：8/8；主变速档位数：4；副变速档位数：2×（1+1）；发动机与离合器联结方式：直联式；翻倾防护装置：安全架；转向系型式：全液压转向；转向系转向操纵机构：方向盘；转向系转向机构型式：前轮转向；变速箱型式：机械平面组成式；主变速换挡方式：机械有级档；副变速换挡方式：机械有级档；轮胎型号：前轮8.3-20或7.50-16，后轮12.4-28或11.2-28或12.4/11-28；轮胎数量：前轮2个/后轮2个","17000","T201932320110","2024-12-30","56000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH20GW0401/FH20GW0411","国家拖拉机质量监督检验中心（洛阳西苑车辆与动力检验所有限公司）","（2017）委检字整机类第2051号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","60-70马力四轮驱动拖拉机","山东瑞泽重工有限公司","轮式拖拉机","RC604","功率:60马力;驱动方式:四轮驱动 ;","驱动方式：四轮驱动  功率：60马力","17000","T202000430099","2025-03-31","65000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。承诺书版本过期；可靠性试验报告与所投产品型号不符。","","NW201909017\t\t\t","山东省农业机械科学研究院产品质量检测中心","WJ2018DKKX002","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","60-70马力四轮驱动拖拉机","山东时风（集团）有限责任公司","轮式拖拉机","SF604-B","功率:60马力;驱动方式:四轮驱动 ;","驱动方式：四轮驱动，4D27ZT32/604，功率：44.2kW，浙江新柴股份有限公司，第三阶段。","17000","T202000370245","2025-07-05","56780.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","防翻架：NW201910026，驾驶室：NW201910024","山东省农业机械科学研究院产品质量检测中心","WJ2018IKKX020","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","60-70马力四轮驱动拖拉机","雷沃重工股份有限公司","轮式拖拉机","M604-BA","功率:60马力;驱动方式:四轮驱动 ;","驱动方式：四轮驱动；功率（kw）：44.2KW","17000","T201900510989","2024-12-30","77900.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","W201606069","山东省农业机械产品质量监督检验站","W2010-293-Ⅱ","山东省农业机械产品质量监督检验站"]
["动力机械","拖拉机","轮式拖拉机","60-70马力四轮驱动拖拉机","河北铠特农业机械有限公司","轮式拖拉机","KT654","功率:65马力;驱动方式:四轮驱动 ;","发动机标定功率:48KW,标定转速2400R/MIN；驱动方式:四轮驱动.","17000","T201900320739","2024-12-30","66000.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过，未提供翻倾防护装置强度检验及可靠性试验报告。","","","","",""]
["动力机械","拖拉机","轮式拖拉机","60-70马力四轮驱动拖拉机","雷沃重工股份有限公司","轮式拖拉机","M604-B","功率:60马力;驱动方式:四轮驱动 ;","驱动方式：四轮驱动；功率（kw）：44.2KW","17000","T201900510989","2024-12-30","85000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","W201606070","山东省农业机械产品质量监督检验站","W2010-293-Ⅱ","山东省农业机械产品质量监督检验站"]
["动力机械","拖拉机","轮式拖拉机","60-70马力四轮驱动拖拉机","潍坊红柳机械开发有限公司","轮式拖拉机","604A","功率:60马力;驱动方式:四轮驱动 ;","发动机标定功率：60马力；驱动方式：四轮驱动","17000","部20180575","2022-12-31","57000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","W201101009","山东省农业机械产品质量监督检验站","W201401035-II","山东省农业机械产品质量监督检验站"]
["动力机械","拖拉机","轮式拖拉机","60-70马力四轮驱动拖拉机","潍坊红柳机械开发有限公司","轮式拖拉机","604D","功率:60马力;驱动方式:四轮驱动 ;","发动机标定功率：60马力；驱动方式：四轮驱动","17000","部20170215","2021-12-31","57000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","W201101009","山东省农业机械产品质量监督检验站","W201401035-II","山东省农业机械产品质量检验站"]
["动力机械","拖拉机","轮式拖拉机","60-70马力四轮驱动拖拉机","山东悍沃农业装备有限公司","轮式拖拉机","604-F","功率:60马力;驱动方式:四轮驱动 ;","整机外廓尺寸（长×宽×高）：3600×1500×2700mm（驾驶室顶部）/3600×1500×2200mm（安全架顶部）；轴距：1950mm；整机型式：4×4四轮驱动；标准配重：前72kg/后56kg；发动机标定功率：44.1kW；轮胎型号：前轮8.3-20/后轮12.4-28；最小使用质量：2000kg（驾驶室）/1800kg（安全架）。","17000","T202032320019","2025-02-27","59500.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019KFH006/WJ2019KFH005","河南省拖拉机柴油机产品质量监督检验中心","YH2019WJ01025","江苏沿海农业机械检测有限公司"]
["动力机械","拖拉机","轮式拖拉机","60-70马力四轮驱动拖拉机","山拖农机装备有限公司","轮式拖拉机","NS604-C","功率:60马力;驱动方式:四轮驱动 ;","外型尺寸（mm）：3410×1430×2240；\n驱动方式：四轮驱动;\n功率（KW）:44.1（国三）;\n轴距（mm）:1860;\n最小使用质量（kg）:1680；\n轮距(前轮/后轮)mm：1040、1200/1050、1200、1300；\n标准配重(前/后)kg:48/72;\n挡位数(前进/倒退):10/10;\n转向系型式：全液压；\n最小使用比质量kg/kW:38.10;\n主变速箱换档方式:机械有级挡;\n轮胎型号(前轮/后轮):6.00-12/13.8-20；6.00-12（水田）/8.3-24（水田）；6.00-16/9.5-24；6.50-16/13.8-20；6.50-16/11.2-24；6.50-16/9.5-28；7.00-12/13.6-16；7.50-16/11.2-28；7.50-16/13.6-24；8.3-20/12.4-28；8.3-20/13.6-28","17000","T201900370866","2024-12-30","63300.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","W201608256","机械工业农业机械产品质量检测中心（济南）","W201308065-Ⅱ","山东省农业机械产品质量监督检验站"]
["动力机械","拖拉机","轮式拖拉机","60-70马力四轮驱动拖拉机","山东五征集团有限公司","轮式拖拉机","NS604","功率:60马力;驱动方式:四轮驱动 ;","功率：60马力；整机驱动型式：四驱；外廓尺寸（长×宽×高及部位）：3470×1500×2499mm（安全架顶）；离合器壳体前端面至后驱动轴轴心线的水平距离：1130mm；最小使用质量：1730kg；翻倾防护装置：安全框架；转向系型式：全液压；变速箱（器）型式：机械平面组成式；主变速换挡方式：机械有级档；副变速换挡方式：机械有级档；悬挂装置型式：后置三点悬挂","17000","T201900370884","2024-12-30","63300.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW201907048；NW201907004","山东省农业机械科学研究院产品质量检测中心","NO201701063","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","60-70马力四轮驱动拖拉机","洛阳福格森机械装备有限公司","轮式拖拉机","MF604","功率:60马力;驱动方式:四轮驱动 ;","发动机标定功率：44.2kW；驱动方式：四轮驱动","17000","鄂2020008","2025-04-11","65000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","HB2019FHZ023","湖北三智农业机械检测有限公司","WJ2018CKKX011","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","60-70马力四轮驱动拖拉机","英轩重工有限公司","轮式拖拉机","YX604-B1","功率:60马力;驱动方式:四轮驱动 ;","驱动方式：四轮驱动；功率(KW)：44.5KW","17000","T201932320056","2024-12-01","65500.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019IFH021","河南省拖拉机柴油机产品质量监督检验中心","(2016)委字整机类第012010223号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","60-70马力四轮驱动拖拉机","山东福尔沃农业装备股份有限公司","轮式拖拉机","FB604-E","功率:60马力;驱动方式:四轮驱动 ;","60马力；驱动方式：四轮驱动；发动机转速：2300r/min；外廓尺寸（长×宽×高）:3275×1300×2070mm；最大牵引力：13.1kN；轴距：1775mm；最小离地间隙及部位：220mm 前桥下沿；最小使用质量：1680kg;功率：44.5Kw（选装功率：44.2kW/44.2kW）.","17000","T201900430039","2024-10-22","68000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019CFH042","河南省拖拉机柴油机产品质量监督检验中心","WJ2018HKKX003","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","60-70马力四轮驱动拖拉机","山东福尔沃农业装备股份有限公司","轮式拖拉机","DN604","功率:60马力;驱动方式:四轮驱动 ;","60马力；驱动方式：四轮驱动；排放标准：囯三排放；发动机转速：2300r/min；外廓尺寸（长×宽×高）:3775×1735×2800mm（选装安全框架3775×1620×2400mm）；轴距：2000mm；最小离地间隙及部位：415mm 牵引支座下沿；最小使用质量：2280kg;功率：44.5Kw.(选装发动机功率：44.2kW/44.2kw)K=38","17000","T201900430036","2024-10-22","68000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019CFH042/NW201905017/WJ2019CFH041","河南省拖拉机柴油机产品质量监督检验中心/山东省农业机械科学研究院产品质量检测中心/河南省拖拉机柴油机产","WJ2018JKKX026","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","60-70马力四轮驱动拖拉机","常力工贸有限公司","轮式拖拉机","CL604-5","功率:60马力;驱动方式:四轮驱动 ;","整机外廓尺寸（长×宽×高mm）:3840×1530×2540防翻架 ；最小使用质量:1906kg；配套动力（kW）:44.1；型式:四轮驱动；轴距（mm）:1830 ； 轮距（前轮/后轮）（mm）:1210、1410/1200、1270、1340； 最小离地间隙（mm）:380；变速箱前端面至后驱动轴轴心线的水平距离：1057 ； 标准配重（kg）:96/160 ； 档位数（前进/倒退/爬行）: 8/2；变速箱型式:（4+1）×2组成式；轮胎型号（前轮/后轮）:7.50-16/11.2-28","17000","T202043430010","2025-03-24","57500.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019KFH014","河南省拖拉机柴油机产品质量监督检验中心","(2019)2240075","潍坊市产品质量检验所"]
["动力机械","拖拉机","轮式拖拉机","60-70马力四轮驱动拖拉机","常力工贸有限公司","轮式拖拉机","CL604-1","功率:60马力;驱动方式:四轮驱动 ;","整机外廓尺寸（长×宽×高mm）:3330×1410×2000(安全框架顶部)；最小使用质量:1690kg；配套动力（kW）:44.1；型式:四轮驱动；轴距（mm）:1750； 轮距（前轮/后轮）（mm）:980、1060/910-1060； 最小离地间隙（mm）:265；变速箱前端面至后驱动轴轴心线的水平距离：965； 标准配重（kg）:0/120； 档位数（前进/倒退/爬行）: 8/2；变速箱型式:（4+1）×2组成式；轮胎型号（前轮/后轮）:6.00-14/9.50-20。","17000","T202000430098","2025-03-31","57000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2020CFH030","河南省拖拉机柴油机产品质量监督检验中心","(2019)2040109","潍坊市产品质量检验所"]
["动力机械","拖拉机","轮式拖拉机","60-70马力四轮驱动拖拉机","道依茨法尔机械有限公司","轮式拖拉机","SH604-C","功率:60马力;驱动方式:四轮驱动 ;","驱动轮数：四轮驱动；发动机标定功率（kW）：44.1或44.2；最小使用质量（kg）:2540；排放标准：第三阶段。","17000","T201900220502","2024-12-30","80400.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。未提供翻倾防护装置强度检验及可靠性试验报告。","","","","",""]
["动力机械","拖拉机","轮式拖拉机","60-70马力四轮驱动拖拉机","江苏沃得高新农业装备有限公司（原：江苏沃得植保机械有限公司、原：沃得重工（中国）有限公司）","轮式拖拉机","WE604","功率:60马力;驱动方式:四轮驱动 ;","标定功率：60马力（44.1kW）；驱动方式：四轮驱动；配套发动机型号：常柴4G33T-60G31E（国Ⅲ排放标准）；标定转速(r/min)：2400；外廓尺寸（长×宽×高）（mm）：3650×1572×2400（至安全架顶）/2460（至驾驶室顶）；轴距或履带接地长（mm）：1845；最小使用质量(kg)：1950（带安全架）/2140（带驾驶室）；发动机与主离合器联接方式：直联；变速箱（器）型式：机械平面组成式；轮胎型号（前轮/后轮）：8.3-20/13.6-28。","17000","T202032320096","2025-06-30","63000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","SAM2020019、SAM2020020","南京赛姆认证科技发展有限公司、南京赛姆认证科技发展有限公司","(2018)委字整机类第01801206555号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","60-70马力四轮驱动拖拉机","洛阳博途农业装备有限公司","轮式拖拉机","BOTON604","功率:60马力;驱动方式:四轮驱动 ;","整机信息： 型号：BOTON604；型式：4*4轮式；用途：一般农业用；外廓尺寸：3340mm*1610mm*2640mm；轴距：2040mm；轮距：1300/1300~1600mm；最小离地间隙：350mm；最小使用质量：2435kg；挡位数：12F+4R。","17000","豫2016043","2020-12-31","70000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH15GW0501","国家拖拉机质量监督检验中心","2015KKX041","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","60-70马力四轮驱动拖拉机","京山三雷重工股份有限公司","轮式拖拉机","雷木604ESS","功率:60马力;驱动方式:四轮驱动 ;","型式:四轮驱动,外廓尺寸(mm):3220×1300×1930,轴距1820mm,最小使用质量1730kg,标准配重（前/后）:60/50（kg）,变速箱型式:机械空间组成式,换挡方式:机械有级挡,发动机型号：4D27ZT32/604,标定功率：44.2kW，制造商：浙江新柴股份有限公司，国三排放阶段","17000","鄂2019341","2024-10-27","57000.00","","通用类","湖北省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019HFH014","河南省拖拉机柴油机产品质量监督检验中心","HBNJ201909039","湖北三智农业机械检测有限公司"]
["动力机械","拖拉机","轮式拖拉机","60-70马力四轮驱动拖拉机","邢台市同德机械有限公司","轮式拖拉机","XT-604","功率:60马力;驱动方式:四轮驱动 ;","发动机功率：44.1KW  驱动方式：四轮驱动","17000","T201900430046","2024-10-22","59500.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019DFH016","河南省拖拉机柴油机产品质量监督检验中心","(2018)委检字整机类2027号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","60-70马力四轮驱动拖拉机","潍坊米基林农业机械有限公司","轮式拖拉机","604-C","功率:60马力;驱动方式:四轮驱动 ;","结构尺寸（长×宽×高mm）:3300×1360×2350；最小使用质量（kg）:1720；轴距（mm）:1800； 轮距（前轮/后轮）（mm）:1050/1050；；选装轮距（前轮/后轮）（mm）:1050、1140/900-1300 ； 最小离地间隙（mm）:350(前桥底部) ;最大配重（kg）:100/240； 档位数（前进/倒退/爬行）:8/2 ；变速箱型式:（4+1）×2 组成式；轮胎型号（前轮/后轮）:6.5-16/12.4-24；","17000","T202000430096","2025-03-31","59800.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，未提供翻倾防护装置强度检验及可靠性试验报告。","","","","",""]
["动力机械","拖拉机","轮式拖拉机","60-70马力四轮驱动拖拉机","潍坊米基林农业机械有限公司","轮式拖拉机","604-H","功率:60马力;驱动方式:四轮驱动 ;","结构尺寸（长×宽×高mm）:4000×1850×2700（驾驶室） 4000×1780×2600（安全架）；最小使用质量（kg）:2650（安全架）、2750（驾驶室）；轴距（mm）:2050； 轮距（前轮/后轮）（mm）:1450/1400；；选装轮距（前轮/后轮）（mm）: 1250、1350、1450/1250～1560； 最小离地间隙（mm）:370（前桥放油螺栓） ;最大配重（kg）:130/60； 档位数（前进/倒退/爬行）: 12/12；变速箱型式:4 ×3×(1+1)组成式；轮胎型号（前轮）:8.3-24/14.9-30；","17000","T202000220045","2025-03-31","65000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，未提供翻倾防护装置强度检验及可靠性试验报告。","","","","",""]
["动力机械","拖拉机","轮式拖拉机","60-70马力四轮驱动拖拉机","潍坊米基林农业机械有限公司","轮式拖拉机","604-N","功率:60马力;驱动方式:四轮驱动 ;","结构尺寸（长×宽×高mm）:3800×1710×2650（驾驶室） 3800×1620×2500（安全架）；最小使用质量（kg）:2470（安全架）、2550（驾驶室）；轴距（mm）:1980； 轮距（前轮/后轮）（mm）:1300/1300；；选装轮距（前轮/后轮）（mm）:1200、1300、1400/1200、1300、1400 ； 最小离地间隙（mm）: 420（后牵引架底部）;最大配重（kg）:64/60； 档位数（前进/倒退/爬行）: 8/8；变速箱型式: 4×2×（1+1） 组成式；轮胎型号（前轮/轮）:8.3-24/11-32；","17000","T202000220044","2025-03-31","63000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，未提供翻倾防护装置强度检验及可靠性试验报告。","","","","",""]
["动力机械","拖拉机","轮式拖拉机","70-80马力四轮驱动拖拉机","洛阳福格森机械装备有限公司","轮式拖拉机","MF704","功率:70马力;驱动方式:四轮驱动 ;","发动机标定功率：51.5kW；驱动方式：四轮驱动","22800","鄂2020008","2025-04-11","81000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","HB2019FHZ023","湖北三智农业机械检测有限公司","WJ2018CKKX011","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","70-80马力四轮驱动拖拉机","山东巨明机械有限公司","轮式拖拉机","JM704","功率:70马力;驱动方式:四轮驱动 ;","发动机标定功率：51.5kW；型式：四轮驱动；外廓尺寸（长×宽×高）：4100×1795×2600mm；轴距：2070mm；最小离地间隙：365mm；最小使用质量：2875kg；最大配重（前/后）：120/360kg；档位数（前进/倒退/爬行）：12/12/0；最大牵引力：≥14kN；变速箱型式：4×3×（1+1）组成式；翻倾防护装置：驾驶室；悬挂装置型式：后置三点悬挂。","22800","部20190460","2023-12-31","78000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2018FFH017","河南省拖拉机柴油机产品质量监督检验中心","WJ2017FKKX036","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","70-80马力四轮驱动拖拉机","山东五征集团有限公司","轮式拖拉机","NS704","功率:70马力;驱动方式:四轮驱动 ;","功率：70马力；整机驱动型式：四驱；外廓尺寸（长×宽×高及部位）：3470×1500×2499mm（安全架顶）；离合器壳体前端面至后驱动轴轴心线的水平距离：1130mm；最小使用质量：1960kg；翻倾防护装置：安全框架；转向系型式：全液压；变速箱（器）型式：机械平面组成式；主变速换挡方式：机械有级档；副变速换挡方式：机械有级档；悬挂装置型式：后置三点悬挂","22800","T201900370884","2024-12-30","83700.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW201907048；NW201907004","山东省农业机械科学研究院产品质量检测中心","NO201701063","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","70-80马力四轮驱动拖拉机","第一拖拉机股份有限公司","轮式拖拉机","MK754","功率:75马力;驱动方式:四轮驱动 ;","功率：55.2kw/75马力；驱动形式：四轮驱动","22800","部20160173","2020-12-31","77000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH13GW0111","国家拖拉机质量监督检验中心","LT13GK0231","国家拖拉机质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","70-80马力四轮驱动拖拉机","第一拖拉机股份有限公司","轮式拖拉机","MK754-1","功率:75马力;驱动方式:四轮驱动 ;","功率：55.2kw/75马力；驱动形式：四轮驱动","22800","部20160173","2020-12-31","81000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","201520","国家拖拉机质量监督检验中心","LT13GK0231","国家拖拉机质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","70-80马力四轮驱动拖拉机","山东悍沃农业装备有限公司","轮式拖拉机","704-F","功率:70马力;驱动方式:四轮驱动 ;","整机外廓尺寸（长×宽×高）：3600×1500×2700mm（驾驶室顶部）/3600×1500×2200mm（安全架顶部）；轴距：1950mm；整机型式：4×4四轮驱动；标准配重：前72kg/后56kg；发动机标定功率：51.5kW；轮胎型号：前轮8.3-20/后轮12.4-28；最小使用质量：2000kg（驾驶室）/1800kg（安全架）。","22800","T202032320019","2025-02-27","81000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019JFH003/WJ2019IFH031","河南省拖拉机柴油机产品质量监督检验中心","YH2019WJ01025","江苏沿海农业机械检测有限公司"]
["动力机械","拖拉机","轮式拖拉机","70-80马力四轮驱动拖拉机","潍坊红柳机械开发有限公司","轮式拖拉机","704A","功率:70马力;驱动方式:四轮驱动 ;","发动机标定功率：70马力；驱动方式：四轮驱动","22800","部20180574","2022-12-31","77000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","W201101009","山东省农业机械产品质量监督检验站","W201401037-11","山东省农业机械产品质量检验站"]
["动力机械","拖拉机","轮式拖拉机","70-80马力四轮驱动拖拉机","潍坊红柳机械开发有限公司","轮式拖拉机","704C","功率:70马力;驱动方式:四轮驱动 ;","发动机标定功率：70马力；驱动方式：四轮驱动","22800","部20180576","2022-12-31","76500.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","W201101009","山东省农业机械产品质量监督检验站","W201401037-11","山东省农业机械产品质量检验站"]
["动力机械","拖拉机","轮式拖拉机","70-80马力四轮驱动拖拉机","山东凯斯迪尔农业装备有限公司","轮式拖拉机","DR704-K","功率:51.5KW（70马力）马力;驱动方式:四轮驱动 ;","功率：51.5KW（70马力）；驱动方式：四轮驱动 ：  最小使用质量  2280kg(驾驶室)；最小使用质量：2075kg(安全架)； 排放标准 ：国家第三阶段；","22800","T202032320012","2025-02-27","77520.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH19GW1341（驾驶室）/FH19GW1331（安全架）","国家拖拉机质量监督检验中心/国家拖拉机质量监督检验中心","（2018）委字整机类第0180800611号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","70-80马力四轮驱动拖拉机","潍坊恒大农业装备有限公司","轮式拖拉机","HD704-B","功率:70马力;驱动方式:四轮驱动 ;","结构尺寸（长×宽×高mm）：3770×1650×2650（驾驶室）3770×1650×2350（安全架） 轴距或履带接地长（mm）：1970，常用轮距（前轮/后轮）或轨距（mm）:1300/1300,最小使用质量（kg）：2250（驾驶室）、2150（安全架）, 标准配重（前/后）kg:60/60,档位数（前进/后退）：8/2，主变速档位*副变速档位数：4+1/2，发动机与主离合器连接方式：直联，起动方式：电启动 翻轻防护装置型式：安全框架，转向系型式：全液压，转向操纵机构：方向盘，主变速换挡方式：机械有级档，副变速箱换挡方式：机械有级档，轮胎型号（前轮/后轮）：8.3-24/11-32，液压悬挂系统型式：分置式，悬挂装置型式：后置三点悬挂，悬挂装置类别：2类，工作装置液压油泵型号：CBN-316,液压输出组数：2，工作装置安全阀全开压力（MPa）:18±0.5,动力输出轴花键数目：8，动力输出轴标准转速（r/min）:540/760","22800","T202000220050","2025-03-31","76500.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019GFH021","河南省拖拉机柴油机产品质量监督检验中心","WJ2018KKKX048","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","70-80马力四轮驱动拖拉机","山东双力现代农业装备有限公司","轮式拖拉机","SL704-B","功率:70马力;驱动方式:四轮驱动 ;","驱动型式：四轮驱动；配套功率：70马力；","22800","T202000430289","2025-07-05","76500.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW202001002","山东省农业机械科学研究院产品质量检测中心","NW201712031","山东省农业机械科学研究院产品质量检测中心"]
["动力机械","拖拉机","轮式拖拉机","70-80马力四轮驱动拖拉机","山东潍坊鲁中拖拉机有限公司","轮式拖拉机","LZ704-C","功率:70马力;驱动方式:四轮驱动 ;","功率：70马力；驱动方式：四轮驱动","22800","T202000370264","2025-07-05","76500.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW202004022","山东省农业机械科学研究院产品质量检测中心","（2019）2240042","潍坊市产品质量检验所"]
["动力机械","拖拉机","轮式拖拉机","70-80马力四轮驱动拖拉机","潍坊奥利达机械有限公司","轮式拖拉机","ALD704-C","功率:70马力;驱动方式:四轮驱动 ;","外廓尺寸：3700×1660×2530（驾驶室顶部） 3700×1660×2370（安全架顶部）；驱动型式：四轮驱动；配套功率：52kW; 发动机型号及制造商：4D32ZT33/704,浙江新柴股份有限公司；轴距：1980; 最小使用质量：2370（驾驶室）/2280（安全架）kg; 配重：72/116; 档位数： 8/2/0; 是否有驾驶室或安全架：驾驶室/安全架。","22800","T201932320094","2024-12-30","80500.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019IFH014/WJ2019IFH016","河南省拖拉机柴油机产品质量监督检验中心","(2018)委检字整机类第01801204020号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","70-80马力四轮驱动拖拉机","山东瑞泽重工有限公司","轮式拖拉机","RC704","功率:70马力;驱动方式:四轮驱动 ;","驱动方式：四轮驱动 功率：70马力","22800","鄂2020064","2025-05-13","75000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。承诺书版本过期；未提供翻倾防护装置强度检验与可靠性试验报告。","","","","",""]
["动力机械","拖拉机","轮式拖拉机","70-80马力四轮驱动拖拉机","安徽天平机械股份有限公司","轮式拖拉机","JH704","功率:70马力;驱动方式:四轮驱动 ;","外廓尺寸(长×宽×高)：3750×1700×2550mm；轴距或履带接地长：1985mm；常用轮距(前轮/后轮)或轨距：1300/1300；轮距(前轮/后轮)调整方式：有级可调/有级可调；最小使用质量：2300kg；标准配重(前/后)：70/160kg；档位数(前进/倒退/爬行)：8/2/0；主变速档位数*副变速档位数/其他档位数：（4+1）/2/0；发动机与离合器联接方式：直联；起动方式：电起动；翻倾防护装置（驾驶室或安全框架）：六柱驾驶室；前照灯型号：D-1DDzhL；转向系型式：前轮液压转向；行车制动系型式：机械操纵、盘式制动器；驻车制动系型式：机械操纵、盘式制动器；前驱动桥型式：旱地型；离合器型式：单片、干式、单作用、常接合；传动系动力输出轴离合器型式：；传动系变速箱型式：圆锥齿轮/内置式、单级直齿圆柱齿轮；主变速箱换档方式：滑动齿轮换挡；副变速箱换档方式：滑动齿轮换挡；轮胎型号(前轮/后轮)：8.3-24/11-32","22800","2019TJ163","2023-12-31","82000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：不通过，可靠性试验报告与所投产品型号不符。","","NW201705043","山东省农业机械科学研究院产品质量检测中心","NJJC20180713","山东宝鼎农业机械检查有限公司"]
["动力机械","拖拉机","轮式拖拉机","70-80马力四轮驱动拖拉机","江苏常发农业装备股份有限公司","轮式拖拉机","CFF754-J","功率:75马力;驱动方式:四轮驱动 ;","整机型式：轮式；整机机架型式：无架；整机驱动型式：四驱；外廓尺寸（长×宽×高）mm：4325×1970×2668；轴距mm：2135；轮距（前轮/后轮）mm：前轮1550，后轮1315、1425、1540、1685、1700、1810、1920；最小使用质量kg：3280；标准配重（前/后）kg：300/540；最小使用比质量kg/kw：59.4；档位数（前进/倒退）：12/12；主变速档位数：4；副变速档位数：3×（1+1）；发动机与离合器联结方式：直联式；翻倾防护装置：简易驾驶室；转向系型式：全液压转向；转向系转向操纵机构：方向盘；转向系转向机构型式：前轮转向；变速箱型式：机械平面组成式；主变速换挡方式：机械有级档；副变速换挡方式：机械有级档；轮胎型号：前轮11.2-24，后轮16.9-30；轮胎数量：前轮2个/后轮2个","22800","T201900320597","2024-12-30","98000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH14GW0461","国家拖拉机质量监督检验中心","（2012）委字01类第309号","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","70-80马力四轮驱动拖拉机","江苏常发农业装备股份有限公司","轮式拖拉机","CFC704B","功率:70马力;驱动方式:四轮驱动 ;","整机型式：轮式；整机机架型式：无架；整机驱动型式：四驱；外廓尺寸（长×宽×高）mm：3713×1615×2640或3713×1365×2640，选装宽1515-1975或1365-1515；轴距mm：1798；轮距（前轮/后轮）mm：前轮1300或1050、1100、1200，后轮1300或1050，选装后轮1200-1660（无极调节）或1050-1200（无极调节）；最小使用质量kg：2140；标准配重kg：后配重180；最小使用比质量kg/kw：41.6；档位数（前进/倒退）：8/8；主变速档位数：4；副变速档位数：2×（1+1）；发动机与离合器联结方式：直联式；翻倾防护装置：安全架；转向系型式：全液压转向；转向系转向操纵机构：方向盘；转向系转向机构型式：前轮转向；变速箱型式：机械平面组成式；主变速换挡方式：机械有级档；副变速换挡方式：机械有级档；轮胎型号：前轮8.3-20或7.50-16，后轮12.4-28或11.2-28或12.4/11-28；轮胎数量：前轮2个/后轮2个","22800","T201932320110","2024-12-30","60000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH20GW0401/FH20GW0411","国家拖拉机质量监督检验中心（洛阳西苑车辆与动力检验所有限公司）","（2017）委检字整机类第2051号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","70-80马力四轮驱动拖拉机","江苏常发农业装备股份有限公司","轮式拖拉机","CFF704-J","功率:70马力;驱动方式:四轮驱动 ;","整机型式：轮式；整机机架型式：无架；整机驱动型式：四驱；外廓尺寸（长×宽×高）mm：4325×1930×2635；轴距mm：2135；轮距（前轮/后轮）mm：前轮1450，后轮1285、1420、1535、1685、1820、1935；最小使用质量kg：3170；标准配重（前/后）kg：300/540；最小使用比质量kg/kw：61.6；档位数（前进/倒退）：12/12；主变速档位数：4；副变速档位数：3×（1+1）；发动机与离合器联结方式：直联式；翻倾防护装置：简易驾驶室；转向系型式：全液压转向；转向系转向操纵机构：方向盘；转向系转向机构型式：前轮转向；变速箱型式：机械平面组成式；主变速换挡方式：机械有级档；副变速换挡方式：机械有级档；轮胎型号：前轮8.3-24，后轮14.9-30；轮胎数量：前轮2个/后轮2个","22800","T201900320597","2024-12-30","95000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH14GW0461","国家拖拉机质量监督检验中心","（2012）委字01类第307号","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","70-80马力四轮驱动拖拉机","潍坊百利拖拉机有限公司","轮式拖拉机","704-A","功率:70马力;驱动方式:四轮驱动 ;","整机外廓尺寸（长×宽×高）：3800×1618×2220mm（安全架顶）；轴距：2030mm；整机型式：4×4四轮驱动；标准配重：前144kg/后360kg；发动机标定功率：51.5kW；轮胎型号：前轮7.50-16/后轮13.6-24；最小使用质量：2434kg。","22800","T201900320722","2024-12-30","78000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2020GFH022","河南省拖拉机柴油机产品质量监督检验中心","W201303041-Ⅱ","山东省农业机械产品质量监督检验站"]
["动力机械","拖拉机","轮式拖拉机","70-80马力四轮驱动拖拉机","江苏沃得农业机械股份有限公司（原：江苏沃得农业机械有限公司）","轮式拖拉机","WD704F","功率:70马力;驱动方式:四轮驱动 ;","标定功率：70马力（51.5kW）；驱动方式：四轮驱动；配套发动机型号：常柴4G33TC（国Ⅲ排放标准）；标定转速(r/min)：2300；外廓尺寸（长×宽×高）（mm）：3820×1710×2550（至安全架顶）/2550（至驾驶室顶）；轴距或履带接地长（mm）：1992；最小使用质量(kg)：2540（带安全架）/2660（带驾驶室）；发动机与主离合器联接方式：直联；变速箱（器）型式：机械平面组成式；轮胎型号（前轮/后轮）：8.3-24/14.9-30。","22800","T201932320117","2024-12-30","89800.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","SAM2020002/FH20GW0211","南京赛姆认证科技发展有限公司/国家拖拉机质量监督检验中心","（2007）委字01类第190号","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","70-80马力四轮驱动拖拉机","江苏沃得高新农业装备有限公司（原：江苏沃得植保机械有限公司、原：沃得重工（中国）有限公司）","轮式拖拉机","WE704","功率:70马力;驱动方式:四轮驱动 ;","标定功率：70马力（51.5kW）；驱动方式：四轮驱动；配套发动机型号：常柴4L88-70G31E（国Ⅲ排放标准）；标定转速(r/min)：2400；外廓尺寸（长×宽×高）（mm）：3650×1572×2400（至安全架顶）/2460（至驾驶室顶）；轴距或履带接地长（mm）：1845；最小使用质量(kg)：2060（带安全架）/2250（带驾驶室）；发动机与主离合器联接方式：直联；变速箱（器）型式：机械平面组成式；轮胎型号（前轮/后轮）：8.3-20/13.6-28。","22800","T202032320096","2025-06-30","81000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","SAM2020019、SAM2020020","南京赛姆认证科技发展有限公司、南京赛姆认证科技发展有限公司","(2018)委字整机类第01801206555号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","70-80马力四轮驱动拖拉机","道依茨法尔机械有限公司","轮式拖拉机","SH704-C1","功率:70马力;驱动方式:四轮驱动 ;","驱动轮数：四轮驱动；发动机标定功率（kW）：51.5；最小使用质量（kg）:2660；排放标准：第三阶段。","22800","T201900220502","2024-12-30","86200.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。未提供翻倾防护装置强度检验与可靠性试验报告。","","","","",""]
["动力机械","拖拉机","轮式拖拉机","70-80马力四轮驱动拖拉机","常力工贸有限公司","轮式拖拉机","CL704-1","功率:70马力;驱动方式:四轮驱动 ;","整机外廓尺寸（长×宽×高mm）:3955×1700×2170（安全框架顶）；最小使用质量:2065kg；配套动力（kW）:51.5；型式:四轮驱动；轴距（mm）:1950； 轮距（前轮/后轮）（mm）:1100、1330/1150-1250； 最小离地间隙（mm）:290；变速箱前端面至后驱动轴轴心线的水平距离：1150； 标准配重（kg）:180/160； 档位数（前进/倒退/爬行）: 12/12；变速箱型式:4×3×（1+1）组成式；轮胎型号（前轮/后轮）:207/80-15/13.8-20","22800","T202000430097","2025-03-31","76500.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019KFH003","河南省拖拉机柴油机产品质量监督检验中心","(2019)2040104","潍坊市产品质量检验所"]
["动力机械","拖拉机","轮式拖拉机","70-80马力四轮驱动拖拉机","常力工贸有限公司","轮式拖拉机","CL704-5","功率:70马力;驱动方式:四轮驱动 ;","整机外廓尺寸（长×宽×高mm）:3860×1500×2540防翻架；最小使用质量:1960 kg；配套动力（kW）:52；型式:四轮驱动；轴距（mm）:1830 ； 轮距（前轮/后轮）（mm）:1210、1410/1200、1270、1340； 最小离地间隙（mm）:380；变速箱前端面至后驱动轴轴心线的水平距离：1057 ； 标准配重（kg）:96/160； 档位数（前进/倒退/爬行）: 8/2；变速箱型式:（4+1）×2组成式；轮胎型号（前轮/后轮）:7.50-16/11.2-28","22800","T202043430010","2025-03-24","77000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019KFH014","河南省拖拉机柴油机产品质量监督检验中心；","(2019)2240075","潍坊市产品质量检验所"]
["动力机械","拖拉机","轮式拖拉机","70-80马力四轮驱动拖拉机","常力工贸有限公司","轮式拖拉机","CL704-2","功率:70马力;驱动方式:四轮驱动 ;","整机外廓尺寸（长×宽×高mm）:4000×1640×2580防翻架 ；最小使用质量:2190kg；配套动力（kW）:52；型式:四轮驱动；轴距（mm）:1950 ； 轮距（前轮/后轮）（mm）:1290、1490/1150、1300、1380； 最小离地间隙（mm）:390；变速箱前端面至后驱动轴轴心线的水平距离：1169 ； 标准配重（kg）:96/160 ； 档位数（前进/倒退/爬行）: 8/2；变速箱型式:（4+1）×2组成式；轮胎型号（前轮/后轮）:8.3-24/11-32。","22800","T202043430011","2025-03-24","78000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019KFH003","河南省拖拉机柴油机产品质量监督检验中心","(2019)2240076","潍坊市产品质量检验所"]
["动力机械","拖拉机","轮式拖拉机","70-80马力四轮驱动拖拉机","山东福尔沃农业装备股份有限公司","轮式拖拉机","FB704","功率:70马力;驱动方式:四轮驱动 ;","70马力；驱动方式：四轮驱动；发动机转速：2300r/min；外廓尺寸（长×宽×高）:3565×1500×2230mm；最大牵引力：14.5kN；轴距：1875mm；最小离地间隙及部位：370mm 前桥下沿；最小使用质量：1975kg;功率：51.5Kw（选装功率：52kW/51.5kW）.","22800","T201900430037","2024-10-22","85000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019CFH042","河南省拖拉机柴油机产品质量监督检验中心","WJ2018HKKX016","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","70-80马力四轮驱动拖拉机","山东福尔沃农业装备股份有限公司","轮式拖拉机","DN704","功率:70马力;驱动方式:四轮驱动 ;","70马力；驱动方式：四轮驱动；排放标准：囯三排放；发动机转速：2300r/min；外廓尺寸（长×宽×高）:3775×1735×2800mm（选装安全框架3775×1620×2400mm）；轴距：2000mm；最小离地间隙及部位：415mm 牵引支座下沿；最小使用质量：2280kg;功率：51.5Kw.(选装发动机功率：52kw/51.5kW)K=32.57","22800","T201900430036","2024-10-22","85000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019CFH042/NW201905017/WJ2019CFH041","河南省拖拉机柴油机产品质量监督检验中心/山东省农业机械科学研究院产品质量检测中心/河南省拖拉机柴油机产","WJ2018JKKX026","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","70-80马力四轮驱动拖拉机","山东飞迅驰农业装备有限公司","轮式拖拉机","飞驰704","功率:70马力;驱动方式:四轮驱动 ;","外廓尺寸：4055×1690×2670(驾驶室：4055×1915×2700)；驱动型式：四轮驱动；配套功率：51.5kW; 发动机型号及制造商：YN4P070-33CR,山东云内动力有限责任公司；轴距：2090; 最小使用质量：2480（驾驶室：2650）; 配重：144/180; 档位数：12+12; 变速箱型式：4×3×(1+1)组成式；是否有驾驶室或安全架：有安全架及驾驶室。","22800","鄂2019377","2024-09-27","77500.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH19GW0721/FH19GW0742","国家拖拉机质量监督检验中心","（2018）委字整机类第0180800641号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","70-80马力四轮驱动拖拉机","宁波北野拖拉机制造有限公司","轮式拖拉机","704-3","功率:70马力;驱动方式:四轮驱动 ;","标定功率：52kw（70马力）；驱动方式：四轮驱动。","22800","T202000230166","2025-07-05","76500.00","","通用类","浙江宁波","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH20GW0681/FH20GW0671","国家拖拉机质量监督检验中心）","(2018)委检字整机类第0073号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","70-80马力四轮驱动拖拉机","潍坊米基林农业机械有限公司","轮式拖拉机","704-N","功率:70马力;驱动方式:四轮驱动 ;","结构尺寸（长×宽×高mm）:3800×1710×2650（驾驶室） 3800×1620×2500（安全架）；最小使用质量（kg）:2470（安全架）、2550（驾驶室）；轴距（mm）:1980； 轮距（前轮/后轮）（mm）:；1300/1300；选装轮距（前轮/后轮）（mm）:1200、1300、1400/1200、1300、1400 ； 最小离地间隙（mm）:420（后牵引架底部） ;最大配重（kg）:64/60； 档位数（前进/倒退/爬行）: 8/8；变速箱型式: 4×2×（1+1） 组成式；轮胎型号（前轮/后轮）:8.3-24/11-32；","22800","T202000220044","2025-03-31","76000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，未提供翻倾防护装置强度检验及可靠性试验报告。","","","","",""]
["动力机械","拖拉机","轮式拖拉机","70-80马力四轮驱动拖拉机","潍坊米基林农业机械有限公司","轮式拖拉机","704-H","功率:70马力;驱动方式:四轮驱动 ;","结构尺寸（长×宽×高mm）:4000×1850×2700（驾驶室） 4000×1780×2600（安全架）；最小使用质量（kg）:2650（安全架）、2750（驾驶室）；轴距（mm）:2050； 轮距（前轮/后轮）（mm）:1450/1400；；选装轮距（前轮/后轮）（mm）:1250、1350、1450/1250～1560 ； 最小离地间隙（mm）:370（前桥放油螺栓） ;最大配重（kg）:130/60； 档位数（前进/倒退/爬行）: 12/12；变速箱型式:4 ×3×(1+1)组成式；轮胎型号（前轮/后轮）:8.3-24/14.9-30；","22800","T202000220045","2025-03-31","78000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，未提供翻倾防护装置强度检验及可靠性试验报告。","","","","",""]
["动力机械","拖拉机","轮式拖拉机","70-80马力四轮驱动拖拉机","邢台市同德机械有限公司","轮式拖拉机","XT-704","功率:70马力;驱动方式:四轮驱动 ;","发动机功率：51.5KW  驱动方式：四轮驱动","22800","T201900430950","2024-12-30","79800.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019DFH016","河南省拖拉机柴油机产品质量监督检验中心","（2018）委检字整机类第2027号","盐城市农业机械实验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","70-80马力四轮驱动拖拉机","潍坊越腾农业机械有限公司","轮式拖拉机","704","功率:70马力;驱动方式:四轮驱动 ;","型号、名称：704轮式拖拉机  ；型式：轮式  ； 机架型式：无架  ； 驱动型式：四驱 ；\n用途：一般用途；外廓尺寸（长×宽×高及部位）：3650mm×1640mm×2500mm安全框架顶部 ；轴距：2000mm；轮距(mm)：1200、1300/1200、1300","22800","T202000430297","2025-07-05","78500.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019GFH011   WJ2019GFH010","河南省拖拉机柴油机产品质量监督检验中心","WJ2018LKKX016","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","70-80马力四轮驱动拖拉机","潍坊福康农业装备有限公司","轮式拖拉机","GF704","功率:70马力;驱动方式:四轮驱动 ;","发动机功率：51.5kw；驱动方式：四轮驱动；整机外廓尺寸（长x宽x高）：4040x1820x2805（mm）；轴距或履带接地长：2030mm；最小使用质量：2560kg；标准配重（前/后）：144/180kg；转向系型式：全液压；悬挂装置类别：二类；","22800","T202000430306","2025-07-05","81000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019JFH020(驾驶室）/WJ2019JFH021(防翻架）","河南省拖拉机柴油机产品质量监督检验中心","（2019）2240069","潍坊市产品质量检验所"]
["动力机械","拖拉机","轮式拖拉机","80-90马力四轮驱动拖拉机","中联重机股份有限公司","轮式拖拉机","RK804","功率:80马力;驱动方式:四轮驱动 ;","功率：80马力；型式：4×4四轮驱动；","25400","T201900511008","2024-12-30","98800.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH19GW0371","国家拖拉机质量监督检验中心","W201301081-Ⅱ","山东省农业机械产品质量监督检验站"]
["动力机械","拖拉机","轮式拖拉机","80-90马力四轮驱动拖拉机","中联重机股份有限公司","轮式拖拉机","RK804-A","功率:80马力;驱动方式:四轮驱动 ;","功率：80马力；型式：4×4四轮驱动；","25400","T201900511008","2024-12-30","94700.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH19GW0381","国家拖拉机质量监督检验中心","W201301081-Ⅱ","山东省农业机械产品质量监督检验站"]
["动力机械","拖拉机","轮式拖拉机","80-90马力四轮驱动拖拉机","江苏常发农业装备股份有限公司","轮式拖拉机","CFF804-J","功率:80马力;驱动方式:四轮驱动 ;","整机型式：轮式；整机机架型式：无架；整机驱动型式：四驱；外廓尺寸（长×宽×高）mm：4325×1970×2668；轴距mm：2135；轮距（前轮/后轮）mm：前轮1550，后轮1315、1425、1540、1685、1700、1810、1920；最小使用质量kg：3280；标准配重（前/后）kg：300/540；最小使用比质量kg/kw：55.6；档位数（前进/倒退）：12/12；主变速档位数：4；副变速档位数：3×（1+1）；发动机与离合器联结方式：直联式；翻倾防护装置：简易驾驶室；转向系型式：全液压转向；转向系转向操纵机构：方向盘；转向系转向机构型式：前轮转向；变速箱型式：机械平面组成式；主变速换挡方式：机械有级档；副变速换挡方式：机械有级档；轮胎型号：前轮11.2-24，后轮16.9-30；轮胎数量：前轮2个/后轮2个","25400","T201900320597","2024-12-30","101000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH14GW0461","国家拖拉机质量监督检验中心","（2012）委字01类第311号","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","80-90马力四轮驱动拖拉机","江苏常发农业装备股份有限公司","轮式拖拉机","CFF854-J","功率:85马力;驱动方式:四轮驱动 ;","整机型式：轮式；整机机架型式：无架；整机驱动型式：四驱；外廓尺寸（长×宽×高）mm：4325×1970×2938；轴距mm：2200；轮距（前轮/后轮）mm：前轮1550，后轮1315、1425、1540、1685、1700、1810、1920；最小使用质量kg：3410；标准配重（前/后）kg：300/540；最小使用比质量kg/kw：54.6；档位数（前进/倒退）：12/12；主变速档位数：4；副变速档位数：3×（1+1）；发动机与离合器联结方式：直联式；翻倾防护装置：简易驾驶室；转向系型式：全液压转向；转向系转向操纵机构：方向盘；转向系转向机构型式：前轮转向；变速箱型式：机械平面组成式；主变速换挡方式：机械有级档；副变速换挡方式：机械有级档；轮胎型号：前轮7.50-20，后轮16.9-34；轮胎数量：前轮2个/后轮2个","25400","T201900320597","2024-12-30","104000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH14GW0461","国家拖拉机质量监督检验中心","（2005）委字01类第130号","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","80-90马力四轮驱动拖拉机","山东时风（集团）有限责任公司","轮式拖拉机","SF804B","功率:80马力;驱动方式:四轮驱动 ;","洛柴4108国Ⅲ、前轮8.3-24后轮14.9-30、8+2档加强型底盘、液压转向、单速输出、差速锁、双作用离合器 不带前后配重。","25400","部20171849","2021-12-31","84836.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","驾驶室：W201606050,防翻架：W201509082。","驾驶室：机械工业农业机械产品质量检测中心。防翻架：山东省农业机械产品监督检验站","WJ2014001148Ⅱ","山东省农业机械产品质量监督检验站"]
["动力机械","拖拉机","轮式拖拉机","80-90马力四轮驱动拖拉机","雷沃重工股份有限公司","轮式拖拉机","M804-A","功率:80马力;驱动方式:四轮驱动 ;","驱动方式：四轮驱动；功率（kw）：59KW","25400","T201900510991","2024-12-30","105000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW201908028","山东省农业机械科学研究院产品质量检测中心","W201109024-Ⅱ","山东省农业机械产品质量监督检验站"]
["动力机械","拖拉机","轮式拖拉机","80-90马力四轮驱动拖拉机","潍坊恒大农业装备有限公司","轮式拖拉机","HD804-A","功率:80马力;驱动方式:四轮驱动 ;","结构尺寸（长×宽×高mm）：4100×1750×2550（安全架）4100×1750×2650（驾驶室） 轴距或履带接地长（mm）：2050，常用轮距（前轮/后轮）或轨距（mm）:1300/1300,最小使用质量（kg）：2700（驾驶室）、2560（安全架）, 标准配重（前/后）kg:140/160,档位数（前进/后退）：12/12，主变速档位*副变速档位数：4/3×（1＋1），发动机与主离合器连接方式：直联，起动方式：电启动  翻轻防护装置型式：安全框架，转向系型式：全液压，转向操纵机构：方向盘，主变速换挡方式：机械有级档，副变速箱换挡方式：机械有级档，轮胎型号（前轮/后轮）：8.3-24/14.9-30，液压悬挂系统型式：分置式，悬挂装置型式：后置三点悬挂，悬挂装置类别：2类，工作装置液压油泵型号：CBN-E320,液压输出组数：2，工作装置安全阀全开压力（MPa）:18±0.5,动力输出轴花键数目：8，动力输出轴标准转速（r/min）:540/760","25400","T202000220049","2025-03-31","85100.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019GFH021","河南省拖拉机柴油机产品质量监督检验中心","WJ2018KKKX049","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","80-90马力四轮驱动拖拉机","潍坊恒大农业装备有限公司","轮式拖拉机","HD804-B","功率:80马力;驱动方式:四轮驱动 ;","结构尺寸（长×宽×高mm）：3770×1650×2650（驾驶室） 轴距或履带接地长（mm）：1970，常用轮距（前轮/后轮）或轨距（mm）:1300/1300,最小使用质量（kg）：2300, 标准配重（前/后）kg:60/60,档位数（前进/后退）：8/2，主变速档位*副变速档位数：4+1/2，发动机与主离合器连接方式：直联，起动方式：电启动  翻轻防护装置型式：简易驾驶室，转向系型式：全液压，转向操纵机构：方向盘，主变速换挡方式：机械有级档，副变速箱换挡方式：机械有级档，轮胎型号（前轮/后轮）：8.3-24/11-32，液压悬挂系统型式：分置式，悬挂装置型式：后置三点悬挂，悬挂装置类别：2类，工作装置液压油泵型号：CBN-316,液压输出组数：2，工作装置安全阀全开压力（MPa）:18±0.5,动力输出轴花键数目：8，动力输出轴标准转速（r/min）:540/760","25400","T202000220050","2025-03-31","85200.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019GFH020","河南省拖拉机柴油机产品质量监督检验中心","WJ2018KKKX048","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","80-90马力四轮驱动拖拉机","山东凯斯迪尔农业装备有限公司","轮式拖拉机","DR804-K","功率:80马力;驱动方式:四轮驱动 ;","功率:59KW(80马力）;驱动方式 ：四轮驱动；最小使用质量:2405kg,最小使用比质量:40.76(驾驶室)；最小使用质量  2310kg，最小使用比质量:39.15（安全架）；\n外廓尺寸(长×宽×高) 3890 mm×1640 mm×2700 mm ；\n轴距或履带接地长 1980  mm；\n轮距(前轮/后轮)或轨距  1200mm、1300mm/ 1200mm、1300mm； \n常用轮距(前轮/后轮)或轨距  1300mm/1300mm ；\n最小离地间隙  395mm； \n标准配重(前/后)  150kg/130kg； \n档位数  前进/倒退/爬行 / 8/2/0 ；\n主变速/副变速/其他 / 4+1/2/0；\n发动机与离合器联接方式 / 直联； \n排放标准：国家第三阶段；","25400","T202032320012","2025-02-27","88900.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH19GW1341（驾驶室）/FH19GW1331（安全架）","国家拖拉机质量监督检验中心/国家拖拉机质量监督检验中心","（2018）委字整机类第0180800611号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","80-90马力四轮驱动拖拉机","潍坊红柳机械开发有限公司","轮式拖拉机","804C","功率:80马力;驱动方式:四轮驱动 ;","发动机标定功率：80马力；驱动方式：四轮驱动","25400","部20180577","2022-12-31","85000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","W201101009","山东省农业机械产品质量监督检验站","W201501019-II","山东省农业机械产品质量检验站"]
["动力机械","拖拉机","轮式拖拉机","80-90马力四轮驱动拖拉机","第一拖拉机股份有限公司","轮式拖拉机","MY804S","功率:80马力;驱动方式:四轮驱动 ;","功率：58.8kw/80马力；驱动形式：四轮驱动","25400","部20171097","2021-12-31","86000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH17GW0191","国家拖拉机质量监督检验中心","W201610047","机械工业农业机械产品质量检测中心（济南）"]
["动力机械","拖拉机","轮式拖拉机","80-90马力四轮驱动拖拉机","第一拖拉机股份有限公司","轮式拖拉机","MY804S-1","功率:80马力;驱动方式:四轮驱动 ;","功率：58.8kw/80马力；驱动形式：四轮驱动","25400","部20171097","2021-12-31","86500.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH17GW0181","国家拖拉机质量监督检验中心","W201610047","机械工业农业机械产品质量检测中心（济南）"]
["动力机械","拖拉机","轮式拖拉机","80-90马力四轮驱动拖拉机","山东飞迅驰农业装备有限公司","轮式拖拉机","飞驰804","功率:80马力;驱动方式:四轮驱动 ;","发动机型号：YN4E085-32CR4 发动机结构型式：直列、水冷、四冲程、直喷 发动机生产厂：昆明云内动力股份有限公司 发动机进气方式：增压 发动机气缸数：4 发动机标定功率：59kW 发动机额定净功率：59kW 发动机标定转速：2300r/min 发动机冷却方式：水冷 排放阶段：国3","25400","鄂2019377","2024-09-27","86500.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH19GW0721/FH19GW0742","国家拖拉机质量监督检验中心","（2018）委字整机类第0180800641号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","80-90马力四轮驱动拖拉机","山东骏玛道机械有限公司","轮式拖拉机","MD804","功率:80马力;驱动方式:四轮驱动 ;","发动机标定功率：58.8kW（80马力）；驱动方式：四轮驱动","25400","T201900370855","2024-12-30","86000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019HFH009","河南省拖拉机柴油机产品质量监督检验中心","（2018）委字整机类第 0180800667 号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","80-90马力四轮驱动拖拉机","山东福尔沃农业装备股份有限公司","轮式拖拉机","DN804","功率:80马力;驱动方式:四轮驱动 ;","80马力；驱动方式：四轮驱动；排放标准：囯三排放；发动机转速：2300r/min；外廓尺寸（长×宽×高）:3850×1735×2800mm（选装安全框架3850×1620×2400mm）；最大牵引力：18.7kN；轴距：2080mm；最小离地间隙及部位：415mm 牵引支座下沿；最小使用质量：2350kg;功率：59Kw(选装功率：58.8kW/59kW).K=29.37","25400","T201900430036","2024-10-22","97650.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019CFH042/NW201905017/WJ2019CFH041","河南省拖拉机柴油机产品质量监督检验中心/山东省农业机械科学研究院产品质量检测中心/河南省拖拉机柴油机产","WJ2018JKKX026","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","80-90马力四轮驱动拖拉机","常力工贸有限公司","轮式拖拉机","CL804-2","功率:80马力;驱动方式:四轮驱动 ;","整机外廓尺寸（长×宽×高mm）:4000×1640×2580安全框架顶端；最小使用质量:2240kg；配套动力（kW）:59；型式:四轮驱动；轴距（mm）:1950； 轮距（前轮/后轮）（mm）:1290、1490/1150、1300、1380； 最小离地间隙（mm）:390；变速箱前端面至后驱动轴轴心线的水平距离：1169； 标准配重（kg）:96/160； 档位数（前进/倒退/爬行）: 8/2；变速箱型式:（4+1）×2组成式；轮胎型号（前轮/后轮）:8.3-24/11-32","25400","T202043430011","2025-03-24","86000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019KFH003","河南省拖拉机柴油机产品质量监督检验中心","(2019)2240076","潍坊市产品质量检验所"]
["动力机械","拖拉机","轮式拖拉机","80-90马力四轮驱动拖拉机","常力工贸有限公司","轮式拖拉机","CL804-1","功率:80马力;驱动方式:四轮驱动 ;","整机外廓尺寸（长×宽×高mm）:4060×1700×2165（安全框架顶）；最小使用质量:2205kg；配套动力（kW）:58.8；型式:四轮驱动；轴距（mm）:1990； 轮距（前轮/后轮）（mm）:1100、1330/1150-1250； 最小离地间隙（mm）:290；变速箱前端面至后驱动轴轴心线的水平距离：1150； 标准配重（kg）:180/160； 档位数（前进/倒退/爬行）: 12/12；变速箱型式:4×3×（1+1）组成式；轮胎型号（前轮/后轮）:207/80-15/13.8-20","25400","T202000430097","2025-03-31","85000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019KFH003","河南省拖拉机柴油机产品质量监督检验中心","(2019)2040104","潍坊市产品质量检验所"]
["动力机械","拖拉机","轮式拖拉机","80-90马力四轮驱动拖拉机","潍坊中驰奔野农业装备有限公司","轮式拖拉机","804-A","功率:80马力;驱动方式:四轮驱动 ;","80马力，功率：59KW；驱动方式：四轮驱动","25400","T202000340192","2025-07-05","84700.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019IFH027,WJ2019IFH028","河南省拖拉机柴油机产品质量监督检验中心,河南省拖拉机柴油机产品质量监督检验中心","WJ2018EKKX006","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","80-90马力四轮驱动拖拉机","洛阳丰收农业机械装备有限公司","轮式拖拉机","芬美得-804","功率:80马力;驱动方式:四轮驱动 ;","发动机标定功率：59kW；驱动方式：四轮驱动；外廓尺寸（mm）长×宽×高：（安全架）3940×1910×2800、（驾驶室）3940×1810×2700；轴距：2020（mm）；最小使用质量：（安全架）2700kg、（驾驶室）2900kg；排放阶段：第三阶段","25400","新2019103","2024-04-10","98560.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","驾驶室报告编号：WJ2018KFH022       安全架报告编号：WJ2018HFH007","河南省拖拉机柴油机产品质量监督检验中心","WJ2018CKKX003","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","80-90马力四轮驱动拖拉机","江苏沃得高新农业装备有限公司（原：江苏沃得植保机械有限公司、原：沃得重工（中国）有限公司）","轮式拖拉机","WE804","功率:80马力;驱动方式:四轮驱动 ;","标定功率：80马力（58.8kW）；驱动方式：四轮驱动；配套发动机型号：常柴4L88-80G31C（国Ⅲ排放标准）；标定转速(r/min)：2400；外廓尺寸（长×宽×高）（mm）：3650×1572×2400（至安全架顶）/2460（至驾驶室顶）；轴距或履带接地长（mm）：1845；最小使用质量(kg)：2300（带安全架）/2390（带驾驶室）；发动机与主离合器联接方式：直联；变速箱（器）型式：机械平面组成式；轮胎型号（前轮/后轮）：8.3-20/13.6-28。","25400","T202032320096","2025-06-30","96500.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","SAM2020019、SAM2020020","南京赛姆认证科技发展有限公司、南京赛姆认证科技发展有限公司","(2018)委字整机类第01801206555号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","80-90马力四轮驱动拖拉机","潍坊富保田拖拉机有限公司","轮式拖拉机","804","功率:80马力;驱动方式:四轮驱动 ;","发动机标定功率：80马力；驱动方式：四轮驱动","25400","部20171770","2021-12-31","105000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW201711024;NW201711025","山东省农业机械科学研究院产品质量检测中心","201701320","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","80-90马力四轮驱动拖拉机","洛阳博途农业装备有限公司","轮式拖拉机","BOTON804","功率:80马力;驱动方式:四轮驱动 ;","整机信息： 型号：BOTON804；型式：4*4轮式；用途：一般农业用；外廓尺寸：4100mm*1900mm*2890mm；轴距：2410mm；轮距：1630~1960/1520~2120mm；最小离地间隙：450mm；最小使用质量：3920kg；挡位数：12F+4R。","25400","豫2016040","2020-12-31","105000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH15GW0511","国家拖拉机质量监督检验中心","2015KKX044","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","80-90马力四轮驱动拖拉机","潍坊福康农业装备有限公司","轮式拖拉机","GF804","功率:80马力;驱动方式:四轮驱动 ;","发动机功率：59kw；驱动方式：四轮驱动；整机外廓尺寸（长x宽x高）：4040x1820x2805（mm）；轴距或履带接地长：2030mm；最小使用质量：2560kg；标准配重（前/后）：144/180kg；转向系型式：全液压；悬挂装置类别：二类；","25400","T202000430306","2025-07-05","91600.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019JFH020(驾驶室）/WJ2019JFH021(防翻架）","河南省拖拉机柴油机产品质量监督检验中心","（2019）2240069","潍坊市产品质量检验所"]
["动力机械","拖拉机","轮式拖拉机","80-90马力四轮驱动拖拉机","山东渊博农业装备有限公司","轮式拖拉机","YB804-2","功率:80马力;驱动方式:四轮驱动 ;","外廓尺寸（长×宽×高mm）:4000×1640×2580（安全架）；最小使用质量:2240；配套动力（kW）:59；型式:四轮驱动；轴距（mm）:1980； 轮距（前轮/后轮）（mm）:1290、1490/1300、1380； 最小离地间隙（mm）:390（前桥底部螺栓）； 标准配重（kg）:128/80； 档位数（前进/倒退/爬行）:8/2/0；变速箱型式:（4+1）×2组成式；轮胎型号（前轮/后轮）:8.3-24/11-32","25400","T202000220147","2025-07-05","86000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019HFH025","河南省拖拉机柴油机产品质量监督检验中心","（2020）2240026","潍坊市产品质量检验所"]
["动力机械","拖拉机","轮式拖拉机","80-90马力四轮驱动拖拉机","潍坊越腾农业机械有限公司","轮式拖拉机","804-A","功率:80马力;驱动方式:四轮驱动 ;","型号、名称：804-A轮式拖拉机  ；型式：轮式  ； 机架型式：无架  ； 驱动型式：四驱 ；\n用途：一般用途；外廓尺寸（长×宽×高及部位）：3850mm×1840mm×2590mm安全框架顶部 ；轴距：2070mm；轮距(mm)：1200、1300/1200、1300","25400","T202000430297","2025-07-05","86800.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019GFH011   WJ2019GFH010","河南省拖拉机柴油机产品质量监督检验中心","WJ2018LKKX016","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","80-90马力四轮驱动拖拉机","艾格瑞巨明农业装备有限公司","轮式拖拉机","JM804","功率:80马力;驱动方式:四轮驱动 ;","发动机标定功率：59kW；型式：四轮驱动；外廓尺寸（长×宽×高）：4100×1795×2600mm；轴距：2072mm；最小离地间隙：365mm；最小使用质量：2875kg；最大配重（前/后）：136/350kg；档位数（前进/倒退/爬行）：12/12/0；最大牵引力：≥19.0kN；变速箱型式：4×3×（1+1）组成式；翻倾防护装置：四柱式安全驾驶室；悬挂装置型式：后置三点悬挂。","25400","部20181231","2022-12-31","93000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2018FFH019","河南省拖拉机柴油机产品质量监督检验中心","WJ2018BKKX009","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","80-90马力四轮驱动拖拉机","潍坊米基林农业机械有限公司","轮式拖拉机","804-N","功率:80马力;驱动方式:四轮驱动 ;","结构尺寸（长×宽×高mm）:3800×1710×2650（驾驶室） 3800×1620×2500（安全架）；最小使用质量（kg）:2470（安全架）、2550（驾驶室）；轴距（mm）:1980； 轮距（前轮/后轮）（mm）:1300/1300；；选装轮距（前轮/后轮）（mm）:1200、1300、1400/1200、1300、1400 ； 最小离地间隙（mm）: 420（后牵引架底部）;最大配重（kg）:64/60； 档位数（前进/倒退/爬行）:8/8 ；变速箱型式: 4×2×（1+1）组成式；轮胎型号（前轮/后轮）:8.3-24/11-32；","25400","T202000220044","2025-03-31","84200.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，未提供翻倾防护装置强度检验及可靠性试验报告。","","","","",""]
["动力机械","拖拉机","轮式拖拉机","80-90马力四轮驱动拖拉机","潍坊米基林农业机械有限公司","轮式拖拉机","804-H","功率:80马力;驱动方式:四轮驱动 ;","结构尺寸（长×宽×高mm）:4000×1850×2700（驾驶室） 4000×1780×2600（安全架）；最小使用质量（kg）:2650（安全架）、2750（驾驶室）；轴距（mm）:2050； 轮距（前轮/后轮）（mm）:1450/1400；；选装轮距（前轮/后轮）（mm）:1250、1350、1450/1250～1560 ； 最小离地间隙（mm）:370（前桥放油螺栓） ;最大配重（kg）:130/60； 档位数（前进/倒退/爬行）: 12/12；变速箱型式:4 ×3×(1+1)组成式；轮胎型号（前轮）:8.3-24/14.9-30；","25400","T202000220045","2025-03-31","84700.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，未提供翻倾防护装置强度检验及可靠性试验报告。","","","","",""]
["动力机械","拖拉机","轮式拖拉机","80-90马力四轮驱动拖拉机","宁波北野拖拉机制造有限公司","轮式拖拉机","804-3","功率:80马力;驱动方式:四轮驱动 ;","标定功率：59kw（80马力）；驱动方式：四轮驱动。","25400","T202000230166","2025-07-05","85200.00","","通用类","浙江宁波","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH20GW0681/FH20GW0671","国家拖拉机质量监督检验中心","(2018)委检字整机类第0073号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","80-90马力四轮驱动拖拉机","洛阳映山红拖拉机有限公司","轮式拖拉机","新东方804","功率:80马力;驱动方式:四轮驱动 ;","功率：58.8Kw；驱动方式：四轮驱动；外廓尺寸（长×宽×高）：3600×1500×2200（至安全架顶）；轮距（前轮/后轮）：1050/1160；轴距：2000；轮距调整方式：不可调/不可调；最小使用质量kg：1700；标准配重(前/后)kg：50/30；档位数(前进/倒退/爬行)：8/2/0；主变速档位数*副变速档位数/其他档位数：4+1/2/0；发动机与离合器联接方式：直联式；起动方式：电起动；翻倾防护装置（驾驶室或安全框架）；两柱式；前照灯型号：SZ550.48.030A/031A；转向系型式：全液压前轮转向；行车制动系型式：盘式；驻车制动系型式：锁定踏板式；离合器型式：干式、双作用；传动系变速箱型式：（4+1）×2机械组成式；主变速箱换档方式：啮合套；副变速箱换档方式：啮合套；轮胎型号(前轮/后轮)：7.00-12/13.6-16。","25400","T202065650003","2025-04-16","85000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH18GW0681","国家拖拉机质量监督检验中心","WJ2018JKKX019","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","90-100马力四轮驱动拖拉机","第一拖拉机股份有限公司","轮式拖拉机","MY904S-1","功率:90马力;驱动方式:四轮驱动 ;","功率：66.2kw/90马力；驱动形式：四轮驱动","31200","部20171098","2021-12-31","110000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH17GW0181","国家拖拉机质量监督检验中心","W201610047","机械工业农业机械产品质量检测中心（济南）"]
["动力机械","拖拉机","轮式拖拉机","90-100马力四轮驱动拖拉机","第一拖拉机股份有限公司","轮式拖拉机","MY904S","功率:90马力;驱动方式:四轮驱动 ;","功率：66.2kw/90马力；驱动形式：四轮驱动","31200","部20171098","2021-12-31","110000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH17GW0191","国家拖拉机质量监督检验中心","W201610047","机械工业农业机械产品质量检测中心（济南）"]
["动力机械","拖拉机","轮式拖拉机","90-100马力四轮驱动拖拉机","山东凯斯迪尔农业装备有限公司","轮式拖拉机","DR904","功率:66.2KW（90马力）马力;驱动方式:四轮驱动 ;","功率：66.2KW（90马力）；驱动方式：四轮驱动；最小使用质量：4095kg；\t\n外廓尺寸(长×宽×高)：4600mm×2100mm×2800mm(高度至空滤顶）；\n轴距或履带接地长：2200mm；\n轮距(前轮/后轮)：1600mm、1700mm、1800mm/1620mm、1696mm、1806mm、1902mm、2012mm；\n轮距(前轮/后轮)调整方式：有级可调/有级可调；最小离地间隙：410mm；常用轮距(前轮/后轮)：1700mm/1620mm；标准配重(前/后)：310kg/360kg；最大配重(前/后)：310kg/360kg；挡位数(前进/倒退/爬行)：16/8/0；","31200","部20171220","2021-12-31","106080.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","W201601011 ","山东省农业机械产品质量监督检验站","LT14GK0131","国家拖拉机质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","90-100马力四轮驱动拖拉机","潍坊恒大农业装备有限公司","轮式拖拉机","HD904-A","功率:90马力;驱动方式:四轮驱动 ;","结构尺寸（长×宽×高mm）：4100×1750×2650（驾驶室） 轴距或履带接地长（mm）：2050，常用轮距（前轮/后轮）或轨距（mm）:1300/1300,最小使用质量（kg）：2750, 标准配重（前/后）kg:140/160,档位数（前进/后退）：12/12，主变速档位*副变速档位数：4/3×（1＋1），发动机与主离合器连接方式：直联，起动方式：电启动  翻轻防护装置型式：简易驾驶室，转向系型式：全液压，转向操纵机构：方向盘，主变速换挡方式：机械有级档，副变速箱换挡方式：机械有级档，轮胎型号（前轮/后轮）：8.3-24/14.9-30，液压悬挂系统型式：分置式，悬挂装置型式：后置三点悬挂，悬挂装置类别：2类，工作装置液压油泵型号：CBN-E320,液压输出组数：2，工作装置安全阀全开压力（MPa）:18±0.5,动力输出轴花键数目：8，动力输出轴标准转速（r/min）:540/760","31200","T202000220049","2025-03-31","104500.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019GFH020","河南省拖拉机柴油机产品质量监督检验中心","WJ2018KKKX049","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","90-100马力四轮驱动拖拉机","江苏常发农业装备股份有限公司","轮式拖拉机","CFF904-J","功率:90马力;驱动方式:四轮驱动 ;","整机型式：轮式；整机机架型式：无架；整机驱动型式：四驱；外廓尺寸（长×宽×高）mm：4325×1970×2715；轴距mm：2200；轮距（前轮/后轮）mm：前轮1550，后轮1315、1425、1540、1685、1700、1810、1920；最小使用质量kg：3410；标准配重（前/后）kg：300/540；最小使用比质量kg/kw：51.5；档位数（前进/倒退）：12/12；主变速档位数：4；副变速档位数：3×（1+1）；发动机与离合器联结方式：直联式；翻倾防护装置：简易驾驶室；转向系型式：全液压转向；转向系转向操纵机构：方向盘；转向系转向机构型式：前轮转向；变速箱型式：机械平面组成式；主变速换挡方式：机械有级档；副变速换挡方式：机械有级档；轮胎型号：前轮11.2-28，后轮16.9-34；轮胎数量：前轮2个/后轮2个","31200","T201900320597","2024-12-30","108000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH14GW0461","国家拖拉机质量监督检验中心","（2005）委字01类第094号","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","90-100马力四轮驱动拖拉机","江苏常发农业装备股份有限公司","轮式拖拉机","CFG904-BJ","功率:90马力;驱动方式:四轮驱动 ;","整机型式：轮式；整机机架型式：无架；整机驱动型式：四驱；外廓尺寸（长×宽×高）mm：4705×2120×2924；轴距mm：2334；轮距（前轮/后轮）mm：前轮1646、1720、1900、1928，后轮1656、1688、1884、2088、；最小使用质量kg：4130；标准配重（前/后）kg：400/540；最小使用比质量kg/kw：62.4；档位数（前进/倒退）：12/12；主变速档位数：4；副变速档位数：3×（1+1）；发动机与离合器联结方式：直联式；翻倾防护装置：简易驾驶室；转向系型式：全液压转向；转向系转向操纵机构：方向盘；转向系转向机构型式：前轮转向；变速箱型式：机械平面组成式；主变速换挡方式：机械有级档；副变速换挡方式：机械有级档；轮胎型号：前轮14.9-26、12.4-28、9.5-24，后轮16.9-38、16.9-34、18.4-34R-2、13.6-38、14.9-30","31200","T201900320606","2024-12-30","129000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH20GW0351","国家拖拉机质量监督检验中心（洛阳西苑车辆与动力检验所有限公司）","（2005）委字01类第094号","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","90-100马力四轮驱动拖拉机","江苏常发农业装备股份有限公司","轮式拖拉机","CFG954-BJ","功率:95马力;驱动方式:四轮驱动 ;","整机型式：轮式；整机机架型式：无架；整机驱动型式：四驱；外廓尺寸（长×宽×高）mm：4705×2120×2924；轴距mm：2334；轮距（前轮/后轮）mm：前轮1646、1720、1900、1928，后轮1656、1688、1884、2088、；最小使用质量kg：4130；标准配重（前/后）kg：400/540；最小使用比质量kg/kw：59；档位数（前进/倒退）：12/12；主变速档位数：4；副变速档位数：3×（1+1）；发动机与离合器联结方式：直联式；翻倾防护装置：简易驾驶室；转向系型式：全液压转向；转向系转向操纵机构：方向盘；转向系转向机构型式：前轮转向；变速箱型式：机械平面组成式；主变速换挡方式：机械有级档；副变速换挡方式：机械有级档；轮胎型号：前轮14.9-26、12.4-28、9.5-24，后轮16.9-38、16.9-34、18.4-34R-2、13.6-38、14.9-30；轮胎数量：前轮2个/后轮2个","31200","T201900320606","2024-12-30","132000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH20GW0351","国家拖拉机质量监督检验中心（洛阳西苑车辆与动力检验所有限公司）","（2011）委字01类第118号","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","90-100马力四轮驱动拖拉机","江苏沃得农业机械股份有限公司（原：江苏沃得农业机械有限公司）","轮式拖拉机","WD904G","功率:90马力;驱动方式:四轮驱动 ;","标定功率：90马力（66.2kW）；驱动方式：四轮驱动；配套发动机型号：一拖LR4A3ZU23/0662E、玉柴YC4A105-T310、一拖LR4A3LR23/0662（国Ⅲ排放标准）；标定转速(r/min)：2300；外廓尺寸（长×宽×高）（mm）：4250×2025×2900（至安全架顶）/2935（至驾驶室顶）；轴距或履带接地长（mm）：2310；最小使用质量(kg)：3542（带安全架）/3648（带驾驶室）；发动机与主离合器联接方式：直联；变速箱（器）型式：机械平面组成式；轮胎型号（前轮/后轮）：12.4-24/16.9-34。","31200","T201932320118","2024-12-30","113500.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","SAM2020001、FH20GW0221","南京赛姆认证科技发展有限公司、国家拖拉机质量监督检验中心","（2007）委字01类第013号","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","90-100马力四轮驱动拖拉机","中联重机股份有限公司","轮式拖拉机","RC904","功率:90马力;驱动方式:四轮驱动 ;","功率：90马力；型式：4×4四轮驱动；","31200","T201900511007","2024-12-30","122900.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH12GW0281","国家拖拉机质量监督检验中心","W201401033-Ⅱ","山东省农业机械产品质量监督检验站"]
["动力机械","拖拉机","轮式拖拉机","90-100马力四轮驱动拖拉机","中联重机股份有限公司","轮式拖拉机","RC904-A","功率:90马力;驱动方式:四轮驱动 ;","功率：90马力；型式：4×4四轮驱动；","31200","T201900511007","2024-12-30","116600.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH13GW0091","国家拖拉机质量监督检验中心","W201401033-Ⅱ","山东省农业机械产品质量监督检验站"]
["动力机械","拖拉机","轮式拖拉机","90-100马力四轮驱动拖拉机","洛阳博途农业装备有限公司","轮式拖拉机","BOTON904","功率:90马力;驱动方式:四轮驱动 ;","整机信息： 型号：BOTON904；型式：4*4轮式；用途：一般农业用；外廓尺寸：3940mm*1900mm*2910mm；轴距：2350mm；轮距：1630~1960/1520~2120mm；最小离地间隙：450mm；最小使用质量：3765kg；挡位数：12F+4R。","31200","豫2016039","2020-12-31","130000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH15GW0511","国家拖拉机质量监督检验中心","2015KKX044","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","90-100马力四轮驱动拖拉机","潍坊富保田拖拉机有限公司","轮式拖拉机","904A","功率:90马力;驱动方式:四轮驱动 ;","发动机标定功率：90马力；驱动方式：四轮驱动","31200","部20171769","2021-12-31","110000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW201711024;NW201711025","山东省农业机械科学研究院产品质量检测中心","201701320","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","90-100马力四轮驱动拖拉机","洛阳丰收农业机械装备有限公司","轮式拖拉机","芬美得-904","功率:90马力;驱动方式:四轮驱动 ;","发动机标定功率：66.2kW；驱动方式：四轮驱动；外廓尺寸（mm）长×宽×高：（安全架）3940×1810×2800、（驾驶室）3940×1810×2700；轴距：2020（mm）；最小使用质量：（安全架）2700kg、（驾驶室）2900kg；排放阶段：第三阶段","31200","新2019104","2024-04-10","115600.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","驾驶室报告编号：WJ2018KFH022       安全架报告编号：WJ2018HFH007","河南省拖拉机柴油机产品质量监督检验中心","WJ2018CKKX003","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","90-100马力四轮驱动拖拉机","潍坊东科重工农业装备有限公司","轮式拖拉机","DK904A","功率:90马力;驱动方式:四轮驱动 ;","外廓尺寸：4100×1810×2580；驱动型式：四轮驱动；配套功率：66.2kW; 发动机型号及制造商：4C6-90C33,安徽全柴动力股份有限公司；轴距：2000; 最小使用质量：2700; 配重：144/360; 档位数：12+12; 变速箱型式：4×3×(1+1)组成式，选装变速箱型式：4×（2+1）；是否有驾驶室或安全架：有驾驶室。","31200","鄂2019386","2024-09-27","115000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019FFH001","河南省拖拉机柴油机产品质量监督检验中心","(2018)委字整机类第0180600170号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","90-100马力四轮驱动拖拉机","潍坊东科重工农业装备有限公司","轮式拖拉机","DK904K","功率:90马力;驱动方式:四轮驱动 ;","外廓尺寸：4100×1810×2710；驱动型式：四轮驱动；配套功率：66.2kW; 发动机型号及制造商：4C6-90C33；安徽全柴动力股份有限公司：轴距：2000; 最小使用质量：2660; 配重：144/360; 档位数：12/12/0; 变速箱型式：4×3×(1+1)组成式；是否有驾驶室或安全架：有安全架。","31200","鄂2020009","2025-04-11","115000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2020AFH010","河南省拖拉机柴油机产品质量监督检验中心","(2016)委字整机类第0120049号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","90-100马力四轮驱动拖拉机","山东骏玛道机械有限公司","轮式拖拉机","MD904","功率:90马力;驱动方式:四轮驱动 ;","发动机标定功率：66.2kW（90马力）；驱动方式：四轮驱动","31200","T201900370855","2024-12-30","106000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019HFH009","河南省拖拉机柴油机产品质量监督检验中心","（2018）委字整机类第 0180800667 号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","90-100马力四轮驱动拖拉机","山东飞迅驰农业装备有限公司","轮式拖拉机","飞驰904","功率:90马力;驱动方式:四轮驱动 ;","外廓尺寸：4055×1690×2670(驾驶室：4055×1915×2700)；驱动型式：四轮驱动；配套功率：66.2kW; 发动机型号及制造商：YN4E095-32CR4,昆明云内动力股份有限公司；轴距：2090; 最小使用质量：2550（驾驶室：2650）; 配重：144/180; 档位数：12+12; 变速箱型式：4×3×(1+1)组成式；是否有驾驶室或安全架：有安全架及驾驶室","31200","鄂2019377","2024-09-27","105800.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","  FH19GW0721/FH19GW0742","国家拖拉机质量监督检验中心","（2018）委字整机类第0180800641号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","90-100马力四轮驱动拖拉机","潍坊米基林农业机械有限公司","轮式拖拉机","904-N","功率:90马力;驱动方式:四轮驱动 ;","结构尺寸（长×宽×高mm）:3800×1710×2650（驾驶室） 3800×1620×2500（安全架）；最小使用质量（kg）:2470（安全架）、2550（驾驶室）；轴距（mm）:1980； 轮距（前轮/后轮）（mm）:1300/1300；；选装轮距（前轮/后轮）（mm）: 1200、1300、1400/1200、1300、1400； 最小离地间隙（mm）:420（后牵引架底部） ;最大配重（kg）:64/60； 档位数（前进/倒退/爬行）:8/8 ；变速箱型式:4×2×（1+1） 组成式；轮胎型号（前轮/后轮）:8.3-24/11-32","31200","T202000220044","2025-03-31","107000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，未提供翻倾防护装置强度检验及可靠性试验报告。","","","","",""]
["动力机械","拖拉机","轮式拖拉机","90-100马力四轮驱动拖拉机","潍坊米基林农业机械有限公司","轮式拖拉机","904-H","功率:90马力;驱动方式:四轮驱动 ;","结构尺寸（长×宽×高mm）:4000×1850×2700（驾驶室） 4000×1780×2600（安全架）；最小使用质量（kg）:2650（安全架）、2750（驾驶室）；轴距（mm）:2050； 轮距（前轮/后轮）（mm）:1450/1400；；选装轮距（前轮/后轮）（mm）:1250、1350、1450/1250～1560 ； 最小离地间隙（mm）:370（前桥放油螺栓） ;最大配重（kg）:130/60； 档位数（前进/倒退/爬行）: 12/12；变速箱型式:4 ×3×(1+1)组成式；轮胎型号（前轮）:8.3-24/14.9-30；","31200","T202000220045","2025-03-31","108500.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，未提供翻倾防护装置强度检验及可靠性试验报告。","","","","",""]
["动力机械","拖拉机","轮式拖拉机","90-100马力四轮驱动拖拉机","京山三雷重工股份有限公司","轮式拖拉机","雷木904BB","功率:90马力;驱动方式:四轮驱动 ;","型式:四轮驱动，外廓尺寸(mm):3830×1650×2650（安全框架）3830×1650×2450（四柱驾驶室）3830×1650×2450（六柱驾驶室），轴距2000mm,最小使用质量2540kg（安全架）2620kg（四柱驾驶室）2700kg（六柱驾驶室）,标准配重（前/后）:180/360（kg）,变速箱型式:机械空间组成式,换挡方式:机械有级挡,发动机型号：4C6-90U32,标定功率：66.2kW,制造商：安徽全柴动力股份有限公司，国三排放阶段。","31200","鄂2019380","2024-10-27","105500.00","","通用类","湖北省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019HFH014/NW201709023/HB2019FHZ195","河南省拖拉机柴油机产品质量监督检验中心/山东省农业机械科学研究院产品质量检测中心/湖北三智农业机械检测","HBNJ201909025","湖北三智农业机械检测有限公司"]
["动力机械","拖拉机","轮式拖拉机","100-120马力四轮驱动拖拉机","中联重机股份有限公司","轮式拖拉机","RC1104","功率:110马力;驱动方式:四轮驱动 ;","功率：110马力；型式：4×4四轮驱动；","32800","T201900511007","2024-12-30","142200.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH12GW0281","国家拖拉机质量监督检验中心","W201401033-Ⅱ","山东省农业机械产品质量监督检验站"]
["动力机械","拖拉机","轮式拖拉机","100-120马力四轮驱动拖拉机","江苏常发农业装备股份有限公司","轮式拖拉机","CFG1004-BJ","功率:100马力;驱动方式:四轮驱动 ;","整机型式：轮式；整机机架型式：无架；整机驱动型式：四驱；外廓尺寸（长×宽×高）mm：4705×2120×2924；轴距mm：2334；轮距（前轮/后轮）mm：前轮1646、1720、1900、1928，后轮1656、1688、1884、2088、；最小使用质量kg：4130；标准配重（前/后）kg：480/540；最小使用比质量kg/kw：56.2；档位数（前进/倒退）：12/12；主变速档位数：4；副变速档位数：3×（1+1）；发动机与离合器联结方式：直联式；翻倾防护装置：简易驾驶室；转向系型式：全液压转向；转向系转向操纵机构：方向盘；转向系转向机构型式：前轮转向；变速箱型式：机械平面组成式；主变速换挡方式：机械有级档；副变速换挡方式：机械有级档；轮胎型号：前轮12.4-28，后轮16.9-34；轮胎数量：前轮2个/后轮2个","32800","T201900320606","2024-12-30","135000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH20GW0351","国家拖拉机质量监督检验中心（洛阳西苑车辆与动力检验所有限公司）","（2011）委字01类第120号","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","100-120马力四轮驱动拖拉机","江苏常发农业装备股份有限公司","轮式拖拉机","CFG1104-BJ","功率:110马力;驱动方式:四轮驱动 ;","整机型式：轮式；整机机架型式：无架；整机驱动型式：四驱；外廓尺寸（长×宽×高）mm：4705×2120×2924；轴距mm：2334；轮距（前轮/后轮）mm：前轮1646、1720、1900、1928，后轮1656、1688、1884、2088、；最小使用质量kg：4140；标准配重（前/后）kg：480/540；最小使用比质量kg/kw：51.1；档位数（前进/倒退）：12/12；主变速档位数：4；副变速档位数：3×（1+1）；发动机与离合器联结方式：直联式；翻倾防护装置：简易驾驶室；转向系型式：全液压转向；转向系转向操纵机构：方向盘；转向系转向机构型式：前轮转向；变速箱型式：机械平面组成式；主变速换挡方式：机械有级档；副变速换挡方式：机械有级档；轮胎型号：前轮12.4-28，后轮16.9-34；轮胎数量：前轮2个/后轮2个","32800","T201900320606","2024-12-30","138000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH20GW0351","国家拖拉机质量监督检验中心（洛阳西苑车辆与动力检验所有限公司）","（2013）委字01类第236号","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","100-120马力四轮驱动拖拉机","山东凯斯迪尔农业装备有限公司","轮式拖拉机","DR1004","功率:73.5KW（100马力）马力;驱动方式:四轮驱动 ;","功率：73.5KW（100马力）；驱动方式：四轮驱动；最小使用质量：4095kg；\n外廓尺寸(长×宽×高)：4600mm×2100mm×2800mm(高度至空滤器顶）；\n轴距或履带接地长：2200mm；\n轮距(前轮/后轮)：1600mm、1700mm、1800mm/1620mm、1696mm、1806mm、1902mm、2012mm；\n轮距(前轮/后轮)调整方式：有级可调/无级可调；段；最小离地间隙：410mm（前桥底部放油螺栓）；\n常用轮距(前轮/后轮)：1700mm/1620mm；标准配重(前/后)：310kg/360kg；最大配重(前/后)：310kg/360kg；\n挡位数(前进/倒退/爬行)：16/8/0；","32800","部20171221","2021-12-31","111520.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","W201601011 ","山东省农业机械产品质量监督检验站","LT14GK0131 "," 国家拖拉机质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","100-120马力四轮驱动拖拉机","潍坊恒大农业装备有限公司","轮式拖拉机","HD1004-A","功率:100马力;驱动方式:四轮驱动 ;","结构尺寸（长×宽×高mm）：4100×1750×2650（驾驶室） 轴距或履带接地长（mm）：2050，常用轮距（前轮/后轮）或轨距（mm）:1300/1300,最小使用质量（kg）：3000, 标准配重（前/后）kg:140/160,档位数（前进/后退）：12/12，主变速档位*副变速档位数：4/3×（1＋1），发动机与主离合器连接方式：直联，起动方式：电启动   翻轻防护装置型式：简易驾驶室，转向系型式：全液压，转向操纵机构：方向盘，主变速换挡方式：机械有级档，副变速箱换挡方式：机械有级档，轮胎型号（前轮/后轮）：8.3-24/14.9-30，液压悬挂系统型式：分置式，悬挂装置型式：后置三点悬挂，悬挂装置类别：2类，工作装置液压油泵型号：CBN-E320,液压输出组数：2，工作装置安全阀全开压力（MPa）:18±0.5,动力输出轴花键数目：8，动力输出轴标准转速（r/min）:540/760","32800","T202000220049","2025-03-31","109800.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，不通过。可靠性试验报告与所投产品型号不符。","","WJ2019GFH020","河南省拖拉机柴油机产品质量监督检验中心","WJ2018KKKX049","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","100-120马力四轮驱动拖拉机","山东飞迅驰农业装备有限公司","轮式拖拉机","飞驰1004","功率:100马力;驱动方式:四轮驱动 ;","外廓尺寸：4055×1690×2670（驾驶室：4055×1915×2700）；驱动型式：四轮驱动；配套功率：73.5kW; 发动机型号及制造商：4C6-100C35,安徽全柴动力股份有限公司；轴距：2060; 最小使用质量：2900（驾驶室：3050）; 配重：144/180; 档位数：12+12; 变速箱型式：4×3×（1+1）组成式；是否有驾驶室或安全架：有驾驶室及安全架。","32800","鄂2019377","2024-09-27","115000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH19GW0721/FH19GW0742","国家拖拉机质量监督检验中心","（2018）委字整机类第0180800641号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","100-120马力四轮驱动拖拉机","洛阳瑞得拖拉机有限公司","轮式拖拉机","RD1004A","功率:100马力;驱动方式:四轮驱动 ;","驱动方式：四轮驱动；发动机标定功率：73.5kw","32800","T202065650012","2025-04-16","110000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019LFH010","河南省拖拉机柴油机产品质量监督检验中心","（2017）委检字整机类第2057号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","100-120马力四轮驱动拖拉机","潍坊富保田拖拉机有限公司","轮式拖拉机","1004C","功率:100马力;驱动方式:四轮驱动 ;","发动机标定功率：100马力；驱动方式：四轮驱动","32800","部20180579","2022-12-31","112000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","W201101009","山东省农业机械产品质量监督检验站","WJ2017IKKX004","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","100-120马力四轮驱动拖拉机","潍坊大申奔野机械有限公司","轮式拖拉机","M1004","功率:100马力;驱动方式:四轮驱动 ;","结构尺寸（长×宽×高mm）:4000×1910×2750，轴距或履带接地长（mm）:2140, 常用轮距（前轮/后轮） 或轨距（mm）:1510/1500，最小使用质量（kg）:3050，标准配重（前/后）kg：144/180，档位数（前进/倒退）:12/12，主变速档位数/副变速档位数4/3×(1+1)，发动机与离合器连接方式：直联，起动方式：电起动，翻倾防护装置：简易驾驶室，转向系型式：全液压，转向操纵机构：方向盘，主变速箱换挡方式：机械有级挡，副变速箱换挡方式：机械有级挡，轮胎型号（前轮/后轮）：9.5-24/16.9-30","32800","T202000220158","2025-07-05","110000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW202003017","山东省农业机械科学研究院产品质量检测中心","WJ2018EKKX004","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","100-120马力四轮驱动拖拉机","洛阳博途农业装备有限公司","轮式拖拉机","BOTON1004","功率:100马力;驱动方式:四轮驱动 ;","整机信息： 型号：BOTON1004；型式：4*4轮式；用途：一般农业用；外廓尺寸：3940mm*1900mm*2910mm；轴距：2350mm；轮距：1630~1960/1520~2120mm；最小离地间隙：450mm；最小使用质量：3765kg；挡位数：12F+4R。","32800","豫2016042","2020-12-31","135000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH15GW0511","国家拖拉机质量监督检验中心","2015KKX044","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","120-140马力四轮驱动拖拉机","潍坊红柳机械开发有限公司","轮式拖拉机","1204A","功率:120马力;驱动方式:四轮驱动 ;","发动机标定功率：120马力；驱动方式:四轮驱动","42300","部20180547","2022-12-31","150000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","W201507077","山东省农业机械产品质量监督检验站","W201403031","山东省农业机械产品质量检验站"]
["动力机械","拖拉机","轮式拖拉机","120-140马力四轮驱动拖拉机","山东凯斯迪尔农业装备有限公司","轮式拖拉机","DR1204","功率:88.2KW（120马力）马力;驱动方式:四轮驱动 ;","功率：88.2KW（120马力）；驱动方式：四轮驱动；最小使用质量：4300kg；\n外廓尺寸（长×宽×高）：4800m\nm×2190mm×2860mm；\n轴距：2500mm；\n轮距(前轮/后轮)：1600mm～1950mm/1800mm～1996mm；\n轮距(前轮/后轮)调整方式：无级可调/无级可调；最小离地间隙(离地部位)：420mm（前桥放油螺栓）；\n前轴质量/后轴质量：1700/2600kg；\t最大配重(前/后)：310/540kg；挡位数(前进/倒退/爬行)：16/8；","42300","部20160440","2020-12-31","143820.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","W201601011","山东省农业机械产品质量监督检验站","LT14GK0131","国家拖拉机质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","120-140马力四轮驱动拖拉机","山拖农机装备有限公司","轮式拖拉机","ME1204A","功率:120马力;驱动方式:四轮驱动 ;","外型尺寸（mm）：4340×2050×2895；\n驱动方式：四轮驱动\n功率（KW）:88.2（国三）\n轴距（mm）:2180\n最小使用质量（kg）:4235；\n轮距(前轮/后轮)（mm）：1610、1710、1750、1810、1850、1950/1490、1605、1700、1815、1890、2005","42300","部20160136","2020-12-31","158700.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","W201508044、W201608032","山东省农业机械产品质量监督检验站、机械工业农业机械产品质量检测中心（济南）","W201210017-Ⅱ","山东省农业机械产品质量监督检验站"]
["动力机械","拖拉机","轮式拖拉机","120-140马力四轮驱动拖拉机","江苏常发农业装备股份有限公司","轮式拖拉机","CFF1204-X","功率:120马力;驱动方式:四轮驱动 ;","型式：四轮驱动；外廓尺寸（长×宽×高）mm：4487×1970×2862（至安全架顶）；轴距mm：2135；轮距（前轮/后轮）mm：1450、1550、1650/1315、1425、1540、1700、1810；最小使用质量kg：3540；标准配重（前/后）kg：0/540； 最小使用比质量kg/kw：40.1；档位数(前进/倒退/爬行)：12/12/0，选装12/12/24；主变速档位数：4；副变速档位数：3×（1+1），选装3×（1+1）×2；发动机与离合器联结方式：直联式；起动方式：电启动；翻倾防护装置：安全框架；转向系型式：全液压；转向系转向操纵机构：方向盘；转向系转向机构型式：前轮转向；变速箱型式：机械平面组成式；主变速换挡方式：机械有级档；副变速换挡方式：机械有级档；轮胎型号（前/后）：11.2-28、8.3-24、9.5-24、8.3-24PR、9.5-24PR、11.2-24PR、11.2-24/16.9-34、14.9-30、11-32PR、14.9-30PR、16.9-30PR、13.6-38PR、16.9-30、12-38；轮胎数量（前轮/后轮）：2/2","42300","T202032320068","2025-05-28","120000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH20GW0321","国家拖拉机质量监督检验中心（洛阳西苑车辆与动力检验所有限公司）","201801004","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","120-140马力四轮驱动拖拉机","中联重机股份有限公司","轮式拖拉机","RC1204","功率:120马力;驱动方式:四轮驱动 ;","功率：120马力；型式：4×4四轮驱动；","42300","T201900511007","2024-12-30","158000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH12GW0281","国家拖拉机质量监督检验中心","W201401033-Ⅱ","山东省农业机械产品质量监督检验站"]
["动力机械","拖拉机","轮式拖拉机","120-140马力四轮驱动拖拉机","河北铠特农业机械有限公司","轮式拖拉机","KT1204","功率:120马力;驱动方式:四轮驱动 ;","发动机标定功率:88.2KW,标定转速2300R/MIN；驱动方式:四轮驱动.","42300","T201900320737","2024-12-30","143000.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过，未提供翻倾防护装置强度检验及可靠性试验报告。","","","","",""]
["动力机械","拖拉机","轮式拖拉机","120-140马力四轮驱动拖拉机","道依茨法尔机械有限公司","轮式拖拉机","CD1204-1","功率:120马力;驱动方式:四轮驱动 ;","整机驱动型式：四驱；发动机标定功率（kW）：88.2；最小使用质量（kg）：4310（驾驶室）、4200（安全架）；排放标准：第三阶段。","42300","T202000230175","2025-07-05","156000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH20GW0601/FH20GW0611","国家拖拉机质量监督检验中心","No201701078","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","120-140马力四轮驱动拖拉机","道依茨法尔机械有限公司","轮式拖拉机","CD1304-6","功率:130马力;驱动方式:四轮驱动 ;","整机驱动型式：四驱；发动机标定功率（kW）：95.6；最小使用质量（kg）：4600（驾驶室）、4490（安全架）；排放标准：第三阶段。","42300","T202000230175","2025-07-05","170000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH20GW0601/FH20GW0611","国家拖拉机质量监督检验中心","No201701078","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","140-160马力四轮驱动拖拉机","河北铠特农业机械有限公司","轮式拖拉机","KT1504","功率:150马力;驱动方式:四轮驱动 ;","发动机标定功率:110.3KW,标定转速2300R/MIN；驱动方式:四轮驱动.","57400","T201900320738","2024-12-30","192000.00","","通用类","河北省","评阅不通过","初评员：不通过","专家：不通过，未提供翻倾防护装置强度检验及可靠性试验报告。","","","","",""]
["动力机械","拖拉机","轮式拖拉机","140-160马力四轮驱动拖拉机","安徽天平机械股份有限公司","轮式拖拉机","1504","功率:150马力;驱动方式:四轮驱动 ;","外廓尺寸(长×宽×高)：5180×2345×3030mm；轴距或履带接地长：2630mm；常用轮距(前轮/后轮)或轨距：1800/1900；轮距(前轮/后轮)调整方式：翻转辐板或轮辋/无极可调；最小使用质量：5230kg；标准配重(前/后)：440/480kg；档位数(前进/倒退/爬行)：16/8/12；主变速档位数*副变速档位数/其他档位数：4/3/2；发动机与离合器联接方式：直联式；起动方式：电起动；翻倾防护装置（驾驶室或安全框架）：六柱式拖拉机驾驶室；前照灯型号：YYDT16-1(12V/24)；转向系型式：全液压转向；行车制动系型式：油浴室式盘式制动；驻车制动系型式：手制动；前驱动桥型式：旱地型；离合器型式：干式、双作用离合器、独立操纵；传动系动力输出轴离合器型式：干式/独立式操纵；传动系变速箱型式：4×（2+1）×2组合式；主变速箱换档方式：啮合套换档；副变速箱换档方式：啮合套换档；轮胎型号(前轮/后轮)：14.9-26/18.4-38","57400","2017TJ740","2021-12-31","200000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：不通过，未提供翻倾防护装置强度检验与可靠性试验报告。","","","","",""]
["动力机械","拖拉机","轮式拖拉机","140-160马力四轮驱动拖拉机","江苏沃得农业机械股份有限公司（原：江苏沃得农业机械有限公司）","轮式拖拉机","WF1404","功率:140马力;驱动方式:四轮驱动 ;","外廓尺寸（长×宽×高）（mm）：5230×2130×2760（至安全架顶）/2820（至驾驶室顶）；驱动方式：4×4四轮驱动；发动机标定功率（kW）：103；轴距（mm）：2799；最小使用质量(kg)：4578（带安全架）/4684（带驾驶室）；最大配重（前/后）（kg)：600/540；档位数（前进/倒退）：24/24；变速箱型式：机械平面组成式；可选装驾驶室或安全架。","57400","T201932320123","2024-12-30","239000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","SAM2020001、FH20GW0221","南京赛姆认证科技发展有限公司、国家拖拉机质量监督检验中心","(2018)委字整机类第01801206464号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","140-160马力四轮驱动拖拉机","江苏沃得农业机械股份有限公司（原：江苏沃得农业机械有限公司）","轮式拖拉机","WF1404-1","功率:140马力;驱动方式:四轮驱动 ;","标定功率：140马力（103kW）；驱动方式：四轮驱动；配套发动机型号：玉柴YC4A160-T303（国Ⅲ排放标准）；标定转速(r/min)：2300；外廓尺寸（长×宽×高）（mm）：4745×2130×2760（至安全架顶）/2820（至驾驶室顶）；轴距或履带接地长（mm）：2368.5；最小使用质量(kg)：4114（带安全架）/4220（带驾驶室）；发动机与主离合器联接方式：直联；变速箱（器）型式：机械平面组成式；轮胎型号（前轮/后轮）：13.6-24/16.9-34。","57400","T201932320123","2024-12-30","239000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","SAM2020001、FH20GW0221","南京赛姆认证科技发展有限公司、国家拖拉机质量监督检验中心","(2018)委字整机类第01801206464号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","140-160马力四轮驱动拖拉机","山东双力现代农业装备有限公司","轮式拖拉机","SL1504-S","功率:150马力;驱动方式:四轮驱动 ;","驱动型式：四轮驱动；配套功率：150马力；","57400","T202000510316","2025-07-05","197000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW201909044","山东省农业机械科学研究院产品质量检测中心","NW201712033","山东省农业机械科学研究院产品质量检测中心"]
["动力机械","拖拉机","轮式拖拉机","140-160马力四轮驱动拖拉机","山东双力现代农业装备有限公司","轮式拖拉机","SL1404-S","功率:140马力;驱动方式:四轮驱动 ;","驱动型式：四轮驱动；配套功率：140马力；","57400","T202000510316","2025-07-05","191500.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW201909044，NW201905012","山东省农业机械科学研究院产品质量检测中心，山东省农业机械科学研究院产品质量检测中心","NW201712033","山东省农业机械科学研究院产品质量检测中心"]
["动力机械","拖拉机","轮式拖拉机","140-160马力四轮驱动拖拉机","英轩重工有限公司","轮式拖拉机","YX1504-F1","功率:150马力;驱动方式:四轮驱动 ;","驱动方式：四轮驱动；功率(KW)：110.3KW","57400","T201932320057","2024-12-01","224300.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019IFH020","河南省拖拉机柴油机产品质量监督检验中心","(2016)委字整机类第012010214号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","140-160马力四轮驱动拖拉机","道依茨法尔机械有限公司","轮式拖拉机","CD1404-1","功率:140马力;驱动方式:四轮驱动 ;","整机驱动型式：四驱；发动机标定功率（kW）：103；最小使用质量（kg）：4310；排放标准：第三阶段。","57400","T202000230175","2025-07-05","190000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH20GW0601","国家拖拉机质量监督检验中心","No201701078","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","140-160马力四轮驱动拖拉机","道依茨法尔机械有限公司","轮式拖拉机","CD1404-6","功率:140马力;驱动方式:四轮驱动 ;","整机驱动型式：四驱；发动机标定功率（kW）：103；最小使用质量（kg）：4600；排放标准：第三阶段。","57400","T202000230175","2025-07-05","192000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH20GW0601","国家拖拉机质量监督检验中心","No201701078","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","140-160马力四轮驱动拖拉机","道依茨法尔机械有限公司","轮式拖拉机","CD1504-6","功率:150马力;驱动方式:四轮驱动 ;","整机驱动型式：四驱；发动机标定功率（kW）：110.3；最小使用质量（kg）：4610；排放标准：第三阶段。","57400","T202000230175","2025-07-05","192000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH20GW0601","国家拖拉机质量监督检验中心","No201701078","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","140-160马力四轮驱动拖拉机","道依茨法尔机械有限公司","轮式拖拉机","CD1504-1","功率:150马力;驱动方式:四轮驱动 ;","整机驱动型式：四驱；发动机标定功率（kW）：110.3；最小使用质量（kg）：4310；排放标准：第三阶段。","57400","T202000230175","2025-07-05","192000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH20GW0601","国家拖拉机质量监督检验中心","No201701078","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","140-160马力四轮驱动拖拉机","潍坊大申奔野机械有限公司","轮式拖拉机","M1404","功率:140马力;驱动方式:四轮驱动 ;","结构尺寸（长×宽×高mm）:4600×2100×2920，轴距或履带接地长（mm）:2320, 常用轮距（前轮/后轮） 或轨距（mm）:1590/1660，最小使用质量（kg）:4360，标准配重（前/后）kg：260/160，档位数（前进/倒退）:16/8，主变速档位数/副变速档位数4/（2+1）×2，发动机与离合器连接方式：直联，起动方式：电起动，翻倾防护装置：简易驾驶室，转向系型式：全液压，转向操纵机构：方向盘，主变速箱换挡方式：机械有级挡，副变速箱换挡方式：机械有级挡，轮胎型号（前轮/后轮）：12.4-24/16.9-34","57400","T202000220159","2025-07-05","192000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW202003017","山东省农业机械科学研究院产品质量检测中心","WJ2018KKKX012","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","140-160马力四轮驱动拖拉机","江苏沃得高新农业装备有限公司（原：江苏沃得植保机械有限公司、原：沃得重工（中国）有限公司）","轮式拖拉机","WF1404","功率:140马力;驱动方式:四轮驱动 ;","标定功率：140马力（103kW）；驱动方式：四轮驱动；配套发动机型号：玉柴YCA07165-T301（国Ⅲ排放标准）；标定转速(r/min)：2300；外廓尺寸（长×宽×高）（mm）：5230×2130×2760（至安全架顶）/2820（至驾驶室顶）；轴距或履带接地长（mm）：2799；最小使用质量(kg)：4578（带安全架）/4684（带驾驶室）；发动机与主离合器联接方式：直联；变速箱（器）型式：机械平面组成式；轮胎型号（前轮/后轮）：13.6-24/16.9-34。","57400","T201932320125","2024-12-30","239000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","SAM2020022、SAM2020023 ","南京赛姆认证科技发展有限公司、南京赛姆认证科技发展有限公司 ","(2018)委字整机类第01801206464号 ","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","140-160马力四轮驱动拖拉机","江苏沃得高新农业装备有限公司（原：江苏沃得植保机械有限公司、原：沃得重工（中国）有限公司）","轮式拖拉机","WF1404-1","功率:140马力;驱动方式:四轮驱动 ;","标定功率：140马力（103kW）；驱动方式：四轮驱动；配套发动机型号：玉柴YC4A160-T303（国Ⅲ排放标准）；标定转速(r/min)：2300；外廓尺寸（长×宽×高）（mm）：4745×2130×2760（至安全架顶）/2820（至驾驶室顶）；轴距或履带接地长（mm）：2368.5；最小使用质量(kg)：4114（带安全架）/4220（带驾驶室）；发动机与主离合器联接方式：直联；变速箱（器）型式：机械平面组成式；轮胎型号（前轮/后轮）：13.6-24/16.9-34。","57400","T201932320125","2024-12-30","232000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","SAM2020022、SAM2020023","南京赛姆认证科技发展有限公司、南京赛姆认证科技发展有限公司","(2018)委字整机类第01801206464号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","140-160马力四轮驱动拖拉机","江苏沃得高新农业装备有限公司（原：江苏沃得植保机械有限公司、原：沃得重工（中国）有限公司）","轮式拖拉机","WF1504","功率:150马力;驱动方式:四轮驱动 ;","标定功率：150马力（110.3kW）；驱动方式：四轮驱动；配套发动机型号：玉柴YCA07175-T301（国Ⅲ排放标准）；标定转速(r/min)：2300；外廓尺寸（长×宽×高）（mm）：5230×2075×2850（至安全架顶）/2930（至驾驶室顶）；轴距或履带接地长（mm）：2799；最小使用质量(kg)：4820（带安全架）/5000（带驾驶室）；发动机与主离合器联接方式：直联；变速箱（器）型式：机械平面组成式；轮胎型号（前轮/后轮）：14.9-26/18.4-38。","57400","T202032320099","2025-06-30","221000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","SAM2020022、SAM2020023","南京赛姆认证科技发展有限公司、南京赛姆认证科技发展有限公司","202001030","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","140-160马力四轮驱动拖拉机","安徽省传奇农业机械制造有限公司","轮式拖拉机","传奇1504-F","功率:150马力;驱动方式:四轮驱动 ;","驱动方式：四轮驱动，外廓尺寸：5040*2355*3035，轴距：2550mm，最小使用质量：5370kg，标定功率：110.3kw，标定转速：2200r/min","57400","T202000340202","2025-07-05","218000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH19GW1161","国家拖拉机质量监督检验中心","（2016）委字整机类第07001204号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","140-160马力四轮驱动拖拉机","凯斯纽荷兰工业(哈尔滨)机械有限公司","轮式拖拉机","T1404","功率:140马力;驱动方式:四轮驱动 ;","外廓尺寸(长×宽×高)：5310×2420×3030mm；轴距：2739mm；常用轮距(前轮/后轮)或轨距：1720/1730mm；轮距(前轮/后轮)调整方式：无级/无级；最小使用质量：5700kg；标准配重(前/后)：520/240kg；档位数(前进/倒退/爬行)：18/6/0；发动机与离合器联接方式：直联；起动方式：电启动；翻倾防护装置（驾驶室或安全框架）：驾驶室；转向系型式：静液压转向；行车制动系型式：液压助力制动；驻车制动系型式：机械制动；前驱动桥型式：旱地型；离合器型式：湿式多片；动力输出轴离合器型式：湿式离合器；传动系变速箱型式：电液控制；主变速箱换档方式：区域动力换档；副变速箱换档方式：动力换向；","57400","T201900020244","2024-12-30","482400.00","","通用类","黑龙江","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FCB200620ROPS","丹麦农业科学研究所比格霍尔姆检测中心","KK-3（2011）016","黑龙江省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","140-160马力四轮驱动拖拉机","凯斯纽荷兰工业(哈尔滨)机械有限公司","轮式拖拉机","T1554","功率:155马力;驱动方式:四轮驱动 ;","外廓尺寸(长×宽×高)：5310×2420×3030mm；轴距：2739mm；常用轮距(前轮/后轮)或轨距：1980/2040mm；轮距(前轮/后轮)调整方式：无级/无级；最小使用质量：6040kg；标准配重(前/后)：520/240kg；档位数(前进/倒退/爬行)：18/6/0；发动机与离合器联接方式：直联；起动方式：电启动；翻倾防护装置（驾驶室或安全框架）：驾驶室；转向系型式：静液压转向；行车制动系型式：液压助力制动；驻车制动系型式：机械制动；前驱动桥型式：旱地型；离合器型式：湿式多片；动力输出轴离合器型式：湿式离合器；传动系变速箱型式：电液控制；主变速箱换档方式：区域动力换档；副变速箱换档方式：动力换向；","57400","T201900020244","2024-12-30","518500.00","","通用类","黑龙江","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FCB200620ROPS","丹麦农业科学研究所比格霍尔姆检测中心","KK-3（2011）016","黑龙江省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","140-160马力四轮驱动拖拉机","凯斯纽荷兰工业(哈尔滨)机械有限公司","轮式拖拉机","1404","功率:140马力;驱动方式:四轮驱动 ;","外廓尺寸(长×宽×高)：4954×2610×2805mm；轴距：2627mm；常用轮距(前轮/后轮)或轨距：1828/2120mm；轮距(前轮/后轮)调整方式：有级/有级；最小使用质量：5225kg；标准配重(前/后)：540/380kg；档位数(前进/倒退/爬行)：16/16/0；主变速档位数*副变速档位数/其他档位数：4/4/0；发动机与离合器联接方式：直联；起动方式：电启动；翻倾防护装置（驾驶室或安全框架）：驾驶室；前照灯型号：0541982；转向系型式：静液压转向；行车制动系型式：液压助力制动；驻车制动系型式：机械制动；前驱动桥型式：旱地型；离合器型式：湿式多片；动力输出轴离合器型式：湿式离合器；传动系变速箱型式：电液控制；主变速箱换档方式：区域动力换挡；副变速箱换档方式：液压助力换挡；","57400","部20170764","2021-12-31","388500.00","","通用类","黑龙江","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FCBS158ext3","丹麦奥胡斯大学比格霍尔姆农用机械检测中心","LT16GK0041","国家拖拉机质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","140-160马力四轮驱动拖拉机","艾格瑞巨明农业装备有限公司","轮式拖拉机","JM1504","功率:150马力;驱动方式:四轮驱动 ;","发动机标定功率：110.3kW；型式：四轮驱动；外廓尺寸（长×宽×高）：5250×2345×3245mm；轴距：2650mm；最小离地间隙：440mm；最小使用质量：5420kg；最大配重（前/后）：490/480kg；档位数（前进/倒退/爬行）：16/8/0；最大牵引力：≥28.0kN；变速箱型式：4×（2+1）×2组成式；翻倾防护装置：六柱式安全驾驶室；悬挂装置型式：后置三点悬挂。","57400","部20181238","2022-12-31","198000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2018FFH020","河南省拖拉机柴油机产品质量监督检验中心","WJ2018BKKX010","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","140-160马力四轮驱动拖拉机","潍坊米基林农业机械有限公司","轮式拖拉机","1404-G","功率:140马力;驱动方式:四轮驱动 ;","结构尺寸（长×宽×高mm）5120×2350×2920（驾驶室顶部）:；最小使用质量（kg）:5255；轴距（mm）:2630； 轮距（前轮/后轮）（mm）:1750/1860；；选装轮距（前轮/后轮）（mm）:1650、1750、1850、1950/1620～2420； 最小离地间隙（mm）: 460（前桥放油螺塞）;最大配重（kg）:440/240； 档位数（前进/倒退/爬行）:16/8 ；变速箱型式:；4×（2+1）×2组成式；轮胎型号（前轮/后轮）:14.9-26/18.4-38","57400","T202000340206","2025-07-05","216000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019IFH006","河南省拖拉机柴油机产品质量监督检验中心","WJ2018DKKX027","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","140-160马力四轮驱动拖拉机","潍坊米基林农业机械有限公司","轮式拖拉机","1504-H","功率:150马力;驱动方式:四轮驱动 ;","结构尺寸（长×宽×高mm）:5020×2125×2810（驾驶室顶部）；最小使用质量（kg）:4603；轴距（mm）:2620； 轮距（前轮/后轮）（mm）:1630/1670；选装轮距（前轮/后轮）（mm）:1630、1750、1850、1950/1620～2420； 最小离地间隙（mm）: 390（前桥放油螺塞）;最大配重（kg）:440/180； 档位数（前进/倒退/爬行）:16/8 ；变速箱型式:；4×（2+1）×2组成式；轮胎型号（前轮/后轮）:12.4-24/16.9-34；","57400","T202000340207","2025-07-05","215000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，可靠性试验报告与所投产品型号不符。","","WJ2019IFH006","河南省拖拉机柴油机产品质量监督检验中心","WJ2018GKKX013","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","140-160马力四轮驱动拖拉机","潍坊米基林农业机械有限公司","轮式拖拉机","1404-H","功率:140马力;驱动方式:四轮驱动 ;","结构尺寸（长×宽×高mm）:5020×2125×2810（驾驶室顶部）；最小使用质量（kg）:4603；轴距（mm）:2620； 轮距（前轮/后轮）（mm）:1630/1670；选装轮距（前轮/后轮）（mm）:1630、1750、1850、1950/1620～2420； 最小离地间隙（mm）: 390（前桥放油螺塞）;最大配重（kg）:440/180； 档位数（前进/倒退/爬行）:16/8 ；变速箱型式:；4×（2+1）×2组成式；轮胎型号（前轮/后轮）:12.4-24/16.9-34","57400","T202000340207","2025-07-05","214000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，可靠性试验报告与所投产品型号不符。","","WJ2019IFH006","河南省拖拉机柴油机产品质量监督检验中心","WJ2018GKKX013","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","140-160马力四轮驱动拖拉机","潍坊米基林农业机械有限公司","轮式拖拉机","1504-A","功率:150马力;驱动方式:四轮驱动 ;","结构尺寸（长×宽×高mm）:4630×2120×2800（驾驶室顶部）；最小使用质量（kg）:4525；轴距（mm）:2320； 轮距（前轮/后轮）（mm）:1630/1680；选装轮距（前轮/后轮）（mm）:1630、1730、1830、1930/1630～2230； 最小离地间隙（mm）: 390（前桥放油螺塞）;最大配重（kg）:440/180； 档位数（前进/倒退/爬行）:16/8 ；变速箱型式:；4×（2+1）×2组成式；轮胎型号（前轮/后轮）:12.4-24/16.9-34；","57400","T202000340207","2025-07-05","215000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，可靠性试验报告与所投产品型号不符。","","WJ2019IFH006","河南省拖拉机柴油机产品质量监督检验中心","WJ2018GKKX013","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","140-160马力四轮驱动拖拉机","潍坊米基林农业机械有限公司","轮式拖拉机","1404-A","功率:140马力;驱动方式:四轮驱动 ;","结构尺寸（长×宽×高mm）:4630×2120×2800（驾驶室顶部）；最小使用质量（kg）:4295；轴距（mm）:2320； 轮距（前轮/后轮）（mm）:1630/1680；选装轮距（前轮/后轮）（mm）:1630、1730、1830、1930/1630～2230； 最小离地间隙（mm）: 390（前桥放油螺塞）;最大配重（kg）:440/180； 档位数（前进/倒退/爬行）:16/8 ；变速箱型式:；4×（2+1）×2组成式；轮胎型号（前轮/后轮）:12.4-24/16.9-34","57400","T202000340207","2025-07-05","212000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，可靠性试验报告与所投产品型号不符。","","WJ2019IFH006","河南省拖拉机柴油机产品质量监督检验中心","WJ2018GKKX013","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","140-160马力四轮驱动拖拉机","潍坊米基林农业机械有限公司","轮式拖拉机","1504-G","功率:150马力;驱动方式:四轮驱动 ;","结构尺寸（长×宽×高mm）:5120×2350×2920（驾驶室顶部）；最小使用质量（kg）:5255；轴距（mm）:2630； 轮距（前轮/后轮）（mm）:1750/1860；；选装轮距（前轮/后轮）（mm）:1650、1750、1850、1950/1620～2420； 最小离地间隙（mm）: 460（前桥放油螺塞）;最大配重（kg）:440/240； 档位数（前进/倒退/爬行）:16/8 ；变速箱型式:；4×（2+1）×2组成式；轮胎型号（前轮/后轮）:14.9-26/18.4-38；","57400","T202000340206","2025-07-05","218000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，可靠性试验报告与所投产品型号不符。","","WJ2019IFH006","河南省拖拉机柴油机产品质量监督检验中心","WJ2018DKKX027","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","160-180马力四轮驱动拖拉机","英轩重工有限公司","轮式拖拉机","YX1604-F1","功率:160马力;驱动方式:四轮驱动 ;","驱动方式：四轮驱动；功率(KW)：118KW","61000","T201932320057","2024-12-01","265700.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019IFH020","河南省拖拉机柴油机产品质量监督检验中心","(2016)委字整机类第012010214号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","160-180马力四轮驱动拖拉机","潍坊鸿创金拖机械制造有限公司","轮式拖拉机","HC1604-A","功率:160马力;驱动方式:四轮驱动 ;","外廓尺寸(长×宽×高)mm:5045×2260×3005（空滤器顶）；轴距或履带接地长:2550mm；常用轮距(前轮/后轮)或轨距:1780/1760mm；轮距(前轮/后轮)调整方式:有级可调/无级可调；最小使用质量:5000kg；标准配重（前/后）：390/480kg； 档位数：前进/倒退/爬行：16/8/0；主变速器档位数：4；副变速器档位数/其他档位数：（2+1）/2","61000","T201900220529","2024-12-30","205000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW201908002","山东省农业机械科学研究院产品质量检测中心","NJJC20180808-CK","山东宝鼎农业机械检测有限公司"]
["动力机械","拖拉机","轮式拖拉机","160-180马力四轮驱动拖拉机","山东双力现代农业装备有限公司","轮式拖拉机","SL1604-S","功率:160马力;驱动方式:四轮驱动 ;","驱动型式：四轮驱动；配套功率：160马力；","61000","T202000510316","2025-07-05","205000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW201909044","山东省农业机械科学研究产品质量检测中心","NW201712033","山东省农业机械科学研究院产品质量检测中心"]
["动力机械","拖拉机","轮式拖拉机","160-180马力四轮驱动拖拉机","雷沃重工股份有限公司","轮式拖拉机","M1654-G","功率:165马力;驱动方式:四轮驱动 ;","驱动方式：四轮驱动；功率（kw）：121.3KW","61000","T201900230540","2024-12-30","373400.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NO.4/1 110","OECD","W2008-055-Ⅱ","山东省农业机械产品质量监督检验站"]
["动力机械","拖拉机","轮式拖拉机","160-180马力四轮驱动拖拉机","山东悍沃农业装备有限公司","轮式拖拉机","1604-D","功率:160马力;驱动方式:四轮驱动 ;","整机外廓尺寸（长×宽×高）：5000×2250×3000mm（驾驶室顶部）；轴距：2600mm；整机型式：4×4四轮驱动；标准配重：前440kg/后516kg；发动机标定功率：118kW；轮胎型号：前轮14.9-26/后轮18.4-38；最小使用质量：5100kg。","61000","T202032320021","2025-02-27","215000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019HFH004","河南省拖拉机柴油机产品质量监督检验中心","YH2019WJ01023","江苏沿海农业机械检测有限公司"]
["动力机械","拖拉机","轮式拖拉机","160-180马力四轮驱动拖拉机","山东飞迅驰农业装备有限公司","轮式拖拉机","飞驰1604","功率:160马力;驱动方式:四轮驱动 ;","外廓尺寸：5100×2100×2905；驱动型式：四轮驱动；配套功率：117.7kW; 发动机型号及制造商：LR6M3LR22/1177,一拖（洛阳）柴油4850;轴距：2500；最小使用质量：4850； 配重：440/240; 档位数：16+8; 变速箱型式：4×(2+1)×2组成式；是否有驾驶室或安全架：有驾驶室。","61000","鄂2019376","2024-09-27","210000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH19GW0732","国家拖拉机质量监督检验中心","（2018）委字整机类第0180800644号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","160-180马力四轮驱动拖拉机","山东福尔沃农业装备股份有限公司","农业轮式拖拉机","FB1604-F","功率:160马力;驱动方式:四轮驱动 ;","160马力；驱动方式：四轮驱动；发动机转速：2200r/min；外廓尺寸（长×宽×高）:5350×2330×3030mm；轴距：2650mm；最小离地间隙离地部位）：475mm；最小使用质量：5500kg;功率：118kW（选装功率：117.6kW;117.7kW.）.","61000","T201900230571","2024-12-30","250000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW201810005","山东省农业机械科学研究院产品质量检测中心","WJ2018AKKX008","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","160-180马力四轮驱动拖拉机","安徽省传奇农业机械制造有限公司","轮式拖拉机","传奇1654-F","功率:165马力;驱动方式:四轮驱动 ;","驱动方式：四轮驱动，外廓尺寸：5045*2340*3020，轴距：2550mm，最小使用质量：5340kg，标定功率：121.3kw，标定转速：2200r/min","61000","T202000340199","2025-07-05","255000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH19GW1161","国家拖拉机质量监督检验中心","（2016）委字整机类第04001204号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","160-180马力四轮驱动拖拉机","江苏沃得高新农业装备有限公司（原：江苏沃得植保机械有限公司、原：沃得重工（中国）有限公司）","轮式拖拉机","WF1604","功率:160马力;驱动方式:四轮驱动 ;","标定功率：160马力（117.6kW）；驱动方式：四轮驱动；配套发动机型号：玉柴YCA07190-T301（国Ⅲ排放标准）；标定转速(r/min)：2300；外廓尺寸（长×宽×高）（mm）：5230×2075×2850（至安全架顶）/2930（至驾驶室顶）；轴距或履带接地长（mm）：2799；最小使用质量(kg)：4820（带安全架）/5000（带驾驶室）；发动机与主离合器联接方式：直联；变速箱（器）型式：机械平面组成式；轮胎型号（前轮/后轮）：14.9-26/18.4-38。","61000","T202032320099","2025-06-30","270000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","SAM2020022、SAM2020023","南京赛姆认证科技发展有限公司、南京赛姆认证科技发展有限公司","202001030","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","160-180马力四轮驱动拖拉机","潍坊富保田拖拉机有限公司","轮式拖拉机","1604","功率:160马力;驱动方式:四轮驱动 ;","发动机标定功率 ：160马力；驱动方式：四轮驱动","61000","部20190067","2023-12-31","210000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","HL1804.45.101","山东省农业机械产品质量监督检验站","WJ2017IKKX005","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","160-180马力四轮驱动拖拉机","潍坊米基林农业机械有限公司","轮式拖拉机","1604-H","功率:160马力;驱动方式:四轮驱动 ;","结构尺寸（长×宽×高mm）:5020×2125×2810（驾驶室顶部）；最小使用质量（kg）:4830；轴距（mm）:2620； 轮距（前轮/后轮）（mm）:1630/1670；选装轮距（前轮/后轮）（mm）:1630、1750、1850、1950/1620～2420； 最小离地间隙（mm）: 460（前桥放油螺塞）;最大配重（kg）:440/180； 档位数（前进/倒退/爬行）:16/8 ；变速箱型式:；4×（2+1）×2组成式；轮胎型号（前轮/后轮）:112.4-24/16.9-34；","61000","T202000340207","2025-07-05","240000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，可靠性试验报告与所投产品型号不符。","","WJ2019IFH006","河南省拖拉机柴油机产品质量监督检验中心","WJ2018GKKX013","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","160-180马力四轮驱动拖拉机","潍坊米基林农业机械有限公司","轮式拖拉机","1604-A","功率:160马力;驱动方式:四轮驱动 ;","结构尺寸（长×宽×高mm）:4630×2120×2800（驾驶室顶部）；最小使用质量（kg）:4825；轴距（mm）:2320； 轮距（前轮/后轮）（mm）:1630/1680；选装轮距（前轮/后轮）（mm）:1630、1730、1830、1930/1630～2230； 最小离地间隙（mm）: 390（前桥放油螺塞）;最大配重（kg）:440/180； 档位数（前进/倒退/爬行）:16/8 ；变速箱型式:；4×（2+1）×2组成式；轮胎型号（前轮/后轮）:12.4-24/16.9-34；","61000","T202000340207","2025-07-05","240000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，可靠性试验报告与所投产品型号不符。","","WJ2019IFH006","河南省拖拉机柴油机产品质量监督检验中心","WJ2018GKKX013","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","160-180马力四轮驱动拖拉机","潍坊米基林农业机械有限公司","轮式拖拉机","1604-G","功率:160马力;驱动方式:四轮驱动 ;","结构尺寸（长×宽×高mm）:5120×2350×2920（驾驶室顶部）；最小使用质量（kg）:5255；轴距（mm）:2630； 轮距（前轮/后轮）（mm）:1750/1860；；选装轮距（前轮/后轮）（mm）:1650、1750、1850、1950/1620～2420； 最小离地间隙（mm）: 460（前桥放油螺塞）;最大配重（kg）:440/240； 档位数（前进/倒退/爬行）:16/8 ；变速箱型式:；4×（2+1）×2组成式；轮胎型号（前轮/后轮）:14.9-26/18.4-38；","61000","T202000340206","2025-07-05","241000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，可靠性试验报告与所投产品型号不符。","","WJ2019IFH006","河南省拖拉机柴油机产品质量监督检验中心","WJ2018DKKX027","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","160-180马力四轮驱动拖拉机","艾格瑞巨明农业装备有限公司","轮式拖拉机","JM1654","功率:165马力;驱动方式:四轮驱动 ;","发动机标定功率：122kW；型式：四轮驱动；外廓尺寸（长×宽×高）：5300×2250×3100mm；轴距：2750mm；最小离地间隙：470mm；最小使用质量：5760kg；最大配重（前/后）：570/720kg；档位数（前进/倒退/爬行）：16/8/0；最大牵引力：≥32.0kN；变速箱型式：4×（2+1）×2组成式；翻倾防护装置：六柱式安全驾驶室；悬挂装置型式：后置三点悬挂。","61000","部20181235","2022-12-31","210000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2018FFH020","河南省拖拉机柴油机产品质量监督检验中心","WJ2018BKKX011","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","180-200马力四轮驱动拖拉机","山东凯斯迪尔农业装备有限公司","轮式拖拉机","DR1804","功率:132.5KW（180马力）马力;驱动方式:四轮驱动 ;","功率：132.5KW（180马力）；驱动方式：四轮驱动；最小使用质量：6900kg,K值（kg/kw）：52.08（单胎）;最小使用质量:7620kg,K值（kg/kw）：57.51（双胎）\n外廓尺寸(长×宽×高)：5400mm×2400mm×3285mm（单胎）；5400mm×3360mm×3285mm（双胎）；\n轴距或履带接地长：2820mm；\n轮距(前轮/后轮)：1720mm、1820mm、1945mm、2000mm、2100mm/1700mm～2790mm（单胎）；1720mm、1820mm、1945mm、2000mm、2100mm/2330mm（双胎）；\n 最小离地间隙：450mm；\n常用轮距(前轮/后轮)：1945mm/1930mm（单胎）；1945mm/2330mm（双胎）；标准配重(前/后)：780kg/480kg（单胎）；780kg/0kg（双胎）；最大配重(前/后)：900kg/1200kg（单胎）；900kg/0kg（双胎）；挡位数(前进/倒退/爬行)：16/16/0；主变速/副变速/其他:4/4/(1+1)","64800","T202032320014","2025-02-27","220320.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH19GW1351","国家拖拉机质量监督检验中心","（2018）委字整机类第0180100228号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","180-200马力四轮驱动拖拉机","雷沃重工股份有限公司","轮式拖拉机","M1854-G","功率:185马力;驱动方式:四轮驱动 ;","驱动方式：四轮驱动；功率（kw）：136KW；","64800","T201900230540","2024-12-30","342900.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NO.4/1 110","OECD","W2008-055-Ⅱ","山东省农业机械产品质量监督检验站 "]
["动力机械","拖拉机","轮式拖拉机","180-200马力四轮驱动拖拉机","安徽天平机械股份有限公司","轮式拖拉机","JH1804","功率:180马力;驱动方式:四轮驱动 ;","外廓尺寸(长×宽×高)：5180×2220×3030mm；轴距或履带接地长：2630mm；常用轮距(前轮/后轮)或轨距：1800/1900；轮距(前轮/后轮)调整方式：有级可调/无级可调；最小使用质量：5460kg；标准配重(前/后)：520/240kg；档位数(前进/倒退/爬行)：16/8/0；主变速档位数*副变速档位数/其他档位数：4/（2+1）×2/0；发动机与离合器联接方式：直联；起动方式：电起动；翻倾防护装置（驾驶室或安全框架）：六柱式；前照灯型号：YYDT16-1；转向系型式：前轮液压转向；行车制动系型式：湿式、盘式制动器、静液压操纵；驻车制动系型式：独立式手制动；前驱动桥型式：旱地型；离合器型式：单片、干式、双作用；传动系动力输出轴离合器型式：单片、干式、双作用；传动系变速箱型式：4×（2+1）×2组成式；主变速箱换档方式：啮合套换挡；副变速箱换档方式：啮合套换挡；轮胎型号(前轮/后轮)：14.9-26/18.4-38","64800","2019TJ159","2023-12-31","270000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：不通过，可靠性试验报告与所投产品型号不符。","","NW201705045","山东省农业机械科学研究院产品质量检测中心","NJJC20180714","山东宝鼎农业机械检查有限公司"]
["动力机械","拖拉机","轮式拖拉机","180-200马力四轮驱动拖拉机","山东瑞泽重工有限公司","轮式拖拉机","RG1804","功率:180马力;驱动方式:四轮驱动 ;","驱动方式：四轮驱动  功率：180马力","64800","部20171017","2021-12-31","250000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。承诺书版本过期；未提供翻倾防护装置强度检验与可靠性试验报告。","","","","",""]
["动力机械","拖拉机","轮式拖拉机","180-200马力四轮驱动拖拉机","山东双力现代农业装备有限公司","轮式拖拉机","SL1804-A","功率:180马力;驱动方式:四轮驱动 ;","驱动型式：四轮驱动；配套功率：180马力；","64800","T202000510317","2025-07-05","216500.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW201909047","山东省农业机械科学研究院产品质量检测中心","NW201712034","山东省农业机械科学研究院产品质量检测中心"]
["动力机械","拖拉机","轮式拖拉机","180-200马力四轮驱动拖拉机","潍坊鸿创金拖机械制造有限公司","轮式拖拉机","HC1804","功率:180马力;驱动方式:四轮驱动 ;","外廓尺寸(长×宽×高)mm:5150×2300×3170（驾驶室）；轴距或履带接地长:2760mm；常用轮距(前轮/后轮)或轨距:1790/1730mm；轮距(前轮/后轮)调整方式:有级可调/无级可调；最小使用质量:5600kg；标准配重（前/后）：200/320kg； 档位数：前进/倒退/爬行：16/8/0；主变速器档位数：4；副变速器档位数/其他档位数：（2+1）/2","64800","T201900220522","2024-12-30","216000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW201908002","山东省农业机械科学研究院产品质量检测中心","NJJC20180808-DK","山东宝鼎农业机械检测有限公司"]
["动力机械","拖拉机","轮式拖拉机","180-200马力四轮驱动拖拉机","英轩重工有限公司","轮式拖拉机","YX1804-G1","功率:180马力;驱动方式:四轮驱动 ;","驱动方式：四轮驱动；功率(KW)：132.5KW","64800","T201932320101","2024-12-30","351800.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019IFH035","河南省拖拉机柴油机产品质量监督检验中心","(2016)委字整机类第012010212号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","180-200马力四轮驱动拖拉机","英轩重工有限公司","轮式拖拉机","YX1804-F1","功率:180马力;驱动方式:四轮驱动 ;","驱动方式：四轮驱动；功率(KW)：132.5KW","64800","T201932320057","2024-12-01","325800.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019KFH011","河南省拖拉机柴油机产品质量监督检验中心","(2016)委字整机类第012010214号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","180-200马力四轮驱动拖拉机","江苏悦达智能农业装备有限公司","轮式拖拉机","YR1804","功率:180马力;驱动方式:四轮驱动 ;","发动机功率：132.5千瓦；国三排放；四轮驱动:(1+1)*4*2*4组合式变速箱；整机最小使用质量：7850kg；整机外廓尺寸(长×宽×高)mm5585*2560*3450；动力输出轴后置独立式","64800","苏农机（2019）第（0147）号","2023-12-31","265000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH19GW0421","国家拖拉机质量监督检验中心","YH2019WJ01016","江苏沿海农业机械检测有限公司"]
["动力机械","拖拉机","轮式拖拉机","180-200马力四轮驱动拖拉机","潍坊华夏拖拉机制造有限公司","轮式拖拉机","HX1804-C","功率:180马力;驱动方式:四轮驱动 ;","发动机功率：180马力；驱动方式：四轮驱动","64800","T202000320184","2025-07-05","217000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW201912030","山东省农业机械科学研究院产品质量检测中心","WJ2017LKKX016","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","180-200马力四轮驱动拖拉机","安徽省传奇农业机械制造有限公司","轮式拖拉机","传奇1854-F","功率:185马力;驱动方式:四轮驱动 ;","驱动方式：四轮驱动，外廓尺寸：5050*2385*3030，轴距：2580mm，最小使用质量：5380kg，标定功率：136kw，标定转速：2200r/min","64800","T202000340199","2025-07-05","256000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH19GW1161","国家拖拉机质量监督检验中心","（2016）委字整机类第04001204号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","180-200马力四轮驱动拖拉机","山东福尔沃农业装备股份有限公司","农业轮式拖拉机","FB1804-F","功率:180马力;驱动方式:四轮驱动 ;","180马力；驱动方式：四轮驱动；发动机转速：2200r/min；外廓尺寸（长×宽×高）:5350×2330×3030mm；最大牵引力：56.5kN；轴距：2650mm；最小离地间隙离地部位）：475mm；最小使用质量：5500kg;功率：132.5kW（功率：132.4kW）.","64800","T201900230571","2024-12-30","260000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW201810005","山东省农业机械科学研究院产品质量检测中心","WJ2018AKKX008","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","180-200马力四轮驱动拖拉机","潍坊东科重工农业装备有限公司","轮式拖拉机","DK1804-A","功率:180马力;驱动方式:四轮驱动 ;","外廓尺寸：5300×2480×3200；驱动型式：四轮驱动；配套功率：132.5kW; 发动机型号及制造商：WP6G180E330,潍柴（潍坊）中型柴油机有限公司；轴距：2710; 最小使用质量：5600; 配重：780/480; 档位数：16+8; 变速箱型式：4×(2+1)×2组成式；是否有驾驶室或安全架：有驾驶室。","64800","T202032320007","2025-02-27","245000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019IFH011","河南省拖拉机柴油机产品质量监督检验中心","(2018)委字整机类第0180100206号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","180-200马力四轮驱动拖拉机","艾格瑞巨明农业装备有限公司","轮式拖拉机","JM1804","功率:180马力;驱动方式:四轮驱动 ;","发动机标定功率：132.5kW；型式：四轮驱动；外廓尺寸（长×宽×高）：5300×2250×3135mm；轴距：2750mm；最小离地间隙：560mm；最小使用质量：6000kg；最大配重（前/后）：741/720kg；档位数（前进/倒退/爬行）：16/8/0；最大牵引力：≥32.0kN；变速箱型式：4×（2+1）×2组成式；翻倾防护装置：六柱式安全驾驶室；悬挂装置型式：后置三点悬挂。","64800","部20181234","2022-12-31","238000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2018FFH020","河南省拖拉机柴油机产品质量监督检验中心","WJ2018BKKX011","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","180-200马力四轮驱动拖拉机","艾格瑞巨明农业装备有限公司","轮式拖拉机","JG1854","功率:185马力;驱动方式:四轮驱动 ;","发动机标定功率：136kW；型式：四轮驱动；外廓尺寸（长×宽×高）：5470×2780×3215mm；轴距：2850mm；最小离地间隙：430mm；最小使用质量：6975kg；最大配重（前/后）：741/720kg；档位数（前进/倒退/爬行）：16/16/0；最大牵引力：≥35.0kN；变速箱型式：4×4×（1+1）组成式；翻倾防护装置：六柱式安全驾驶室；悬挂装置型式：后置三点悬挂。","64800","部20181239","2022-12-31","248000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2018FFH020","河南省拖拉机柴油机产品质量监督检验中心","WJ2018BKKX008","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","180-200马力四轮驱动拖拉机","潍坊米基林农业机械有限公司","轮式拖拉机","1804-S","功率:180马力;驱动方式:四轮驱动 ;","结构尺寸（长×宽×高mm）:5340×2350×3220（排气管）；最小使用质量（kg）:6740；轴距（mm）:2850； 轮距（前轮/后轮）（mm）:2000/1870；选装轮距（前轮/后轮）（mm）:1720、1820、2000、2100/1700～2300； 最小离地间隙（mm）:425（后牵引架）;最大配重（kg）:780/480； 档位数（前进/倒退/爬行）:16/16 ；变速箱型式:；4×4×（1+1）组成式；轮胎型号（前轮/后轮）:16.9-28/18.4-42","64800","T202000340209","2025-07-05","315000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，可靠性试验报告与所投产品型号不符。","","WJ2019IFH002","河南省拖拉机柴油机产品质量监督检验中心","WJ2018DKKX028","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","180-200马力四轮驱动拖拉机","潍坊米基林农业机械有限公司","轮式拖拉机","1804-G","功率:180马力;驱动方式:四轮驱动 ;","结构尺寸（长×宽×高mm）:5120×2350×2920（驾驶室顶部）；最小使用质量（kg）:5450；轴距（mm）:2630； 轮距（前轮/后轮）（mm）:1750/1860；；选装轮距（前轮/后轮）（mm）:1650、1750、1850、1950/1620～2420； 最小离地间隙（mm）: 460（前桥放油螺塞）;最大配重（kg）:440/240； 档位数（前进/倒退/爬行）:16/8 ；变速箱型式:；4×（2+1）×2组成式；轮胎型号（前轮/后轮）:14.9-26/18.4-38；","64800","T202000340206","2025-07-05","303000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，可靠性试验报告与所投产品型号不符。","","WJ2019IFH006","河南省拖拉机柴油机产品质量监督检验中心","TF2004/WJ2018DKKX027","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","180-200马力四轮驱动拖拉机","潍坊米基林农业机械有限公司","轮式拖拉机","1804-C","功率:180马力;驱动方式:四轮驱动 ;","结构尺寸（长×宽×高mm）:5210×2340×2970（驾驶室顶）；最小使用质量（kg）:5450；轴距（mm）:2700； 轮距（前轮/后轮）（mm）:1950/1860；选装轮距（前轮/后轮）（mm）:1610、1720、1810、1950/1620-2420； 最小离地间隙（mm）: 470（前桥放油螺塞）;最大配重（kg）:440/240； 档位数（前进/倒退/爬行）:16/8 ；变速箱型式:；4×（2+1）×2组成式；轮胎型号（前轮/后轮）:14.9-26/18.4-38","64800","T202000340208","2025-07-05","311000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，可靠性试验报告与所投产品型号不符。","","WJ2019IFH006","河南省拖拉机柴油机产品质量监督检验中心","（2019）2240009","潍坊市产品质量检验所"]
["动力机械","拖拉机","轮式拖拉机","200马力及以上四轮驱动拖拉机","江苏悦达智能农业装备有限公司","轮式拖拉机","YR2004","功率:200马力;驱动方式:四轮驱动 ;","发动机功率：147.5千瓦；国三排放；四轮驱动:(1+1)*4*2*4组合式变速箱；整机最小使用质量：7850kg；整机外廓尺寸(长×宽×高)mm5585*2560*3450；动力输出轴独立式","64800","苏农机（2019）第（0148）号","2023-12-31","280000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH19GW0421","国家拖拉机质量监督检验中心","YH2019WJ01016","江苏沿海农业机械检测有限公司"]
["动力机械","拖拉机","轮式拖拉机","200马力及以上四轮驱动拖拉机","英轩重工有限公司","轮式拖拉机","YX2204-G1","功率:220马力;驱动方式:四轮驱动 ;","驱动方式：四轮驱动；功率(KW)：162KW","64800","T201932320101","2024-12-30","434500.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019LFH001","河南省拖拉机柴油机产品质量监督检验中心","(2016)委字整机类第012010212号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","200马力及以上四轮驱动拖拉机","英轩重工有限公司","轮式拖拉机","YX2004-G1","功率:200马力;驱动方式:四轮驱动 ;","驱动方式：四轮驱动；功率(KW)：147KW","64800","T201932320101","2024-12-30","407500.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019LFH001","河南省拖拉机柴油机产品质量监督检验中心","(2016)委字整机类第012010212号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","200马力及以上四轮驱动拖拉机","江苏悦达智能农业装备有限公司","轮式拖拉机","YR2204","功率:220马力;驱动方式:四轮驱动 ;","发动机功率：162千瓦；国三排放；整机外廓尺寸(长×宽×高)mm5585*2560*3450；四轮驱动:(1+1)*4*2*4组合式变速箱；液压转向；整机最小使用质量：7850kg；动力输出轴独立式","64800","苏农机（2019）第（0149）号","2023-12-31","290000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。未提供翻倾防护装置强度检验与可靠性试验报告。","","","","",""]
["动力机械","拖拉机","轮式拖拉机","200马力及以上四轮驱动拖拉机","潍坊鸿创金拖机械制造有限公司","轮式拖拉机","HC2104-A","功率:210马力;驱动方式:四轮驱动 ;","外廓尺寸(长×宽×高)mm:5200×2300×3200（驾驶室顶）；轴距或履带接地长:2750mm；常用轮距(前轮/后轮)或轨距:1850/1850mm；轮距(前轮/后轮)调整方式:有级可调/无级可调；最小使用质量:6350kg；最小使用比质量：41.13；标准配重（前/后）：350/480kg； 档位数：前进/倒退/爬行：16/8/0；主变速器档位数：4；副变速器档位数/其他档位数：2×（2+1）","64800","T202000220155","2025-07-05","216000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW202003042","山东省农业机械科学研究院产品质量检测中心","NJJC20180808-DK","山东宝鼎农业机械检测有限公司"]
["动力机械","拖拉机","轮式拖拉机","200马力及以上四轮驱动拖拉机","潍坊鸿创金拖机械制造有限公司","轮式拖拉机","HC2004","功率:200马力;驱动方式:四轮驱动 ;","外廓尺寸(长×宽×高)mm:5150×2300×3170（驾驶室）；轴距或履带接地长:2760mm；常用轮距(前轮/后轮)或轨距:1790/1730mm；轮距(前轮/后轮)调整方式:有级可调/无级可调；最小使用质量:6100kg；标准配重（前/后）：200/320kg； 档位数：前进/倒退/爬行：16/8/0；主变速器档位数：4；副变速器档位数/其他档位数：（2+1）/2","64800","T201900220522","2024-12-30","216000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW201908002","山东省农业机械科学研究院产品质量检测中心","NJJC20180808-DK","山东宝鼎农业机械检测有限公司"]
["动力机械","拖拉机","轮式拖拉机","200马力及以上四轮驱动拖拉机","泰安泰山国泰拖拉机制造有限公司","轮式拖拉机","GT2104","功率:210马力;驱动方式:四轮驱动 ;","外廓尺寸（长*宽*高mm）：5300×2360×3200(驾驶室顶），驱动型式：四轮驱动，配套功率（kw）：155，发动机商标或品牌：潍柴，发动机型号：WP6G220E330，轴距（mm）：2700，最小使用质量（kg）：6480，配重（kg）(前/后)：720/720，档位数（前进/倒退）：16/8，变速箱（器）型式：机械平面组成式，机架型式：无架","64800","T202000320182","2025-07-05","221000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW202004008","山东省农业机械科学研究院产品质量检测中心","№201901130","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","200马力及以上四轮驱动拖拉机","徐州凯尔农业装备股份有限公司","轮式拖拉机","KAT2104-B","功率:210马力;驱动方式:四轮驱动 ;","发动机功率：154.4KW，驱动方式：四轮驱动。","64800","T201932320048","2024-12-01","335500.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH19GW1101","国家拖拉机质量监督检验中心","201801007","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","200马力及以上四轮驱动拖拉机","徐州凯尔农业装备股份有限公司","轮式拖拉机","KAT2004-C","功率:200马力;驱动方式:四轮驱动 ;","发动机功率：147KW，驱动方式：四轮驱动。","64800","T201932320048","2024-12-01","270000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH19GW1101","国家拖拉机质量监督检验中心","201801007","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","200马力及以上四轮驱动拖拉机","江苏常发农业装备股份有限公司","轮式拖拉机","CFH2004-X","功率:200马力;驱动方式:四轮驱动 ;","型式：四轮驱动；外廓尺寸（长×宽×高）mm：5230×2155×3110（至驾驶室顶），选装5230×（2123-3055）×3110（至驾驶室顶）；轴距mm：2677；轮距（前轮/后轮）mm：1736/1688，选装1736/1656-2588（无极调节）；最小使用质量kg：6170；标准配重（前/后）kg：0/400； 最小使用比质量kg/kw：42；档位数(前进/倒退)：16/16；主变速档位数：4；副变速档位数：4×（1+1）；发动机与离合器联结方式：直联式；起动方式：电启动；翻倾防护装置：简易驾驶室；转向系型式：全液压；转向系转向操纵机构：方向盘；转向系转向机构型式：前轮转向；变速箱型式：机械平面组成式；主变速换挡方式：机械有级档；副变速换挡方式：机械有级档；轮胎型号（前/后）：14.9-28、14.9-26、12.4/11-28PR、14.9-26PR-2、14.9R28、12.4-26PR/18.4-38、16.9-38、18.4-34R-2、18.4-38R-2、18.4R38、18.4-34PR、18.4-38PR；轮胎数量（前轮/后轮）：2/2","64800","T202032320069","2025-05-28","245000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH20GW0351","国家拖拉机质量监督检验中心（洛阳西苑车辆与动力检验所有限公司）","201801086","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","200马力及以上四轮驱动拖拉机","安徽天平机械股份有限公司","轮式拖拉机","JH2104","功率:210马力;驱动方式:四轮驱动 ;","外廓尺寸(长×宽×高)：5180×2220×3030mm；轴距或履带接地长：2630mm；常用轮距(前轮/后轮)或轨距：1800/1900；轮距(前轮/后轮)调整方式：有级可调/无级可调；最小使用质量：5550kg；标准配重(前/后)：520/480kg；档位数(前进/倒退/爬行)：16/8/0；主变速档位数*副变速档位数/其他档位数：4/（2+1）×2/0；发动机与离合器联接方式：直联；起动方式：电起动；翻倾防护装置（驾驶室或安全框架）：六柱式；前照灯型号：YYDT16-1；转向系型式：前轮液压转向；行车制动系型式：湿式、盘式制动器、静液压操纵；驻车制动系型式：独立式手制动；前驱动桥型式：旱地型；离合器型式：单片、干式、双作用；传动系动力输出轴离合器型式：单片、干式、双作用；传动系变速箱型式：4×（2+1）×2组成式；主变速箱换档方式：啮合套换挡；副变速箱换档方式：啮合套换挡；轮胎型号(前轮/后轮)：14.9-26/18.4-38","64800","2019TJ160","2023-12-31","300000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：不通过，可靠性试验报告与所投产品型号不符。","","NW201705045","山东省农业机械科学研究院产品质量检测中心","NJJC20180714","山东宝鼎农业机械检查有限公司"]
["动力机械","拖拉机","轮式拖拉机","200马力及以上四轮驱动拖拉机","山东双力现代农业装备有限公司","轮式拖拉机","SL2004-A","功率:200马力;驱动方式:四轮驱动 ;","驱动型式：四轮驱动；配套功率：200马力；","64800","T202000510317","2025-07-05","225000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW201909047","山东省农业机械科学研究院产品质量检测中心","NW201712034","山东省农业机械科学研究院产品质量检测中心"]
["动力机械","拖拉机","轮式拖拉机","200马力及以上四轮驱动拖拉机","山东时风（集团）有限责任公司","轮式拖拉机","SF2204","功率:220马力;驱动方式:四轮驱动 ;","驱动方式：四轮驱动，LR6M3LR22/1620，功率：162kW，一拖（洛阳）柴油机有限公司，第三阶段。","64800","T202000370243","2025-07-05","216432.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。。","","NW201909029-X01","山东省农业机械科学研究院产品质量检测中心","WJ2018JKKX013","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","200马力及以上四轮驱动拖拉机","潍坊奥利达机械有限公司","轮式拖拉机","ALD2104-B","功率:210马力;驱动方式:四轮驱动 ;","外廓尺寸：5190×2350×3030（消音器顶部顶部） ；驱动型式：四轮驱动；配套功率：154.4kW; 发动机型号及制造商：WP6G220E330,潍柴（潍坊）中型柴油机有限公司；轴距：2710; 最小使用质量：6405kg; 配重：720/480; 档位数： 16/8/0; 是否有驾驶室或安全架：驾驶室。","64800","T201932320093","2024-12-30","235000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019IFH015","河南省拖拉机柴油机产品质量监督检验中心","(2018)委字整机类第01801204026号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","200马力及以上四轮驱动拖拉机","潍坊奥利达机械有限公司","轮式拖拉机","ALD2204-G","功率:220马力;驱动方式:四轮驱动 ;","外廓尺寸：5450×2370×3160；驱动型式：四轮驱动；配套功率：162kW; 发动机型号及制造商：WP6G220E330,潍柴（潍坊）中型柴油机有限公司；轴距：2870; 最小使用质量：6710; 配重：780/480; 档位数：16/16; 变速箱型式：4×4×（1+1）；是否有驾驶室或安全架：有驾驶室。","64800","T201932320092","2024-12-30","235000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019IFH015","河南省拖拉机柴油机产品质量监督检验中心","(2018)委字整机类第0180100217号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","200马力及以上四轮驱动拖拉机","山东凯斯迪尔农业装备有限公司","轮式拖拉机","DR2004","功率:147KW（200马力）马力;驱动方式:四轮驱动 ;","功率：147KW（200马力） ；\n型式：四轮驱动；最小使用质量:7060kg, 最小使用比质量(kg/kw):48.02（单胎）。最小使用质量:7660kg, 最小使用比质量(kg/kw):52.10（双胎）\n外廓尺寸(长×宽×高): 5400 mm×2900 mm×3150 mm ；\n轴距或履带接地长: 2820 ；\n轮距(前轮/后轮)或轨距 : 1830mm、1900mm、1990mm/1700mm～2790mm ；\n常用轮距(前轮/后轮)或轨距; 1990mm /2050mm；  最小离地间隙：410mm ； \n 标准配重(前/后)：660/720 kg；  档位数：  前进/倒退/爬行 / 16/16/0 ；主变速/副变速/其他 ：/ 4/(1+1)；","64800","T202032320014","2025-02-27","220320.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH19GW1351","国家拖拉机质量监督检验中心","（2018）委字整机类第0180100228号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","200马力及以上四轮驱动拖拉机","山东凯斯迪尔农业装备有限公司","轮式拖拉机","DR2204-V","功率:162KW(220马力 ）马力;驱动方式:四轮驱动 ;","功率：162KW(220马力 ）；驱动方式：四轮驱动；最小使用质量:7100kg（单胎）最小使用比质量:（kg/kw）：43.82;    最小使用质量: 7700kg(双胎) ；最小使用比质量:（kg/kw）：47.53；排放阶段：国家第三阶段；","64800","T202032320014","2025-02-27","220320.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH19GW1351","国家拖拉机质量监督检验中心","（2018）委字整机类第0180100228号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","200马力及以上四轮驱动拖拉机","安徽省传奇农业机械制造有限公司","轮式拖拉机","CQ2204-G","功率:220马力;驱动方式:四轮驱动 ;","驱动方式：四轮驱动，外廓尺寸：5600*2800*3150，轴距：2880mm，最小使用质量：7100kg，标定功率：162kw，标定转速：2200r/min","64800","T202000340201","2025-07-05","296000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH19GW1881","国家拖拉机质量监督检验中心","（2016）委字整机类第07001202号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","200马力及以上四轮驱动拖拉机","潍坊东科重工农业装备有限公司","轮式拖拉机","DK-2004","功率:200马力;驱动方式:四轮驱动 ;","外廓尺寸：5300×2480×3200；驱动型式：四轮驱动；配套功率：147kW; 发动机型号及制造商：WP6G200E330,潍柴（潍坊）中型柴油机有限公司；轴距：2710; 最小使用质量：6100; 配重：780/480; 档位数：16+8; 变速箱型式：4×(2+1)×2组成式；是否有驾驶室或安全架：有驾驶室。","64800","T202032320007","2025-02-27","245000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019IFH011","河南省拖拉机柴油机产品质量监督检验中心","(2018)委字整机类第0180100206号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","200马力及以上四轮驱动拖拉机","潍坊东科重工农业装备有限公司","轮式拖拉机","DK2204-A","功率:220马力;驱动方式:四轮驱动 ;","外廓尺寸：5400×2480×3200；驱动型式：四轮驱动；配套功率：162kW; 发动机型号及制造商：WP6G220E330,潍柴（潍坊）中型柴油机有限公司；轴距：2710; 最小使用质量：6660; 配重：780/480; 档位数：16+8; 变速箱型式：4×(2+1)×2组成式；是否有驾驶室或安全架：有驾驶室。","64800","T202032320007","2025-02-27","253000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019IFH011","河南省拖拉机柴油机产品质量监督检验中心","(2018)委字整机类第0180100206号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","200马力及以上四轮驱动拖拉机","安徽省传奇农业机械制造有限公司","轮式拖拉机","传奇2104-C","功率:210马力;驱动方式:四轮驱动 ;","驱动方式：四轮驱动，外廓尺寸：5230*2360*3090，轴距：2670mm，最小使用质量：5890kg，标定功率：155kw，标定转速：2200r/min","64800","T202000340200","2025-07-05","268000.00","","通用类","安徽省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH19GW1161","国家拖拉机质量监督检验中心","（2018）委字整机类第0180606547号","（2018）委字整机类第0180606547号"]
["动力机械","拖拉机","轮式拖拉机","200马力及以上四轮驱动拖拉机","山东飞迅驰农业装备有限公司","轮式拖拉机","飞驰-2204","功率:220马力;驱动方式:四轮驱动 ;","外廓尺寸：5500×2480×3080；驱动型式：四轮驱动；配套功率：162kW; 发动机型号及制造商：WP6G220E330,潍柴（潍坊）中型柴油机有限公司；轴距：2840; 最小使用质量：6850; 配重：600/480; 档位数：16+16; 变速箱型式：4×4×(1+1)组成式；是否有驾驶室或安全架：有驾驶室。","64800","新2019279","2024-12-31","220000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH19GW0711","国家拖拉机质量监督检验中心","（2018）委字整机类第0180800646号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","200马力及以上四轮驱动拖拉机","山东骏玛道机械有限公司","轮式拖拉机","MC2004","功率:210马力;驱动方式:四轮驱动 ;","发动机标定功率：147kW（200马力）；驱动方式：四轮驱动","64800","T201900230567","2024-12-30","240000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019GHF005","河南省拖拉机柴油机产品质量监督检验中心","WJ2018LKKX004","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","200马力及以上四轮驱动拖拉机","山东骏玛道机械有限公司","轮式拖拉机","MC2104","功率:210马力;驱动方式:四轮驱动 ;","发动机标定功率：154.4kW（210马力）；驱动方式：四轮驱动","64800","T201900370854","2024-12-30","242000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019DFH025","河南省拖拉机柴油机产品质量监督检验中心","WJ2018LKKX004","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","200马力及以上四轮驱动拖拉机","山东骏玛道机械有限公司","轮式拖拉机","MG2204","功率:220马力;驱动方式:四轮驱动 ;","发动机标定功率：162kW（220马力）；驱动方式：四轮驱动","64800","T201900370853","2024-12-30","247000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019DFH024","河南省拖拉机柴油机产品质量监督检验中心","WJ2018LKKX005","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","200马力及以上四轮驱动拖拉机","潍坊富保田拖拉机有限公司","轮式拖拉机","2104","功率:210马力;驱动方式:四轮驱动 ;","标定功率：210马力；驱动方式：四轮驱动","64800","部20171771","2021-12-31","400000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","HL1804.45.101","山东省农业机械产品质量监督检验站","201701321","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","200马力及以上四轮驱动拖拉机","潍坊富保田拖拉机有限公司","轮式拖拉机","2104A","功率:210马力;驱动方式:四轮驱动 ;","发动机标定功率：210马力；驱动方式：四轮驱动","64800","部20180581","2022-12-31","370000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","HL1804.45.101","山东省农业机械产品质量监督检验站","WJ2017IKKX006","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","200马力及以上四轮驱动拖拉机","潍坊大申奔野机械有限公司","轮式拖拉机","M2204","功率:220马力;驱动方式:四轮驱动 ;","结构尺寸（长×宽×高mm）::5480×2500×3050，轴距或履带接地长（mm）:2820, 常用轮距（前轮/后轮） 或轨距（mm）:1940/1785，最小使用质量（kg）：6800，标准配重（前/后）kg：320/240，档位数（前进/倒退）:16/16，主变速档位数*副变速档位数4/4×（1+1），发动机与离合器连接方式：直联，起动方式：电起动，防翻架装置：安全框架/驾驶室，转向系型式：全液压，转向操纵机构：方向盘，主变速箱换挡方式：机械有级挡，副变速箱换挡方式：机械有级挡，轮胎型号（前轮/后轮）：18.4-26/20.8-38","64800","T202000220057","2025-03-31","380000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW201906017","山东省农业机械科学研究院产品质量检测中心","WJ2018KKKX013","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","200马力及以上四轮驱动拖拉机","潍坊大申奔野机械有限公司","轮式拖拉机","M2104-A","功率:210马力;驱动方式:四轮驱动 ;","结构尺寸（长×宽×高mm）::5480×2800×3050，轴距或履带接地长（mm）:2820, 常用轮距（前轮/后轮） 或轨距（mm）:1940/1785，最小使用质量（kg）:6750，标准配重（前/后）kg：320/240，档位数（前进/倒退）:16/16，主变速档位数*副变速档位数4/4×（1+1），发动机与离合器连接方式：直联，起动方式：电起动，防翻架装置：安全框架/驾驶室，转向系型式：全液压，转向操纵机构：方向盘，主变速箱换挡方式：机械有级挡，副变速箱换挡方式：机械有级挡，轮胎型号（前轮/后轮）：18.4-26/20.8-38","64800","T202000220057","2025-03-31","375000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW201906017","山东省农业机械科学研究院产品质量检测中心","WJ2018KKKX013","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","200马力及以上四轮驱动拖拉机","江苏沃得高新农业装备有限公司（原：江苏沃得植保机械有限公司、原：沃得重工（中国）有限公司）","轮式拖拉机","WG2404","功率:240马力;驱动方式:四轮驱动 ;","标定功率：240马力（176.5kW）；驱动方式：四轮驱动；配套发动机型号：一拖LR6M3LR22/1765（国Ⅲ排放标准）；标定转速(r/min)：2200；外廓尺寸（长×宽×高）（mm）：5510×2665（后轮单胎）/3600（后轮双胎）×3140（至驾驶室顶）；轴距或履带接地长（mm）：2860；最小使用质量(kg)：7250（后轮单胎）/7550（后轮双胎）；发动机与主离合器联接方式：直联；变速箱（器）型式：机械平面组成式；轮胎型号（前轮/后轮）：（460/85R30）/（650/70R42）（单胎）、16.9-28/20.8-38（双胎）。","64800","T202032320101","2025-06-30","440000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","SAM2020018","南京赛姆认证科技发展有限公司","202001032","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","200马力及以上四轮驱动拖拉机","江苏沃得高新农业装备有限公司（原：江苏沃得植保机械有限公司、原：沃得重工（中国）有限公司）","轮式拖拉机","WG2204","功率:220马力;驱动方式:四轮驱动 ;","标定功率：220马力（162kW）；驱动方式：四轮驱动；配套发动机型号：一拖LR6M3LR22/1620（国Ⅲ排放标准）；标定转速(r/min)：2200；外廓尺寸（长×宽×高）（mm）：5510×2665（后轮单胎）/3600（后轮双胎）×3140（至驾驶室顶）；轴距或履带接地长（mm）：2860；最小使用质量(kg)：7250（后轮单胎）/7550（后轮双胎）；发动机与主离合器联接方式：直联；变速箱（器）型式：机械平面组成式；轮胎型号（前轮/后轮）：（460/85R30）/（710/70R38）（单胎）、16.9-28/20.8-38（双胎）。","64800","T202032320101","2025-06-30","430000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","SAM2020018","南京赛姆认证科技发展有限公司","202001032","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","200马力及以上四轮驱动拖拉机","江苏沃得高新农业装备有限公司（原：江苏沃得植保机械有限公司、原：沃得重工（中国）有限公司）","轮式拖拉机","WG2004","功率:200马力;驱动方式:四轮驱动 ;","标定功率：200马力（147.5kW）；驱动方式：四轮驱动；配套发动机型号：一拖LR6M3LR23/1475（国Ⅲ排放标准）；标定转速(r/min)：2300；外廓尺寸（长×宽×高）（mm）：5510×2665（后轮单胎）/3600（后轮双胎）×3140（至驾驶室顶）；轴距或履带接地长（mm）：2860；最小使用质量(kg)：7250（后轮单胎）/7550（后轮双胎）；发动机与主离合器联接方式：直联；变速箱（器）型式：机械平面组成式；轮胎型号（前轮/后轮）：（460/85R30）/（710/70R38）（单胎）、16.9-28/20.8-38（双胎）。","64800","T202032320101","2025-06-30","429000.00","","通用类","江苏省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","SAM2020018","南京赛姆认证科技发展有限公司","202001032","江苏省农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","200马力及以上四轮驱动拖拉机","洛阳丰收农业机械装备有限公司","轮式拖拉机","芬美得-2104","功率:210马力;驱动方式:四轮驱动 ;","潍柴发动机标定功率：154.4kW；东方红发动机标定功率：155kW；驱动方式：四轮驱动；外廓尺寸（mm）长×宽×高：5230×2320×3130（空滤顶部）；轴距：2689（mm）；最小使用质量：6520（kg）排放阶段：第三阶段","64800","新2019108","2024-04-10","432000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2019IFH001","河南省拖拉机柴油机产品质量监督检验中心","WJ2018DKKX007","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","200马力及以上四轮驱动拖拉机","潍坊米基林农业机械有限公司","轮式拖拉机","2104-S","功率:210马力;驱动方式:四轮驱动 ;","结构尺寸（长×宽×高mm）:5340×2350×3220（排气管）；最小使用质量（kg）:6740；轴距（mm）:2850； 轮距（前轮/后轮）（mm）:2000/1870；选装轮距（前轮/后轮）（mm）:1720、1820、2000、2100/1700～2300； 最小离地间隙（mm）:425（后牵引架）;最大配重（kg）:780/480； 档位数（前进/倒退/爬行）:16/16 ；变速箱型式:；4×4×（1+1）组成式；轮胎型号（前轮/后轮）:16.9-28/18.4-42；","64800","T202000340209","2025-07-05","413000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过，可靠性试验报告与所投产品型号不符。","","WJ2019IFH002","河南省拖拉机柴油机产品质量监督检验中心","WJ2018DKKX028","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","200马力及以上四轮驱动拖拉机","山东天海农业装备有限公司","轮式拖拉机","GA2204S","功率:220马力;驱动方式:四轮驱动 ;","功率：220马力，162kW；驱动型式：四轮驱动；长×宽×高（mm）：5470×2500×3200(单胎)，5470×3580×3200(选装双胎）；轴距（mm）：2830；最小使用质量（kg）：6820（单胎）、7420（选装双胎）。","64800","部20181284","2022-12-31","360000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","WJ2018GFH008","河南省拖拉机柴油机产品质量监督检验中心","（2018）委检字整机类第0180600225号","盐城市农业机械试验鉴定站"]
["动力机械","拖拉机","轮式拖拉机","200马力及以上四轮驱动拖拉机","潍坊同和动力装备有限公司","轮式拖拉机","TH2104","功率:210马力;驱动方式:四轮驱动 ;","210马力；驱动方式：四轮驱动；发动机转速：2200r/min；外廓尺寸（长×宽×高）:5350×2400×3030mm；最大牵引力：54.21kN；轴距：2670mm；最小离地间隙离地部位：510mm；最小使用质量：6355kg;功率：154.4kW.","64800","T202000220138","2025-07-05","440000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW201907053","山东省农业机械科学研究院产品质量检测中心","WJ2017LKKX020","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","200马力及以上四轮驱动拖拉机","潍坊同和动力装备有限公司","轮式拖拉机","TH2004","功率:200马力;驱动方式:四轮驱动 ;","200马力；驱动方式：四轮驱动；发动机转速：2200r/min；外廓尺寸（长×宽×高）:5350×2330×3030mm；最大牵引力：35.8kN；动力输出轴标定功率下限：111.82kw；轴距：2670mm；最小离地间隙离地部位）：460mm；最小使用质量：6045kg;功率：147kW（选装功率：147.5kW；147kW）。","64800","部20190485","2023-12-31","440000.00","","通用类","山东省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","NW201907053","山东省农业机械科学研究院产品质量检测中心","WJ2017LKKX020","河南省拖拉机柴油机产品质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","80-90马力四轮驱动拖拉机(动力换档、动力换向)","第一拖拉机股份有限公司","轮式拖拉机","LX804-C","功率:80马力;驱动方式:四轮驱动 ;动力换档、动力换向:是 ;","功率：58.8KW/80马力；驱动方式：四驱；变速箱换挡方式：机械有级挡、动力换向，选装：机械有级挡、 Hi-Lo 挡（2 速动力换挡）","26200","T202000410270","2025-07-05","128000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH19GW0861/FH19GW0871/FH19GW0881","国家拖拉机质量监督检验中心","LT09GK0111","国家拖拉机质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","90-100马力四轮驱动拖拉机(动力换档、动力换向)","第一拖拉机股份有限公司","轮式拖拉机","LX954-C","功率:95马力;驱动方式:四轮驱动 ;动力换档、动力换向:是 ;","功率：70KW/95马力；驱动方式：四驱；变速箱换挡方式：机械有级挡、动力换向，选装：机械有级挡、 Hi-Lo 挡（2 速动力换挡）","33800","T202000410270","2025-07-05","140000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH19GW0861/FH19GW0871/FH19GW0881","国家拖拉机质量监督检验中心","LT09GK0111","国家拖拉机质量监督检验中心"]
["动力机械","拖拉机","轮式拖拉机","90-100马力四轮驱动拖拉机(动力换档、动力换向)","第一拖拉机股份有限公司","轮式拖拉机","LX904-C","功率:90马力;驱动方式:四轮驱动 ;动力换档、动力换向:是 ;","功率：66.2KW/90马力；驱动方式：四驱；变速箱换挡方式：机械有级挡、动力换向，选装：机械有级挡、 Hi-Lo 挡（2 速动力换挡）","33800","T202000410270","2025-07-05","135000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。可靠性试验报告与所投产品型号不符。","","FH19GW0861/FH19GW0871/FH19GW0881","国家拖拉机质量监督检验中心","LT09GK0111","国家拖拉机质量监督检验中心"]
["动力机械","拖拉机","履带式拖拉机","70-80马力履带式拖拉机","益阳富佳科技有限公司","履带拖拉机","FJ-752","功率:75马力;驱动方式:履带式:是 ;","发动机标定功率： 55.2 kW；发动机标定转速：2300r/min；履带式","36700","T202043430027","2025-04-09","138800.00","","通用类","湖南省","评阅不通过","初评员：不通过","专家：不通过。分档错误，应为50马力及以上轻型履带式拖拉机。","","","","",""]
["动力机械","拖拉机","履带式拖拉机","80-90马力履带式拖拉机","益阳富佳科技有限公司","履带拖拉机","FJ-802","功率:80马力;驱动方式:履带式:是 ;","标定功率：58.8KW;标定转速：2400r/min; 履带式","36700","湘20180803044","2022-12-31","148800.00","","通用类","湖南省","评阅不通过","初评员：不通过","专家：不通过。分档错误，应为50马力及以上轻型履带式拖拉机。","","","","",""]
["动力机械","拖拉机","履带式拖拉机","90-100马力履带式拖拉机","益阳富佳科技有限公司","履带拖拉机","FJ-902","功率:90马力;驱动方式:履带式:是 ;","发动机标定功率：66.2KW; \n发动机标定转速:2300r/min; \n驱动方式:履带式","42700","T202043430001","2025-03-24","158880.00","","通用类","湖南省","评阅不通过","初评员：不通过","专家：不通过。分档错误，应为50马力及以上轻型履带式拖拉机。","","","","",""]
["动力机械","拖拉机","履带式拖拉机","100-110马力履带式拖拉机","益阳富佳科技有限公司","履带拖拉机","FJ-1002","功率:100马力;驱动方式:履带式:是 ;","发动机标定功率：73.5KW;驱动方式:履带式","46300","T202043430001","2025-03-24","168800.00","","通用类","湖南省","评阅不通过","初评员：不通过","专家：不通过。分档错误，应为50马力及以上轻型履带式拖拉机。","","","","",""]
["动力机械","拖拉机","履带式拖拉机","100-110马力履带式拖拉机","中重开诚（重庆）机器人有限公司","履带拖拉机","CRT1002","功率:100马力;驱动方式:履带式:是 ;","整机型式：全履带式，机架型式：全架式，长宽高3340X1800X2470mm，履带接地长度1540mm，轨距1346mm,最小离地间隙410mm, 最小使用质量2700KG，最小使用比质量36.7KG/KW，档位数：前进8档/后退8档。","46300","T202032320071","2025-05-28","146000.00","","通用类","重庆市","评阅不通过","初评员：不通过","专家：不通过。分档错误，应为50马力及以上轻型履带式拖拉机。","","","","",""]
["动力机械","拖拉机","履带式拖拉机","160马力及以上履带式拖拉机","第一拖拉机股份有限公司","履带式拖拉机","C1802","功率:180马力;驱动方式:履带式:是 ;","功率：133KW/180马力；整机型式：全履带式；整机驱动型式：两驱","106900","T201900020260","2024-12-30","490000.00","","通用类","河南省","评阅不通过","初评员：不通过","专家：不通过。分档错误，应为50马力及以上轻型履带式拖拉机。","","","","",""]
["其他机械","其他机械","简易保鲜储藏设备","库容50m³以下简易保鲜储藏设备","沈阳沈一冷冷冻机有限公司","组合式冷库","ZK37","库容:37m³;","外形尺寸（长×宽×高)mm：4750×3600×2600；制冷型式：直膨式；制冷剂：R22；设计库温度（℃）：-2 ~ +10；配套总功率：5.35KW；冷凝器型式：平板式；蒸发器型式：吊顶式风机；冷风机型号：DD60；功率：1.1KW；冷风机数量：1台；库板材料（外层：彩钢板、内芯：阻燃型硬质聚氨酯）；库门尺寸（800×1800×100）；门框尺寸（1000×2000）","120","GZNJ/TJ 2019-174","2024-08-11","36000.00","","非通用类","辽宁省","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["其他机械","其他机械","简易保鲜储藏设备","库容50-100m³简易保鲜储藏设备","沈阳沈一冷冷冻机有限公司","组合式冷库","ZK86","库容:86m³;","外形尺寸（长×宽×高)mm：7400×5400×2500；制冷型式：直膨式；制冷剂：R22；设计库温度（℃）：-2 ~ +10；配套总功率：5.35KW；冷凝器型式：平板式；蒸发器型式：吊顶式冷风机；冷风机型号：DD60；功率：1.1KW；冷风机数量：1台；库板材料（外层彩钢板、内芯阻燃型硬质聚氨酯）；库门尺寸（800宽×1800高×100厚）；门框尺寸（1000宽×2000厚）","90","GZNJ/TJ 2019-175","2024-08-11","56000.00","","非通用类","辽宁省","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["其他机械","其他机械","简易保鲜储藏设备","库容200-400m³简易保鲜储藏设备","沈阳沈一冷冷冻机有限公司","组合式冷库","ZK250","库容:250m³;","外形尺寸（长×宽×高)mm：12200×6200×3700；制冷型式：直膨式；制冷剂：R22；设计库温度（℃）：0 ~ 10；配套总功率：8.64KW；冷凝器型式：平板式；蒸发器型式：吊顶式冷风机；冷风机型号：DD60；功率:：1.1KW；冷风机数量：2台；库板材料（外层彩钢板、内芯阻燃型硬质聚氨酯）；库门尺寸（800宽×1800高×100厚）；门框尺寸（1000宽×2000厚）","50","GZNJ/TJ 2019-176","2024-08-12","105000.00","","非通用类","辽宁省","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["其他机械","其他机械","简易保鲜储藏设备","库容200-400m³简易保鲜储藏设备","江苏精英冷暖设备工程有限公司","组合式冷库","ZKJY-260","库容:260m³;","库容:容积260M3 工作时间系数:≤0.8设计库温:-15至24℃ 库内温度不均匀性:≤5.0℃  压缩机冷却方式:风冷/水冷m132; 制冷压缩机功率:制冷机11.19KW(风冷)冷却器90W*4台风幕120W/220VkW;","50","苏农机（2016）第（0509）号","2020-12-31","130000.00","","非通用类","江苏省","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["其他机械","其他机械","简易保鲜储藏设备","库容400m³及以上简易保鲜储藏设备","沈阳沈一冷冷冻机有限公司","组合式冷库","ZK525","库容:525m³;","外形尺寸（长×宽×高)mm：长18000×宽9000×高3550；制冷型式：直膨式；制冷剂：R22；设计库温度（℃）：1 ~ 10 ；配套总功率：27.6KW；冷凝器型式：平板式；蒸发器型式：吊顶式冷风机；冷风机型号：DD80；功率：1.1KW；冷风机数量：4台；库板材料（外层彩钢板、内芯阻燃型硬质聚氨酯）；库门尺寸（800宽×1800高×100厚）；门框尺寸（1000宽×2000厚）","40","GZNJ/TJ 2019-177","2024-08-11","155000.00","","非通用类","辽宁省","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["其他机械","其他机械","简易保鲜储藏设备","库容400m³及以上简易保鲜储藏设备","瑞冬集团股份有限公司","组合冷库","ZK750","库容:750m³;","库容量：750立方米，主机由压缩机组（制冷系统（风冷机组）、空气循环系统、控制系统，冷风输送和回风管道，库房等组成），机组制冷量为47000W，总功率为17＋12KW，总制冷量夺：4700W，压缩机型号：C－SC603H8H，压缩机结构型式：涡旋式，压缩机制冷量：2350W，压缩机台数：2台，冷凝方式：风冷，融霜方式：加热","40","GZNJ/TJ 2019-289","2024-11-25","340000.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["其他机械","其他机械","简易保鲜储藏设备","库容400m³及以上简易保鲜储藏设备","江苏精英冷暖设备工程有限公司","组合式冷库","ZKJY-500","库容:500m³;","库容:容积500M3  库内温度不均匀性:≤5.0℃ 工作时间系数:≤0.8  设计库温:-15至24℃  压缩机冷却方式:风冷/水冷  水泵3.0KWm134;制冷压缩机功率:制冷机22.37KW冷却器150W*2台风幕120W/220VkW;","40","苏农机（2016）第（0510）号","2020-12-31","175000.00","","非通用类","江苏省","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["其他机械","其他机械","农业用北斗终端（含渔船用）","液压控制转向机,直线精度±2.5cm的北斗导航自动驾驶系统","浙江联辉智能科技有限公司","北斗农机自动导航驾驶系统","LFC800BD-2.5RY","液压控制转向机:是 ;北斗导航自动驾驶系统:是 ;直线精度:2.5cm;","液压控制转向机，北斗导航自动驾驶系统，直线精度±2.5cm；","28000","T20190606066","2024-12-31","75000.00","","非通用类","浙江省","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["其他机械","其他机械","农业用北斗终端（含渔船用）","液压控制转向机,直线精度±2.5cm的北斗导航自动驾驶系统","上海华测导航技术股份有限公司","农业机械自动驾驶系统","领航员NX100BD-2.5RY","液压控制转向机:是 ;北斗导航自动驾驶系统:是 ;直线精度:±2cm;","转向控制型式：液压；卫星接收机类型及频点：测地型GNSS接收机/北斗B1、B2、GPSL1、L2、GLONASSL1、L2；卫星接收机差分类型：CMR、RTCM3.0、RTCM3.2；卫星接收机数据更新率：10HZ；卫星接收机接收天线形式：小盘天线；移动基站信号覆盖范围≥5km；固定基站信号覆盖范围≥15km；无线电发射设备频率：223.025-235MHZ；移动基站无线电发射设备功率：2.5W；固定基站无线电发射设备功率≤25W；集成部分组成：转向控制器与卫星接收机集成；直线度精度±2cm","28000","T20190606079","2024-12-31","95000.00","","非通用类","上海市","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["其他机械","其他机械","农业用北斗终端（含渔船用）","液压控制转向机,直线精度±2.5cm的北斗导航自动驾驶系统","北京奥腾岩石科技有限公司","北斗农机自动导航驾驶系统","YanWaFreeGo2","液压控制转向机:是 ;北斗导航自动驾驶系统:是 ;直线精度:±2.5cm;","液压控制转向机，直线精度±2.5cm，行间距精度±2.5cm","28000","黑垦鉴2018131","2022-12-31","95000.00","","非通用类","北京市","评阅不通过","初评员：不通过","专家：承诺书过期；产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["其他机械","其他机械","农业用北斗终端（含渔船用）","液压控制转向机,直线精度±2.5cm的北斗导航自动驾驶系统","无锡卡尔曼导航技术有限公司","液压式北斗农机自动驾驶仪","KM-502","液压控制转向机:是 ;北斗导航自动驾驶系统:是 ;直线精度:2.5cm;","液压控制转向机 直线精度2.5cm,北斗自动驾驶系统;设备配套:含移动基站、终端显示屏、导航控制器、电磁阀、接收电台、接收天线、角度传感器等","28000","黑垦鉴2018101","2022-12-31","94000.00","","非通用类","江苏省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["其他机械","其他机械","农业用北斗终端（含渔船用）","电动方向盘,直线精度±10cm的北斗导航辅助驾驶系统","浙江联辉智能科技有限公司","北斗导航插秧机自动驾驶系统","AC01BD-5GD","直线精度:5cm;电动方向盘:是 ;北斗导航辅助(自动)驾驶系统:是 ;","型号 AC01BD-5GD型北斗 导航插秧机动驾驶系统\n转向控制型式\t/\t力矩电机控制\n车载计算机处理器型号\t/\tD2550\n车载计算机内存\tGB\t2\n车载计算机硬盘\tGB\t16\n车载计算机操作系统及软件版本\t/\tWindows xp，AZ300 v1.00\n车载计算机显示分辨率\t/\t210×135×50mm， 800×480\n车载计算机接口种类\t/\tLAN、USB、RS-232、RS422、485、GPIO\n车载计算机数据输入输出协议\t/\t支持以太网协议、CAN口协议、串口协议\n卫星接收机类型及频点\t/\tGPS(L1/L2)、GLONASS(L1/L2)、BDS(B1/B2)\n卫星接收机主板固件版本\t/\tBuild19856\n卫星接收机通道数\t/\t432通道\n卫星接收机接口种类\t/\tRS-232\n卫星接收机差分类型\t/\tDGPS、SBAS、RTK\n卫星接收机数据更新率\tHz\t10\n卫星接收机接收天线型式\t/\tGPS500 双测量天线\n转向控制器主板固件版本\t/\tAC300_V2.00\n转动电机型号规格\t/\tCTSM170-30\n角度传感器型号规格\t/\t/\n移动机站信号覆盖范围\tkm\t/\n固定基站信号覆盖范围\tkm\t/\n基站无线电发射设备频率\tMHz\t/\n移动基站无线电发射设备功率\tW\t/\n固定基站无线电发射设备功率\tW\t/\n集成部分组成\t/\t/","23800","T20190606107","2024-12-31","65000.00","","非通用类","浙江省","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["其他机械","其他机械","农业用北斗终端（含渔船用）","电动方向盘,直线精度±10cm的北斗导航辅助驾驶系统","雷沃重工股份有限公司","农业机械导航及自动作业系统","AG4BD-2.5RD","直线精度:±2.5cm;电动方向盘:是 ;北斗导航辅助(自动)驾驶系统:是 ;","电动控制转向机，直线精度±2.5cm的北斗导航自动驾驶系统","23800","GZNJ/TJ 2019-423","2025-01-20","84000.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["其他机械","其他机械","农业用北斗终端（含渔船用）","电动方向盘,直线精度±10cm的北斗导航辅助驾驶系统","雷沃重工股份有限公司","农业机械导航及自动作业系统","AG5BD-2.5RD","直线精度:±2.5cm;电动方向盘:是 ;北斗导航辅助(自动)驾驶系统:是 ;","电动控制转向机，直线精度±2.5cm的北斗导航自动驾驶系统","23800","GZNJ/TJ 2019-424","2025-01-20","86000.00","","非通用类","山东省","评阅不通过","初评员：不通过","专家：产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["其他机械","其他机械","农业用北斗终端（含渔船用）","电动方向盘,直线精度±10cm的北斗导航辅助驾驶系统","上海联适导航技术有限公司","北斗自动导航驾驶系统","AF305BD-2.5GD","直线精度:±2.5cm;电动方向盘:是 ;北斗导航辅助(自动)驾驶系统:是 ;","电动方向盘控制转向机,直线精度±2.5CM的北斗导航自动驾驶系统","23800","T20190606127","2024-12-31","80000.00","","非通用类","上海市","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["其他机械","其他机械","农业用北斗终端（含渔船用）","电动方向盘,直线精度±10cm的北斗导航辅助驾驶系统","无锡卡尔曼导航技术有限公司","电机式北斗农机自动驾驶仪","KM-503","直线精度:2.5cm;电动方向盘:是 ;北斗导航辅助(自动)驾驶系统:否 ;","电动方向盘，直线精度2.5cm 北斗自动驾驶系统;设备配套:含移动基站、终端显示屏、导航控制器、电磁阀、接收电台、接收天线、角度传感器等","23800","黑垦鉴2018147","2022-12-31","80000.00","","非通用类","江苏省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["其他机械","其他机械","驱动耙","作业幅宽≥3m","天津库恩农业机械有限公司","驱动耙","HRB302D","作业幅宽:3m;","结构型式：水平旋转\n工作状态外形尺寸（长x宽x高）：1600x3100x1200\n工作宽幅：3000mm\n耙齿间距：290mm\n耙组数量：10组\n耙齿数量：20个\n主轴转速：1000r/min","4000","T202012120037","2025-06-28","80000.00","","非通用类","天津市","评阅不通过","初评员：不通过","专家：承诺书过期；产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["其他机械","其他机械","驱动耙","作业幅宽≥3m","天津库恩农业机械有限公司","驱动耙","1BQH-4(HR4030)","作业幅宽:4m;","结构型式：水平旋转\n工作状态外形尺寸（长x宽x高）：1550x4050x1200mm\n耙组数：14个\n耙刀数：28个\n工作宽幅：4m","4000","新2019125","2024-04-10","178800.00","","非通用类","天津市","评阅不通过","初评员：不通过","专家：承诺书过期；产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["其他机械","其他机械","驱动耙","作业幅宽≥3m","天津库恩农业机械有限公司","驱动耙","HR4530","作业幅宽:4.5m;","整机配置形式：耙刀组，镇压辊，刮土器\n结构形式：水平旋转\n工作状态外形尺寸（长x宽x高）：1600x4510x1330mm\n耙组数：16个\n耙刀数：22个\n工作宽幅：4.5米","4000","新2019269","2024-08-14","206000.00","","非通用类","天津市","评阅不通过","初评员：不通过","专家：承诺书过期；产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["其他机械","其他机械","驱动耙","作业幅宽≥3m","天津库恩农业机械有限公司","驱动耙","1BQ-4(HR4004D)","作业幅宽:4m;","整机配置形式：耙刀组，镇压辊，刮土器\n结构形式：水平旋转\n工作状态外形尺寸（长x宽x高）：1600x4200x200mm\n耙组数：14个\n耙刀数：28个\n工作宽幅：4米","4000","新2019123","2024-04-10","170000.00","","非通用类","天津市","评阅不通过","初评员：不通过","专家：承诺书过期；产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]
["其他机械","其他机械","旋耕播种机","2m-2.3m旋耕施肥播种机","保定市鑫飞达农机装备有限公司","旋耕施肥播种机","2BFG-12(6)(200)","旋幅:2m;","\"结构尺寸（长*宽*高mm）： 2120*2450*1220  整机质量（kg）： 720  \n配套动力（kw）： 66.17-73.5  工作幅宽（cm）： 200  \n动力输出轴转速（r/min）： 720/540  旋耕部分耕深（cm）： 80-140  \n旋耕部分传动方式： 中间齿轮转动  旋耕部分刀辊设计转速r/min： 269/262  \n旋耕部分刀辊最大回转半径： 245  旋耕部分刀辊总安装刀数： 58  \n条播部分传动方式： 链传动  条播部分运输间隙： ≥300mm  \n播种行数（行）： 12 \n\"","3000","冀2018T-139（续）","2022-12-31","13000.00","","非通用类","河北省","评阅不通过","初评员：不通过","专家：承诺书过期。","","","","",""]
["其他机械","其他机械","旋耕播种机","2m-2.3m旋耕施肥播种机","石家庄农业机械股份有限公司","旋耕播种机","2BFG-14（8）（215）","旋幅:2.15m;","外形尺寸（长×宽×高）\t1815×2380×1435\tmm\n结构质量\t750\tkg\n纯工作小时生产率\t0.44～1.1\thm2/h\n配套拖拉机标定功率\t47.8～48.8\tkW\n配套拖拉机动力输出轴转速\t720\tr/min\n配套拖拉机常用作业挡挡次\t低Ⅱ\t挡\n配套拖拉机常用作业挡理论前进速度\t2～5\tkm/h\n旋耕部分耕深\t12～16\tcm\n旋耕部分传动方式\t中间齿轮传动\t\n旋耕部分与拖拉机联接方式\t三点悬挂\t\n旋耕部分刀辊设计转速\t267\tr/min\n旋耕部分刀辊最大回转半径\t245\tmm\n旋耕部分刀辊总安装刀数\t60\t把\n旋耕部分旋耕刀型号\tIT245\t\n条播部分传动方式\t链传动\t\n条播部分种子/肥箱容积\t74/73\tL\n条播部分运输间隙\t≥310\tmm\n条播部分排种/肥器型式\t外槽轮/外槽轮\t\n条播部分排种/肥器数量\t8月14日\t个\n条播部分排种/肥器排量调节方式\t螺纹调节\t\n条播部分开沟器型式\t双轴承双圆盘式\t\n条播部分开沟器铲尖材料\t65Mn\t\n条播部分开沟器数量\t14\t个\n条播部分开沟器深度调节范围\t40～80\tmm","3000","冀2018T—264（续）","2022-12-31","13800.00","","非通用类","河北省","评阅不通过","初评员：不通过","专家：承诺书过期；产品铭牌无铆钉，无法确认为整机铭牌。","","","","",""]