{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":396,"n_cols":9,"rows_kept":396,"merged":[[1,0,1,8],[3,0,38,0],[3,1,31,1],[3,2,10,2],[11,2,20,2],[21,2,22,2],[23,2,24,2],[25,2,30,2],[25,8,27,8],[32,1,38,1],[32,2,34,2],[35,2,36,2],[37,2,38,2],[39,0,91,0],[39,1,40,1],[39,2,40,2],[41,1,77,1],[41,2,50,2],[51,2,58,2],[59,2,69,2],[67,8,69,8],[70,2,77,2],[78,1,82,1],[78,2,82,2],[83,1,90,1],[83,2,88,2],[92,0,111,0],[92,1,95,1],[92,2,93,2],[94,2,95,2],[96,1,109,1],[96,2,109,2],[110,1,111,1],[110,2,111,2],[112,0,119,0],[112,1,115,1],[112,2,115,2],[116,1,119,1],[116,2,119,2],[120,0,184,0],[120,1,151,1],[120,2,121,2],[122,2,135,2],[136,2,148,2],[149,2,151,2],[152,1,173,1],[152,2,161,2],[162,2,173,2],[174,1,178,1],[174,2,175,2],[176,2,178,2],[179,1,182,1],[179,2,182,2],[183,1,184,1],[183,2,184,2],[183,8,184,8],[186,0,187,0],[186,1,187,1],[186,2,187,2],[188,0,256,0],[188,1,234,1],[189,2,193,2],[194,2,207,2],[209,2,234,2],[215,8,217,8],[235,1,256,1],[235,2,240,2],[241,2,250,2],[251,2,253,2],[254,2,256,2],[257,0,259,0],[258,1,259,1],[258,2,259,2],[260,0,275,0],[260,1,271,1],[260,2,265,2],[266,2,271,2],[272,1,275,1],[272,2,275,2],[276,0,277,0],[276,1,277,1],[276,2,277,2],[279,0,307,0],[279,1,299,1],[279,2,288,2],[289,2,290,2],[291,2,296,2],[297,2,299,2],[300,1,307,1],[300,2,304,2],[305,2,307,2],[308,0,343,0],[308,1,320,1],[308,2,315,2],[316,2,320,2],[321,1,343,1],[321,2,323,2],[324,2,327,2],[328,2,329,2],[330,2,332,2],[333,2,339,2],[340,2,341,2],[342,2,343,2],[344,0,384,0],[344,1,384,1],[344,2,372,2],[356,8,372,8],[373,2,374,2],[375,2,384,2],[379,8,382,8],[385,0,391,0],[385,1,391,1],[385,2,388,2],[389,2,391,2],[392,0,393,0],[392,1,393,1],[394,0,395,0],[394,1,395,1],[394,2,395,2]]}
["附件2"]
["河南省2021-2023年农机购置补贴机具补贴额一览表（第一批、第二批2022修订）（公告稿）"]
["大类","小类","品目","档次编号","档次名称","基本配置和参数","类型","中央财政补贴额（元）","备注"]
["耕整地机械","耕地机械","犁",1,"犁体幅宽35cm以下，1—2铧翻转犁","犁体幅宽＜35cm；铧体个数1、2铧","非通用类",590]
[{"$nulls":3},2,"犁体幅宽35cm以下，3—4铧翻转犁","犁体幅宽＜35cm；铧体个数3、4铧","非通用类",990]
[{"$nulls":3},3,"犁体幅宽35cm以下，5铧及以上翻转犁","犁体幅宽＜35cm；铧体个数≥5铧","非通用类",1900]
[{"$nulls":3},4,"犁体幅宽35cm及以上，1—2铧翻转犁","犁体幅宽≥35cm；铧体个数1、2铧","非通用类",590]
[{"$nulls":3},5,"犁体幅宽35cm及以上，3—4铧翻转犁","犁体幅宽≥35cm；铧体个数3、4铧","非通用类",2300]
[{"$nulls":3},6,"犁体幅宽35cm及以上，5—6铧翻转犁","犁体幅宽≥35cm；铧体个数5、6铧","非通用类",3000]
[{"$nulls":3},7,"犁体幅宽35—45cm，7铧及以上翻转犁","35cm≤犁体幅宽＜45cm；铧体个数≥7铧","非通用类",3100]
[{"$nulls":3},8,"犁体幅宽45cm及以上，7铧及以上翻转犁","犁体幅宽≥45cm；铧体个数≥7铧","非通用类",3100]
[null,null,"旋耕机",1,"单轴1—1.5m旋耕机","单轴；1m≤耕幅＜1.5m","通用类",300]
[{"$nulls":3},2,"单轴1.5—2m旋耕机","单轴；1.5m≤耕幅＜2m","通用类",900]
[{"$nulls":3},3,"单轴2—2.5m旋耕机","单轴；2m≤耕幅＜2.5m","通用类",1600]
[{"$nulls":3},4,"单轴2.5m及以上旋耕机","单轴；耕幅≥2.5m","通用类",2200]
[{"$nulls":3},5,"双轴1—1.5m旋耕机","双轴；1m≤耕幅＜1.5m","通用类",500]
[{"$nulls":3},6,"双轴1.5—2m旋耕机","双轴；1.5m≤耕幅＜2m","通用类",1200]
[{"$nulls":3},7,"双轴2—2.5m旋耕机","双轴；2m≤耕幅＜2.5m","通用类",2600]
[{"$nulls":3},8,"双轴2.5m及以上旋耕机","双轴；耕幅≥2.5m","通用类",2900]
[{"$nulls":3},9,"1.2—2m履带自走式旋耕机","型式：履带自走式；1.2m≤耕幅＜2m","通用类",7600]
[{"$nulls":3},10,"2m及以上履带自走式旋耕机","型式：履带自走式；耕幅≥2m","通用类",15100]
[null,null,"微型耕耘机",1,"功率4kW以下微耕机","配套发动机功率＜4kW","非通用类",510]
[{"$nulls":3},2,"功率4kW及以上微耕机","配套发动机功率≥4kW","非通用类",700]
[null,null,"耕整机",1,"功率4kW以下耕整机","配套发动机功率＜4kW","非通用类",510]
[{"$nulls":3},2,"功率4kW及以上耕整机","配套发动机功率≥4kW","非通用类",700]
[null,null,"深松机",1,"2—3铲凿铲式深松机","深松部件2、3个；深松铲结构形式：凿铲式；铲间距≥180mm","通用类",1000,"凿铲式深松机档次的深松铲结构型式既包含凿铲式的单一型式，也包含凿铲式和偏柱式的混合型式，相关产品均可按深松部件和铲间距要求投档。"]
[{"$nulls":3},2,"4—5铲凿铲式深松机","深松部件4、5个；深松铲结构形式：凿铲式；铲间距≥180mm","通用类",1700]
[{"$nulls":3},3,"6铲及以上凿铲式深松机","深松部件6个及以上；深松铲结构形式：凿铲式；铲间距≥180mm","通用类",2500]
[{"$nulls":3},4,"2—3铲偏柱式、全方位式深松机","深松部件2、3个；深松铲结构形式：偏柱式或全方位式；铲间距≥330mm","通用类",1200]
[{"$nulls":3},5,"4—5铲偏柱式、全方位式深松机","深松部件4、5个；深松铲结构形式：偏柱式或全方位式；铲间距≥330mm","通用类",2300]
[{"$nulls":3},6,"6铲及以上偏柱式、全方位式深松机","深松部件6个及以上；深松铲结构形式：偏柱式或全方位式；铲间距≥330mm","通用类",2900]
[null,null,"开沟机",1,"开沟深度50cm以下配套轮式拖拉机开沟机","开沟深度＜50cm；配套轮式拖拉机","非通用类",840]
[null,"整地机械","耙（限圆盘耙、驱动耙）",1,"2—3m圆盘耙","2m≤工作幅宽＜3m","非通用类",900]
[{"$nulls":3},2,"3—3.5m圆盘耙","3m≤工作幅宽＜3.5m","非通用类",2000]
[{"$nulls":3},3,"3.5m及以上圆盘耙","工作幅宽≥3.5m","非通用类",2900]
[null,null,"埋茬起浆机",1,"2—2.5m埋茬起浆机","2m≤工作幅宽＜2.5m","非通用类",1600]
[{"$nulls":3},2,"2.5m及以上埋茬起浆机","工作幅宽≥2.5m","非通用类",2200]
[null,null,"起垄机",1,"1-2m起垄机","1m≤工作幅宽＜2m","非通用类",720]
[{"$nulls":3},2,"2m及以上起垄机","工作幅宽≥2m","非通用类",1000]
["种植施肥机械","种子播前处理和育苗机械设备","育秧（苗）播种设备",1,"生产率200—500盘/h秧盘播种成套设备","200盘/h≤生产率＜500盘/h；含铺底土、播种、洒水、覆土功能","非通用类",1000]
[{"$nulls":3},2,"生产率500盘/h及以上秧盘播种成套设备","生产率≥500盘/h；含铺底土、播种、洒水、覆土功能","非通用类",2500]
[null,"播种机械（可含施肥功能）","条播机",1,"6行条播机","播种行数：6行","非通用类",350]
[{"$nulls":3},2,"7—11行条播机","7行≤播种行数≤11行","非通用类",670]
[{"$nulls":3},3,"12—18行条播机","12行≤播种行数≤18行","非通用类",890]
[{"$nulls":3},4,"19—24行条播机","19行≤播种行数≤24行","非通用类",1400]
[{"$nulls":3},5,"25行及以上条播机","播种行数≥25行","非通用类",2000]
[{"$nulls":3},6,"6行及以下免耕条播机","播种行数≤6行；作业幅宽≥1m","通用类",810]
[{"$nulls":3},7,"7—11行免耕条播机","7行≤播种行数≤11行","通用类",2300]
[{"$nulls":3},8,"12—18行免耕条播机","12行≤播种行数≤18行","通用类",3500]
[{"$nulls":3},9,"19—24行免耕条播机","19行≤播种行数≤24行","通用类",4300]
[{"$nulls":3},10,"25行及以上免耕条播机","播种行数≥25行","通用类",4300]
[null,null,"穴播机",1,"2—3行穴播机","播种行数2、3行","通用类",560]
[{"$nulls":3},2,"4—5行穴播机","播种行数4、5行","通用类",1000]
[{"$nulls":3},3,"6行及以上穴播机","播种行数≥6行","通用类",1400]
[{"$nulls":3},4,"2—3行免耕穴播机","普通排种器；播种行数2、3行","通用类",840]
[{"$nulls":3},5,"4—5行免耕穴播机","普通排种器；播种行数4、5行","通用类",1400]
[{"$nulls":3},6,"6行及以上免耕穴播机","普通排种器；播种行数≥6行","通用类",2700]
[{"$nulls":3},7,"8行及以上悬挂式或牵引式穴播水稻直播机","播种行数≥8行；型式：悬挂式或牵引式","非通用类",2500]
[{"$nulls":3},8,"8行及以上四轮乘坐自走式穴播水稻直播机","播种行数≥8行；型式：四轮乘坐自走式；专用底盘","非通用类",10000,"专用底盘：是针对自走式水稻直播机专门设计，拆除水稻直播系统外不能作为其他机械使用的底盘。"]
[null,null,"单粒（精密）播种机",1,"2—3行机械式精量播种机","结构型式：机械式；播种行数2、3行","通用类",790]
[{"$nulls":3},2,"4—5行机械式精量播种机","结构型式：机械式；播种行数4、5行","通用类",1600]
[{"$nulls":3},3,"6—10行机械式精量播种机","结构型式：机械式；6行≤播种行数≤10行","通用类",3100]
[{"$nulls":3},4,"11行及以上机械式精量播种机","结构型式：机械式；播种行数≥11行","通用类",3100]
[{"$nulls":3},5,"2—3行气力式精量播种机","结构型式：气力式；播种行数2、3行","通用类",930]
[{"$nulls":3},6,"4—5行气力式精量播种机","结构型式：气力式；播种行数4、5行","通用类",2200]
[{"$nulls":3},7,"6—10行气力式精量播种机","结构型式：气力式；6行≤播种行数≤10行","通用类",3900]
[{"$nulls":3},8,"11行及以上气力式精量播种机","结构型式：气力式；播种行数≥11行","通用类",3900]
[{"$nulls":3},9,"2—3行免耕精量播种机","精量排种器；播种行数2、3行","通用类",850,"精量排种器包括气力式和达到精量要求的指夹式，其他列为普通型式。"]
[{"$nulls":3},10,"4—5行免耕精量播种机","精量排种器；播种行数4、5行","通用类",1400]
[{"$nulls":3},11,"6行及以上免耕精量播种机","精量排种器；播种行数≥6行","通用类",3200]
[null,null,"根（块）茎种子播种机",1,"3行及以下手扶自走式大蒜播种机","手扶自走式；播种行数≤3行；空穴率≤1.5%；正芽率≥80%","非通用类",1600]
[{"$nulls":3},2,"4行及以上手扶自走式大蒜播种机","手扶自走式；播种行数≥4行；空穴率≤1.5%；正芽率≥80%","非通用类",3200]
[{"$nulls":3},3,"5行及以下自走式大蒜播种机","自走式；播种行数≤5行；空穴率≤1.5%；正芽率≥80%","非通用类",5700]
[{"$nulls":3},4,"6—9行自走式大蒜播种机","自走式；6行≤播种行数≤9行；空穴率≤1.5%；正芽率≥80%","非通用类",19000]
[{"$nulls":3},5,"10行及以上自走式大蒜播种机","自走式；播种行数≥10行；空穴率≤1.5%；正芽率≥80%","非通用类",24800]
[{"$nulls":3},6,"5行及以下悬挂式或牵引式大蒜播种机","悬挂式或牵引式；播种行数≤5行；空穴率≤1.5%；正芽率≥80%","非通用类",5000]
[{"$nulls":3},7,"6—9行悬挂式或牵引式大蒜播种机","悬挂式或牵引式；6行≤播种行数≤9行；空穴率≤1.5%；正芽率≥80%","非通用类",12500]
[{"$nulls":3},8,"10行及以上悬挂式或牵引式大蒜播种机","悬挂式或牵引式；播种行数≥10行；空穴率≤1.5%；正芽率≥80%","非通用类",23200]
[null,"耕整地播种作业机械（可含施肥功能）","旋耕播种机",1,"6行及以下旋耕施肥播种机","播种行数≥6行；工作幅宽≥1m","非通用类",810]
[{"$nulls":3},2,"7-11行旋耕施肥播种机","7行≤播种行数≤11行","非通用类",2300]
[{"$nulls":3},3,"12—18行旋耕施肥播种机","12行≤播种行数≤18行","非通用类",3500]
[{"$nulls":3},4,"19—24行旋耕施肥播种机","19行≤播种行数≤24行","非通用类",4300]
[{"$nulls":3},5,"25行及以上旋耕施肥播种机","播种行数≥25行","非通用类",4300]
[null,"栽植机械","插秧机",1,"4行手扶步进式水稻插秧机","手扶步进式；4行","通用类",4500]
[{"$nulls":3},2,"6行及以上手扶步进式水稻插秧机","手扶步进式；6行及以上","通用类",5700]
[{"$nulls":3},3,"6行及以上独轮乘坐式水稻插秧机","独轮乘坐式；6行及以上","通用类",3400]
[{"$nulls":3},4,"4—5行四轮乘坐式水稻插秧机","四轮乘坐式；4、5行","通用类",12400]
[{"$nulls":3},5,"6—7行四轮乘坐式水稻插秧机","四轮乘坐式；6、7行","通用类",29000]
[{"$nulls":3},6,"8行及以上四轮乘坐式水稻插秧机","四轮乘坐式；8行及以上","通用类",37400]
[null,null,"抛秧机",1,"13行及以上四轮乘坐式水稻有序抛秧机","工作行数≥13行；四轮乘坐式；有序抛秧","非通用类",30300]
[null,null,"移栽机",1,"2行及以上四轮乘坐自走式秧苗移栽机","工作行数≥2行；四轮乘坐自走式","非通用类",5200]
[null,"施肥机械","侧深施肥装置",1,"6行及以上水稻侧深施肥装置","行数≥6行；配置强制施肥装置、漏施堵塞报警装置、插秧施肥同步控制装置、施肥量调节装置","非通用类",4600]
["田间管理机械","中耕机械","中耕机",1,"1—2m中耕机","1m≤作业幅宽＜2m","非通用类",400]
[{"$nulls":3},2,"2—3m中耕机","2m≤作业幅宽＜3m","非通用类",600]
[null,null,"田园管理机",1,"功率4kW以下田园管理机","配套发动机功率＜4kW","非通用类",510]
[{"$nulls":3},2,"功率4kW及以上田园管理机","配套发动机功率≥4kW","非通用类",700]
[null,"植保机械","喷雾机",1,"4—12m悬挂式喷杆喷雾机","4m≤喷杆长度＜12m；药箱≥400L；型式：悬挂式","通用类",730]
[{"$nulls":3},2,"12—18m悬挂式喷杆喷雾机","12m≤喷杆长度＜18m；药箱≥600L；型式：悬挂式","通用类",1400]
[{"$nulls":3},3,"18m及以上悬挂式喷杆喷雾机","喷杆长度≥18m；药箱≥800L；型式：悬挂式","通用类",4400]
[{"$nulls":3},4,"18m及以上牵引式喷杆喷雾机","喷杆长度≥18m；药箱≥2000L；型式：牵引式","通用类",4400]
[{"$nulls":3},5,"11-18马力自走式两轮转向喷杆喷雾机","11马力＜功率＜18马力；药箱≥200L；喷杆长度≥8m；离地间隙≥0.8m；型式：自走式；两轮驱动、四轮驱动；两轮转向","通用类",2400]
[{"$nulls":3},6,"18—50马力自走式两轮转向喷杆喷雾机","18马力≤功率＜50马力；药箱≥400L；喷杆长度≥8m；离地间隙≥0.8m；型式：自走式；两轮驱动、四轮驱动；两轮转向","通用类",11000]
[{"$nulls":3},7,"50—100马力自走式两轮转向喷杆喷雾机","50马力≤功率＜100马力；药箱≥700L；喷杆长度≥10m；离地间隙≥0.8m；型式：自走式；两轮驱动、四轮驱动；两轮转向","通用类",11500]
[{"$nulls":3},8,"100马力及以上自走式两轮转向喷杆喷雾机","功率≥100马力；药箱≥1000L；喷杆长度≥20m；离地间隙≥0.8m；型式：自走式；两轮驱动、四轮驱动；两轮转向","通用类",17300]
[{"$nulls":3},9,"11—18马力自走式四轮转向喷杆喷雾机","11马力＜功率＜18马力；药箱≥200L；喷杆长度≥8m；离地间隙≥0.8m；型式：自走式；四轮驱动；四轮转向","通用类",4900]
[{"$nulls":3},10,"18—50马力自走式四轮转向喷杆喷雾机","18马力≤功率＜50马力；药箱≥400L；喷杆长度≥8m；离地间隙≥0.8m；型式：自走式；四轮驱动；四轮转向","通用类",13400]
[{"$nulls":3},11,"50—100马力自走式四轮转向喷杆喷雾机","50马力≤功率＜100马力；药箱≥700L；喷杆长度≥10m；离地间隙≥0.8m；型式：自走式；四轮驱动；四轮转向","通用类",13900]
[{"$nulls":3},12,"100马力及以上自走式四轮转向喷杆喷雾机","功率≥100马力；药箱≥1000L；喷杆长度≥20m；离地间隙≥0.8m；型式：自走式；四轮驱动；四轮转向","通用类",19700]
[{"$nulls":3},13,"药箱容积350L及以上牵引式风送喷雾机","药箱容积≥350L；水平射程或喷幅≥12m；型式：牵引式","非通用类",2000]
[{"$nulls":3},14,"药箱容积300L及以上自走式风送喷雾机","药箱容积≥300L；水平射程或喷幅≥20m；型式：自走式","非通用类",3000]
[null,"修剪防护管理机械","修剪机",1,"单人手提式茶树修剪机","作业幅宽＜1m；单人手提式；自带动力","非通用类",240]
[{"$nulls":3},2,"双人抬式茶树修剪机","作业幅宽≥1m；双人抬式；自带动力","非通用类",600]
["灌溉机械","喷灌机械","喷灌机",1,"管径65mm以下绞盘式喷灌机","管径＜65mm；卷管长度≥150m；绞盘式","非通用类",3300]
[{"$nulls":3},2,"管径65—75mm绞盘式喷灌机","65mm≤管径＜75mm；卷管长度≥300m；绞盘式","非通用类",6600]
[{"$nulls":3},3,"管径75—85mm绞盘式喷灌机","75mm≤管径＜85mm；卷管长度≥300m；绞盘式","非通用类",8000]
[{"$nulls":3},4,"管径85mm及以上绞盘式喷灌机","管径≥85mm；卷管长度≥300m；绞盘式","非通用类",12300]
[null,"微灌设备","灌溉首部",1,"流量50—80m³/h灌溉首部","50m³/h≤流量＜80m³/h；首部(含灌溉水增压设备、过滤设备、水质软化设备、灌溉施肥一体化设备以及营养液消毒设备等)","非通用类",200]
[{"$nulls":3},2,"流量80—130m³/h灌溉首部","80m³/h≤流量＜130m³/h；首部(含灌溉水增压设备、过滤设备、水质软化设备、灌溉施肥一体化设备以及营养液消毒设备等)","非通用类",300]
[{"$nulls":3},3,"流量130—180m³/h灌溉首部","130m³/h≤流量＜180m³/h；首部(含灌溉水增压设备、过滤设备、水质软化设备、灌溉施肥一体化设备以及营养液消毒设备等)","非通用类",400]
[{"$nulls":3},4,"流量180m³/h及以上灌溉首部","流量≥180m³/h；首部(含灌溉水增压设备、过滤设备、水质软化设备、灌溉施肥一体化设备以及营养液消毒设备等)","非通用类",400]
["收获机械","粮食作物收获机械","脱粒机",1,"生产率300kg/h及以上稻麦脱粒机","生产率≥300kg/h；含动力","非通用类",300]
[{"$nulls":3},2,"生产率10t/h及以上玉米脱粒机","生产率≥10t/h","非通用类",1200]
[null,null,"谷物联合收割机",1,"2—3kg/s自走轮式谷物联合收割机","2kg/s≤喂入量＜3kg/s；自走轮式；喂入方式：全喂入","通用类",9400]
[{"$nulls":3},2,"3—4kg/s自走轮式谷物联合收割机","3kg/s≤喂入量＜4kg/s；自走轮式；喂入方式：全喂入","通用类",12300]
[{"$nulls":3},3,"4—5kg/s自走轮式谷物联合收割机","4kg/s≤喂入量＜5kg/s；自走轮式；喂入方式：全喂入","通用类",13400]
[{"$nulls":3},4,"5—6kg/s自走轮式谷物联合收割机","5kg/s≤喂入量＜6kg/s；自走轮式；喂入方式：全喂入","通用类",29300]
[{"$nulls":3},5,"6—7kg/s自走轮式谷物联合收割机","6kg/s≤喂入量＜7kg/s；自走轮式；喂入方式：全喂入","通用类",29300]
[{"$nulls":3},6,"7kg/s及以上自走轮式谷物联合收割机","喂入量≥7kg/s；自走轮式；喂入方式：全喂入","通用类",34600]
[{"$nulls":3},7,"0.6—1kg/s自走履带式谷物联合收割机（全喂入），包含1—1.5kg/s自走履带式水稻联合收割机（全喂入）","0.6kg/s≤喂入量＜1kg/s，1kg/s≤水稻机喂入量＜1.5kg/s；自走履带式；喂入方式：全喂入","通用类",6100]
[{"$nulls":3},8,"1—1.5kg/s自走履带式谷物联合收割机（全喂入），包含1.5—2.1kg/s自走履带式水稻联合收割机（全喂入）","1kg/s≤喂入量＜1.5kg/s，1.5kg/s≤水稻机喂入量＜2.1kg/s；自走履带式；喂入方式：全喂入","通用类",7700]
[{"$nulls":3},9,"1.5—2.1kg/s自走履带式谷物联合收割机（全喂入），包含2.1—3kg/s自走履带式水稻联合收割机（全喂入）","1.5kg/s≤喂入量＜2.1kg/s，2.1kg/s≤水稻机喂入量＜3kg/s；自走履带式；喂入方式：全喂入","通用类",10700]
[{"$nulls":3},10,"2.1—3kg/s自走履带式谷物联合收割机（全喂入），包含3—4kg/s自走履带式水稻联合收割机（全喂入）","2.1kg/s≤喂入量＜3kg/s，3kg/s≤水稻机喂入量＜4kg/s；自走履带式；喂入方式：全喂入","通用类",16900]
[{"$nulls":3},11,"3—4kg/s自走履带式谷物联合收割机（全喂入），包含4kg/s及以上自走履带式水稻联合收割机（全喂入）","3kg/s≤喂入量＜4kg/s，水稻机喂入量≥4kg/s；自走履带式；喂入方式：全喂入","通用类",19900]
[{"$nulls":3},12,"4kg/s及以上自走履带式谷物联合收割机（全喂入）","喂入量≥4kg/s；自走履带式；喂入方式：全喂入","通用类",26700]
[{"$nulls":3},13,"3行35马力及以上半喂入联合收割机","收获行数：3行；喂入方式：半喂入；功率≥35马力","通用类",17100]
[{"$nulls":3},14,"4行及以上35马力及以上半喂入联合收割机","收获行数≥4行；喂入方式：半喂入；功率≥35马力","通用类",44500]
[null,null,"玉米收获机",1,"2行摘穗剥皮型自走式玉米收获机","2行割台；1m≤工作幅宽＜1.6m；型式：自走式（摘穗剥皮型）","通用类",21300]
[{"$nulls":3},2,"3行摘穗剥皮型自走式玉米收获机","3行割台；1.6m≤工作幅宽＜2.2m；型式：自走式（摘穗剥皮型）","通用类",37700]
[{"$nulls":3},3,"4行摘穗剥皮型自走式玉米收获机","4行割台；2.2m≤工作幅宽＜2.8m；型式：自走式（摘穗剥皮型）","通用类",53500]
[{"$nulls":3},4,"5行及以上摘穗剥皮型自走式玉米收获机","5行及以上割台；工作幅宽≥2.8m；型式：自走式（摘穗剥皮型）","通用类",53500]
[{"$nulls":3},5,"3行自走式玉米籽粒联合收获机","3行割台；工作幅宽＜2.2m；型式：自走式","通用类",18000]
[{"$nulls":3},6,"4行自走式玉米籽粒联合收获机","4行割台；2.2m≤工作幅宽＜2.8m；型式：自走式","通用类",35800]
[{"$nulls":3},7,"5行及以上自走式玉米籽粒联合收获机（横轴流）","5行及以上割台；工作幅宽≥2.8m；型式：自走式；脱粒滚筒型式：横轴流；脱粒滚筒数量：1个","通用类",35800]
[{"$nulls":3},8,"5行及以上自走式玉米籽粒联合收获机（纵轴流）","5行及以上割台；工作幅宽≥2.8m；型式:自走式；脱粒滚筒型式：纵轴流；滚脱粒筒数量：1个","通用类",44400]
[{"$nulls":3},9,"5行及以上自走式玉米籽粒联合收获机（双滚筒）","5行及以上割台；工作幅宽≥2.8m；型式:自走式；脱粒滚筒数量：2个","通用类",44400]
[{"$nulls":3},10,"2行穗茎兼收玉米收获机","2行割台；1m≤工作幅宽＜1.6m；型式：自走式","通用类",21300]
[{"$nulls":3},11,"3行穗茎兼收玉米收获机","3行割台；1.6m≤工作幅宽＜2.2m；型式：自走式","通用类",37700]
[{"$nulls":3},12,"4行穗茎兼收玉米收获机","4行割台；2.2m≤工作幅宽＜2.8m；型式：自走式","通用类",56200]
[{"$nulls":3},13,"5行及以上穗茎兼收玉米收获机","5行及以上割台；工作幅宽≥2.8m；型式：自走式","通用类",56200]
[null,null,"薯类收获机",1,"0.7—1m薯类收获机","0.7m≤工作幅宽＜1m","非通用类",940]
[{"$nulls":3},2,"1—1.5m薯类收获机","1m≤工作幅宽＜1.5m","非通用类",1800]
[{"$nulls":3},3,"1.5m及以上薯类收获机","工作幅宽≥1.5m","非通用类",2700]
[null,"油料作物收获机械","花生收获机",1,"0.8—1.5m花生收获机","0.8m≤挖掘机构工作幅宽＜1.5m；悬挂式或牵引式","非通用类",1000]
[{"$nulls":3},2,"1.5—2.1m花生收获机","1.5m≤挖掘机构工作幅宽＜2.1m；悬挂式或牵引式","非通用类",2700]
[{"$nulls":3},3,"2.1m及以上花生收获机","挖掘机构工作幅宽≥2.1m；悬挂式或牵引式","非通用类",3000]
[{"$nulls":3},4,"自走式花生联合收获机","工作幅宽≥0.5m；型式：自走式；含挖掘、秧土分离、摘果、清选、集果等功能","非通用类",21700]
[{"$nulls":3},5,"2.5m及以上自走式花生捡拾收获机","捡拾幅宽≥2.5m；配套发动机功率≥88kW；型式：自走式；具有捡拾、摘果、清选、集果等功能","非通用类",39500]
[{"$nulls":3},6,"其他花生捡拾收获机","捡拾幅宽≥1m，具有捡拾、摘果、清选、集果等功能","非通用类",5000]
[{"$nulls":3},7,"配套动力3—7kW花生摘果机","3kW≤配套动力功率＜7kW","非通用类",570]
[{"$nulls":3},8,"配套动力7—11kW花生摘果机","7kW≤配套动力功率＜11kW","非通用类",660]
[{"$nulls":3},9,"配套动力11—15kW花生摘果机","11kW≤配套动力功率＜15kW","非通用类",1200]
[{"$nulls":3},10,"配套动力15kW及以上花生摘果机","配套动力功率≥15kW","非通用类",1400]
[null,null,"油菜籽收获机",1,"0.6—1kg/s自走履带式油菜籽收获机","0.6kg/s≤喂入量＜1kg/s；自走履带式","通用类",6100]
[{"$nulls":3},2,"1—1.5kg/s自走履带式油菜籽收获机","1kg/s≤喂入量＜1.5kg/s；自走履带式","通用类",7700]
[{"$nulls":3},3,"1.5—2.1kg/s自走履带式油菜籽收获机","1.5kg/s≤喂入量＜2.1kg/s；自走履带式","通用类",10700]
[{"$nulls":3},4,"2.1—3kg/s自走履带式油菜籽收获机","2.1kg/s≤喂入量＜3kg/s；自走履带式","通用类",16900]
[{"$nulls":3},5,"3—4kg/s自走履带式油菜籽收获机","3kg/s≤喂入量＜4kg/s；自走履带式","通用类",19900]
[{"$nulls":3},6,"4kg/s及以上自走履带式油菜籽收获机","喂入量≥4kg/s；自走履带式","通用类",26700]
[{"$nulls":3},7,"2—3kg/s自走轮式油菜籽收获机","2kg/s≤喂入量＜3kg/s；自走轮式","通用类",9400]
[{"$nulls":3},8,"3—4kg/s自走轮式油菜籽收获机","3kg/s≤喂入量＜4kg/s；自走轮式","通用类",12300]
[{"$nulls":3},9,"4—5kg/s自走轮式油菜籽收获机","4kg/s≤喂入量＜5kg/s；自走轮式","通用类",13400]
[{"$nulls":3},10,"5—6kg/s自走轮式油菜籽收获机","5kg/s≤喂入量＜6kg/s；自走轮式","通用类",29300]
[{"$nulls":3},11,"6—7kg/s自走轮式油菜籽收获机","6kg/s≤喂入量＜7kg/s；自走轮式","通用类",29300]
[{"$nulls":3},12,"7kg/s及以上自走轮式油菜籽收获机","喂入量≥7kg/s；自走轮式","通用类",34600]
[null,"果菜茶烟草药收获机械","叶类采收机",1,"单人手提式采茶机","切割器宽度＜1m；单人手提式；自带动力","非通用类",240]
[{"$nulls":3},2,"双人抬式采茶机","切割器宽度≥1m；双人抬式；自带动力","非通用类",600]
[null,null,"根（茎）类收获机",1,"悬挂式或牵引式大蒜收获机","工作幅宽≥1m；悬挂式或牵引式","非通用类",500]
[{"$nulls":3},2,"手扶式大蒜收获机","配套发动机功率≥3.5kW；手扶式","非通用类",500]
[{"$nulls":3},3,"自走式大蒜联合收获机","工作行数≥6行；自走式；联合收获；具备挖掘、切茎、分离、输送、收集等装置","非通用类",4100]
[null,"秸秆收集处理机械","秸秆粉碎还田机",1,"1—1.5m秸秆粉碎还田机","1m≤作业幅宽＜1.5m","通用类",800]
[{"$nulls":3},2,"1.5—2m秸秆粉碎还田机","1.5m≤作业幅宽＜2m","通用类",1600]
[{"$nulls":3},3,"2—2.5m秸秆粉碎还田机","2m≤作业幅宽＜2.5m","通用类",1800]
[{"$nulls":3},4,"2.5m及以上秸秆粉碎还田机","作业幅宽≥2.5m","通用类",2200]
[null,"收获割台","玉米收获专用割台",1,"4行玉米收获专用割台","4行割台；2.2m≤工作幅宽＜2.8m","非通用类",7000,"含脱粒、清选装置"]
[{"$nulls":3},2,"5行及以上玉米收获专用割台","5行及以上割台；工作幅宽≥2.8m","非通用类",9000]
["田间监测及作业监控设备","田间作业监控设备","辅助驾驶（系统）设备",1,"农业用北斗终端","卫星接收机类型及频点：BDS（北斗）；直线度精度≤2.5cm（拖拉机用）、直线度精度≤5cm（插秧机用）","非通用类",5000]
["种植业废弃物处理设备","农作物废弃物处理设备","秸秆压块（粒、棒）机",1,"1—2t/h秸秆压块机","1t/h≤生产率＜2t/h","非通用类",4000]
[{"$nulls":3},2,"2t/h及以上秸秆压块机","生产率≥2t/h","非通用类",6000]
["饲料（草）收获加工运输设备","饲料（草）收获机械","割草（压扁）机",1,"2.8m及以上旋转式割草机","割幅宽度≥2.8m；旋转式","非通用类",11500]
[null,null,"搂草机",1,"6m及以上机引横向搂草机","搂幅≥6m；结构型式：机引横向式","非通用类",1500]
[{"$nulls":3},2,"5.4m以下指轮式搂草机","搂幅＜5.4m；结构型式：指轮式","非通用类",2200]
[{"$nulls":3},3,"5.4m及以上指轮式搂草机","搂幅宽度≥5.4m；液压折叠式；结构型式：指轮式","非通用类",3600]
[{"$nulls":3},4,"4.5m以下旋转式搂草机","搂幅＜4.5m；结构型式：旋转式","非通用类",3000]
[{"$nulls":3},5,"4.5m及以上旋转式搂草机","搂幅≥4.5m；结构型式：旋转式","非通用类",4300]
[null,null,"打（压）捆机",1,"压缩室截面积（宽×高）0.102m2及以上方捆捡拾压捆机","方捆；压缩室截面积（宽×高）≥0.102m²；打结器数量≥2个；捡拾宽度≥0.7m","通用类",5400]
[{"$nulls":3},2,"压缩室截面积（宽×高）0.1344m2及以上方捆捡拾压捆机","方捆；压缩室截面积（宽×高）≥0.1344m²；打结器数量≥2个；捡拾宽度≥1.2m","通用类",10800]
[{"$nulls":3},3,"压缩室截面积（宽×高）0.154m2及以上方捆捡拾压捆机","方捆；压缩室截面积（宽×高）≥0.154m²；打结器数量≥2个；捡拾宽度≥1.7m","通用类",16300]
[{"$nulls":3},4,"压缩室截面积（宽×高）0.162m2及以上方捆捡拾压捆机","方捆；压缩室截面积（宽×高）≥0.162m²；打结器数量≥2个；捡拾宽度≥2.2m","通用类",16300]
[{"$nulls":3},5,"压缩室截面积（宽×高）0.1998m2及以上方捆捡拾压捆机（3个及以上打结器）","方捆；压缩室截面积（宽×高）≥0.1998m2；打结器数量≥3个；捡拾宽度≥2.2m","通用类",29200]
[{"$nulls":3},6,"压缩室直径0.5m及以上圆捆捡拾压捆机","圆捆；压缩室直径≥0.5m；压缩室宽度≥0.7m；捡拾宽度≥0.7m","通用类",5600]
[{"$nulls":3},7,"压缩室直径0.8m及以上圆捆捡拾压捆机","圆捆；压缩室直径≥0.8m；压缩室宽度≥0.8m；捡拾宽度≥1.2m","通用类",12000]
[{"$nulls":3},8,"压缩室直径1m及以上圆捆捡拾压捆机","圆捆；压缩室直径≥1m；压缩室宽度≥1m；捡拾宽度≥1.7m","通用类",16300]
[{"$nulls":3},9,"压缩室直径1.2m及以上圆捆捡拾压捆机","圆捆；压缩室直径≥1.2m；压缩室宽度≥1.2m；捡拾宽度≥2.2m","通用类",23700]
[{"$nulls":3},10,"压缩室直径0.52m及以上圆捆压捆机","圆捆；压缩室直径≥0.52m；压缩室宽度≥0.52m；功率≥4kW","通用类",5600]
[{"$nulls":3},11,"压缩室截面积（宽×高）0.081m2及以上方捆压捆机","方捆；压缩室截面积（宽×高）≥0.081m²；7.5kW≤功率＜15kW","通用类",2300]
[{"$nulls":3},12,"压缩室截面积（宽×高）0.105m2及以上方捆压捆机","方捆；压缩室截面积（宽×高）≥0.105m²；功率≥15kW","通用类",5400]
[{"$nulls":3},13,"压缩室截面积（宽×高）0.0936m2及以上无打结器自动套袋方捆捡拾压捆机","方捆；压缩室截面积（宽×高）≥0.0936m2；捡拾宽度≥1.7m；自动套袋","通用类",15400]
[{"$nulls":3},14,"压缩室截面积（宽×高）0.1344m2及以上无打结器自动套袋方捆捡拾压捆机","方捆；压缩室截面积（宽×高）≥0.1344m2；捡拾宽度≥2.2m；自动套袋","通用类",18300]
[null,null,"草捆包膜机",1,"1.1kW及以上圆草捆包膜机","配套动力功率≥1.1kW；适用草捆直径≥400mm","非通用类",1000]
[null,null,"青（黄）饲料收获机",1,"0.9—1.1m悬挂单圆盘式青饲料收获机","悬挂单圆盘式；0.9m≤割幅＜1.1m","通用类",2200]
[{"$nulls":3},2,"1.1m及以上悬挂单圆盘式青饲料收获机","悬挂单圆盘式；割幅≥1.1m","通用类",7100]
[{"$nulls":3},3,"0.9—1.1m悬挂双圆盘式青饲料收获机","悬挂双圆盘式；0.9m≤割幅＜1.1m","通用类",2200]
[{"$nulls":3},4,"1.1—2.1m悬挂双圆盘式青饲料收获机","悬挂双圆盘式；1.1m≤割幅＜2.1m","通用类",7100]
[{"$nulls":3},5,"2.1—2.2m悬挂双圆盘式青饲料收获机","悬挂双圆盘式；2.1m≤割幅＜2.2m","通用类",17800]
[{"$nulls":3},6,"2.2m及以上悬挂双圆盘式青饲料收获机","悬挂双圆盘式；割幅≥2.2m","通用类",18700]
[{"$nulls":3},7,"1.6—1.9m悬挂其他式青饲料收获机","悬挂其他式；1.6m≤割幅＜1.9m","通用类",6700,"割台切割器型式不包含甩刀（锤爪）式。"]
[{"$nulls":3},8,"1.9—2.2m悬挂其他式青饲料收获机","悬挂其他式；1.9m≤割幅＜2.2m","通用类",7100]
[{"$nulls":3},9,"2.2m及以上悬挂其他式青饲料收获机","悬挂其他式；割幅≥2.2m","通用类",7900]
[{"$nulls":3},10,"1.1m及以上牵引式青饲料收获机","牵引式；割幅≥1.1m","通用类",2300]
[{"$nulls":3},11,"2—2.6m自走圆盘式青饲料收获机","自走圆盘式；2m≤割幅＜2.6m；籽粒破碎机构：无或非对辊式；配套发动机功率≥110kW","通用类",31900]
[{"$nulls":3},12,"2—2.6m自走圆盘式青饲料收获机，带对辊式籽粒破碎机构","自走圆盘式；2m≤割幅＜2.6m；籽粒破碎机构：对辊式；配套发动机功率≥115kW","通用类",63700]
[{"$nulls":3},13,"2.6m及以上自走圆盘式青饲料收获机","自走圆盘式；割幅≥2.6m；籽粒破碎机构：无或非对辊式；配套发动机功率≥130kW","通用类",58600]
[{"$nulls":3},14,"2.6m及以上自走圆盘式青饲料收获机，带对辊式籽粒破碎机构","自走圆盘式；割幅≥2.6m；籽粒破碎机构：对辊式；配套发动机功率≥150kW","通用类",117200]
[{"$nulls":3},15,"1.8—2.2m自走其他式青饲料收获机","自走其他式；1.8m≤割幅＜2.2m；籽粒破碎机构：无或非对辊式；配套发动机功率≥90kW","通用类",20000]
[{"$nulls":3},16,"1.8—2.2m自走其他式青饲料收获机，带对辊式籽粒破碎机构","自走其他式；1.8m≤割幅＜2.2m；籽粒破碎机构：对辊式；配套发动机功率≥105kW","通用类",41500]
[{"$nulls":3},17,"2.2—2.6m自走其他式青饲料收获机","自走其他式；2.2m≤割幅＜2.6m；籽粒破碎机构：无或非对辊式；配套发动机功率≥115kW","通用类",29600]
[{"$nulls":3},18,"2.2—2.6m自走其他式青饲料收获机，带对辊式籽粒破碎机构","自走其他式；2.2m≤割幅＜2.6m；籽粒破碎机构：对辊式；配套发动机功率≥115kW","通用类",59300]
[{"$nulls":3},19,"2.6—2.9m自走其他式青饲料收获机","自走其他式；2.6m≤割幅＜2.9m；籽粒破碎机构：无或非对辊式；配套发动机功率≥150kW","通用类",34800]
[{"$nulls":3},20,"2.6—2.9m自走其他式青饲料收获机，带对辊式籽粒破碎机构","自走其他式；2.6m≤割幅＜2.9m；籽粒破碎机构：对辊式；配套发动机功率≥150kW","通用类",69600]
[{"$nulls":3},21,"2.9m及以上自走其他式青饲料收获机","自走其他式；割幅≥2.9m；籽粒破碎机构：无或非对辊式；配套发动机功率≥190kW","通用类",53600]
[{"$nulls":3},22,"2.9m及以上自走其他式青饲料收获机，带对辊式籽粒破碎机构","自走其他式；割幅≥2.9m；籽粒破碎机构：对辊式；配套发动机功率≥215kW","通用类",107200]
[{"$nulls":3},23,"1—1.5m秸秆收集机","1m≤作业幅宽＜1.5m；收集器型式：甩刀式、锤爪式、弹齿式","非通用类",800]
[{"$nulls":3},24,"1.5—2m秸秆收集机","1.5m≤作业幅宽＜2m；收集器型式：甩刀式、锤爪式、弹齿式","非通用类",1600]
[{"$nulls":3},25,"2—2.5m秸秆收集机","2m≤作业幅宽＜2.5m；收集器型式：甩刀式、锤爪式、弹齿式","非通用类",1800]
[{"$nulls":3},26,"2.5m及以上秸秆收集机","作业幅宽≥2.5m；收集器型式：甩刀式、锤爪式、弹齿式","非通用类",2200]
[null,"饲料（草）加工机械","铡草机",1,"1—3t/h铡草机","1t/h≤生产率（干秸秆）＜3t/h","非通用类",390]
[{"$nulls":3},2,"3—6t/h铡草机","3t/h≤生产率（干秸秆）＜6t/h","非通用类",630]
[{"$nulls":3},3,"6—9t/h铡草机","6t/h≤生产率（干秸秆）＜9t/h","非通用类",1200]
[{"$nulls":3},4,"9—15t/h铡草机","9t/h≤生产率（干秸秆）＜15t/h","非通用类",2500]
[{"$nulls":3},5,"15—20t/h铡草机","15t/h≤生产率（干秸秆）＜20t/h","非通用类",2500]
[{"$nulls":3},6,"20t/h及以上铡草机","生产率（干秸秆）≥20t/h","非通用类",3600]
[null,null,"饲料（草）粉碎机",1,"1t/h以下揉丝机","生产率（干秸秆）＜1t/h，1t/h≤生产率（青秸秆）＜2t/h","非通用类",290]
[{"$nulls":3},2,"1—2t/h揉丝机","1t/h≤生产率（干秸秆）＜2t/h，2t/h≤生产率（青秸秆）＜4t/h","非通用类",370]
[{"$nulls":3},3,"2—4t/h揉丝机","2t/h≤生产率（干秸秆）＜4t/h，4t/h≤生产率（青秸秆）＜6t/h","非通用类",420]
[{"$nulls":3},4,"4—6t/h揉丝机","4t/h≤生产率（干秸秆）＜6t/h，6t/h≤生产率（青秸秆）＜10t/h","非通用类",770]
[{"$nulls":3},5,"6—10t/h揉丝机","6t/h≤生产率（干秸秆）＜10t/h，10t/h≤生产率（青秸秆）＜15t/h","非通用类",1900]
[{"$nulls":3},6,"10—15t/h揉丝机","10t/h≤生产率（干秸秆）＜15t/h，生产率（青秸秆）≥15t/h","非通用类",2300]
[{"$nulls":3},7,"15t/h及以上揉丝机","生产率（干秸秆）≥15t/h","非通用类",2700]
[{"$nulls":3},8,"400mm以下饲料粉碎机","转子工作直径＜400mm","非通用类",190]
[{"$nulls":3},9,"400—550mm饲料粉碎机","400mm≤转子工作直径＜550mm","非通用类",490]
[{"$nulls":3},10,"550mm及以上饲料粉碎机","转子工作直径≥550mm","非通用类",820]
[null,null,"颗粒饲料压制机",1,"平模直径200mm及以上颗粒饲料压制机","平模直径≥200mm","非通用类",700]
[{"$nulls":3},2,"环模直径200-250mm颗粒饲料压制机","200mm≤环模直径＜250mm，电机功率＜17kW","非通用类",2500]
[{"$nulls":3},3,"环模直径250mm及以上颗粒饲料压制机","环模直径≥250mm，电机功率≥17kW","非通用类",3500]
[null,null,"全混合日粮制备机",1,"4—9m³饲料全混合日粮制备机","4m³≤搅拌室容积＜9m³","非通用类",11300]
[{"$nulls":3},2,"9—12m³饲料全混合日粮制备机","9m³≤搅拌室容积＜12m³","非通用类",13900]
[{"$nulls":3},3,"12m³及以上饲料全混合日粮制备机","搅拌室容积≥12m³","非通用类",15000]
["畜禽养殖机械","畜禽养殖成套设备","蜜蜂养殖设备",1,"移动式养蜂平台","适用蜂箱数量≥80个；含联动式蜂箱踏板、蜂箱保湿装置、蜜蜂饲喂装置、电动摇浆机、电动取浆器、花粉干燥箱","非通用类",7600]
[null,"畜禽繁育设备","孵化机",1,"10000—50000枚孵化机","10000枚≤蛋容量＜50000枚","非通用类",4100]
[{"$nulls":3},2,"50000枚及以上孵化机","蛋容量≥50000枚","非通用类",9400]
["畜禽产品采集储运设备","畜禽产品采集设备","挤奶机",1,"1杯组手动移动式挤奶机","杯组数：1；脱杯方式：手动；型式：移动式","通用类",1200]
[{"$nulls":3},2,"2杯组手动移动式挤奶机","杯组数：2；脱杯方式：手动；型式：移动式","通用类",1600]
[{"$nulls":3},3,"24—40杯组鱼骨式挤奶机","24≤杯组数＜40；型式：鱼骨式；脉动器型式：电子；计量方式：电子计量；脱杯方式：自动","通用类",84200]
[{"$nulls":3},4,"40杯组及以上鱼骨式挤奶机","杯组数≥40；型式：鱼骨式；脉动器型式：电子；计量方式：电子计量；脱杯方式：自动","通用类",84200]
[{"$nulls":3},5,"16—20杯组并列式挤奶机","16≤杯组数＜20；型式：并列式；脉动器型式：电子；计量方式：电子计量；脱杯方式：自动","通用类",100000]
[{"$nulls":3},6,"20杯组及以上并列（转盘）式挤奶机","杯组数≥20；型式：并列（转盘）式；脉动器型式：电子；计量方式：电子计量；脱杯方式：自动","通用类",100000]
[null,null,"散装乳冷藏罐",1,"1000—3000L非全自动清洗冷藏罐","1000L≤容量＜3000L；清洗方式：非全自动清洗","通用类",3500]
[{"$nulls":3},2,"3000—6000L非全自动清洗冷藏罐","3000L≤容量＜6000L；清洗方式：非全自动清洗","通用类",8400]
[{"$nulls":3},3,"6000L及以上非全自动清洗冷藏罐","容量≥6000L；清洗方式：非全自动清洗","通用类",11800]
[{"$nulls":3},4,"1000—3000L全自动清洗冷藏罐","1000L≤容量＜3000L；清洗方式：全自动清洗","通用类",3800]
[{"$nulls":3},5,"3000—6000L全自动清洗冷藏罐","3000L≤容量＜6000L；清洗方式：全自动清洗","通用类",8400]
[{"$nulls":3},6,"6000L及以上全自动清洗冷藏罐","容量≥6000L；清洗方式：全自动清洗","通用类",16500]
[null,"畜禽产品储运设备","储奶罐",1,"3000—6000L储奶罐","3000L≤容量＜6000L","通用类",7100]
[{"$nulls":3},2,"6000—12000L储奶罐","6000L≤容量＜12000L","通用类",10500]
[{"$nulls":3},3,"12000—20000L储奶罐","12000L≤容量＜20000L","通用类",10500]
[{"$nulls":3},4,"20000L及以上储奶罐","容量≥20000L","通用类",18800]
["畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","畜禽粪便发酵处理设备",1,"100m³及以上罐式畜禽粪便发酵处理机","盛料容器容积≥100m³；罐式","非通用类",49000]
[{"$nulls":3},2,"30m³及以上层叠式畜禽粪便发酵处理机","盛料容器容积≥30m³；层叠式；具有破碎、装盘布料机构","非通用类",49000]
["水产养殖机械","水质调控设备","增氧机",1,"叶轮（水车、涌浪）式增氧机","增氧结构型式：叶轮式、水车式、涌浪式；叶轮数≥3个；配套电机功率≥1.5kW","非通用类",310]
["粮油糖初加工机械","粮食初加工机械","谷物（粮食）干燥机",1,"批处理量2—4t循环式谷物烘干机","2t≤批处理量＜4t；循环式","通用类",4500]
[{"$nulls":3},2,"批处理量4—10t循环式谷物烘干机","4t≤批处理量＜10t；循环式","通用类",14700]
[{"$nulls":3},3,"批处理量10—20t循环式谷物烘干机","10t≤批处理量＜20t；循环式","通用类",22600]
[{"$nulls":3},4,"批处理量20—30t循环式谷物烘干机","20t≤批处理量＜30t；循环式","通用类",26300]
[{"$nulls":3},5,"批处理量30t及以上循环式谷物烘干机","批处理量≥30t；循环式","通用类",46900]
[{"$nulls":3},6,"处理量20—50t/d连续式谷物烘干机","20t≤处理量＜50t/d；连续式","通用类",15000]
[{"$nulls":3},7,"处理量50—100t/d连续式谷物烘干机","50t/d≤处理量＜100t/d；连续式","通用类",31000]
[{"$nulls":3},8,"处理量100t/d及以上连续式谷物烘干机","处理量≥100t/d；连续式","通用类",69000]
[{"$nulls":3},9,"3—5t平床式谷物烘干机","3t≤装载量＜5t；平床式","通用类",4500]
[{"$nulls":3},10,"5t及以上平床式谷物烘干机","装载量≥5t；平床式","通用类",7100]
[null,null,"碾米机",1,"2.2kW及以上碾米机","配套功率≥2.2kW；含电机、碾米装置","非通用类",200]
[{"$nulls":3},2,"2.2kW及以上砻碾组合米机","配套功率≥2.2kW；具有砻碾功能","非通用类",700]
[null,null,"粮食色选机",1,"总执行单元数60个以下大米色选机","总执行单元数＜60个","非通用类",2800]
[{"$nulls":3},2,"总执行单元数60—300个大米色选机","60个≤总执行单元数＜300个","非通用类",9500]
[{"$nulls":3},3,"总执行单元数300个及以上大米色选机","总执行单元数≥300个","非通用类",21400]
[{"$nulls":3},4,"总执行单元数60个以下杂粮色选机","总执行单元数＜60个","非通用类",2800]
[{"$nulls":3},5,"总执行单元数60—300个杂粮色选机","60个≤总执行单元数＜300个","非通用类",9500]
[{"$nulls":3},6,"总执行单元数300个及以上杂粮色选机","总执行单元数≥300个","非通用类",21400]
[null,null,"磨粉机",1,"磨辊长度300—400mm磨粉机","300mm≤磨辊长度＜400mm","非通用类",3000]
[{"$nulls":3},2,"磨辊长度400—600mm磨粉机","400mm≤磨辊长度＜600mm","非通用类",4000]
[{"$nulls":3},3,"磨辊长度600mm及以上磨粉机","磨辊长度≥600mm","非通用类",5000]
[null,"油料初加工机械","油菜籽干燥机",1,"批处理量2—4t循环式油菜籽烘干机","2t≤批处理量＜4t；循环式","非通用类",4500]
[{"$nulls":3},2,"批处理量4—10t循环式油菜籽烘干机","4t≤批处理量＜10t；循环式","非通用类",14700]
[{"$nulls":3},3,"批处理量10—20t循环式油菜籽烘干机","10t≤批处理量＜20t；循环式","非通用类",22600]
[{"$nulls":3},4,"批处理量20—30t循环式油菜籽烘干机","20t≤批处理量＜30t；循环式","非通用类",26300]
[{"$nulls":3},5,"批处理量30t及以上循环式油菜籽烘干机","批处理量≥30t；循环式","非通用类",46900]
[null,null,"油料果（籽）脱（剥）壳机",1,"1—1.5t/h花生脱壳机","1t/h≤生产率＜1.5t/h","非通用类",600]
[{"$nulls":3},2,"1.5—3t/h花生脱壳机","1.5t/h≤生产率＜3t/h；含自动上料设备","非通用类",2200]
[{"$nulls":3},3,"3t/h及以上花生脱壳机","生产率≥3t/h；含自动上料、去杂设备","非通用类",4200]
["果菜茶初加工机械","果蔬初加工机械","果蔬干燥机",1,"容积1—5m³厢式果蔬烘干机","1m³≤有效烘干容积＜5m³；结构型式：厢式；热源装置：非燃煤型","非通用类",900]
[{"$nulls":3},2,"容积5—20m³厢式果蔬烘干机","5m³≤有效烘干容积＜20m³；结构型式：厢式；热源装置：非燃煤型","非通用类",1500]
[{"$nulls":3},3,"容积20—40m³厢式果蔬烘干机","20m³≤有效烘干容积＜40m³；结构型式：厢式；热源装置：非燃煤型","非通用类",3000]
[{"$nulls":3},4,"容积40m³及以上厢式果蔬烘干机","有效烘干容积≥40m³；结构型式：厢式；热源装置：非燃煤型","非通用类",4500]
[{"$nulls":3},5,"容积1—5m³热泵型厢式果蔬烘干机","1m³≤有效烘干容积＜5m³；结构型式：厢式；热源装置：热泵；热泵额定功率（不含电辅助加热）≥2.1kW","非通用类",1200]
[{"$nulls":3},6,"容积5—20m³热泵型厢式果蔬烘干机","5m³≤有效烘干容积＜20m³；结构型式：厢式；热源装置：热泵；热泵额定功率（不含电辅助加热）≥2.4kW","非通用类",5500]
[{"$nulls":3},7,"容积20—40m³热泵型厢式果蔬烘干机","20m³≤有效烘干容积＜40m³；结构型式：厢式；热源装置：热泵；热泵额定功率（不含电辅助加热）≥4.5kW","非通用类",7500]
[{"$nulls":3},8,"容积40m³及以上热泵型厢式果蔬烘干机","有效烘干容积≥40m³；结构型式：厢式；热源装置：热泵；热泵额定功率（不含电辅助加热）≥9kW","非通用类",9500]
[null,null,"果蔬冷藏保鲜设备",1,"库容50m³以下简易保鲜储藏设备","库容＜50m³","非通用类","93元/m³"]
[{"$nulls":3},2,"库容50—100m³简易保鲜储藏设备","50m³≤库容＜100m³","非通用类","80元/m³"]
[{"$nulls":3},3,"库容100—200m³简易保鲜储藏设备","100m³≤库容＜200m³","非通用类","66元/m³"]
[{"$nulls":3},4,"库容200—400m³简易保鲜储藏设备","200m³≤库容＜400m³","非通用类","38元/m³"]
[{"$nulls":3},5,"库容400m³及以上简易保鲜储藏设备","库容≥400m³","非通用类","28元/m³（上限5万元）"]
[null,"茶叶初加工机械","茶叶杀青机",1,"滚筒外径300—400mm杀青机","滚筒式；300mm≤滚筒外径＜400mm；含热源装置","非通用类",1100]
[{"$nulls":3},2,"滚筒外径400—600mm杀青机","滚筒式；400mm≤滚筒外径＜600mm；含热源装置","非通用类",1500]
[{"$nulls":3},3,"滚筒外径600mm及以上杀青机","滚筒式；滚筒外径≥600mm；滚筒长度≥3m；含热源装置","非通用类",2400]
[null,null,"茶叶揉捻机",1,"揉桶直径350mm以下揉捻机","揉桶直径＜350mm","非通用类",800]
[{"$nulls":3},2,"揉桶直径350—500mm揉捻机","350mm≤揉桶直径＜500mm","非通用类",1100]
[{"$nulls":3},3,"揉桶直径500—600mm揉捻机","500mm≤揉桶直径＜600mm","非通用类",1700]
[{"$nulls":3},4,"揉桶直径60cm及以上揉捻机（含揉捻机组）","揉桶直径≥60cm","非通用类",2800]
[null,null,"茶叶压扁机",1,"600mm及以上非全自动茶叶压扁机","压辊长度≥600mm；非全自动","非通用类",1400]
[{"$nulls":3},2,"600mm及以上全自动茶叶压扁机","压辊长度≥600mm；全自动","非通用类",2000]
[null,null,"茶叶理条机",1,"0.5—1m²茶叶理条机","0.5m²≤槽锅面积＜1m²","非通用类",1500]
[{"$nulls":3},2,"1—2.5m²茶叶理条机","1m²≤槽锅面积＜2.5m²","非通用类",2800]
[{"$nulls":3},3,"2.5m²及以上茶叶理条机","槽锅面积≥2.5m²","非通用类",2800]
[null,null,"茶叶炒（烘）干机",1,"非全自动茶叶炒干机（含扁形茶炒制机）","非全自动茶叶炒干机、扁形茶炒制机","非通用类",590]
[{"$nulls":3},2,"1—2锅（槽）全自动茶叶炒干机","全自动控制作业；1、2锅（槽）","非通用类",1600]
[{"$nulls":3},3,"3—4锅（槽）全自动茶叶炒干机","全自动控制作业；3、4锅（槽）","非通用类",3200]
[{"$nulls":3},4,"10m²以下百叶式茶叶烘干机","烘干面积＜10m²；百叶式","非通用类",600]
[{"$nulls":3},5,"10m²及以上百叶式茶叶烘干机","烘干面积≥10m²；百叶式","非通用类",1100]
[{"$nulls":3},6,"10m²以下连续自动式茶叶烘干机","烘干面积＜10m²；连续自动式","非通用类",4400]
[{"$nulls":3},7,"10m²及以上连续自动式茶叶烘干机","烘干面积≥10m²；连续自动式","非通用类",9000]
[null,null,"茶叶色选机",1,"总执行单元数60-384个茶叶色选机","60个≤总执行单元数＜384个","非通用类",16000]
[{"$nulls":3},2,"总执行单元数384个及以上茶叶色选机","总执行单元数≥384个","非通用类",36000]
[null,null,"茶叶输送机",1,"带宽300mm及以上带式茶叶输送机","带式；带宽≥300mm；输送长度≥2m","非通用类",600]
[{"$nulls":3},2,"槽宽200-600mm振动式茶叶输送机","振动式；200mm≤槽宽＜600mm","非通用类",600]
["农用动力机械","拖拉机","轮式拖拉机",1,"30—40马力两轮驱动拖拉机","30马力≤功率＜40马力；驱动方式：两轮驱动","通用类",6900]
[{"$nulls":3},2,"40—50马力两轮驱动拖拉机","40马力≤功率＜50马力；驱动方式：两轮驱动","通用类",7500]
[{"$nulls":3},3,"50—60马力两轮驱动拖拉机","50马力≤功率＜60马力；驱动方式：两轮驱动","通用类",8200]
[{"$nulls":3},4,"60—70马力两轮驱动拖拉机","60马力≤功率＜70马力；驱动方式：两轮驱动","通用类",9000]
[{"$nulls":3},5,"70—80马力两轮驱动拖拉机","70马力≤功率＜80马力；驱动方式：两轮驱动","通用类",11300]
[{"$nulls":3},6,"80—90马力两轮驱动拖拉机","80马力≤功率＜90马力；驱动方式：两轮驱动","通用类",13600]
[{"$nulls":3},7,"90—100马力两轮驱动拖拉机","90马力≤功率＜100马力；驱动方式：两轮驱动","通用类",18400]
[{"$nulls":3},8,"100马力及以上两轮驱动拖拉机","功率≥100马力；驱动方式：两轮驱动","通用类",24100]
[{"$nulls":3},9,"30—40马力四轮驱动拖拉机","30马力≤功率＜40马力；驱动方式：四轮驱动","通用类",8000]
[{"$nulls":3},10,"40—50马力四轮驱动拖拉机","40马力≤功率＜50马力；驱动方式：四轮驱动","通用类",9900]
[{"$nulls":3},11,"50—60马力四轮驱动拖拉机","50马力≤功率＜60马力；驱动方式：四轮驱动","通用类",10900]
[{"$nulls":3},12,"60—70马力四轮驱动拖拉机","60马力≤功率＜70马力；驱动方式：四轮驱动","通用类",12000]
[{"$nulls":3},13,"70—80马力四轮驱动拖拉机","70马力≤功率＜80马力；驱动方式：四轮驱动；最小使用比质量≥38kg/kW","通用类",15300,"最小使用比质量（kg/kW）=最小使用质量/配套发动机标定功率。"]
[{"$nulls":3},14,"80—90马力四轮驱动拖拉机","80马力≤功率＜90马力；驱动方式：四轮驱动；最小使用比质量≥40kg/kW","通用类",18500]
[{"$nulls":3},15,"80—90马力四轮驱动动力换挡拖拉机","80马力≤功率＜90马力；驱动方式：四轮驱动；换挡方式：部分动力换挡、动力换挡/换向、无级变速；最小使用比质量≥40kg/kW","通用类",21500]
[{"$nulls":3},16,"90—100马力四轮驱动拖拉机","90马力≤功率＜100马力；驱动方式：四轮驱动；最小使用比质量≥40kg/kW","通用类",21500]
[{"$nulls":3},17,"90—100马力四轮驱动动力换挡拖拉机","90马力≤功率＜100马力；驱动方式：四轮驱动；换挡方式：部分动力换挡、动力换挡/换向、无级变速；最小使用比质量≥40kg/kW","通用类",24500]
[{"$nulls":3},18,"100—120马力四轮驱动拖拉机","100马力≤功率＜120马力；驱动方式：四轮驱动；最小使用比质量≥43kg/kW","通用类",24500]
[{"$nulls":3},19,"100—120马力四轮驱动动力换挡拖拉机","100马力≤功率＜120马力；驱动方式：四轮驱动；换挡方式：部分动力换挡、动力换挡/换向、无级变速；最小使用比质量≥43kg/kW","通用类",27500]
[{"$nulls":3},20,"120—140马力四轮驱动拖拉机","120马力≤功率＜140马力；驱动方式：四轮驱动；最小使用比质量≥43kg/kW","通用类",31900]
[{"$nulls":3},21,"120—140马力四轮驱动动力换挡拖拉机","120马力≤功率＜140马力；驱动方式：四轮驱动；换挡方式：部分动力换挡、动力换挡/换向、无级变速；最小使用比质量≥43kg/kW","通用类",34900]
[{"$nulls":3},22,"140—160马力四轮驱动拖拉机","140马力≤功率＜160马力；驱动方式：四轮驱动；最小使用比质量≥43kg/kW","通用类",38800]
[{"$nulls":3},23,"140—160马力四轮驱动动力换挡拖拉机","140马力≤功率＜160马力；驱动方式：四轮驱动；换挡方式：部分动力换挡、动力换挡/换向、无级变速；最小使用比质量≥43kg/kW","通用类",42800]
[{"$nulls":3},24,"160—180马力四轮驱动拖拉机","160马力≤功率＜180马力；驱动方式：四轮驱动；最小使用比质量≥43kg/kW","通用类",45700]
[{"$nulls":3},25,"160—180马力四轮驱动动力换挡拖拉机","160马力≤功率＜180马力；驱动方式：四轮驱动；换挡方式：部分动力换挡、动力换挡/换向、无级变速；最小使用比质量≥43kg/kW","通用类",49700]
[{"$nulls":3},26,"180—200马力四轮驱动拖拉机","180马力≤功率＜200马力；驱动方式：四轮驱动；最小使用比质量≥43kg/kW","通用类",51200]
[{"$nulls":3},27,"180—200马力四轮驱动动力换挡拖拉机","180马力≤功率＜200马力；驱动方式：四轮驱动；换挡方式：部分动力换挡、动力换挡/换向、无级变速；最小使用比质量≥43kg/kW","通用类",55200]
[{"$nulls":3},28,"200马力及以上四轮驱动拖拉机","功率≥200马力；驱动方式：四轮驱动；最小使用比质量≥43kg/kW","通用类",51200]
[{"$nulls":3},29,"200马力及以上四轮驱动动力换挡拖拉机","功率≥200马力；驱动方式：四轮驱动；换挡方式：部分动力换挡、动力换挡/换向、无级变速；最小使用比质量≥43kg/kW","通用类",55200]
[null,null,"手扶拖拉机",1,"8马力及以上皮带传动手扶拖拉机","传动方式：皮带传动；功率≥8马力","非通用类",1000]
[{"$nulls":3},2,"11—15马力直联传动手扶拖拉机","传动方式：直联传动；11马力≤功率≤15马力","非通用类",1650]
[null,null,"履带式拖拉机",1,"80—100马力重型履带式拖拉机","80马力≤功率＜100马力；驱动方式：履带式；最小使用质量≥6000kg","通用类",36700]
[{"$nulls":3},2,"100—130马力重型履带式拖拉机","100马力≤功率＜130马力；驱动方式：履带式；最小使用质量≥6500kg","通用类",46300]
[{"$nulls":3},3,"130—160马力重型履带式拖拉机","130马力≤功率＜160马力；驱动方式：履带式；最小使用质量≥7000kg","通用类",56100]
[{"$nulls":3},4,"160马力及以上重型履带式拖拉机","功率≥160马力；驱动方式：履带式；最小使用质量≥8000kg","通用类",76500]
[{"$nulls":3},5,"50—70马力差速转向履带式拖拉机","50马力≤功率＜70马力；驱动方式：履带式；转向型式：差速式转向；最大牵引功率≥70%发动机标定功率；最小使用比质量≥35kg/kW","通用类",21200,"差速式转向是指用于液压机械双功率流驱动差速转向机构，实现履带车辆转向的差速式转向系统。"]
[{"$nulls":3},6,"70—90马力差速转向履带式拖拉机","70马力≤功率＜90马力；驱动方式：履带式；转向型式：差速式转向；最大牵引功率≥70%发动机标定功率；最小使用比质量≥35kg/kW","通用类",23800]
[{"$nulls":3},7,"90—110马力差速转向履带式拖拉机","90马力≤功率＜110马力；驱动方式：履带式；转向型式：差速式转向；最大牵引功率≥70%发动机标定功率；最小使用比质量≥35kg/kW","通用类",31500]
[{"$nulls":3},8,"110马力及以上差速转向履带式拖拉机","功率≥110马力；驱动方式：履带式；转向型式：差速式转向；最大牵引功率≥70%发动机标定功率；最小使用比质量≥45kg/kW","通用类",31500]
[{"$nulls":3},9,"50—70马力轻型履带式拖拉机","50马力≤功率＜70马力；驱动方式：履带式；橡胶履带","通用类",14400]
[{"$nulls":3},10,"70—100马力轻型履带式拖拉机","70马力≤功率＜100马力；驱动方式：履带式；橡胶履带","通用类",14400]
["农用水泵","农用水泵","潜水电泵",1,"4—7.5kW潜水电泵","4kW≤电机功率＜7.5kW","非通用类",120]
[{"$nulls":3},2,"7.5—9.2kW潜水电泵","7.5kW≤电机功率＜9.2kW","非通用类",300]
[{"$nulls":3},3,"9.2—18.5kW潜水电泵","9.2kW≤电机功率＜18.5kW","非通用类",490]
[{"$nulls":3},4,"18.5—37kW潜水电泵","18.5kW≤电机功率＜37kW","非通用类",900]
[null,null,"地面泵（机组）",1,"3.8—5.5kW离心泵","3.8kW≤配套功率＜5.5kW；含机座、底阀","非通用类",190]
[{"$nulls":3},2,"5.5—22kW离心泵","5.5kW≤配套功率＜22kW；含机座、底阀","非通用类",350]
[{"$nulls":3},3,"22—55kW离心泵","22kW≤配套功率＜55kW；含机座、底阀","非通用类",1000]
["设施环境控制设备","设施环境控制设备","拉幕（卷帘）设备",1,"1kW及以上电动卷帘机","配套电机功率≥1kW","非通用类",200]
[null,null,"湿帘降温设备",1,"水帘风机降温设备","风机功率≥1.1kW；水帘面积≥4m²","非通用类",500]
["农田基本建设机械","平地机械（限与拖拉机配套）","平地机",1,"2—3m激光（卫星）平地机","2m≤工作幅宽＜3m","非通用类",8600]
[{"$nulls":3},2,"3m及以上激光（卫星）平地机","工作幅宽≥3m","非通用类",10400]