{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet2"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet2","index":0,"n_rows":139,"n_cols":9,"rows_kept":139,"merged":[[1,0,1,8],[80,8,84,8],[85,8,86,8]]}
["附件"]
["河南省2021-2023年农机购置补贴机具补贴额一览表（第三批）"]
["序号","大类","小类","品目","档次名称","基本配置和参数","类型","中央财政补贴额（元）","备注"]
[1,"耕整地机械","整地机械","耙（限圆盘耙、驱动耙）","3m及以上驱动耙","作业幅宽≥3m","非通用类",3700]
[2,"耕整地机械","整地机械","筑埂机","筑埂高度25cm及以上筑埂机","筑埂高度≥25cm；配套动力功率≥36.7kW","非通用类",1000]
[3,"耕整地机械","整地机械","铺膜机","60-120cm普通铺膜机","60cm≤作业幅宽＜120cm","非通用类",260]
[4,"耕整地机械","整地机械","铺膜机","120cm及以上普通铺膜机","作业幅宽≥120cm","非通用类",300]
[5,"耕整地机械","整地机械","铺膜机","1m及以上起垄铺膜机","作业幅宽≥1m；带起垄、施肥、膜面覆土等作业功能","非通用类",1000]
[6,"耕整地机械","整地机械","铺膜机","1m及以上旋耕起垄铺膜机","作业幅宽≥1m；带旋耕、起垄、施肥、膜面覆土等作业功能","非通用类",1500]
[7,"耕整地机械","耕整地联合作业机械（可含施肥功能）","联合整地机","2.5m及以上联合整地机","作业幅宽≥2.5m","非通用类",2100]
[8,"耕整地机械","耕整地联合作业机械（可含施肥功能）","深松整地联合作业机","1.5m以下深松整地联合作业机","作业幅宽＜1.5m","非通用类",370]
[9,"耕整地机械","耕整地联合作业机械（可含施肥功能）","深松整地联合作业机","1.5-2m深松整地联合作业机","1.5m≤作业幅宽＜2m","非通用类",680]
[10,"耕整地机械","耕整地联合作业机械（可含施肥功能）","深松整地联合作业机","2-2.5m深松整地联合作业机","2m≤作业幅宽＜2.5m","非通用类",1400]
[11,"耕整地机械","耕整地联合作业机械（可含施肥功能）","深松整地联合作业机","2.5m及以上深松整地联合作业机","作业幅宽≥2.5m","非通用类",2400]
[12,"种植施肥机械","种子播前处理和育苗机械设备","种子催芽机","生产率20kg/h及以上箱体式自动温控水稻种子催芽机","箱体式；自动温控喷淋装置；催芽生产率≥20kg/h","非通用类",500]
[13,"种植施肥机械","种子播前处理和育苗机械设备","苗床用土粉碎机","生产率4t/h及以上苗床用土粉碎机","额定（标定）功率≥3kW；纯工作小时生产率≥4t/h；含电机、粉碎装置、清选装置","非通用类",600]
[14,"种植施肥机械","耕整地播种作业机械（可含施肥功能）","铺膜（带）播种机","2行铺膜播种机","作业行数2行","非通用类",960]
[15,"种植施肥机械","耕整地播种作业机械（可含施肥功能）","铺膜（带）播种机","3-5行铺膜播种机","3行≤作业行数≤5行","非通用类",1400]
[16,"种植施肥机械","耕整地播种作业机械（可含施肥功能）","铺膜（带）播种机","6行及以上铺膜播种机","作业行数≥6行","非通用类",1600]
[17,"种植施肥机械","施肥机械","施肥机","配套动力14.7kW及以上施肥机","配套动力≥14.7kW","非通用类",270]
[18,"种植施肥机械","施肥机械","撒（抛）肥机","0.2-0.5m³悬挂式固态肥抛撒机","0.2m³≤料厢(肥箱)容积＜0.5m³；抛撒宽度≥5m","非通用类",180]
[19,"种植施肥机械","施肥机械","撒（抛）肥机","0.5-1m³悬挂式固态肥抛撒机","0.5m³≤料厢(肥箱)容积＜1m³；抛撒宽度≥5m","非通用类",450]
[20,"种植施肥机械","施肥机械","撒（抛）肥机","1m³及以上悬挂式固态肥抛撒机","料厢(肥箱)容积≥1m³；抛撒宽度≥5m","非通用类",900]
[21,"种植施肥机械","施肥机械","撒（抛）肥机","2-5m³固态肥抛撒机","2m³≤料厢容积＜5m³；抛撒宽度≥4m；承重车桥数量≥1；具有肥料输送功能；非自走式","非通用类",5000]
[22,"种植施肥机械","施肥机械","撒（抛）肥机","5-8m³固态肥抛撒机","5m³≤料厢容积＜8m³；抛撒宽度≥4m；承重车桥数量≥1；具有肥料输送功能；非自走式","非通用类",7000]
[23,"种植施肥机械","施肥机械","撒（抛）肥机","8-10m³固态肥抛撒机","8m³≤料厢容积＜10m³；抛撒宽度≥4m；承重车桥数量≥1；具有肥料输送功能；非自走式","非通用类",9000]
[24,"种植施肥机械","施肥机械","撒（抛）肥机","10-15m³固态肥抛撒机","10m³≤料厢容积＜15m³；抛撒宽度≥4m；承重车桥数量≥1；具有肥料输送功能；非自走式","非通用类",11000]
[25,"种植施肥机械","施肥机械","撒（抛）肥机","15m³及以上固态肥抛撒机","料厢容积≥15m³；抛撒宽度≥4m；承重车桥数量≥1；具有肥料输送功能；非自走式","非通用类",16000]
[26,"种植施肥机械","施肥机械","撒（抛）肥机","5-10m³液态肥撒施机","5m³≤罐体容积＜10m³；承重车桥数量≥1；作业方式为表面施、浅施或深施时，施肥行数≥10行或作业方式为喷洒时；喷洒幅宽≥6m；非自走式","非通用类",20000]
[27,"种植施肥机械","施肥机械","撒（抛）肥机","10-15m³液态肥撒施机","10m³≤罐体容积＜15m³；承重车桥数量≥1；作业方式为表面施、浅施或深施时，施肥行数≥10行或作业方式为喷洒时；喷洒幅宽≥6m；非自走式","非通用类",33000]
[28,"种植施肥机械","施肥机械","撒（抛）肥机","15m³及以上液态肥撒施机","罐体容积≥15m³；承重车桥数量≥2；作业方式为表面施或浅施时，施肥行数≥10行或作业方式为喷洒时；喷洒幅宽≥6m；非自走式","非通用类",45000]
[29,"种植施肥机械","施肥机械","撒（抛）肥机","15m³及以上液态肥深施撒施机","罐体容积≥15m³；承重车桥数量≥2；作业方式：深施；施肥行数≥20行；施肥幅宽≥7m；非自走式","非通用类",50000]
[30,"田间管理机械","修剪防护管理机械","修剪机","最大剪切直径25mm及以上电动手持式果树修剪机","锂电池2组；每组电池容量≥2Ah；额定电压≥16.8V；最大剪切直径≥25mm；电动手持式","非通用类",150]
[31,"田间管理机械","修剪防护管理机械","修剪机","最大剪切直径30mm及以上电动背负式果树修剪机","锂电池；电池容量≥4Ah；额定电压≥16.8V；最大剪切直径≥30mm；电动背负式","非通用类",200]
[32,"田间管理机械","修剪防护管理机械","枝条切碎机","最大切碎直径5cm及以上枝条切碎机","配套动力（功率）≥4.7kW；最大切碎直径≥5cm","非通用类",600]
[33,"田间管理机械","修剪防护管理机械","枝条切碎机","最大切碎直径7.5cm及以上枝条切碎机","配套动力（功率）≥7.35kW；最大切碎直径≥7.5cm","非通用类",800]
[34,"田间管理机械","修剪防护管理机械","埋藤机","60cm及以上埋藤机","工作幅宽≥60cm","非通用类",1800]
[35,"田间管理机械","修剪防护管理机械","农用升降作业平台","举升负载量250kg及以上自走式果园作业平台","结构型式：自走式；升降机构类型：液压剪叉式或液压导轨式；举升负载量≥250kg；最小离地间隙≥110mm；配套动力≥3kW","非通用类",4000,"不含三轮底盘"]
[36,"收获机械","粮食作物收获机械","割晒机","1m及以上悬挂式或牵引式割晒机","悬挂式或牵引式；工作幅宽≥1m","非通用类",330]
[37,"收获机械","粮食作物收获机械","玉米剥皮机","2对辊及以上玉米剥皮机","剥皮辊数量（对）≥2","非通用类",200]
[38,"收获机械","棉麻作物收获机械","棉花收获机","3行及以上自走式棉花收获机","作业行数≥3行；自走式","非通用类",285000]
[39,"收获机械","油料作物收获机械","花生收获机","配套电动机功率22kW及以上复式花生摘果机","配套电动机总功率≥22kW；结构型式：复式；摘果滚筒数量≥2个；带电机","非通用类",3000]
[40,"收获机械","果菜茶烟草药收获机械","果类收获机","2000mm及以上自走式辣椒收获机","工作幅宽≥2000mm；自走式","非通用类",6600]
[41,"设施种植机械","食用菌生产设备","菌料灭菌设备","10-30m³食用菌培养基蒸汽灭菌设备","蒸汽灭菌；10m³≤有效容积＜30m³","非通用类",8000]
[42,"设施种植机械","食用菌生产设备","菌料灭菌设备","30-50m³食用菌培养基蒸汽灭菌设备","蒸汽灭菌；30m³≤有效容积＜50m³","非通用类",15000]
[43,"设施种植机械","食用菌生产设备","菌料灭菌设备","50m³及以上食用菌培养基蒸汽灭菌设备","蒸汽灭菌；有效容积≥50m³","非通用类",20000]
[44,"设施种植机械","食用菌生产设备","菌料装瓶（袋）机","手动供瓶（套袋）菌料装瓶（袋）机","手动供瓶（套袋）","非通用类",400]
[45,"设施种植机械","食用菌生产设备","菌料装瓶（袋）机","生产率700瓶（袋）/h及以上自动供瓶（套袋）菌料装瓶（袋）机","自动供瓶（套袋）；生产率≥700瓶（袋）/h","非通用类",2800]
[46,"设施种植机械","食用菌生产设备","菌料装瓶（袋）机","生产率600瓶（袋）/h及以上自动供瓶（套袋）、封口菌料装瓶（袋）机","自动供瓶（套袋）、封口；生产率≥600瓶（袋）/h","非通用类",5000]
[47,"种植业废弃物处理设备","农田废弃物收集设备","残膜回收机","1-2m扒齿搂膜式残膜回收机","扒齿搂膜式；1m≤工作幅宽＜2m","非通用类",400]
[48,"种植业废弃物处理设备","农田废弃物收集设备","残膜回收机","2-3m扒齿搂膜式残膜回收机","扒齿搂膜式；2m≤工作幅宽＜3m","非通用类",600]
[49,"种植业废弃物处理设备","农田废弃物收集设备","残膜回收机","3m及以上扒齿搂膜式残膜回收机","扒齿搂膜式；工作幅宽≥3m","非通用类",800]
[50,"种植业废弃物处理设备","农田废弃物收集设备","残膜回收机","1.2-1.8m带膜杂分离机构、残膜收集机构残膜回收机","1.2m≤工作幅宽＜1.8m；带膜杂分离机构、残膜收集机构","非通用类",10000]
[51,"种植业废弃物处理设备","农田废弃物收集设备","残膜回收机","1.8m及以上带膜杂分离机构、残膜收集机构残膜回收机","工作幅宽≥1.8m；带膜杂分离机构、残膜收集机构","非通用类",12500]
[52,"种植业废弃物处理设备","农作物废弃物处理设备","生物质气化设备","50-100kW沼气发电机组","50kW≤额定功率＜100kW；气缸数≥4","非通用类",22000]
[53,"种植业废弃物处理设备","农作物废弃物处理设备","生物质气化设备","100-150kW沼气发电机组","100kW≤额定功率＜150kW；气缸数≥6","非通用类",30000]
[54,"种植业废弃物处理设备","农作物废弃物处理设备","生物质气化设备","150-200kW沼气发电机组","150kW≤额定功率＜200kW；气缸数≥8","非通用类",38000]
[55,"种植业废弃物处理设备","农作物废弃物处理设备","生物质气化设备","200kW及以上沼气发电机组","额定功率≥200kW；气缸数≥12","非通用类",46000]
[56,"饲料（草）收获加工运输设备","饲料（草）加工机械","青贮切碎机","1-3t/h青贮切碎机","1t/h≤生产率＜3t/h","非通用类",100]
[57,"饲料（草）收获加工运输设备","饲料（草）加工机械","青贮切碎机","3-6t/h青贮切碎机","3t/h≤生产率＜6t/h","非通用类",300]
[58,"饲料（草）收获加工运输设备","饲料（草）加工机械","青贮切碎机","6-9t/h青贮切碎机","6t/h≤生产率＜9t/h","非通用类",400]
[59,"饲料（草）收获加工运输设备","饲料（草）加工机械","青贮切碎机","9-15t/h青贮切碎机","9t/h≤生产率＜15t/h","非通用类",500]
[60,"饲料（草）收获加工运输设备","饲料（草）加工机械","青贮切碎机","15-20t/h青贮切碎机","15t/h≤生产率＜20t/h","非通用类",800]
[61,"饲料（草）收获加工运输设备","饲料（草）加工机械","青贮切碎机","20t/h及以上青贮切碎机","生产率≥20t/h","非通用类",1200]
[62,"饲料（草）收获加工运输设备","饲料（草）加工机械","饲料混合机","1-2m³立式饲料混合机","1m³≤混合室容积＜2m³；立式","非通用类",600]
[63,"饲料（草）收获加工运输设备","饲料（草）加工机械","饲料混合机","2m³及以上立式饲料混合机","混合室容积≥2m³；立式","非通用类",800]
[64,"饲料（草）收获加工运输设备","饲料（草）加工机械","饲料混合机","1-2m³卧式（单轴）饲料混合机","1m³≤混合室容积＜2m³；卧式；单轴","非通用类",1100]
[65,"饲料（草）收获加工运输设备","饲料（草）加工机械","饲料混合机","2m³及以上卧式（单轴）饲料混合机","混合室容积≥2m³；卧式；单轴","非通用类",2500]
[66,"饲料（草）收获加工运输设备","饲料（草）加工机械","饲料混合机","1-2m³卧式（双轴）饲料混合机","1m³≤混合室容积＜2m³；卧式；双轴","非通用类",4000]
[67,"饲料（草）收获加工运输设备","饲料（草）加工机械","饲料混合机","2m³及以上卧式（双轴）饲料混合机","混合室容积≥2m³；卧式；双轴","非通用类",5000]
[68,"饲料（草）收获加工运输设备","饲料（草）加工机械","饲料膨化机","500kg/h以下秸秆膨化机","秸秆膨化率≥95%；作业小时生产率＜500kg/h","非通用类",450]
[69,"饲料（草）收获加工运输设备","饲料（草）加工机械","饲料膨化机","500kg/h及以上秸秆膨化机","秸秆膨化率≥95%；作业小时生产率≥500kg/h","非通用类",600]
[70,"畜禽养殖机械","饲养设备","喂（送）料机","20-50m输送带式喂料机","输送带式；20m≤输送带有效长度＜50m；含电机、驱动滚筒","非通用类",500]
[71,"畜禽养殖机械","饲养设备","喂（送）料机","50m及以上输送带式喂料机","输送带式；输送带有效长度≥50m；含电机、驱动滚筒","非通用类",800]
[72,"畜禽养殖机械","饲养设备","喂（送）料机","直径36mm及以上螺旋弹簧式喂（送）料机","螺旋弹簧式；螺旋弹簧直径≥36mm；输送料管长度≥50m；含电机、料斗、驱动装置、控制装置","非通用类",2000]
[73,"畜禽养殖机械","饲养设备","喂（送）料机","60m及以上行车式喂料机","行车式；行车行程≥60m；喂料层数≥3层；含电机、料斗、驱动装置、控制装置","非通用类",2500]
[74,"畜禽产品采集储运设备","畜禽产品采集设备","剪毛机","软轴式剪羊毛机","传动形式：软轴式；功率≥0.25kW","非通用类",200]
[75,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","清粪机","0.75kW及以上刮板式清粪机","刮板式；电机额定功率≥0.75kW；刮粪板数量≥1；工作幅宽（刮板宽度）≥1m","非通用类",650]
[76,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","清粪机","1.5kW及以上刮板式清粪机","刮板式；电机额定功率≥1.5kW；刮粪板数量≥2；工作幅宽（刮板宽度）≥1m","非通用类",900]
[77,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","清粪机","1.5kW及以上不锈钢刮板式清粪机","不锈钢刮板式；电机额定功率≥1.5kW；刮粪板数量≥2；工作幅宽（刮板宽度）≥1m","非通用类",1300]
[78,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","清粪机","90-200m²输送带式清粪机","输送带式；90m²≤输送带面积＜200m²","非通用类",2000,"输送带面积=粪带宽度×辊筒上方粪带长度×粪带层数"]
[79,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","清粪机","200-300m²输送带式清粪机","输送带式；200m²≤输送带面积＜300m²","非通用类",3300]
[80,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","清粪机","300-400m²输送带式清粪机","输送带式；300m²≤输送带面积＜400m²","非通用类",4400]
[81,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","清粪机","400-500m²输送带式清粪机","输送带式；400m²≤输送带面积＜500m²","非通用类",5500]
[82,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","清粪机","500m²及以上输送带式清粪机","输送带式；输送带面积≥500m²","非通用类",6600]
[83,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","畜禽粪污固液分离机","筛筒面积0.2-0.5m²粪污固液分离机","0.2m²≤筛筒面积＜0.5m²；结构型式：螺旋挤压式","非通用类",1700,"筛筒面积=3.14×筛筒直径×筛筒长度"]
[84,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","畜禽粪污固液分离机","筛筒面积0.5m²及以上粪污固液分离机","筛筒面积≥0.5m²；结构型式：螺旋挤压式","非通用类",2200]
[85,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","畜禽粪污固液分离机","斜筛面积0.35-0.8m²粪污固液分离机","0.35m²≤斜筛面积＜0.8m²；结构型式：筛分（斜筛）+螺旋挤压式","非通用类",3000]
[86,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","畜禽粪污固液分离机","斜筛面积0.8m²及以上粪污固液分离机","斜筛面积≥0.8m²；结构型式：筛分（斜筛）+螺旋挤压式；配备振动电机","非通用类",3800]
[87,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","畜禽粪便翻堆设备","1.5-3m电动有机废弃物好氧发酵翻堆机","1.5m≤工作幅宽＜3m；配套动力型式：电动机；配套总功率≥7kW","非通用类",2100]
[88,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","畜禽粪便翻堆设备","3-4m电动有机废弃物好氧发酵翻堆机","3m≤工作幅宽＜4m；配套动力型式：电动机；配套总功率≥10kW","非通用类",3100]
[89,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","畜禽粪便翻堆设备","4m及以上电动有机废弃物好氧发酵翻堆机","工作幅宽≥4m；配套动力型式：电动机；配套总功率≥12kW","非通用类",4000]
[90,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","畜禽粪便翻堆设备","翻堆高度（深度）1.5m及以上电动有机废弃物好氧发酵翻堆机","工作幅宽≥0.9m；配套动力型式：电动机；配套总功率≥23kW；物料最大堆放高度（深度）≥1.5m","非通用类",5000]
[91,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","畜禽粪便翻堆设备","2-2.5m油动有机废弃物好氧发酵翻堆机","2m≤工作幅宽＜2.5m；配套动力型式：柴油机；配套总功率≥22.1kW","非通用类",8000]
[92,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","畜禽粪便翻堆设备","2.5-3m油动有机废弃物好氧发酵翻堆机","2.5m≤工作幅宽＜3m；配套动力型式：柴油机；配套总功率≥51.5kW","非通用类",15000]
[93,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","畜禽粪便翻堆设备","3m及以上油动有机废弃物好氧发酵翻堆机","工作幅宽≥3m；配套动力型式：柴油机；配套总功率≥73.5kW","非通用类",22000]
[94,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","沼液沼渣抽排设备","1.5kW及以上沼渣沼液抽排机","具有切碎切割机构；额定功率≥1.5kW","非通用类",200]
[95,"畜禽养殖废弃物及病死畜禽处理设备","病死畜禽储运及处理设备","病死畜禽处理设备","0.5-1m³降解式病死畜禽无害化处理","降解法；0.5m³≤箱体容积＜1m³","非通用类",2000]
[96,"畜禽养殖废弃物及病死畜禽处理设备","病死畜禽储运及处理设备","病死畜禽处理设备","1-2m³降解式病死畜禽无害化处理","降解法；1m³≤箱体容积＜2m³","非通用类",4000]
[97,"畜禽养殖废弃物及病死畜禽处理设备","病死畜禽储运及处理设备","病死畜禽处理设备","2-3m³降解式病死畜禽无害化处理设备","降解法；2m³≤箱体容积＜3m³","非通用类",6000]
[98,"畜禽养殖废弃物及病死畜禽处理设备","病死畜禽储运及处理设备","病死畜禽处理设备","3m³及以上降解式病死畜禽无害化处理设备","降解法；箱体容积≥3m³","非通用类",12000]
[99,"畜禽养殖废弃物及病死畜禽处理设备","病死畜禽储运及处理设备","病死畜禽处理设备","0.9-2m³干化式病死畜禽无害化处理设备","干化法；0.9m³≤箱体容积＜2m³；工作压力≥200kPa（属于压力容器）","非通用类",18000]
[100,"畜禽养殖废弃物及病死畜禽处理设备","病死畜禽储运及处理设备","病死畜禽处理设备","2-4m³干化式病死畜禽无害化处理设备","干化法；2m³≤箱体容积＜4m³；工作压力≥200kPa（属于压力容器）","非通用类",31000]
[101,"畜禽养殖废弃物及病死畜禽处理设备","病死畜禽储运及处理设备","病死畜禽处理设备","4m³及以上干化式病死畜禽无害化处理设备","干化法；箱体容积≥4m³；工作压力≥200kPa（属于压力容器）","非通用类",41000]
[102,"水产养殖机械","投饲机械","投（饲）饵机","1.5kW及以上风送式投（饲）饵机","结构型式：风送式；风机功率（空气压缩机功率）≥1.5kW；料箱容量≥300kg；最大投（饲）饵能力≥300kg/h","非通用类",900]
[103,"种子初加工机械","种子初加工机械","种子清选机","生产率1.5-3t/h种子清选机","1.5t/h≤纯工作小时生产率＜3t/h","非通用类",1000]
[104,"种子初加工机械","种子初加工机械","种子清选机","生产率3-5t/h种子清选机","3t/h≤纯工作小时生产率＜5t/h","非通用类",1800]
[105,"种子初加工机械","种子初加工机械","种子清选机","生产率5-15t/h种子清选机","5t/h≤纯工作小时生产率＜15t/h","非通用类",3400]
[106,"种子初加工机械","种子初加工机械","种子清选机","生产率15-25t/h种子清选机","15t/h≤纯工作小时生产率＜25t/h","非通用类",5000]
[107,"种子初加工机械","种子初加工机械","种子清选机","生产率25t/h及以上种子清选机","纯工作小时生产率≥25t/h","非通用类",7000]
[108,"粮油糖初加工机械","粮食初加工机械","粮食清选机","生产率3-5t/h粮食清选机","3t/h≤纯工作小时生产率＜5t/h","非通用类",1500]
[109,"粮油糖初加工机械","粮食初加工机械","粮食清选机","生产率5-15t/h粮食清选机","5t/h≤纯工作小时生产率＜15t/h","非通用类",2000]
[110,"粮油糖初加工机械","粮食初加工机械","粮食清选机","生产率15-25t/h粮食清选机","15t/h≤纯工作小时生产率＜25t/h","非通用类",4500]
[111,"粮油糖初加工机械","粮食初加工机械","粮食清选机","生产率25t/h及以上粮食清选机","纯工作小时生产率≥25t/h","非通用类",6000]
[112,"粮油糖初加工机械","粮食初加工机械","磨浆机","1.1kW及以上磨浆机","配套功率≥1.1kW；含电机、支架","非通用类",90]
[113,"果菜茶初加工机械","果蔬初加工机械","果蔬分级机","生产率3t/h及以上机械式水果分级机","机械式水果分级；纯工作小时生产率≥3t/h","非通用类",1400]
[114,"果菜茶初加工机械","果蔬初加工机械","果蔬分级机","生产率1-3t/h电子式水果分级机","电子式水果分级；分选等级≥8个；1t/h≤纯工作小时生产率＜3t/h","非通用类",18000]
[115,"果菜茶初加工机械","果蔬初加工机械","果蔬分级机","生产率3t/h及以上电子式水果分级机","电子式水果分级；分选等级≥8个；纯工作小时生产率≥3t/h","非通用类",21000]
[116,"果菜茶初加工机械","果蔬初加工机械","果蔬清洗机","生产率1-2.5t/h水果清洗机","1t/h≤纯工作小时生产率＜2.5t/h","非通用类",1200]
[117,"果菜茶初加工机械","果蔬初加工机械","果蔬清洗机","生产率2.5-5t/h水果清洗机","2.5t/h≤纯工作小时生产率＜5t/h","非通用类",3600]
[118,"果菜茶初加工机械","果蔬初加工机械","果蔬清洗机","生产率5t/h及以上水果清洗机","纯工作小时生产率≥5t/h","非通用类",6000]
[119,"果菜茶初加工机械","果蔬初加工机械","果蔬清洗机","生产率1000-5000kg/h蔬菜清洗机","1000kg/h≤纯工作小时生产率＜5000kg/h","非通用类",2000]
[120,"果菜茶初加工机械","果蔬初加工机械","果蔬清洗机","生产率5000kg/h及以上蔬菜清洗机","纯工作小时生产率≥5000kg/h","非通用类",3500]
[121,"果菜茶初加工机械","果蔬初加工机械","水果打蜡机","生产率1-2t/h水果清洗打蜡机","1t/h≤纯工作小时生产率＜2t/h；含提升机构","非通用类",4200]
[122,"果菜茶初加工机械","果蔬初加工机械","水果打蜡机","生产率2-3t/h水果清洗打蜡机","2t/h≤纯工作小时生产率＜3t/h；含提升机构","非通用类",6000]
[123,"果菜茶初加工机械","果蔬初加工机械","水果打蜡机","生产率3t/h及以上水果清洗打蜡机","纯工作小时生产率≥3t/h；含提升机构","非通用类",8000]
[124,"果菜茶初加工机械","果蔬初加工机械","果蔬干燥机","容积5m³以下果蔬烘干机","有效烘干容积(容积)＜5m³","非通用类",640]
[125,"果菜茶初加工机械","果蔬初加工机械","脱蓬（脯）机","生产率200kg/h及以上板栗脱蓬机","生产率≥200kg/h；含电机","非通用类",240]
[126,"果菜茶初加工机械","果蔬初加工机械","青果（豆）脱壳机","生产率30kg/h及以上莲子剥壳去皮一体机","纯工作小时生产率≥30kg/h；配套电机额定功率≥2kW；含剥壳、去皮功能","非通用类",4700]
[127,"农用搬运机械","农用运输机械","果园轨道运输机","自走式平地轨道运输机","包含驱动传动装置、载物货厢、轨道。驱动型式：自走式；配套动力类型：汽油机、柴油机或电动机（动力为电动机时；功率≥0.35kW；电池容量≥20A·h）；结构型式：双向；轨道长度≥50米；轨道型式：齿条式、平面导轨式、打孔式、其他式；额定装载质量≥200kg；轨道材料型号：Q235（镀锌）碳素结构钢、ML04Al冷镦钢或45号中碳钢；轨道壁厚≥2.3mm","非通用类","1000元+10元/米（轨道长度）","按成套设备补贴，单台套补贴上限1万元。轨道长度去尾取整。安装、验收完成后补贴。"]
[128,"农用搬运机械","农用运输机械","果园轨道运输机","自走式山地轨道运输机","包含驱动传动装置、载物货厢、轨道。驱动型式：自走式；配套动力类型：汽油机、柴油机或电动机（动力为电动机时；功率≥2.2kW；电池容量≥40A·h）；最大爬坡度≥35°；结构型式：双向；轨道长度≥100米；轨道型式：齿条式、打孔式；额定装载质量≥200kg；轨道材料型号：Q235（镀锌）碳素结构钢；轨道壁厚≥2.5mm","非通用类","3000元+30元/米（轨道长度）","按成套设备补贴，单台套补贴上限3万元。轨道长度去尾取整。安装、验收完成后补贴。"]
[129,"农用搬运机械","农用运输机械","果园轨道运输机","牵引式山地轨道运输机","包含牵引传动装置、载物货厢、轨道。驱动型式：牵引式；配套动力类型：电动机；功率≥3kW；最大爬坡度≥35°；轨道长度≥100米；轨道型式：平面导轨式；额定装载质量≥200kg；轨道材料型号：Q235（镀锌）碳素结构钢；单轨轨道壁厚≥2.5mm、双轨轨道壁厚≥1.5mm","非通用类","2000元+30元/米（轨道长度）","按成套设备补贴，单台套补贴上限3万元。轨道长度去尾取整。安装、验收完成后补贴。"]
[130,"农用水泵","农用水泵","潜水电泵","37kW及以上潜水电泵","电机功率≥37kW","非通用类",1600]
[131,"农用水泵","农用水泵","地面泵（机组）","55kW及以上离心泵","配套功率≥55kW；含机座、底阀","非通用类",1500]
[132,"设施环境控制设备","设施环境控制设备","加温设备","0.1-0.2MW生物质热风炉","0.1MW≤热功率＜0.2MW；燃料种类：生物质","非通用类",2000]
[133,"设施环境控制设备","设施环境控制设备","加温设备","0.2-0.3MW生物质热风炉","0.2MW≤热功率＜0.3MW；燃料种类：生物质","非通用类",4000]
[134,"设施环境控制设备","设施环境控制设备","加温设备","0.3-0.5MW生物质热风炉","0.3MW≤热功率＜0.5MW；燃料种类：生物质","非通用类",9000]
[135,"设施环境控制设备","设施环境控制设备","加温设备","0.5-0.9MW生物质热风炉","0.5MW≤热功率＜0.9MW；燃料种类：生物质","非通用类",14000]
[136,"设施环境控制设备","设施环境控制设备","加温设备","0.9MW及以上生物质热风炉","热功率≥0.9MW；燃料种类：生物质","非通用类",18000]